__constant char *DTV_BLITTER_ALU = (char *) 54078
__constant char * const DTV_BLITTER_CONTROL = (char *) 54074
__constant char * const DTV_BLITTER_CONTROL2 = (char *) 54079
__constant char * const DTV_BLITTER_DEST_HI = (char *) 54066
__constant char * const DTV_BLITTER_DEST_LIN_HI = (char *) 54070
__constant char * const DTV_BLITTER_DEST_LIN_LO = (char *) 54069
__constant char * const DTV_BLITTER_DEST_LO = (char *) 54064
__constant char * const DTV_BLITTER_DEST_MI = (char *) 54065
__constant char * const DTV_BLITTER_DEST_MOD_HI = (char *) 54068
__constant char * const DTV_BLITTER_DEST_MOD_LO = (char *) 54067
__constant char * const DTV_BLITTER_DEST_STEP = (char *) 54071
__constant char * const DTV_BLITTER_LEN_HI = (char *) 54073
__constant char * const DTV_BLITTER_LEN_LO = (char *) 54072
__constant char * const DTV_BLITTER_SRCA_HI = (char *) 54050
__constant char * const DTV_BLITTER_SRCA_LIN_HI = (char *) 54054
__constant char * const DTV_BLITTER_SRCA_LIN_LO = (char *) 54053
__constant char * const DTV_BLITTER_SRCA_LO = (char *) 54048
__constant char * const DTV_BLITTER_SRCA_MI = (char *) 54049
__constant char * const DTV_BLITTER_SRCA_MOD_HI = (char *) 54052
__constant char * const DTV_BLITTER_SRCA_MOD_LO = (char *) 54051
__constant char * const DTV_BLITTER_SRCA_STEP = (char *) 54055
__constant char * const DTV_BLITTER_SRCB_HI = (char *) 54058
__constant char * const DTV_BLITTER_SRCB_LIN_HI = (char *) 54062
__constant char * const DTV_BLITTER_SRCB_LIN_LO = (char *) 54061
__constant char * const DTV_BLITTER_SRCB_LO = (char *) 54056
__constant char * const DTV_BLITTER_SRCB_MI = (char *) 54057
__constant char * const DTV_BLITTER_SRCB_MOD_HI = (char *) 54060
__constant char * const DTV_BLITTER_SRCB_MOD_LO = (char *) 54059
__constant char * const DTV_BLITTER_SRCB_STEP = (char *) 54063
__constant char * const DTV_BLITTER_TRANSPARANCY = (char *) 54075
__constant const char DTV_BLIT_ADD = $30
__constant const char DTV_BLIT_CLEAR_IRQ = 1
__constant const char DTV_BLIT_DEST_CONT = 8
__constant const char DTV_BLIT_DEST_FWD = 8
__constant const char DTV_BLIT_FORCE_START = 1
__constant const char DTV_BLIT_SRCA_FWD = 2
__constant const char DTV_BLIT_SRCB_FWD = 4
__constant const char DTV_BLIT_STATUS_BUSY = 1
__constant const char DTV_BLIT_TRANSPARANCY_NONE = 0
__constant char * const DTV_FEATURE = (char *) 53311
__constant const char DTV_FEATURE_ENABLE = 1
__constant char * const SCREEN = (char *) 1024
__constant const char SRCA[] = { 'c', 'a', 'm', 'e', 'l', 'o', 't', '!', ' ' }
__constant const char SRCA_LEN = 9
__constant const char SRCB[] = { $80 }
void main()
char main::$0 // reg byte a 202.0
char main::r
char main::r#1 // reg byte x 16.5
char main::r#2 // reg byte x 56.0

reg byte x [ main::r#2 main::r#1 ]
reg byte a [ main::$0 ]
