__constant char * const BORDER_COLOR = (char *) 53280
__constant char * const CHUNKY = (char *) 32768
__constant struct MOS6526_CIA * const CIA2 = (struct MOS6526_CIA *) 56576
__constant const char DTV_BADLINE_OFF = $20
__constant const char DTV_CHUNKY = $40
__constant const char DTV_COLORRAM_OFF = $10
__constant char * const DTV_CONTROL = (char *) 53308
__constant char * const DTV_FEATURE = (char *) 53311
__constant const char DTV_FEATURE_ENABLE = 1
__constant const char DTV_HIGHCOLOR = 4
__constant const char DTV_LINEAR = 1
__constant char * const DTV_PALETTE = (char *) 53760
__constant char * const DTV_PLANEB_MODULO_HI = (char *) 53320
__constant char * const DTV_PLANEB_MODULO_LO = (char *) 53319
__constant char * const DTV_PLANEB_START_HI = (char *) 53323
__constant char * const DTV_PLANEB_START_LO = (char *) 53321
__constant char * const DTV_PLANEB_START_MI = (char *) 53322
__constant char * const DTV_PLANEB_STEP = (char *) 53324
__constant char OFFSET_STRUCT_MOS6526_CIA_PORT_A_DDR = 2
__constant char * const PROCPORT = (char *) 1
__constant char * const PROCPORT_DDR = (char *) 0
__constant const char PROCPORT_DDR_MEMORY_MASK = 7
__constant const char PROCPORT_RAM_IO = 5
__constant char * const RASTER = (char *) 53266
__constant char * const VICII_CONTROL1 = (char *) 53265
__constant char * const VICII_CONTROL2 = (char *) 53270
__constant const char VICII_CSEL = 8
__constant const char VICII_DEN = $10
__constant const char VICII_ECM = $40
__constant const char VICII_MCM = $10
__constant char * const VICII_MEMORY = (char *) 53272
__constant const char VICII_RSEL = 8
void dtvSetCpuBankSegment1(char cpuBankIdx)
__constant char *dtvSetCpuBankSegment1::cpuBank = (char *) 255
char dtvSetCpuBankSegment1::cpuBankIdx
char dtvSetCpuBankSegment1::cpuBankIdx#1 // reg byte a 2002.0
char dtvSetCpuBankSegment1::cpuBankIdx#3 // reg byte a 11002.0
void gfx_init_chunky()
unsigned int gfx_init_chunky::$5 // zp[2]:6 1001.0
char gfx_init_chunky::c
char gfx_init_chunky::c#0 // reg byte a 2002.0
char *gfx_init_chunky::gfxb
char *gfx_init_chunky::gfxb#1 // gfxb zp[2]:2 420.59999999999997
char *gfx_init_chunky::gfxb#3 // gfxb zp[2]:2 1552.0
char *gfx_init_chunky::gfxb#4 // gfxb zp[2]:2 750.75
char *gfx_init_chunky::gfxb#5 // gfxb zp[2]:2 202.0
char gfx_init_chunky::gfxbCpuBank
char gfx_init_chunky::gfxbCpuBank#2 // reg byte x 2002.0
char gfx_init_chunky::gfxbCpuBank#4 // reg byte x 1026.25
char gfx_init_chunky::gfxbCpuBank#7 // reg byte x 202.0
char gfx_init_chunky::gfxbCpuBank#8 // reg byte x 344.8888888888889
unsigned int gfx_init_chunky::x
unsigned int gfx_init_chunky::x#1 // x zp[2]:4 1501.5
unsigned int gfx_init_chunky::x#2 // x zp[2]:4 300.29999999999995
char gfx_init_chunky::y
char gfx_init_chunky::y#1 // y zp[1]:8 151.5
char gfx_init_chunky::y#6 // y zp[1]:8 92.53846153846155
void main()
char main::$3 // reg byte a 202.0
char main::$4 // reg byte a 202.0
char main::$5 // reg byte a 202.0
char main::j
char main::j#1 // reg byte x 16.5
char main::j#2 // reg byte x 22.0
char main::rst
char main::rst#1 // reg byte x 57.714285714285715

reg byte x [ main::j#2 main::j#1 ]
zp[1]:8 [ gfx_init_chunky::y#6 gfx_init_chunky::y#1 ]
zp[2]:4 [ gfx_init_chunky::x#2 gfx_init_chunky::x#1 ]
reg byte x [ gfx_init_chunky::gfxbCpuBank#4 gfx_init_chunky::gfxbCpuBank#7 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::gfxbCpuBank#2 ]
zp[2]:2 [ gfx_init_chunky::gfxb#4 gfx_init_chunky::gfxb#3 gfx_init_chunky::gfxb#5 gfx_init_chunky::gfxb#1 ]
reg byte a [ dtvSetCpuBankSegment1::cpuBankIdx#3 dtvSetCpuBankSegment1::cpuBankIdx#1 ]
reg byte x [ main::rst#1 ]
reg byte a [ main::$3 ]
reg byte a [ main::$4 ]
reg byte a [ main::$5 ]
zp[2]:6 [ gfx_init_chunky::$5 ]
reg byte a [ gfx_init_chunky::c#0 ]
