(module Oscillators:Oscillator_DIP-14 (layer F.Cu) (tedit 5C2770BD)
  (descr "Oscillator, DIP14, http://cdn-reichelt.de/documents/datenblatt/B400/OSZI.pdf")
  (tags oscillator)
  (fp_text reference X1 (at 7.62 -5.08) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "3.579545 MHz" (at 7.62 -3.175) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 7.62 -5.08) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 18.22 2.79) (end 18.22 -10.41) (layer F.CrtYd) (width 0.05))
  (fp_line (start 18.22 -10.41) (end -2.98 -10.41) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.98 -10.41) (end -2.98 2.79) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.98 2.79) (end 18.22 2.79) (layer F.CrtYd) (width 0.05))
  (fp_line (start 16.97 1.19) (end 16.97 -8.81) (layer F.Fab) (width 0.1))
  (fp_line (start -1.38 -9.16) (end 16.62 -9.16) (layer F.Fab) (width 0.1))
  (fp_line (start -1.73 1.54) (end -1.73 -8.81) (layer F.Fab) (width 0.1))
  (fp_line (start -1.73 1.54) (end 16.62 1.54) (layer F.Fab) (width 0.1))
  (fp_line (start -2.83 -9.51) (end -2.83 2.64) (layer F.SilkS) (width 0.12))
  (fp_line (start 17.32 -10.26) (end -2.08 -10.26) (layer F.SilkS) (width 0.12))
  (fp_line (start 18.07 1.89) (end 18.07 -9.51) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.83 2.64) (end 17.32 2.64) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.73 2.54) (end 17.32 2.54) (layer F.Fab) (width 0.1))
  (fp_line (start 17.97 -9.51) (end 17.97 1.89) (layer F.Fab) (width 0.1))
  (fp_line (start -2.08 -10.16) (end 17.32 -10.16) (layer F.Fab) (width 0.1))
  (fp_line (start -2.73 2.54) (end -2.73 -9.51) (layer F.Fab) (width 0.1))
  (fp_arc (start 16.62 1.19) (end 16.97 1.19) (angle 90) (layer F.Fab) (width 0.1))
  (fp_arc (start 16.62 -8.81) (end 16.62 -9.16) (angle 90) (layer F.Fab) (width 0.1))
  (fp_arc (start -1.38 -8.81) (end -1.73 -8.81) (angle 90) (layer F.Fab) (width 0.1))
  (fp_arc (start 17.32 1.89) (end 18.07 1.89) (angle 90) (layer F.SilkS) (width 0.12))
  (fp_arc (start 17.32 -9.51) (end 17.32 -10.26) (angle 90) (layer F.SilkS) (width 0.12))
  (fp_arc (start -2.08 -9.51) (end -2.83 -9.51) (angle 90) (layer F.SilkS) (width 0.12))
  (fp_arc (start 17.32 1.89) (end 17.97 1.89) (angle 90) (layer F.Fab) (width 0.1))
  (fp_arc (start 17.32 -9.51) (end 17.32 -10.16) (angle 90) (layer F.Fab) (width 0.1))
  (fp_arc (start -2.08 -9.51) (end -2.73 -9.51) (angle 90) (layer F.Fab) (width 0.1))
  (pad 7 thru_hole circle (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 7.62 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 14 thru_hole circle (at 0 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 15.24 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Oscillators.3dshapes/Oscillator_DIP-14.wrl
    (at (xyz 0 0 0))
    (scale (xyz 0.3937 0.3937 0.3937))
    (rotate (xyz 0 0 0))
  )
)
