(module Amplifier (layer F.Cu) (tedit 5C128446)
  (fp_text reference U11 (at 0 1.27) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value VDU_Port (at 0 -1.905) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 16.51 -10.16) (end 16.51 -12.065) (layer F.SilkS) (width 0.15))
  (fp_line (start 16.51 -12.065) (end -20.32 -12.065) (layer F.SilkS) (width 0.15))
  (fp_line (start -20.32 -12.065) (end -20.32 -10.16) (layer F.SilkS) (width 0.15))
  (fp_line (start -16.51 5.715) (end -20.32 5.715) (layer F.SilkS) (width 0.15))
  (fp_line (start -20.32 5.715) (end -20.32 -10.16) (layer F.SilkS) (width 0.15))
  (fp_line (start -14.605 1.27) (end -10.795 1.27) (layer F.SilkS) (width 0.15))
  (fp_line (start -10.795 -1.27) (end -14.605 -1.27) (layer F.SilkS) (width 0.15))
  (fp_line (start -16.51 5.715) (end 16.51 5.715) (layer F.SilkS) (width 0.15))
  (fp_line (start 16.51 5.715) (end 16.51 5.08) (layer F.SilkS) (width 0.15))
  (fp_line (start 16.51 5.08) (end 16.51 -10.16) (layer F.SilkS) (width 0.15))
  (fp_line (start -10.795 1.27) (end -10.16 1.27) (layer F.SilkS) (width 0.15))
  (fp_line (start -10.16 -1.27) (end -10.795 -1.27) (layer F.SilkS) (width 0.15))
  (fp_line (start -10.16 1.27) (end -7.62 3.81) (layer F.SilkS) (width 0.15))
  (fp_line (start -7.62 3.81) (end 0 3.81) (layer F.SilkS) (width 0.15))
  (fp_line (start -10.16 -1.27) (end -7.62 -3.81) (layer F.SilkS) (width 0.15))
  (fp_line (start -7.62 -3.81) (end 0 -3.81) (layer F.SilkS) (width 0.15))
  (fp_line (start 10.16 3.81) (end 9.525 4.445) (layer F.SilkS) (width 0.15))
  (fp_line (start 10.16 3.81) (end 9.525 3.175) (layer F.SilkS) (width 0.15))
  (fp_line (start 10.16 -3.81) (end 9.525 -3.175) (layer F.SilkS) (width 0.15))
  (fp_line (start 10.16 -3.81) (end 9.525 -4.445) (layer F.SilkS) (width 0.15))
  (fp_line (start 10.16 3.81) (end 8.89 3.81) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 3.81) (end 10.16 3.81) (layer F.SilkS) (width 0.15))
  (fp_line (start 10.16 -3.81) (end 0 -3.81) (layer F.SilkS) (width 0.15))
  (fp_text user GND (at 12.7 -1.27) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user GND (at 12.7 1.27) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user AUD (at 12.7 3.81) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user VID (at 12.7 -3.81) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user AUD (at -16.51 1.27) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user VID (at -16.51 -1.27) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user GND (at -16.51 3.81) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user VCC (at -16.51 -3.81) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 thru_hole circle (at -19.05 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -19.05 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at -19.05 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at -19.05 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 15.24 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 15.24 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 15.24 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 15.24 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
)
