(module resonator_awscr (layer F.Cu)
  (descr "Abracon AWSCR SMD Resonator unit")
  (fp_text reference X*** (at 0 -1.69926) (layer F.SilkS)
    (effects (font (size 0.49784 0.49784) (thickness 0.09906)))
  )
  (fp_text value resonator_awscr (at 0 1.89992) (layer F.SilkS)
    (effects (font (size 0.49784 0.49784) (thickness 0.09906)))
  )
  (fp_line (start -1.25 -1) (end -1.25 1) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.25 1) (end 1.25 1) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.25 1) (end 1.25 -1) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.25 -1) (end -1.25 -1) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at -1 0.9) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.06858))
  (pad 3 smd rect (at 1 0.9) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.06858))
  (pad 2 smd rect (at 0 0.9) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 1 -0.9) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0 -0.9) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -1 -0.9) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask))
  (model walter/crystal/resonator_awscr.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
