(module DIP-16_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 5FFA52B8)
  (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
  (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
  (fp_text reference A1 (at 3.81 2.54) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Game_IO (at 3.81 20.11) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 6.35 19.05) (end 6.35 -1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start 8.89 19.05) (end 6.35 19.05) (layer F.SilkS) (width 0.12))
  (fp_line (start 8.89 -1.27) (end 8.89 19.05) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.35 -1.27) (end 8.89 -1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.27 -1.27) (end 1.27 19.05) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.27 -1.27) (end 1.27 -1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start 9.15 -1.6) (end -1.55 -1.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9.15 19.4) (end 9.15 -1.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.55 19.4) (end 9.15 19.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.55 -1.6) (end -1.55 19.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9.06 -1.39) (end -1.44 -1.39) (layer B.SilkS) (width 0.12))
  (fp_line (start 9.06 19.17) (end 9.06 -1.39) (layer B.SilkS) (width 0.12))
  (fp_line (start -1.44 19.17) (end 9.06 19.17) (layer B.SilkS) (width 0.12))
  (fp_line (start -1.44 -1.39) (end -1.44 19.17) (layer B.SilkS) (width 0.12))
  (fp_line (start 6.06 -1.33) (end 4.81 -1.33) (layer B.SilkS) (width 0.12))
  (fp_line (start 6.06 19.11) (end 6.06 -1.33) (layer B.SilkS) (width 0.12))
  (fp_line (start 1.56 19.11) (end 6.06 19.11) (layer B.SilkS) (width 0.12))
  (fp_line (start 1.56 -1.33) (end 1.56 19.11) (layer B.SilkS) (width 0.12))
  (fp_line (start 2.81 -1.33) (end 1.56 -1.33) (layer B.SilkS) (width 0.12))
  (fp_line (start 8.89 -1.33) (end -1.27 -1.33) (layer F.Fab) (width 0.1))
  (fp_line (start 8.89 19.11) (end 8.89 -1.33) (layer F.Fab) (width 0.1))
  (fp_line (start -1.27 19.11) (end 8.89 19.11) (layer F.Fab) (width 0.1))
  (fp_line (start -1.27 -1.33) (end -1.27 19.11) (layer F.Fab) (width 0.1))
  (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
  (fp_line (start 0.635 19.05) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
  (fp_line (start 6.985 19.05) (end 0.635 19.05) (layer F.Fab) (width 0.1))
  (fp_line (start 6.985 -1.27) (end 6.985 19.05) (layer F.Fab) (width 0.1))
  (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
  (fp_arc (start 3.81 -1.33) (end 2.81 -1.33) (angle -180) (layer B.SilkS) (width 0.12))
  (fp_text user %R (at 3.81 2.54) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 1.905 0) (end 2.54 -0.635) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.54 -0.635) (end 2.54 0.635) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.54 0.635) (end 1.905 0) (layer F.SilkS) (width 0.12))
  (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 9 thru_hole oval (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 10 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 11 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 12 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 13 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 14 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 15 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 8 thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 16 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm_Socket.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
