PAD Specification File
***************************

PART TYPE:        LCMXO2-640HC
Performance Grade:      4
PACKAGE:          TQFP100
Package Status:                     Final          Version 1.39

Thu Dec 28 23:23:38 2023

Pinout by Port Name:
+-----------+----------+---------------+-------+-----------+-----------+------------------------------------------------------------+
| Port Name | Pin/Bank | Buffer Type   | Site  | PG Enable | BC Enable | Properties                                                 |
+-----------+----------+---------------+-------+-----------+-----------+------------------------------------------------------------+
| Ain[0]    | 3/3      | LVCMOS33_IN   | PL2C  |           |           | CLAMP:ON HYSTERESIS:SMALL                                  |
| Ain[1]    | 2/3      | LVCMOS33_IN   | PL2B  |           |           | CLAMP:ON HYSTERESIS:SMALL                                  |
| Ain[2]    | 7/3      | LVCMOS33_IN   | PL3A  |           |           | CLAMP:ON HYSTERESIS:SMALL                                  |
| Ain[3]    | 4/3      | LVCMOS33_IN   | PL2D  |           |           | CLAMP:ON HYSTERESIS:SMALL                                  |
| Ain[4]    | 78/0     | LVCMOS33_IN   | PT11A |           |           | CLAMP:ON HYSTERESIS:SMALL                                  |
| Ain[5]    | 84/0     | LVCMOS33_IN   | PT10A |           |           | CLAMP:ON HYSTERESIS:SMALL                                  |
| Ain[6]    | 86/0     | LVCMOS33_IN   | PT9C  |           |           | CLAMP:ON HYSTERESIS:SMALL                                  |
| Ain[7]    | 8/3      | LVCMOS33_IN   | PL3B  |           |           | CLAMP:ON HYSTERESIS:SMALL                                  |
| BA[0]     | 58/1     | LVCMOS33_OUT  | PR6C  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| BA[1]     | 60/1     | LVCMOS33_OUT  | PR6A  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| C14M      | 62/1     | LVCMOS33_IN   | PR5D  |           |           | CLAMP:ON HYSTERESIS:SMALL                                  |
| CKEout    | 53/1     | LVCMOS33_OUT  | PR7B  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| DQMH      | 49/2     | LVCMOS33_OUT  | PB14D |           |           | DRIVE:4mA SLEW:SLOW                                        |
| DQML      | 48/2     | LVCMOS33_OUT  | PB14C |           |           | DRIVE:4mA SLEW:SLOW                                        |
| Din[0]    | 96/0     | LVCMOS33_IN   | PT6D  |           |           | CLAMP:ON HYSTERESIS:SMALL                                  |
| Din[1]    | 97/0     | LVCMOS33_IN   | PT6C  |           |           | CLAMP:ON HYSTERESIS:SMALL                                  |
| Din[2]    | 98/0     | LVCMOS33_IN   | PT6B  |           |           | CLAMP:ON HYSTERESIS:SMALL                                  |
| Din[3]    | 9/3      | LVCMOS33_IN   | PL3C  |           |           | CLAMP:ON HYSTERESIS:SMALL                                  |
| Din[4]    | 1/3      | LVCMOS33_IN   | PL2A  |           |           | CLAMP:ON HYSTERESIS:SMALL                                  |
| Din[5]    | 99/0     | LVCMOS33_IN   | PT6A  |           |           | CLAMP:ON HYSTERESIS:SMALL                                  |
| Din[6]    | 88/0     | LVCMOS33_IN   | PT9A  |           |           | CLAMP:ON HYSTERESIS:SMALL                                  |
| Din[7]    | 87/0     | LVCMOS33_IN   | PT9B  |           |           | CLAMP:ON HYSTERESIS:SMALL                                  |
| Dout[0]   | 30/2     | LVCMOS33_OUT  | PB4D  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| Dout[1]   | 27/2     | LVCMOS33_OUT  | PB4A  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| Dout[2]   | 25/3     | LVCMOS33_OUT  | PL7D  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| Dout[3]   | 28/2     | LVCMOS33_OUT  | PB4B  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| Dout[4]   | 24/3     | LVCMOS33_OUT  | PL7C  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| Dout[5]   | 21/3     | LVCMOS33_OUT  | PL7B  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| Dout[6]   | 31/2     | LVCMOS33_OUT  | PB6A  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| Dout[7]   | 32/2     | LVCMOS33_OUT  | PB6B  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| LED       | 35/2     | LVCMOS33_OUT  | PB6D  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| PHI1      | 85/0     | LVCMOS33_IN   | PT9D  |           |           | CLAMP:ON HYSTERESIS:SMALL                                  |
| RAout[0]  | 66/1     | LVCMOS33_OUT  | PR3D  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| RAout[10] | 64/1     | LVCMOS33_OUT  | PR5B  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| RAout[11] | 59/1     | LVCMOS33_OUT  | PR6B  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| RAout[1]  | 68/1     | LVCMOS33_OUT  | PR3B  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| RAout[2]  | 70/1     | LVCMOS33_OUT  | PR2D  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| RAout[3]  | 74/1     | LVCMOS33_OUT  | PR2B  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| RAout[4]  | 75/1     | LVCMOS33_OUT  | PR2A  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| RAout[5]  | 71/1     | LVCMOS33_OUT  | PR2C  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| RAout[6]  | 69/1     | LVCMOS33_OUT  | PR3A  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| RAout[7]  | 67/1     | LVCMOS33_OUT  | PR3C  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| RAout[8]  | 65/1     | LVCMOS33_OUT  | PR5A  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| RAout[9]  | 63/1     | LVCMOS33_OUT  | PR5C  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| RD[0]     | 36/2     | LVCMOS33_BIDI | PB10A |           |           | DRIVE:4mA PULL:KEEPER CLAMP:ON HYSTERESIS:SMALL SLEW:SLOW  |
| RD[1]     | 37/2     | LVCMOS33_BIDI | PB10B |           |           | DRIVE:4mA PULL:KEEPER CLAMP:ON HYSTERESIS:SMALL SLEW:SLOW  |
| RD[2]     | 38/2     | LVCMOS33_BIDI | PB10C |           |           | DRIVE:4mA PULL:KEEPER CLAMP:ON HYSTERESIS:SMALL SLEW:SLOW  |
| RD[3]     | 39/2     | LVCMOS33_BIDI | PB10D |           |           | DRIVE:4mA PULL:KEEPER CLAMP:ON HYSTERESIS:SMALL SLEW:SLOW  |
| RD[4]     | 40/2     | LVCMOS33_BIDI | PB12A |           |           | DRIVE:4mA PULL:KEEPER CLAMP:ON HYSTERESIS:SMALL SLEW:SLOW  |
| RD[5]     | 41/2     | LVCMOS33_BIDI | PB12B |           |           | DRIVE:4mA PULL:KEEPER CLAMP:ON HYSTERESIS:SMALL SLEW:SLOW  |
| RD[6]     | 42/2     | LVCMOS33_BIDI | PB12C |           |           | DRIVE:4mA PULL:KEEPER CLAMP:ON HYSTERESIS:SMALL SLEW:SLOW  |
| RD[7]     | 43/2     | LVCMOS33_BIDI | PB12D |           |           | DRIVE:4mA PULL:KEEPER CLAMP:ON HYSTERESIS:SMALL SLEW:SLOW  |
| Vout[0]   | 18/3     | LVCMOS33_OUT  | PL6C  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| Vout[1]   | 15/3     | LVCMOS33_OUT  | PL5D  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| Vout[2]   | 17/3     | LVCMOS33_OUT  | PL6B  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| Vout[3]   | 13/3     | LVCMOS33_OUT  | PL5B  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| Vout[4]   | 19/3     | LVCMOS33_OUT  | PL6D  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| Vout[5]   | 16/3     | LVCMOS33_OUT  | PL6A  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| Vout[6]   | 14/3     | LVCMOS33_OUT  | PL5C  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| Vout[7]   | 12/3     | LVCMOS33_OUT  | PL5A  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| nC07X     | 34/2     | LVCMOS33_IN   | PB6C  |           |           | CLAMP:ON HYSTERESIS:SMALL                                  |
| nCASout   | 52/1     | LVCMOS33_OUT  | PR7C  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| nCSout    | 57/1     | LVCMOS33_OUT  | PR6D  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| nDOE      | 20/3     | LVCMOS33_OUT  | PL7A  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| nEN80     | 82/0     | LVCMOS33_IN   | PT10C |           |           | CLAMP:ON HYSTERESIS:SMALL                                  |
| nRASout   | 54/1     | LVCMOS33_OUT  | PR7A  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| nRWEout   | 51/1     | LVCMOS33_OUT  | PR7D  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| nVOE      | 10/3     | LVCMOS33_OUT  | PL3D  |           |           | DRIVE:4mA SLEW:SLOW                                        |
| nWE       | 29/2     | LVCMOS33_IN   | PB4C  |           |           | CLAMP:ON HYSTERESIS:SMALL                                  |
+-----------+----------+---------------+-------+-----------+-----------+------------------------------------------------------------+

Vccio by Bank:
+------+-------+
| Bank | Vccio |
+------+-------+
| 0    | 3.3V  |
| 1    | 3.3V  |
| 2    | 3.3V  |
| 3    | 3.3V  |
+------+-------+

Vref by Bank:
+------+-----+-----------------+---------+
| Vref | Pin | Bank # / Vref # | Load(s) |
+------+-----+-----------------+---------+
+------+-----+-----------------+---------+

Pinout by Pin Number:
+----------+-----------------------+------------+---------------+-------+---------------+-----------+-----------+
| Pin/Bank | Pin Info              | Preference | Buffer Type   | Site  | Dual Function | PG Enable | BC Enable |
+----------+-----------------------+------------+---------------+-------+---------------+-----------+-----------+
| 1/3      | Din[4]                | LOCATED    | LVCMOS33_IN   | PL2A  |               |           |           |
| 2/3      | Ain[1]                | LOCATED    | LVCMOS33_IN   | PL2B  |               |           |           |
| 3/3      | Ain[0]                | LOCATED    | LVCMOS33_IN   | PL2C  | PCLKT3_2      |           |           |
| 4/3      | Ain[3]                | LOCATED    | LVCMOS33_IN   | PL2D  | PCLKC3_2      |           |           |
| 7/3      | Ain[2]                | LOCATED    | LVCMOS33_IN   | PL3A  |               |           |           |
| 8/3      | Ain[7]                | LOCATED    | LVCMOS33_IN   | PL3B  |               |           |           |
| 9/3      | Din[3]                | LOCATED    | LVCMOS33_IN   | PL3C  |               |           |           |
| 10/3     | nVOE                  | LOCATED    | LVCMOS33_OUT  | PL3D  |               |           |           |
| 12/3     | Vout[7]               | LOCATED    | LVCMOS33_OUT  | PL5A  | PCLKT3_1      |           |           |
| 13/3     | Vout[3]               | LOCATED    | LVCMOS33_OUT  | PL5B  | PCLKC3_1      |           |           |
| 14/3     | Vout[6]               | LOCATED    | LVCMOS33_OUT  | PL5C  |               |           |           |
| 15/3     | Vout[1]               | LOCATED    | LVCMOS33_OUT  | PL5D  |               |           |           |
| 16/3     | Vout[5]               | LOCATED    | LVCMOS33_OUT  | PL6A  |               |           |           |
| 17/3     | Vout[2]               | LOCATED    | LVCMOS33_OUT  | PL6B  |               |           |           |
| 18/3     | Vout[0]               | LOCATED    | LVCMOS33_OUT  | PL6C  |               |           |           |
| 19/3     | Vout[4]               | LOCATED    | LVCMOS33_OUT  | PL6D  |               |           |           |
| 20/3     | nDOE                  | LOCATED    | LVCMOS33_OUT  | PL7A  | PCLKT3_0      |           |           |
| 21/3     | Dout[5]               | LOCATED    | LVCMOS33_OUT  | PL7B  | PCLKC3_0      |           |           |
| 24/3     | Dout[4]               | LOCATED    | LVCMOS33_OUT  | PL7C  |               |           |           |
| 25/3     | Dout[2]               | LOCATED    | LVCMOS33_OUT  | PL7D  |               |           |           |
| 27/2     | Dout[1]               | LOCATED    | LVCMOS33_OUT  | PB4A  | CSSPIN        |           |           |
| 28/2     | Dout[3]               | LOCATED    | LVCMOS33_OUT  | PB4B  |               |           |           |
| 29/2     | nWE                   | LOCATED    | LVCMOS33_IN   | PB4C  |               |           |           |
| 30/2     | Dout[0]               | LOCATED    | LVCMOS33_OUT  | PB4D  |               |           |           |
| 31/2     | Dout[6]               | LOCATED    | LVCMOS33_OUT  | PB6A  | MCLK/CCLK     |           |           |
| 32/2     | Dout[7]               | LOCATED    | LVCMOS33_OUT  | PB6B  | SO/SPISO      |           |           |
| 34/2     | nC07X                 | LOCATED    | LVCMOS33_IN   | PB6C  | PCLKT2_0      |           |           |
| 35/2     | LED                   | LOCATED    | LVCMOS33_OUT  | PB6D  | PCLKC2_0      |           |           |
| 36/2     | RD[0]                 | LOCATED    | LVCMOS33_BIDI | PB10A |               |           |           |
| 37/2     | RD[1]                 | LOCATED    | LVCMOS33_BIDI | PB10B |               |           |           |
| 38/2     | RD[2]                 | LOCATED    | LVCMOS33_BIDI | PB10C | PCLKT2_1      |           |           |
| 39/2     | RD[3]                 | LOCATED    | LVCMOS33_BIDI | PB10D | PCLKC2_1      |           |           |
| 40/2     | RD[4]                 | LOCATED    | LVCMOS33_BIDI | PB12A |               |           |           |
| 41/2     | RD[5]                 | LOCATED    | LVCMOS33_BIDI | PB12B |               |           |           |
| 42/2     | RD[6]                 | LOCATED    | LVCMOS33_BIDI | PB12C |               |           |           |
| 43/2     | RD[7]                 | LOCATED    | LVCMOS33_BIDI | PB12D |               |           |           |
| 45/2     |     unused, PULL:DOWN |            |               | PB14A |               |           |           |
| 47/2     |     unused, PULL:DOWN |            |               | PB14B |               |           |           |
| 48/2     | DQML                  | LOCATED    | LVCMOS33_OUT  | PB14C | SN            |           |           |
| 49/2     | DQMH                  | LOCATED    | LVCMOS33_OUT  | PB14D | SI/SISPI      |           |           |
| 51/1     | nRWEout               | LOCATED    | LVCMOS33_OUT  | PR7D  |               |           |           |
| 52/1     | nCASout               | LOCATED    | LVCMOS33_OUT  | PR7C  |               |           |           |
| 53/1     | CKEout                | LOCATED    | LVCMOS33_OUT  | PR7B  |               |           |           |
| 54/1     | nRASout               | LOCATED    | LVCMOS33_OUT  | PR7A  |               |           |           |
| 57/1     | nCSout                | LOCATED    | LVCMOS33_OUT  | PR6D  |               |           |           |
| 58/1     | BA[0]                 | LOCATED    | LVCMOS33_OUT  | PR6C  |               |           |           |
| 59/1     | RAout[11]             | LOCATED    | LVCMOS33_OUT  | PR6B  |               |           |           |
| 60/1     | BA[1]                 | LOCATED    | LVCMOS33_OUT  | PR6A  |               |           |           |
| 62/1     | C14M                  | LOCATED    | LVCMOS33_IN   | PR5D  | PCLKC1_0      |           |           |
| 63/1     | RAout[9]              | LOCATED    | LVCMOS33_OUT  | PR5C  | PCLKT1_0      |           |           |
| 64/1     | RAout[10]             | LOCATED    | LVCMOS33_OUT  | PR5B  |               |           |           |
| 65/1     | RAout[8]              | LOCATED    | LVCMOS33_OUT  | PR5A  |               |           |           |
| 66/1     | RAout[0]              | LOCATED    | LVCMOS33_OUT  | PR3D  |               |           |           |
| 67/1     | RAout[7]              | LOCATED    | LVCMOS33_OUT  | PR3C  |               |           |           |
| 68/1     | RAout[1]              | LOCATED    | LVCMOS33_OUT  | PR3B  |               |           |           |
| 69/1     | RAout[6]              | LOCATED    | LVCMOS33_OUT  | PR3A  |               |           |           |
| 70/1     | RAout[2]              | LOCATED    | LVCMOS33_OUT  | PR2D  |               |           |           |
| 71/1     | RAout[5]              | LOCATED    | LVCMOS33_OUT  | PR2C  |               |           |           |
| 74/1     | RAout[3]              | LOCATED    | LVCMOS33_OUT  | PR2B  |               |           |           |
| 75/1     | RAout[4]              | LOCATED    | LVCMOS33_OUT  | PR2A  |               |           |           |
| 76/0     |     unused, PULL:DOWN |            |               | PT11D | DONE          |           |           |
| 77/0     |     unused, PULL:DOWN |            |               | PT11C | INITN         |           |           |
| 78/0     | Ain[4]                | LOCATED    | LVCMOS33_IN   | PT11A |               |           |           |
| 81/0     |     unused, PULL:DOWN |            |               | PT10D | PROGRAMN      |           |           |
| 82/0     | nEN80                 | LOCATED    | LVCMOS33_IN   | PT10C | JTAGENB       |           |           |
| 83/0     |     unused, PULL:DOWN |            |               | PT10B |               |           |           |
| 84/0     | Ain[5]                | LOCATED    | LVCMOS33_IN   | PT10A |               |           |           |
| 85/0     | PHI1                  | LOCATED    | LVCMOS33_IN   | PT9D  | SDA/PCLKC0_0  |           |           |
| 86/0     | Ain[6]                | LOCATED    | LVCMOS33_IN   | PT9C  | SCL/PCLKT0_0  |           |           |
| 87/0     | Din[7]                | LOCATED    | LVCMOS33_IN   | PT9B  | PCLKC0_1      |           |           |
| 88/0     | Din[6]                | LOCATED    | LVCMOS33_IN   | PT9A  | PCLKT0_1      |           |           |
| 90/0     | Reserved: sysCONFIG   |            |               | PT7D  | TMS           |           |           |
| 91/0     | Reserved: sysCONFIG   |            |               | PT7C  | TCK           |           |           |
| 94/0     | Reserved: sysCONFIG   |            |               | PT7B  | TDI           |           |           |
| 95/0     | Reserved: sysCONFIG   |            |               | PT7A  | TDO           |           |           |
| 96/0     | Din[0]                | LOCATED    | LVCMOS33_IN   | PT6D  |               |           |           |
| 97/0     | Din[1]                | LOCATED    | LVCMOS33_IN   | PT6C  |               |           |           |
| 98/0     | Din[2]                | LOCATED    | LVCMOS33_IN   | PT6B  |               |           |           |
| 99/0     | Din[5]                | LOCATED    | LVCMOS33_IN   | PT6A  |               |           |           |
| PT11B/0  |     unused, PULL:DOWN |            |               | PT11B |               |           |           |
+----------+-----------------------+------------+---------------+-------+---------------+-----------+-----------+

sysCONFIG Pins:
+----------+--------------------+--------------------+----------+-------------+-------------------+
| Pad Name | sysCONFIG Pin Name | sysCONFIG Settings | Pin/Bank | Buffer Type | Config Pull Mode  |
+----------+--------------------+--------------------+----------+-------------+-------------------+
| PT7D     | TMS                | JTAG_PORT=ENABLE   | 90/0     |             | PULLUP            |
| PT7C     | TCK/TEST_CLK       | JTAG_PORT=ENABLE   | 91/0     |             | NO pull up/down   |
| PT7B     | TDI/MD7            | JTAG_PORT=ENABLE   | 94/0     |             | PULLUP            |
| PT7A     | TDO                | JTAG_PORT=ENABLE   | 95/0     |             | PULLUP            |
+----------+--------------------+--------------------+----------+-------------+-------------------+

Dedicated sysCONFIG Pins:


List of All Pins' Locate Preferences Based on Final Placement After PAR 
to Help Users Lock Down ALL the Pins Easily (by Simply Copy & Paste): 

LOCATE  COMP  "Ain[0]"  SITE  "3";
LOCATE  COMP  "Ain[1]"  SITE  "2";
LOCATE  COMP  "Ain[2]"  SITE  "7";
LOCATE  COMP  "Ain[3]"  SITE  "4";
LOCATE  COMP  "Ain[4]"  SITE  "78";
LOCATE  COMP  "Ain[5]"  SITE  "84";
LOCATE  COMP  "Ain[6]"  SITE  "86";
LOCATE  COMP  "Ain[7]"  SITE  "8";
LOCATE  COMP  "BA[0]"  SITE  "58";
LOCATE  COMP  "BA[1]"  SITE  "60";
LOCATE  COMP  "C14M"  SITE  "62";
LOCATE  COMP  "CKEout"  SITE  "53";
LOCATE  COMP  "DQMH"  SITE  "49";
LOCATE  COMP  "DQML"  SITE  "48";
LOCATE  COMP  "Din[0]"  SITE  "96";
LOCATE  COMP  "Din[1]"  SITE  "97";
LOCATE  COMP  "Din[2]"  SITE  "98";
LOCATE  COMP  "Din[3]"  SITE  "9";
LOCATE  COMP  "Din[4]"  SITE  "1";
LOCATE  COMP  "Din[5]"  SITE  "99";
LOCATE  COMP  "Din[6]"  SITE  "88";
LOCATE  COMP  "Din[7]"  SITE  "87";
LOCATE  COMP  "Dout[0]"  SITE  "30";
LOCATE  COMP  "Dout[1]"  SITE  "27";
LOCATE  COMP  "Dout[2]"  SITE  "25";
LOCATE  COMP  "Dout[3]"  SITE  "28";
LOCATE  COMP  "Dout[4]"  SITE  "24";
LOCATE  COMP  "Dout[5]"  SITE  "21";
LOCATE  COMP  "Dout[6]"  SITE  "31";
LOCATE  COMP  "Dout[7]"  SITE  "32";
LOCATE  COMP  "LED"  SITE  "35";
LOCATE  COMP  "PHI1"  SITE  "85";
LOCATE  COMP  "RAout[0]"  SITE  "66";
LOCATE  COMP  "RAout[10]"  SITE  "64";
LOCATE  COMP  "RAout[11]"  SITE  "59";
LOCATE  COMP  "RAout[1]"  SITE  "68";
LOCATE  COMP  "RAout[2]"  SITE  "70";
LOCATE  COMP  "RAout[3]"  SITE  "74";
LOCATE  COMP  "RAout[4]"  SITE  "75";
LOCATE  COMP  "RAout[5]"  SITE  "71";
LOCATE  COMP  "RAout[6]"  SITE  "69";
LOCATE  COMP  "RAout[7]"  SITE  "67";
LOCATE  COMP  "RAout[8]"  SITE  "65";
LOCATE  COMP  "RAout[9]"  SITE  "63";
LOCATE  COMP  "RD[0]"  SITE  "36";
LOCATE  COMP  "RD[1]"  SITE  "37";
LOCATE  COMP  "RD[2]"  SITE  "38";
LOCATE  COMP  "RD[3]"  SITE  "39";
LOCATE  COMP  "RD[4]"  SITE  "40";
LOCATE  COMP  "RD[5]"  SITE  "41";
LOCATE  COMP  "RD[6]"  SITE  "42";
LOCATE  COMP  "RD[7]"  SITE  "43";
LOCATE  COMP  "Vout[0]"  SITE  "18";
LOCATE  COMP  "Vout[1]"  SITE  "15";
LOCATE  COMP  "Vout[2]"  SITE  "17";
LOCATE  COMP  "Vout[3]"  SITE  "13";
LOCATE  COMP  "Vout[4]"  SITE  "19";
LOCATE  COMP  "Vout[5]"  SITE  "16";
LOCATE  COMP  "Vout[6]"  SITE  "14";
LOCATE  COMP  "Vout[7]"  SITE  "12";
LOCATE  COMP  "nC07X"  SITE  "34";
LOCATE  COMP  "nCASout"  SITE  "52";
LOCATE  COMP  "nCSout"  SITE  "57";
LOCATE  COMP  "nDOE"  SITE  "20";
LOCATE  COMP  "nEN80"  SITE  "82";
LOCATE  COMP  "nRASout"  SITE  "54";
LOCATE  COMP  "nRWEout"  SITE  "51";
LOCATE  COMP  "nVOE"  SITE  "10";
LOCATE  COMP  "nWE"  SITE  "29";





PAR: Place And Route Diamond (64-bit) 3.12.1.454.
Copyright (c) 1991-1994 by NeoCAD Inc. All rights reserved.
Copyright (c) 1995 AT&T Corp.   All rights reserved.
Copyright (c) 1995-2001 Lucent Technologies Inc.  All rights reserved.
Copyright (c) 2001 Agere Systems   All rights reserved.
Copyright (c) 2002-2020 Lattice Semiconductor Corporation,  All rights reserved.
Thu Dec 28 23:23:41 2023

