Loading design for application iotiming from file ram2e_lcmxo2_1200hc_impl1.ncd.
Design name: RAM2E
NCD version: 3.3
Vendor:      LATTICE
Device:      LCMXO2-1200HC
Package:     TQFP100
Performance: 5
Package Status:                     Final          Version 1.44.
Performance Hardware Data Status:   Final          Version 34.4.
Loading design for application iotiming from file ram2e_lcmxo2_1200hc_impl1.ncd.
Design name: RAM2E
NCD version: 3.3
Vendor:      LATTICE
Device:      LCMXO2-1200HC
Package:     TQFP100
Performance: 6
Package Status:                     Final          Version 1.44.
Performance Hardware Data Status:   Final          Version 34.4.
Loading design for application iotiming from file ram2e_lcmxo2_1200hc_impl1.ncd.
Design name: RAM2E
NCD version: 3.3
Vendor:      LATTICE
Device:      LCMXO2-1200HC
Package:     TQFP100
Performance: M
Package Status:                     Final          Version 1.44.
Performance Hardware Data Status:   Final          Version 34.4.
// Design: RAM2E
// Package: TQFP100
// ncd File: ram2e_lcmxo2_1200hc_impl1.ncd
// Version: Diamond (64-bit) 3.12.1.454
// Written on Thu Dec 28 23:23:48 2023
// M: Minimum Performance Grade
// iotiming RAM2E_LCMXO2_1200HC_impl1.ncd RAM2E_LCMXO2_1200HC_impl1.prf -gui -msgset //Mac/iCloud/Repos/RAM2E/CPLD/LCMXO2-1200HC/promote.xml

I/O Timing Report (All units are in ns)

Worst Case Results across Performance Grades (M, 6, 5, 4):

// Input Setup and Hold Times

Port   Clock Edge  Setup Performance_Grade  Hold Performance_Grade
----------------------------------------------------------------------
Ain[0] C14M  R     0.163      4       1.694     4
Ain[1] C14M  R    -0.150      M       2.217     4
Ain[2] C14M  R    -0.080      M       2.156     4
Ain[3] C14M  R     0.466      4       1.338     4
Ain[4] C14M  R     0.215      4       1.597     4
Ain[5] C14M  R    -0.331      M       2.651     4
Ain[6] C14M  R     0.065      M       1.882     4
Ain[7] C14M  R     0.284      4       1.683     4
Din[0] C14M  R     6.887      4       2.257     4
Din[1] C14M  R     8.753      4       2.907     4
Din[2] C14M  R     6.379      4       2.740     4
Din[3] C14M  R     7.129      4       1.402     4
Din[4] C14M  R     6.869      4       2.791     4
Din[5] C14M  R     6.514      4       2.334     4
Din[6] C14M  R     6.735      4       1.914     4
Din[7] C14M  R     8.094      4       1.968     4
PHI1   C14M  R     1.557      4       4.842     4
RD[0]  C14M  R    -0.266      M       2.342     4
RD[1]  C14M  R    -0.248      M       2.283     4
RD[2]  C14M  R    -0.407      M       2.610     4
RD[3]  C14M  R    -0.243      M       2.193     4
RD[4]  C14M  R    -0.246      M       2.201     4
RD[5]  C14M  R    -0.243      M       2.193     4
RD[6]  C14M  R    -0.087      M       1.756     4
RD[7]  C14M  R    -0.092      M       1.769     4
nC07X  C14M  R    -0.320      M       2.703     4
nEN80  C14M  R     4.607      4       1.925     4
nWE    C14M  R     4.609      4       2.010     4


// Clock to Output Delay

Port      Clock Edge  Max_Delay Performance_Grade  Min_Delay Performance_Grade
------------------------------------------------------------------------
BA[0]     C14M  R    10.424         4        3.355          M
BA[1]     C14M  R    10.424         4        3.355          M
CKEout    C14M  F    10.424         4        3.355          M
DQMH      C14M  R    10.404         4        3.362          M
DQML      C14M  R    10.404         4        3.362          M
LED       C14M  R    22.936         4        8.890          M
RAout[0]  C14M  F    10.490         4        3.360          M
RAout[10] C14M  F    10.490         4        3.360          M
RAout[11] C14M  F    10.424         4        3.355          M
RAout[1]  C14M  F    10.490         4        3.360          M
RAout[2]  C14M  F    10.490         4        3.360          M
RAout[3]  C14M  F    10.490         4        3.360          M
RAout[4]  C14M  F    10.490         4        3.360          M
RAout[5]  C14M  F    10.490         4        3.360          M
RAout[6]  C14M  F    10.490         4        3.360          M
RAout[7]  C14M  F    10.490         4        3.360          M
RAout[8]  C14M  F    10.490         4        3.360          M
RAout[9]  C14M  F    10.490         4        3.360          M
RD[0]     C14M  R    13.733         4        3.707          M
RD[1]     C14M  R    13.745         4        3.707          M
RD[2]     C14M  R    14.285         4        3.790          M
RD[3]     C14M  R    13.348         4        3.790          M
RD[4]     C14M  R    14.450         4        3.952          M
RD[5]     C14M  R    14.480         4        3.952          M
RD[6]     C14M  R    14.784         4        3.952          M
RD[7]     C14M  R    14.247         4        3.952          M
Vout[0]   C14M  R    11.348         4        3.872          M
Vout[1]   C14M  R    11.434         4        3.871          M
Vout[2]   C14M  R    11.348         4        3.872          M
Vout[3]   C14M  R    11.434         4        3.871          M
Vout[4]   C14M  R    11.348         4        3.872          M
Vout[5]   C14M  R    11.348         4        3.872          M
Vout[6]   C14M  R    11.434         4        3.871          M
Vout[7]   C14M  R    11.434         4        3.871          M
nCASout   C14M  F    10.424         4        3.355          M
nDOE      C14M  R    13.929         4        4.309          M
nRASout   C14M  F    10.424         4        3.355          M
nRWEout   C14M  F    10.424         4        3.355          M
nVOE      C14M  R    13.926         4        4.281          M
WARNING: you must also run trce with hold speed: 4
WARNING: you must also run trce with setup speed: M
