Loading design for application iotiming from file ram2e_lcmxo2_640hc_impl1.ncd.
Design name: RAM2E
NCD version: 3.3
Vendor:      LATTICE
Device:      LCMXO2-640HC
Package:     TQFP100
Performance: 5
Package Status:                     Final          Version 1.39.
Performance Hardware Data Status:   Final          Version 34.4.
Loading design for application iotiming from file ram2e_lcmxo2_640hc_impl1.ncd.
Design name: RAM2E
NCD version: 3.3
Vendor:      LATTICE
Device:      LCMXO2-640HC
Package:     TQFP100
Performance: 6
Package Status:                     Final          Version 1.39.
Performance Hardware Data Status:   Final          Version 34.4.
Loading design for application iotiming from file ram2e_lcmxo2_640hc_impl1.ncd.
Design name: RAM2E
NCD version: 3.3
Vendor:      LATTICE
Device:      LCMXO2-640HC
Package:     TQFP100
Performance: M
Package Status:                     Final          Version 1.39.
Performance Hardware Data Status:   Final          Version 34.4.
// Design: RAM2E
// Package: TQFP100
// ncd File: ram2e_lcmxo2_640hc_impl1.ncd
// Version: Diamond (64-bit) 3.12.1.454
// Written on Thu Dec 28 23:23:47 2023
// M: Minimum Performance Grade
// iotiming RAM2E_LCMXO2_640HC_impl1.ncd RAM2E_LCMXO2_640HC_impl1.prf -gui -msgset //Mac/iCloud/Repos/ram2e/CPLD/LCMXO2-640HC/promote.xml

I/O Timing Report (All units are in ns)

Worst Case Results across Performance Grades (M, 6, 5, 4):

// Input Setup and Hold Times

Port   Clock Edge  Setup Performance_Grade  Hold Performance_Grade
----------------------------------------------------------------------
Ain[0] C14M  R     2.463      4      -0.066     M
Ain[1] C14M  R     1.330      4       0.135     6
Ain[2] C14M  R     1.221      4       0.223     4
Ain[3] C14M  R     2.776      4      -0.165     M
Ain[4] C14M  R     1.603      4       0.140     M
Ain[5] C14M  R     0.021      6       1.287     4
Ain[6] C14M  R     1.444      4       0.205     M
Ain[7] C14M  R     1.816      4       0.114     M
Din[0] C14M  R     8.919      4       0.723     4
Din[1] C14M  R     8.410      4       1.156     4
Din[2] C14M  R     8.503      4       1.181     4
Din[3] C14M  R     8.783      4       0.110     M
Din[4] C14M  R    10.420      4       1.022     4
Din[5] C14M  R     8.001      4       0.566     4
Din[6] C14M  R     9.731      4       1.050     4
Din[7] C14M  R    10.052      4       0.862     4
PHI1   C14M  R     2.579      4       3.047     4
RD[0]  C14M  R     0.267      4       0.866     4
RD[1]  C14M  R     0.173      4       0.937     4
RD[2]  C14M  R     0.100      4       1.018     4
RD[3]  C14M  R     0.267      4       0.866     4
RD[4]  C14M  R     0.172      4       0.936     4
RD[5]  C14M  R     0.267      4       0.866     4
RD[6]  C14M  R     0.766      4       0.420     4
RD[7]  C14M  R     0.267      4       0.866     4
nC07X  C14M  R     0.998      4       0.405     6
nEN80  C14M  R     6.107      4       0.114     M
nWE    C14M  R     6.726      4       0.069     M


// Clock to Output Delay

Port      Clock Edge  Max_Delay Performance_Grade  Min_Delay Performance_Grade
------------------------------------------------------------------------
BA[0]     C14M  R     8.629         4        2.885          M
BA[1]     C14M  R     8.629         4        2.885          M
CKEout    C14M  F     8.629         4        2.885          M
DQMH      C14M  R     8.609         4        2.892          M
DQML      C14M  R     8.609         4        2.892          M
LED       C14M  R    19.935         4        8.161          M
RAout[0]  C14M  F     8.695         4        2.890          M
RAout[10] C14M  F     8.629         4        2.885          M
RAout[11] C14M  F     8.629         4        2.885          M
RAout[1]  C14M  F     8.695         4        2.890          M
RAout[2]  C14M  F     8.695         4        2.890          M
RAout[3]  C14M  F     8.695         4        2.890          M
RAout[4]  C14M  F     8.695         4        2.890          M
RAout[5]  C14M  F     8.695         4        2.890          M
RAout[6]  C14M  F     8.695         4        2.890          M
RAout[7]  C14M  F     8.695         4        2.890          M
RAout[8]  C14M  F     8.629         4        2.885          M
RAout[9]  C14M  F     8.629         4        2.885          M
RD[0]     C14M  R    11.414         4        3.265          M
RD[1]     C14M  R    11.811         4        3.265          M
RD[2]     C14M  R    11.925         4        3.265          M
RD[3]     C14M  R    11.384         4        3.265          M
RD[4]     C14M  R    12.301         4        3.371          M
RD[5]     C14M  R    12.767         4        3.371          M
RD[6]     C14M  R    12.010         4        3.371          M
RD[7]     C14M  R    12.313         4        3.371          M
Vout[0]   C14M  R     9.553         4        3.402          M
Vout[1]   C14M  R     9.553         4        3.402          M
Vout[2]   C14M  R     9.553         4        3.402          M
Vout[3]   C14M  R     9.553         4        3.402          M
Vout[4]   C14M  R     9.553         4        3.402          M
Vout[5]   C14M  R     9.553         4        3.402          M
Vout[6]   C14M  R     9.553         4        3.402          M
Vout[7]   C14M  R     9.553         4        3.402          M
nCASout   C14M  F     8.629         4        2.885          M
nDOE      C14M  R    12.048         4        3.811          M
nRASout   C14M  F     8.629         4        2.885          M
nRWEout   C14M  F     8.629         4        2.885          M
nVOE      C14M  R    12.164         4        3.783          M
WARNING: you must also run trce with hold speed: 4
WARNING: you must also run trce with setup speed: 6
WARNING: you must also run trce with hold speed: 6
