PAD Specification File
***************************

PART TYPE:        LCMXO256C
Performance Grade:      3
PACKAGE:          TQFP100
Package Status:                     Final          Version 1.19

Thu Sep 21 05:38:42 2023

Pinout by Port Name:
+-----------+----------+---------------+------+----------------------------------+
| Port Name | Pin/Bank | Buffer Type   | Site | Properties                       |
+-----------+----------+---------------+------+----------------------------------+
| CROW[0]   | 32/1     | LVCMOS33_IN   | PB2C | SLEW:FAST                        |
| CROW[1]   | 34/1     | LVCMOS33_IN   | PB2D | SLEW:FAST                        |
| Din[0]    | 21/1     | LVCMOS33_IN   | PL8A | SLEW:FAST                        |
| Din[1]    | 15/1     | LVCMOS33_IN   | PL6A | SLEW:FAST                        |
| Din[2]    | 14/1     | LVCMOS33_IN   | PL5D | SLEW:FAST                        |
| Din[3]    | 16/1     | LVCMOS33_IN   | PL6B | SLEW:FAST                        |
| Din[4]    | 18/1     | LVCMOS33_IN   | PL7B | SLEW:FAST                        |
| Din[5]    | 17/1     | LVCMOS33_IN   | PL7A | SLEW:FAST                        |
| Din[6]    | 20/1     | LVCMOS33_IN   | PL7D | SLEW:FAST                        |
| Din[7]    | 19/1     | LVCMOS33_IN   | PL7C | SLEW:FAST                        |
| Dout[0]   | 1/1      | LVCMOS33_OUT  | PL2A | DRIVE:4mA SLEW:FAST              |
| Dout[1]   | 7/1      | LVCMOS33_OUT  | PL4A | DRIVE:4mA SLEW:FAST              |
| Dout[2]   | 8/1      | LVCMOS33_OUT  | PL4B | DRIVE:4mA SLEW:FAST              |
| Dout[3]   | 6/1      | LVCMOS33_OUT  | PL3D | DRIVE:4mA SLEW:FAST              |
| Dout[4]   | 4/1      | LVCMOS33_OUT  | PL3B | DRIVE:4mA SLEW:FAST              |
| Dout[5]   | 5/1      | LVCMOS33_OUT  | PL3C | DRIVE:4mA SLEW:FAST              |
| Dout[6]   | 2/1      | LVCMOS33_OUT  | PL2B | DRIVE:4mA SLEW:FAST              |
| Dout[7]   | 3/1      | LVCMOS33_OUT  | PL3A | DRIVE:4mA SLEW:FAST              |
| LED       | 57/0     | LVCMOS33_OUT  | PR7B | DRIVE:14mA SLEW:SLOW             |
| MAin[0]   | 23/1     | LVCMOS33_IN   | PL9A | SLEW:FAST                        |
| MAin[1]   | 38/1     | LVCMOS33_IN   | PB3C | SLEW:FAST                        |
| MAin[2]   | 37/1     | LVCMOS33_IN   | PB3B | SLEW:FAST                        |
| MAin[3]   | 47/1     | LVCMOS33_IN   | PB5A | SLEW:FAST                        |
| MAin[4]   | 46/1     | LVCMOS33_IN   | PB4D | SLEW:FAST                        |
| MAin[5]   | 45/1     | LVCMOS33_IN   | PB4C | SLEW:FAST                        |
| MAin[6]   | 49/1     | LVCMOS33_IN   | PB5C | SLEW:FAST                        |
| MAin[7]   | 44/1     | LVCMOS33_IN   | PB4B | SLEW:FAST                        |
| MAin[8]   | 50/1     | LVCMOS33_IN   | PB5D | SLEW:FAST                        |
| MAin[9]   | 51/0     | LVCMOS33_IN   | PR9B | SLEW:FAST                        |
| PHI2      | 39/1     | LVCMOS33_IN   | PB3D | SLEW:FAST                        |
| RA[0]     | 98/0     | LVCMOS33_OUT  | PT2C | DRIVE:4mA SLEW:SLOW              |
| RA[10]    | 87/0     | LVCMOS33_OUT  | PT3D | DRIVE:4mA SLEW:SLOW              |
| RA[11]    | 79/0     | LVCMOS33_OUT  | PT5A | DRIVE:4mA SLEW:SLOW              |
| RA[1]     | 89/0     | LVCMOS33_OUT  | PT3C | DRIVE:4mA SLEW:SLOW              |
| RA[2]     | 94/0     | LVCMOS33_OUT  | PT3A | DRIVE:4mA SLEW:SLOW              |
| RA[3]     | 97/0     | LVCMOS33_OUT  | PT2D | DRIVE:4mA SLEW:SLOW              |
| RA[4]     | 99/0     | LVCMOS33_OUT  | PT2B | DRIVE:4mA SLEW:SLOW              |
| RA[5]     | 95/0     | LVCMOS33_OUT  | PT2F | DRIVE:4mA SLEW:SLOW              |
| RA[6]     | 91/0     | LVCMOS33_OUT  | PT3B | DRIVE:4mA SLEW:SLOW              |
| RA[7]     | 100/0    | LVCMOS33_OUT  | PT2A | DRIVE:4mA SLEW:SLOW              |
| RA[8]     | 96/0     | LVCMOS33_OUT  | PT2E | DRIVE:4mA SLEW:SLOW              |
| RA[9]     | 85/0     | LVCMOS33_OUT  | PT4B | DRIVE:4mA SLEW:SLOW              |
| RBA[0]    | 63/0     | LVCMOS33_OUT  | PR5D | DRIVE:4mA SLEW:SLOW              |
| RBA[1]    | 83/0     | LVCMOS33_OUT  | PT4C | DRIVE:4mA SLEW:SLOW              |
| RCKE      | 82/0     | LVCMOS33_OUT  | PT4D | DRIVE:4mA SLEW:SLOW              |
| RCLK      | 86/0     | LVCMOS33_IN   | PT4A | SLEW:FAST                        |
| RDQMH     | 76/0     | LVCMOS33_OUT  | PR2A | DRIVE:4mA SLEW:SLOW              |
| RDQML     | 61/0     | LVCMOS33_OUT  | PR6A | DRIVE:4mA SLEW:SLOW              |
| RD[0]     | 64/0     | LVCMOS33_BIDI | PR5C | DRIVE:4mA SLEW:SLOW PULL:KEEPER  |
| RD[1]     | 65/0     | LVCMOS33_BIDI | PR5B | DRIVE:4mA SLEW:SLOW PULL:KEEPER  |
| RD[2]     | 66/0     | LVCMOS33_BIDI | PR5A | DRIVE:4mA SLEW:SLOW PULL:KEEPER  |
| RD[3]     | 67/0     | LVCMOS33_BIDI | PR4B | DRIVE:4mA SLEW:SLOW PULL:KEEPER  |
| RD[4]     | 68/0     | LVCMOS33_BIDI | PR4A | DRIVE:4mA SLEW:SLOW PULL:KEEPER  |
| RD[5]     | 69/0     | LVCMOS33_BIDI | PR3D | DRIVE:4mA SLEW:SLOW PULL:KEEPER  |
| RD[6]     | 70/0     | LVCMOS33_BIDI | PR3C | DRIVE:4mA SLEW:SLOW PULL:KEEPER  |
| RD[7]     | 71/0     | LVCMOS33_BIDI | PR3B | DRIVE:4mA SLEW:SLOW PULL:KEEPER  |
| UFMCLK    | 58/0     | LVCMOS33_OUT  | PR7A | DRIVE:4mA SLEW:SLOW              |
| UFMSDI    | 56/0     | LVCMOS33_OUT  | PR7C | DRIVE:4mA SLEW:SLOW              |
| UFMSDO    | 55/0     | LVCMOS33_IN   | PR7D | SLEW:FAST                        |
| nCCAS     | 27/1     | LVCMOS33_IN   | PL9B | SLEW:FAST                        |
| nCRAS     | 43/1     | LVCMOS33_IN   | PB4A | SLEW:FAST                        |
| nFWE      | 22/1     | LVCMOS33_IN   | PL8B | SLEW:FAST                        |
| nRCAS     | 78/0     | LVCMOS33_OUT  | PT5B | DRIVE:4mA SLEW:SLOW              |
| nRCS      | 77/0     | LVCMOS33_OUT  | PT5C | DRIVE:4mA SLEW:SLOW              |
| nRRAS     | 73/0     | LVCMOS33_OUT  | PR2B | DRIVE:4mA SLEW:SLOW              |
| nRWE      | 72/0     | LVCMOS33_OUT  | PR3A | DRIVE:4mA SLEW:SLOW              |
| nUFMCS    | 53/0     | LVCMOS33_OUT  | PR8B | DRIVE:4mA SLEW:SLOW              |
+-----------+----------+---------------+------+----------------------------------+

Vccio by Bank:
+------+-------+
| Bank | Vccio |
+------+-------+
| 0    | 3.3V  |
| 1    | 3.3V  |
+------+-------+

Vref by Bank:
+------+-----+-----------------+---------+
| Vref | Pin | Bank # / Vref # | Load(s) |
+------+-----+-----------------+---------+
+------+-----+-----------------+---------+

Pinout by Pin Number:
+----------+---------------------+------------+---------------+------+---------------+
| Pin/Bank | Pin Info            | Preference | Buffer Type   | Site | Dual Function |
+----------+---------------------+------------+---------------+------+---------------+
| 1/1      | Dout[0]             | LOCATED    | LVCMOS33_OUT  | PL2A |               |
| 2/1      | Dout[6]             | LOCATED    | LVCMOS33_OUT  | PL2B |               |
| 3/1      | Dout[7]             | LOCATED    | LVCMOS33_OUT  | PL3A |               |
| 4/1      | Dout[4]             | LOCATED    | LVCMOS33_OUT  | PL3B |               |
| 5/1      | Dout[5]             | LOCATED    | LVCMOS33_OUT  | PL3C |               |
| 6/1      | Dout[3]             | LOCATED    | LVCMOS33_OUT  | PL3D |               |
| 7/1      | Dout[1]             | LOCATED    | LVCMOS33_OUT  | PL4A |               |
| 8/1      | Dout[2]             | LOCATED    | LVCMOS33_OUT  | PL4B |               |
| 9/1      |     unused, PULL:UP |            |               | PL5A |               |
| 11/1     |     unused, PULL:UP |            |               | PL5B |               |
| 13/1     |     unused, PULL:UP |            |               | PL5C |               |
| 14/1     | Din[2]              | LOCATED    | LVCMOS33_IN   | PL5D | GSR_PADN      |
| 15/1     | Din[1]              | LOCATED    | LVCMOS33_IN   | PL6A |               |
| 16/1     | Din[3]              | LOCATED    | LVCMOS33_IN   | PL6B | TSALLPAD      |
| 17/1     | Din[5]              | LOCATED    | LVCMOS33_IN   | PL7A |               |
| 18/1     | Din[4]              | LOCATED    | LVCMOS33_IN   | PL7B |               |
| 19/1     | Din[7]              | LOCATED    | LVCMOS33_IN   | PL7C |               |
| 20/1     | Din[6]              | LOCATED    | LVCMOS33_IN   | PL7D |               |
| 21/1     | Din[0]              | LOCATED    | LVCMOS33_IN   | PL8A |               |
| 22/1     | nFWE                | LOCATED    | LVCMOS33_IN   | PL8B |               |
| 23/1     | MAin[0]             | LOCATED    | LVCMOS33_IN   | PL9A |               |
| 27/1     | nCCAS               | LOCATED    | LVCMOS33_IN   | PL9B |               |
| 29/1     |     unused, PULL:UP |            |               | PB2A |               |
| 30/1     |     unused, PULL:UP |            |               | PB2B |               |
| 32/1     | CROW[0]             | LOCATED    | LVCMOS33_IN   | PB2C |               |
| 34/1     | CROW[1]             | LOCATED    | LVCMOS33_IN   | PB2D |               |
| 36/1     |     unused, PULL:UP |            |               | PB3A | PCLKT1_1      |
| 37/1     | MAin[2]             | LOCATED    | LVCMOS33_IN   | PB3B |               |
| 38/1     | MAin[1]             | LOCATED    | LVCMOS33_IN   | PB3C | PCLKT1_0      |
| 39/1     | PHI2                | LOCATED    | LVCMOS33_IN   | PB3D |               |
| 43/1     | nCRAS               | LOCATED    | LVCMOS33_IN   | PB4A |               |
| 44/1     | MAin[7]             | LOCATED    | LVCMOS33_IN   | PB4B |               |
| 45/1     | MAin[5]             | LOCATED    | LVCMOS33_IN   | PB4C |               |
| 46/1     | MAin[4]             | LOCATED    | LVCMOS33_IN   | PB4D |               |
| 47/1     | MAin[3]             | LOCATED    | LVCMOS33_IN   | PB5A |               |
| 49/1     | MAin[6]             | LOCATED    | LVCMOS33_IN   | PB5C |               |
| 50/1     | MAin[8]             | LOCATED    | LVCMOS33_IN   | PB5D |               |
| 51/0     | MAin[9]             | LOCATED    | LVCMOS33_IN   | PR9B |               |
| 52/0     |     unused, PULL:UP |            |               | PR9A |               |
| 53/0     | nUFMCS              | LOCATED    | LVCMOS33_OUT  | PR8B |               |
| 54/0     |     unused, PULL:UP |            |               | PR8A |               |
| 55/0     | UFMSDO              | LOCATED    | LVCMOS33_IN   | PR7D |               |
| 56/0     | UFMSDI              | LOCATED    | LVCMOS33_OUT  | PR7C |               |
| 57/0     | LED                 | LOCATED    | LVCMOS33_OUT  | PR7B |               |
| 58/0     | UFMCLK              | LOCATED    | LVCMOS33_OUT  | PR7A |               |
| 59/0     |     unused, PULL:UP |            |               | PR6B |               |
| 61/0     | RDQML               | LOCATED    | LVCMOS33_OUT  | PR6A |               |
| 63/0     | RBA[0]              | LOCATED    | LVCMOS33_OUT  | PR5D |               |
| 64/0     | RD[0]               | LOCATED    | LVCMOS33_BIDI | PR5C |               |
| 65/0     | RD[1]               | LOCATED    | LVCMOS33_BIDI | PR5B |               |
| 66/0     | RD[2]               | LOCATED    | LVCMOS33_BIDI | PR5A |               |
| 67/0     | RD[3]               | LOCATED    | LVCMOS33_BIDI | PR4B |               |
| 68/0     | RD[4]               | LOCATED    | LVCMOS33_BIDI | PR4A |               |
| 69/0     | RD[5]               | LOCATED    | LVCMOS33_BIDI | PR3D |               |
| 70/0     | RD[6]               | LOCATED    | LVCMOS33_BIDI | PR3C |               |
| 71/0     | RD[7]               | LOCATED    | LVCMOS33_BIDI | PR3B |               |
| 72/0     | nRWE                | LOCATED    | LVCMOS33_OUT  | PR3A |               |
| 73/0     | nRRAS               | LOCATED    | LVCMOS33_OUT  | PR2B |               |
| 76/0     | RDQMH               | LOCATED    | LVCMOS33_OUT  | PR2A |               |
| 77/0     | nRCS                | LOCATED    | LVCMOS33_OUT  | PT5C |               |
| 78/0     | nRCAS               | LOCATED    | LVCMOS33_OUT  | PT5B |               |
| 79/0     | RA[11]              | LOCATED    | LVCMOS33_OUT  | PT5A |               |
| 80/0     |     unused, PULL:UP |            |               | PT4F |               |
| 81/0     |     unused, PULL:UP |            |               | PT4E |               |
| 82/0     | RCKE                | LOCATED    | LVCMOS33_OUT  | PT4D |               |
| 83/0     | RBA[1]              | LOCATED    | LVCMOS33_OUT  | PT4C |               |
| 85/0     | RA[9]               | LOCATED    | LVCMOS33_OUT  | PT4B | PCLKT0_1      |
| 86/0     | RCLK                | LOCATED    | LVCMOS33_IN   | PT4A | PCLKT0_0      |
| 87/0     | RA[10]              | LOCATED    | LVCMOS33_OUT  | PT3D |               |
| 89/0     | RA[1]               | LOCATED    | LVCMOS33_OUT  | PT3C |               |
| 91/0     | RA[6]               | LOCATED    | LVCMOS33_OUT  | PT3B |               |
| 94/0     | RA[2]               | LOCATED    | LVCMOS33_OUT  | PT3A |               |
| 95/0     | RA[5]               | LOCATED    | LVCMOS33_OUT  | PT2F |               |
| 96/0     | RA[8]               | LOCATED    | LVCMOS33_OUT  | PT2E |               |
| 97/0     | RA[3]               | LOCATED    | LVCMOS33_OUT  | PT2D |               |
| 98/0     | RA[0]               | LOCATED    | LVCMOS33_OUT  | PT2C |               |
| 99/0     | RA[4]               | LOCATED    | LVCMOS33_OUT  | PT2B |               |
| 100/0    | RA[7]               | LOCATED    | LVCMOS33_OUT  | PT2A |               |
| PB5B/0   |     unused, PULL:UP |            |               | PB5B |               |
| PT5D/0   |     unused, PULL:UP |            |               | PT5D |               |
| TCK/1    |                     |            |               | TCK  | TCK           |
| TDI/1    |                     |            |               | TDI  | TDI           |
| TDO/1    |                     |            |               | TDO  | TDO           |
| TMS/1    |                     |            |               | TMS  | TMS           |
+----------+---------------------+------------+---------------+------+---------------+


List of All Pins' Locate Preferences Based on Final Placement After PAR 
to Help Users Lock Down ALL the Pins Easily (by Simply Copy & Paste): 

LOCATE  COMP  "CROW[0]"  SITE  "32";
LOCATE  COMP  "CROW[1]"  SITE  "34";
LOCATE  COMP  "Din[0]"  SITE  "21";
LOCATE  COMP  "Din[1]"  SITE  "15";
LOCATE  COMP  "Din[2]"  SITE  "14";
LOCATE  COMP  "Din[3]"  SITE  "16";
LOCATE  COMP  "Din[4]"  SITE  "18";
LOCATE  COMP  "Din[5]"  SITE  "17";
LOCATE  COMP  "Din[6]"  SITE  "20";
LOCATE  COMP  "Din[7]"  SITE  "19";
LOCATE  COMP  "Dout[0]"  SITE  "1";
LOCATE  COMP  "Dout[1]"  SITE  "7";
LOCATE  COMP  "Dout[2]"  SITE  "8";
LOCATE  COMP  "Dout[3]"  SITE  "6";
LOCATE  COMP  "Dout[4]"  SITE  "4";
LOCATE  COMP  "Dout[5]"  SITE  "5";
LOCATE  COMP  "Dout[6]"  SITE  "2";
LOCATE  COMP  "Dout[7]"  SITE  "3";
LOCATE  COMP  "LED"  SITE  "57";
LOCATE  COMP  "MAin[0]"  SITE  "23";
LOCATE  COMP  "MAin[1]"  SITE  "38";
LOCATE  COMP  "MAin[2]"  SITE  "37";
LOCATE  COMP  "MAin[3]"  SITE  "47";
LOCATE  COMP  "MAin[4]"  SITE  "46";
LOCATE  COMP  "MAin[5]"  SITE  "45";
LOCATE  COMP  "MAin[6]"  SITE  "49";
LOCATE  COMP  "MAin[7]"  SITE  "44";
LOCATE  COMP  "MAin[8]"  SITE  "50";
LOCATE  COMP  "MAin[9]"  SITE  "51";
LOCATE  COMP  "PHI2"  SITE  "39";
LOCATE  COMP  "RA[0]"  SITE  "98";
LOCATE  COMP  "RA[10]"  SITE  "87";
LOCATE  COMP  "RA[11]"  SITE  "79";
LOCATE  COMP  "RA[1]"  SITE  "89";
LOCATE  COMP  "RA[2]"  SITE  "94";
LOCATE  COMP  "RA[3]"  SITE  "97";
LOCATE  COMP  "RA[4]"  SITE  "99";
LOCATE  COMP  "RA[5]"  SITE  "95";
LOCATE  COMP  "RA[6]"  SITE  "91";
LOCATE  COMP  "RA[7]"  SITE  "100";
LOCATE  COMP  "RA[8]"  SITE  "96";
LOCATE  COMP  "RA[9]"  SITE  "85";
LOCATE  COMP  "RBA[0]"  SITE  "63";
LOCATE  COMP  "RBA[1]"  SITE  "83";
LOCATE  COMP  "RCKE"  SITE  "82";
LOCATE  COMP  "RCLK"  SITE  "86";
LOCATE  COMP  "RDQMH"  SITE  "76";
LOCATE  COMP  "RDQML"  SITE  "61";
LOCATE  COMP  "RD[0]"  SITE  "64";
LOCATE  COMP  "RD[1]"  SITE  "65";
LOCATE  COMP  "RD[2]"  SITE  "66";
LOCATE  COMP  "RD[3]"  SITE  "67";
LOCATE  COMP  "RD[4]"  SITE  "68";
LOCATE  COMP  "RD[5]"  SITE  "69";
LOCATE  COMP  "RD[6]"  SITE  "70";
LOCATE  COMP  "RD[7]"  SITE  "71";
LOCATE  COMP  "UFMCLK"  SITE  "58";
LOCATE  COMP  "UFMSDI"  SITE  "56";
LOCATE  COMP  "UFMSDO"  SITE  "55";
LOCATE  COMP  "nCCAS"  SITE  "27";
LOCATE  COMP  "nCRAS"  SITE  "43";
LOCATE  COMP  "nFWE"  SITE  "22";
LOCATE  COMP  "nRCAS"  SITE  "78";
LOCATE  COMP  "nRCS"  SITE  "77";
LOCATE  COMP  "nRRAS"  SITE  "73";
LOCATE  COMP  "nRWE"  SITE  "72";
LOCATE  COMP  "nUFMCS"  SITE  "53";





PAR: Place And Route Diamond (64-bit) 3.12.1.454.
Copyright (c) 1991-1994 by NeoCAD Inc. All rights reserved.
Copyright (c) 1995 AT&T Corp.   All rights reserved.
Copyright (c) 1995-2001 Lucent Technologies Inc.  All rights reserved.
Copyright (c) 2001 Agere Systems   All rights reserved.
Copyright (c) 2002-2020 Lattice Semiconductor Corporation,  All rights reserved.
Thu Sep 21 05:38:42 2023

