Loading design for application iotiming from file ram2gs_lcmxo2_1200hc_impl1.ncd.
Design name: RAM2GS
NCD version: 3.3
Vendor:      LATTICE
Device:      LCMXO2-1200HC
Package:     TQFP100
Performance: 5
Package Status:                     Final          Version 1.44.
Performance Hardware Data Status:   Final          Version 34.4.
Loading design for application iotiming from file ram2gs_lcmxo2_1200hc_impl1.ncd.
Design name: RAM2GS
NCD version: 3.3
Vendor:      LATTICE
Device:      LCMXO2-1200HC
Package:     TQFP100
Performance: 6
Package Status:                     Final          Version 1.44.
Performance Hardware Data Status:   Final          Version 34.4.
Loading design for application iotiming from file ram2gs_lcmxo2_1200hc_impl1.ncd.
Design name: RAM2GS
NCD version: 3.3
Vendor:      LATTICE
Device:      LCMXO2-1200HC
Package:     TQFP100
Performance: M
Package Status:                     Final          Version 1.44.
Performance Hardware Data Status:   Final          Version 34.4.
// Design: RAM2GS
// Package: TQFP100
// ncd File: ram2gs_lcmxo2_1200hc_impl1.ncd
// Version: Diamond (64-bit) 3.12.1.454
// Written on Thu Oct 19 23:51:14 2023
// M: Minimum Performance Grade
// iotiming RAM2GS_LCMXO2_1200HC_impl1.ncd RAM2GS_LCMXO2_1200HC_impl1.prf -gui -msgset //Mac/iCloud/Repos/RAM2GS/CPLD/LCMXO2-1200HC/promote.xml

I/O Timing Report (All units are in ns)

Worst Case Results across Performance Grades (M, 6, 5, 4):

// Input Setup and Hold Times

Port    Clock Edge  Setup Performance_Grade  Hold Performance_Grade
----------------------------------------------------------------------
CROW[0] nCRAS F     1.569      4       0.268     6
CROW[1] nCRAS F     1.013      4       0.820     4
Din[0]  PHI2  F     5.478      4       4.293     4
Din[0]  nCCAS F     2.010      4      -0.119     M
Din[1]  PHI2  F     4.088      4       4.173     4
Din[1]  nCCAS F     0.601      4       0.796     4
Din[2]  PHI2  F     4.967      4       4.173     4
Din[2]  nCCAS F     0.811      4       0.583     4
Din[3]  PHI2  F     3.810      4       4.173     4
Din[3]  nCCAS F     1.136      4       0.322     4
Din[4]  PHI2  F     4.400      4       4.173     4
Din[4]  nCCAS F     0.762      4       0.590     4
Din[5]  PHI2  F     5.595      4       4.173     4
Din[5]  nCCAS F     0.779      4       0.576     4
Din[6]  PHI2  F     5.120      4       4.293     4
Din[6]  nCCAS F     2.036      4      -0.117     M
Din[7]  PHI2  F     5.630      4       4.293     4
Din[7]  nCCAS F     2.301      4      -0.192     M
MAin[0] PHI2  F     4.196      4       1.086     4
MAin[0] nCRAS F     0.152      6       1.567     4
MAin[1] PHI2  F     3.875      4       1.164     4
MAin[1] nCRAS F    -0.177      M       2.102     4
MAin[2] PHI2  F     8.381      4      -0.693     M
MAin[2] nCRAS F    -0.315      M       2.358     4
MAin[3] PHI2  F     7.199      4      -0.405     M
MAin[3] nCRAS F    -0.173      M       1.962     4
MAin[4] PHI2  F     8.710      4      -0.769     M
MAin[4] nCRAS F     0.292      4       1.419     4
MAin[5] PHI2  F     8.562      4      -0.730     M
MAin[5] nCRAS F    -0.055      M       1.752     4
MAin[6] PHI2  F     7.862      4      -0.604     M
MAin[6] nCRAS F    -0.126      M       1.965     4
MAin[7] PHI2  F     8.829      4      -0.836     M
MAin[7] nCRAS F    -0.122      M       1.960     4
MAin[8] nCRAS F    -0.288      M       2.424     4
MAin[9] nCRAS F    -0.212      M       2.196     4
PHI2    RCLK  R    -0.133      M       2.360     4
nCCAS   RCLK  R     3.627      4      -0.577     M
nCCAS   nCRAS F     3.154      4      -0.145     M
nCRAS   RCLK  R     1.461      4      -0.017     M
nFWE    PHI2  F     6.933      4      -0.318     M
nFWE    nCRAS F     0.403      4       1.860     4


// Clock to Output Delay

Port    Clock Edge  Max_Delay Performance_Grade  Min_Delay Performance_Grade
------------------------------------------------------------------------
LED     RCLK  R    10.948         4        3.270          M
LED     nCRAS F    12.507         4        3.690          M
RA[0]   RCLK  R    13.208         4        4.000          M
RA[0]   nCRAS F    13.040         4        3.935          M
RA[10]  RCLK  R     7.888         4        2.711          M
RA[11]  PHI2  R     9.755         4        3.200          M
RA[1]   RCLK  R    13.332         4        4.024          M
RA[1]   nCRAS F    12.944         4        3.885          M
RA[2]   RCLK  R    13.624         4        4.099          M
RA[2]   nCRAS F    13.220         4        3.993          M
RA[3]   RCLK  R    13.506         4        4.055          M
RA[3]   nCRAS F    13.322         4        4.022          M
RA[4]   RCLK  R    12.512         4        3.834          M
RA[4]   nCRAS F    14.534         4        4.331          M
RA[5]   RCLK  R    13.530         4        4.069          M
RA[5]   nCRAS F    13.126         4        3.963          M
RA[6]   RCLK  R    14.238         4        4.245          M
RA[6]   nCRAS F    13.589         4        4.077          M
RA[7]   RCLK  R    13.759         4        4.129          M
RA[7]   nCRAS F    13.371         4        3.990          M
RA[8]   RCLK  R    11.858         4        3.632          M
RA[8]   nCRAS F    13.338         4        4.026          M
RA[9]   RCLK  R    11.007         4        3.423          M
RA[9]   nCRAS F    12.651         4        3.856          M
RBA[0]  nCRAS F    10.201         4        3.325          M
RBA[1]  nCRAS F    10.201         4        3.325          M
RCKE    RCLK  R     9.754         4        3.167          M
RCLKout RCLK  R     7.971         4        2.504          M
RDQMH   RCLK  R    11.153         4        3.458          M
RDQML   RCLK  R    11.133         4        3.466          M
RD[0]   nCCAS F     9.354         4        3.132          M
RD[1]   nCCAS F     9.354         4        3.132          M
RD[2]   nCCAS F     9.354         4        3.132          M
RD[3]   nCCAS F     9.354         4        3.132          M
RD[4]   nCCAS F     9.354         4        3.132          M
RD[5]   nCCAS F     9.354         4        3.132          M
RD[6]   nCCAS F     9.354         4        3.132          M
RD[7]   nCCAS F     9.354         4        3.132          M
nRCAS   RCLK  R     7.822         4        2.706          M
nRCS    RCLK  R     7.822         4        2.706          M
nRRAS   RCLK  R     7.822         4        2.706          M
nRWE    RCLK  R     7.803         4        2.713          M
WARNING: you must also run trce with hold speed: 4
WARNING: you must also run trce with setup speed: 6
WARNING: you must also run trce with hold speed: 6
WARNING: you must also run trce with setup speed: M
