# I/O Timing Report

    I/O Timing Report
    Loading design for application iotiming from file ram2gs_lcmxo2_1200hc_impl1.ncd.
    Design name: RAM2GS
    NCD version: 3.3
    Vendor:      LATTICE
    Device:      LCMXO2-1200HC
    Package:     TQFP100
    Performance: 5
    Package Status:                     Final          Version 1.44.
    Performance Hardware Data Status:   Final          Version 34.4.
    Loading design for application iotiming from file ram2gs_lcmxo2_1200hc_impl1.ncd.
    Design name: RAM2GS
    NCD version: 3.3
    Vendor:      LATTICE
    Device:      LCMXO2-1200HC
    Package:     TQFP100
    Performance: 6
    Package Status:                     Final          Version 1.44.
    Performance Hardware Data Status:   Final          Version 34.4.
    Loading design for application iotiming from file ram2gs_lcmxo2_1200hc_impl1.ncd.
    Design name: RAM2GS
    NCD version: 3.3
    Vendor:      LATTICE
    Device:      LCMXO2-1200HC
    Package:     TQFP100
    Performance: M
    Package Status:                     Final          Version 1.44.
    Performance Hardware Data Status:   Final          Version 34.4.
    // Design: RAM2GS
    // Package: TQFP100
    // ncd File: ram2gs_lcmxo2_1200hc_impl1.ncd
    // Version: Diamond (64-bit) 3.12.1.454
    // Written on Thu Oct 19 23:51:14 2023
    // M: Minimum Performance Grade
    // iotiming RAM2GS_LCMXO2_1200HC_impl1.ncd RAM2GS_LCMXO2_1200HC_impl1.prf -gui -msgset //Mac/iCloud/Repos/RAM2GS/CPLD/LCMXO2-1200HC/promote.xml

    I/O Timing Report (All units are in ns)

    Worst Case Results across Performance Grades (M, 6, 5, 4):

    // Input Setup and Hold Times

    Port    Clock Edge  Setup Performance_Grade  Hold Performance_Grade
    ----------------------------------------------------------------------
    CROW[0] nCRAS F     1.569      4       0.268     6
    CROW[1] nCRAS F     1.013      4       0.820     4
    Din[0]  PHI2  F     5.478      4       4.293     4
    Din[0]  nCCAS F     2.010      4      -0.119     M
    Din[1]  PHI2  F     4.088      4       4.173     4
    Din[1]  nCCAS F     0.601      4       0.796     4
    Din[2]  PHI2  F     4.967      4       4.173     4
    Din[2]  nCCAS F     0.811      4       0.583     4
    Din[3]  PHI2  F     3.810      4       4.173     4
    Din[3]  nCCAS F     1.136      4       0.322     4
    Din[4]  PHI2  F     4.400      4       4.173     4
    Din[4]  nCCAS F     0.762      4       0.590     4
    Din[5]  PHI2  F     5.595      4       4.173     4
    Din[5]  nCCAS F     0.779      4       0.576     4
    Din[6]  PHI2  F     5.120      4       4.293     4
    Din[6]  nCCAS F     2.036      4      -0.117     M
    Din[7]  PHI2  F     5.630      4       4.293     4
    Din[7]  nCCAS F     2.301      4      -0.192     M
    MAin[0] PHI2  F     4.196      4       1.086     4
    MAin[0] nCRAS F     0.152      6       1.567     4
    MAin[1] PHI2  F     3.875      4       1.164     4
    MAin[1] nCRAS F    -0.177      M       2.102     4
    MAin[2] PHI2  F     8.381      4      -0.693     M
    MAin[2] nCRAS F    -0.315      M       2.358     4
    MAin[3] PHI2  F     7.199      4      -0.405     M
    MAin[3] nCRAS F    -0.173      M       1.962     4
    MAin[4] PHI2  F     8.710      4      -0.769     M
    MAin[4] nCRAS F     0.292      4       1.419     4
    MAin[5] PHI2  F     8.562      4      -0.730     M
    MAin[5] nCRAS F    -0.055      M       1.752     4
    MAin[6] PHI2  F     7.862      4      -0.604     M
    MAin[6] nCRAS F    -0.126      M       1.965     4
    MAin[7] PHI2  F     8.829      4      -0.836     M
    MAin[7] nCRAS F    -0.122      M       1.960     4
    MAin[8] nCRAS F    -0.288      M       2.424     4
    MAin[9] nCRAS F    -0.212      M       2.196     4
    PHI2    RCLK  R    -0.133      M       2.360     4
    nCCAS   RCLK  R     3.627      4      -0.577     M
    nCCAS   nCRAS F     3.154      4      -0.145     M
    nCRAS   RCLK  R     1.461      4      -0.017     M
    nFWE    PHI2  F     6.933      4      -0.318     M
    nFWE    nCRAS F     0.403      4       1.860     4

    // Clock to Output Delay

    Port    Clock Edge  Max_Delay Performance_Grade  Min_Delay Performance_Grade
    ------------------------------------------------------------------------
    LED     RCLK  R    10.948         4        3.270          M
    LED     nCRAS F    12.507         4        3.690          M
    RA[0]   RCLK  R    13.208         4        4.000          M
    RA[0]   nCRAS F    13.040         4        3.935          M
    RA[10]  RCLK  R     7.888         4        2.711          M
    RA[11]  PHI2  R     9.755         4        3.200          M
    RA[1]   RCLK  R    13.332         4        4.024          M
    RA[1]   nCRAS F    12.944         4        3.885          M
    RA[2]   RCLK  R    13.624         4        4.099          M
    RA[2]   nCRAS F    13.220         4        3.993          M
    RA[3]   RCLK  R    13.506         4        4.055          M
    RA[3]   nCRAS F    13.322         4        4.022          M
    RA[4]   RCLK  R    12.512         4        3.834          M
    RA[4]   nCRAS F    14.534         4        4.331          M
    RA[5]   RCLK  R    13.530         4        4.069          M
    RA[5]   nCRAS F    13.126         4        3.963          M
    RA[6]   RCLK  R    14.238         4        4.245          M
    RA[6]   nCRAS F    13.589         4        4.077          M
    RA[7]   RCLK  R    13.759         4        4.129          M
    RA[7]   nCRAS F    13.371         4        3.990          M
    RA[8]   RCLK  R    11.858         4        3.632          M
    RA[8]   nCRAS F    13.338         4        4.026          M
    RA[9]   RCLK  R    11.007         4        3.423          M
    RA[9]   nCRAS F    12.651         4        3.856          M
    RBA[0]  nCRAS F    10.201         4        3.325          M
    RBA[1]  nCRAS F    10.201         4        3.325          M
    RCKE    RCLK  R     9.754         4        3.167          M
    RCLKout RCLK  R     7.971         4        2.504          M
    RDQMH   RCLK  R    11.153         4        3.458          M
    RDQML   RCLK  R    11.133         4        3.466          M
    RD[0]   nCCAS F     9.354         4        3.132          M
    RD[1]   nCCAS F     9.354         4        3.132          M
    RD[2]   nCCAS F     9.354         4        3.132          M
    RD[3]   nCCAS F     9.354         4        3.132          M
    RD[4]   nCCAS F     9.354         4        3.132          M
    RD[5]   nCCAS F     9.354         4        3.132          M
    RD[6]   nCCAS F     9.354         4        3.132          M
    RD[7]   nCCAS F     9.354         4        3.132          M
    nRCAS   RCLK  R     7.822         4        2.706          M
    nRCS    RCLK  R     7.822         4        2.706          M
    nRRAS   RCLK  R     7.822         4        2.706          M
    nRWE    RCLK  R     7.803         4        2.713          M
    WARNING: you must also run trce with hold speed: 4
    WARNING: you must also run trce with setup speed: 6
    WARNING: you must also run trce with hold speed: 6
    WARNING: you must also run trce with setup speed: M