# I/O Timing Report

    I/O Timing Report
    Loading design for application iotiming from file ram2gs_lcmxo640c_impl1.ncd.
    Design name: RAM2GS
    NCD version: 3.3
    Vendor:      LATTICE
    Device:      LCMXO640C
    Package:     TQFP100
    Performance: 4
    Package Status:                     Final          Version 1.17.
    Performance Hardware Data Status: Version 1.124.
    Loading design for application iotiming from file ram2gs_lcmxo640c_impl1.ncd.
    Design name: RAM2GS
    NCD version: 3.3
    Vendor:      LATTICE
    Device:      LCMXO640C
    Package:     TQFP100
    Performance: 5
    Package Status:                     Final          Version 1.17.
    Performance Hardware Data Status: Version 1.124.
    Loading design for application iotiming from file ram2gs_lcmxo640c_impl1.ncd.
    Design name: RAM2GS
    NCD version: 3.3
    Vendor:      LATTICE
    Device:      LCMXO640C
    Package:     TQFP100
    Performance: M
    Package Status:                     Final          Version 1.17.
    Performance Hardware Data Status: Version 1.124.
    // Design: RAM2GS
    // Package: TQFP100
    // ncd File: ram2gs_lcmxo640c_impl1.ncd
    // Version: Diamond (64-bit) 3.12.1.454
    // Written on Thu Sep 21 05:38:44 2023
    // M: Minimum Performance Grade
    // iotiming RAM2GS_LCMXO640C_impl1.ncd RAM2GS_LCMXO640C_impl1.prf -gui -msgset //Mac/iCloud/Repos/RAM2GS/CPLD/LCMXO640C/promote.xml

    I/O Timing Report (All units are in ns)

    Worst Case Results across Performance Grades (M, 5, 4, 3):

    // Input Setup and Hold Times

    Port    Clock Edge  Setup Performance_Grade  Hold Performance_Grade
    ----------------------------------------------------------------------
    CROW[0] nCRAS F    -0.012      M       2.299     3
    CROW[1] nCRAS F    -0.094      M       2.568     3
    Din[0]  PHI2  F     5.117      3       2.324     3
    Din[0]  nCCAS F     1.863      3      -0.129     M
    Din[1]  PHI2  F     4.727      3       3.095     3
    Din[1]  nCCAS F     0.973      3       0.261     3
    Din[2]  PHI2  F     4.040      3       2.270     3
    Din[2]  nCCAS F     1.372      3      -0.027     M
    Din[3]  PHI2  F     4.809      3       1.454     3
    Din[3]  nCCAS F     0.916      3       0.298     3
    Din[4]  PHI2  F     6.041      3       2.279     3
    Din[4]  nCCAS F     1.531      3      -0.100     M
    Din[5]  PHI2  F     5.903      3       2.260     3
    Din[5]  nCCAS F     2.338      3      -0.268     M
    Din[6]  PHI2  F     6.028      3       1.422     3
    Din[6]  nCCAS F     1.099      3       0.266     3
    Din[7]  PHI2  F     6.673      3       2.385     3
    Din[7]  nCCAS F     0.940      3       0.417     3
    MAin[0] PHI2  F     4.543      3       0.820     3
    MAin[0] nCRAS F    -0.219      M       3.000     3
    MAin[1] PHI2  F     4.179      3       1.515     3
    MAin[1] nCRAS F    -0.122      M       2.681     3
    MAin[2] PHI2  F     9.178      3      -0.474     M
    MAin[2] nCRAS F    -0.219      M       3.000     3
    MAin[3] PHI2  F     9.642      3      -0.572     M
    MAin[3] nCRAS F    -0.200      M       2.949     3
    MAin[4] PHI2  F     9.311      3      -0.515     M
    MAin[4] nCRAS F     0.454      3       1.905     3
    MAin[5] PHI2  F     8.033      3      -0.256     M
    MAin[5] nCRAS F    -0.214      M       2.985     3
    MAin[6] PHI2  F     8.467      3      -0.339     M
    MAin[6] nCRAS F     0.019      3       2.253     3
    MAin[7] PHI2  F     8.283      3      -0.303     M
    MAin[7] nCRAS F    -0.200      M       2.949     3
    MAin[8] nCRAS F    -0.239      M       3.098     3
    MAin[9] nCRAS F    -0.200      M       2.952     3
    PHI2    RCLK  R     2.024      3      -0.115     M
    UFMSDO  RCLK  R     2.747      3      -0.023     M
    nCCAS   RCLK  R     1.461      3       0.049     3
    nCCAS   nCRAS F     0.041      3       2.233     3
    nCRAS   RCLK  R     1.492      3       0.026     3
    nFWE    PHI2  F     9.958      3      -0.643     M
    nFWE    nCRAS F    -0.200      M       2.952     3

    // Clock to Output Delay

    Port   Clock Edge  Max_Delay Performance_Grade  Min_Delay Performance_Grade
    ------------------------------------------------------------------------
    LED    RCLK  R    13.643         3        4.416          M
    LED    nCRAS F    18.132         3        5.318          M
    RA[0]  RCLK  R    10.790         3        2.216          M
    RA[0]  nCRAS F    13.344         3        2.709          M
    RA[10] RCLK  R     6.926         3        1.431          M
    RA[11] PHI2  R     9.183         3        1.867          M
    RA[1]  RCLK  R    11.242         3        2.314          M
    RA[1]  nCRAS F    14.215         3        2.899          M
    RA[2]  RCLK  R    10.691         3        2.207          M
    RA[2]  nCRAS F    13.021         3        2.641          M
    RA[3]  RCLK  R    11.553         3        2.371          M
    RA[3]  nCRAS F    13.307         3        2.703          M
    RA[4]  RCLK  R    10.653         3        2.186          M
    RA[4]  nCRAS F    12.915         3        2.624          M
    RA[5]  RCLK  R    11.976         3        2.463          M
    RA[5]  nCRAS F    13.269         3        2.696          M
    RA[6]  RCLK  R     9.986         3        2.078          M
    RA[6]  nCRAS F    12.404         3        2.531          M
    RA[7]  RCLK  R    10.257         3        2.107          M
    RA[7]  nCRAS F    12.647         3        2.563          M
    RA[8]  RCLK  R    11.577         3        2.383          M
    RA[8]  nCRAS F    13.570         3        2.740          M
    RA[9]  RCLK  R    11.562         3        2.371          M
    RA[9]  nCRAS F    14.266         3        2.895          M
    RBA[0] nCRAS F    10.698         3        2.157          M
    RBA[1] nCRAS F    12.177         3        2.478          M
    RCKE   RCLK  R     6.926         3        1.431          M
    RDQMH  RCLK  R    11.068         3        2.337          M
    RDQML  RCLK  R    11.619         3        2.421          M
    RD[0]  nCCAS F     8.787         3        1.927          M
    RD[1]  nCCAS F     8.785         3        1.927          M
    RD[2]  nCCAS F     8.076         3        1.799          M
    RD[3]  nCCAS F     9.246         3        2.027          M
    RD[4]  nCCAS F     9.626         3        2.112          M
    RD[5]  nCCAS F     9.183         3        2.015          M
    RD[6]  nCCAS F     8.537         3        1.898          M
    RD[7]  nCCAS F     9.704         3        2.117          M
    UFMCLK RCLK  R     8.800         3        1.847          M
    UFMSDI RCLK  R     8.079         3        1.714          M
    nRCAS  RCLK  R     6.926         3        1.431          M
    nRCS   RCLK  R     7.765         3        1.590          M
    nRRAS  RCLK  R     8.554         3        1.749          M
    nRWE   RCLK  R     8.704         3        1.789          M
    nUFMCS RCLK  R     9.262         3        1.937          M
    WARNING: you must also run trce with hold speed: 3
    WARNING: you must also run trce with setup speed: M