#Build: Synplify Pro (R) R-2021.03L-SP1, Build 093R, Aug 10 2021
#install: C:\lscc\diamond\3.12\synpbase
#OS: Windows 8 6.2
#Hostname: ZANEMACWIN11

# Thu Sep 21 05:39:33 2023

#Implementation: impl1


Copyright (C) 1994-2021 Synopsys, Inc.
This Synopsys software and all associated documentation are proprietary to Synopsys, Inc.
and may only be used pursuant to the terms and conditions of a written license agreement
with Synopsys, Inc. All other use, reproduction, modification, or distribution of the
Synopsys software or the associated documentation is strictly prohibited.
Tool: Synplify Pro (R)
Build: R-2021.03L-SP1
Install: C:\lscc\diamond\3.12\synpbase
OS: Windows 6.2

Hostname: ZANEMACWIN11

Implementation : impl1
Synopsys HDL Compiler, Version comp202103synp2, Build 093R, Built Aug 10 2021 09:15:36, @

@N|Running in 64-bit mode
###########################################################[

Copyright (C) 1994-2021 Synopsys, Inc.
This Synopsys software and all associated documentation are proprietary to Synopsys, Inc.
and may only be used pursuant to the terms and conditions of a written license agreement
with Synopsys, Inc. All other use, reproduction, modification, or distribution of the
Synopsys software or the associated documentation is strictly prohibited.
Tool: Synplify Pro (R)
Build: R-2021.03L-SP1
Install: C:\lscc\diamond\3.12\synpbase
OS: Windows 6.2

Hostname: ZANEMACWIN11

Implementation : impl1
Synopsys Verilog Compiler, Version comp202103synp2, Build 093R, Built Aug 10 2021 09:15:36, @

@N|Running in 64-bit mode
@I::"C:\lscc\diamond\3.12\synpbase\lib\lucent\machxo2.v" (library work)
@I::"C:\lscc\diamond\3.12\synpbase\lib\lucent\pmi_def.v" (library work)
@I::"C:\lscc\diamond\3.12\synpbase\lib\vlog\hypermods.v" (library __hyper__lib__)
@I::"C:\lscc\diamond\3.12\synpbase\lib\vlog\umr_capim.v" (library snps_haps)
@I::"C:\lscc\diamond\3.12\synpbase\lib\vlog\scemi_objects.v" (library snps_haps)
@I::"C:\lscc\diamond\3.12\synpbase\lib\vlog\scemi_pipes.svh" (library snps_haps)
@I::"\\Mac\iCloud\Repos\RAM2GS\CPLD\RAM2GS-LCMXO2.v" (library work)
@I::"\\Mac\iCloud\Repos\RAM2GS\CPLD\LCMXO2-640HC\REFB.v" (library work)
Verilog syntax check successful!
Selecting top level module RAM2GS
@N: CG364 :"C:\lscc\diamond\3.12\synpbase\lib\lucent\machxo2.v":1120:7:1120:9|Synthesizing module VHI in library work.
Running optimization stage 1 on VHI .......
Finished optimization stage 1 on VHI (CPU Time 0h:00m:00s, Memory Used current: 98MB peak: 98MB)
@N: CG364 :"C:\lscc\diamond\3.12\synpbase\lib\lucent\machxo2.v":1124:7:1124:9|Synthesizing module VLO in library work.
Running optimization stage 1 on VLO .......
Finished optimization stage 1 on VLO (CPU Time 0h:00m:00s, Memory Used current: 98MB peak: 99MB)
@N: CG364 :"C:\lscc\diamond\3.12\synpbase\lib\lucent\machxo2.v":1800:7:1800:9|Synthesizing module EFB in library work.
Running optimization stage 1 on EFB .......
Finished optimization stage 1 on EFB (CPU Time 0h:00m:00s, Memory Used current: 99MB peak: 99MB)
@N: CG364 :"\\Mac\iCloud\Repos\RAM2GS\CPLD\LCMXO2-640HC\REFB.v":8:7:8:10|Synthesizing module REFB in library work.
Running optimization stage 1 on REFB .......
Finished optimization stage 1 on REFB (CPU Time 0h:00m:00s, Memory Used current: 99MB peak: 99MB)
@N: CG364 :"\\Mac\iCloud\Repos\RAM2GS\CPLD\RAM2GS-LCMXO2.v":1:7:1:12|Synthesizing module RAM2GS in library work.
Running optimization stage 1 on RAM2GS .......
Finished optimization stage 1 on RAM2GS (CPU Time 0h:00m:00s, Memory Used current: 101MB peak: 101MB)
Running optimization stage 2 on RAM2GS .......
Finished optimization stage 2 on RAM2GS (CPU Time 0h:00m:00s, Memory Used current: 102MB peak: 102MB)
Running optimization stage 2 on REFB .......
Finished optimization stage 2 on REFB (CPU Time 0h:00m:00s, Memory Used current: 102MB peak: 102MB)
Running optimization stage 2 on EFB .......
Finished optimization stage 2 on EFB (CPU Time 0h:00m:00s, Memory Used current: 102MB peak: 102MB)
Running optimization stage 2 on VLO .......
Finished optimization stage 2 on VLO (CPU Time 0h:00m:00s, Memory Used current: 102MB peak: 102MB)
Running optimization stage 2 on VHI .......
Finished optimization stage 2 on VHI (CPU Time 0h:00m:00s, Memory Used current: 102MB peak: 102MB)

At c_ver Exit (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 101MB peak: 102MB)

Process took 0h:00m:01s realtime, 0h:00m:01s cputime

Process completed successfully.
# Thu Sep 21 05:39:33 2023

###########################################################]
###########################################################[

Copyright (C) 1994-2021 Synopsys, Inc.
This Synopsys software and all associated documentation are proprietary to Synopsys, Inc.
and may only be used pursuant to the terms and conditions of a written license agreement
with Synopsys, Inc. All other use, reproduction, modification, or distribution of the
Synopsys software or the associated documentation is strictly prohibited.
Tool: Synplify Pro (R)
Build: R-2021.03L-SP1
Install: C:\lscc\diamond\3.12\synpbase
OS: Windows 6.2

Hostname: ZANEMACWIN11

Implementation : impl1
Synopsys Synopsys Netlist Linker, Version comp202103synp2, Build 093R, Built Aug 10 2021 09:15:36, @

@N|Running in 64-bit mode

At syn_nfilter Exit (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 98MB peak: 98MB)

Process took 0h:00m:01s realtime, 0h:00m:01s cputime

Process completed successfully.
# Thu Sep 21 05:39:34 2023

###########################################################]

For a summary of runtime and memory usage for all design units, please see file:
==========================================================
@L: A:\\Mac\iCloud\Repos\RAM2GS\CPLD\LCMXO2-640HC\impl1\synwork\RAM2GS_LCMXO2_640HC_impl1_comp.rt.csv

@END

At c_hdl Exit (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 30MB peak: 31MB)

Process took 0h:00m:01s realtime, 0h:00m:01s cputime

Process completed successfully.
# Thu Sep 21 05:39:34 2023

###########################################################]
###########################################################[

Copyright (C) 1994-2021 Synopsys, Inc.
This Synopsys software and all associated documentation are proprietary to Synopsys, Inc.
and may only be used pursuant to the terms and conditions of a written license agreement
with Synopsys, Inc. All other use, reproduction, modification, or distribution of the
Synopsys software or the associated documentation is strictly prohibited.
Tool: Synplify Pro (R)
Build: R-2021.03L-SP1
Install: C:\lscc\diamond\3.12\synpbase
OS: Windows 6.2

Hostname: ZANEMACWIN11

Implementation : impl1
Synopsys Synopsys Netlist Linker, Version comp202103synp2, Build 093R, Built Aug 10 2021 09:15:36, @

@N|Running in 64-bit mode

At syn_nfilter Exit (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 98MB peak: 99MB)

Process took 0h:00m:01s realtime, 0h:00m:01s cputime

Process completed successfully.
# Thu Sep 21 05:39:35 2023

###########################################################]
Premap Report

# Thu Sep 21 05:39:35 2023


Copyright (C) 1994-2021 Synopsys, Inc.
This Synopsys software and all associated documentation are proprietary to Synopsys, Inc.
and may only be used pursuant to the terms and conditions of a written license agreement
with Synopsys, Inc. All other use, reproduction, modification, or distribution of the
Synopsys software or the associated documentation is strictly prohibited.
Tool: Synplify Pro (R)
Build: R-2021.03L-SP1
Install: C:\lscc\diamond\3.12\synpbase
OS: Windows 6.2

Hostname: ZANEMACWIN11

Implementation : impl1
Synopsys Lattice Technology Pre-mapping, Version map202103lat, Build 070R, Built Oct  6 2021 11:12:38, @


Mapper Startup Complete (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 128MB peak: 128MB)


Done reading skeleton netlist (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 131MB peak: 140MB)

Reading constraint file: \\Mac\iCloud\Repos\RAM2GS\CPLD\RAM2GS.sdc
@L: \\Mac\iCloud\Repos\RAM2GS\CPLD\LCMXO2-640HC\impl1\RAM2GS_LCMXO2_640HC_impl1_scck.rpt 
See clock summary report "\\Mac\iCloud\Repos\RAM2GS\CPLD\LCMXO2-640HC\impl1\RAM2GS_LCMXO2_640HC_impl1_scck.rpt"
@N: MF916 |Option synthesis_strategy=base is enabled. 
@N: MF248 |Running in 64-bit mode.
@N: MF666 |Clock conversion enabled. (Command "set_option -fix_gated_and_generated_clocks 1" in the project file.)

Design Input Complete (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 136MB peak: 140MB)


Mapper Initialization Complete (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 136MB peak: 140MB)


Start loading timing files (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 149MB peak: 149MB)


Finished loading timing files (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 150MB peak: 151MB)

@N: FX493 |Applying initial value "0" on instance InitReady.
@W: FX474 |User-specified initial value defined for some sequential elements which can prevent optimum synthesis results from being achieved. 
@N: FX493 |Applying initial value "0" on instance Ready.
@N: FX493 |Applying initial value "0" on instance RCKE.
@N: FX493 |Applying initial value "0" on instance LEDEN.
@N: FX493 |Applying initial value "0" on instance n8MEGEN.
@N: FX493 |Applying initial value "1" on instance nRCAS.
@N: FX493 |Applying initial value "0" on instance CmdLEDEN.
@N: FX493 |Applying initial value "0" on instance CmdUFMShift.
@N: FX493 |Applying initial value "0" on instance CmdUFMWrite.
@N: FX493 |Applying initial value "0" on instance Cmdn8MEGEN.
@N: FX493 |Applying initial value "0" on instance CmdValid.
@N: FX493 |Applying initial value "1" on instance nRCS.
@N: FX493 |Applying initial value "1" on instance nRRAS.
@N: FX493 |Applying initial value "0" on instance CmdUFMData.
@N: FX493 |Applying initial value "0" on instance C1Submitted.
@N: FX493 |Applying initial value "0" on instance ADSubmitted.
@N: FX493 |Applying initial value "0" on instance XOR8MEG.
@N: FX493 |Applying initial value "0" on instance CmdEnable.
@N: FX493 |Applying initial value "1" on instance nRWE.

Starting clock optimization phase (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 181MB peak: 181MB)


Finished clock optimization phase (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 181MB peak: 181MB)


Starting clock optimization report phase (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 181MB peak: 182MB)


Finished clock optimization report phase (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 182MB peak: 182MB)

@N: FX1184 |Applying syn_allowed_resources blockrams=2 on top level netlist RAM2GS 

Finished netlist restructuring (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 182MB peak: 182MB)



Clock Summary
******************

          Start      Requested     Requested     Clock        Clock                Clock
Level     Clock      Frequency     Period        Type         Group                Load 
----------------------------------------------------------------------------------------
0 -       RCLK       62.5 MHz      16.000        declared     default_clkgroup     65   
                                                                                        
0 -       PHI2       2.9 MHz       350.000       declared     default_clkgroup     19   
                                                                                        
0 -       nCRAS      2.9 MHz       350.000       declared     default_clkgroup     14   
                                                                                        
0 -       nCCAS      2.9 MHz       350.000       declared     default_clkgroup     8    
                                                                                        
0 -       System     100.0 MHz     10.000        system       system_clkgroup      0    
========================================================================================



Clock Load Summary
***********************

           Clock     Source          Clock Pin       Non-clock Pin     Non-clock Pin     
Clock      Load      Pin             Seq Example     Seq Example       Comb Example      
-----------------------------------------------------------------------------------------
RCLK       65        RCLK(port)      CASr2.C         -                 -                 
                                                                                         
PHI2       19        PHI2(port)      Bank[7:0].C     PHI2r.D[0]        un1_PHI2.I[0](inv)
                                                                                         
nCRAS      14        nCRAS(port)     CBR.C           RASr.D[0]         RASr_2.I[0](inv)  
                                                                                         
nCCAS      8         nCCAS(port)     WRD[7:0].C      CASr.D[0]         CASr_2.I[0](inv)  
                                                                                         
System     0         -               -               -                 -                 
=========================================================================================

ICG Latch Removal Summary:
Number of ICG latches removed: 0
Number of ICG latches not removed:	0
For details review file gcc_ICG_report.rpt


@S |Clock Optimization Summary



#### START OF PREMAP CLOCK OPTIMIZATION REPORT #####[

4 non-gated/non-generated clock tree(s) driving 106 clock pin(s) of sequential element(s)
0 gated/generated clock tree(s) driving 0 clock pin(s) of sequential element(s)
0 instances converted, 0 sequential instances remain driven by gated/generated clocks

=========================== Non-Gated/Non-Generated Clocks ============================
Clock Tree ID     Driving Element     Drive Element Type     Fanout     Sample Instance
---------------------------------------------------------------------------------------
@KP:ckid0_0       RCLK                port                   65         nRWE           
@KP:ckid0_1       PHI2                port                   19         RA11           
@KP:ckid0_2       nCCAS               port                   8          WRD[7:0]       
@KP:ckid0_3       nCRAS               port                   14         RowA[9:0]      
=======================================================================================


##### END OF CLOCK OPTIMIZATION REPORT ######

@N: FX1143 |Skipping assigning INTERNAL_VREF to iobanks, because the table of mapping from pin to iobank is not initialized.
Finished Pre Mapping Phase.

Starting constraint checker (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 182MB peak: 182MB)


Finished constraint checker preprocessing (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 182MB peak: 182MB)


Finished constraint checker (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 183MB peak: 183MB)

Pre-mapping successful!

At Mapper Exit (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 103MB peak: 185MB)

Process took 0h:00m:01s realtime, 0h:00m:01s cputime
# Thu Sep 21 05:39:37 2023

###########################################################]
Map & Optimize Report

# Thu Sep 21 05:39:37 2023


Copyright (C) 1994-2021 Synopsys, Inc.
This Synopsys software and all associated documentation are proprietary to Synopsys, Inc.
and may only be used pursuant to the terms and conditions of a written license agreement
with Synopsys, Inc. All other use, reproduction, modification, or distribution of the
Synopsys software or the associated documentation is strictly prohibited.
Tool: Synplify Pro (R)
Build: R-2021.03L-SP1
Install: C:\lscc\diamond\3.12\synpbase
OS: Windows 6.2

Hostname: ZANEMACWIN11

Implementation : impl1
Synopsys Lattice Technology Mapper, Version map202103lat, Build 070R, Built Oct  6 2021 11:12:38, @


Mapper Startup Complete (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 127MB peak: 127MB)

@N: MF916 |Option synthesis_strategy=base is enabled. 
@N: MF248 |Running in 64-bit mode.
@N: MF666 |Clock conversion enabled. (Command "set_option -fix_gated_and_generated_clocks 1" in the project file.)

Design Input Complete (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 129MB peak: 139MB)


Mapper Initialization Complete (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 129MB peak: 139MB)


Start loading timing files (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 143MB peak: 143MB)


Finished loading timing files (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 145MB peak: 146MB)



Starting Optimization and Mapping (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 179MB peak: 179MB)


Finished RTL optimizations (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 183MB peak: 183MB)

@N: MO231 :"\\mac\icloud\repos\ram2gs\cpld\ram2gs-lcmxo2.v":163:4:163:9|Found counter in view:work.RAM2GS(verilog) instance IS[3:0] 
@N: MO231 :"\\mac\icloud\repos\ram2gs\cpld\ram2gs-lcmxo2.v":150:4:150:9|Found counter in view:work.RAM2GS(verilog) instance FS[17:0] 
@N: FX493 |Applying initial value "0" on instance IS[0].
@W: FX474 |User-specified initial value defined for some sequential elements which can prevent optimum synthesis results from being achieved. 
@N: FX493 |Applying initial value "0" on instance IS[1].
@N: FX493 |Applying initial value "0" on instance IS[2].
@N: FX493 |Applying initial value "0" on instance IS[3].

Starting factoring (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:00s; Memory used current: 185MB peak: 185MB)


Finished factoring (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 187MB peak: 187MB)


Available hyper_sources - for debug and ip models
	None Found


Finished generic timing optimizations - Pass 1 (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 187MB peak: 187MB)


Starting Early Timing Optimization (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 187MB peak: 187MB)


Finished Early Timing Optimization (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 187MB peak: 187MB)


Finished generic timing optimizations - Pass 2 (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 188MB peak: 188MB)


Finished preparing to map (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 188MB peak: 188MB)


Finished technology mapping (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 197MB peak: 197MB)

Pass		 CPU time		Worst Slack		Luts / Registers
------------------------------------------------------------
   1		0h:00m:01s		    -2.98ns		 201 /       106
   2		0h:00m:01s		    -2.98ns		 217 /       106
   3		0h:00m:01s		    -2.76ns		 215 /       106
@N: FX271 :"\\mac\icloud\repos\ram2gs\cpld\ram2gs-lcmxo2.v":121:4:121:9|Replicating instance CBR (in view: work.RAM2GS(verilog)) with 6 loads 1 time to improve timing.
@N: FX271 :"\\mac\icloud\repos\ram2gs\cpld\ram2gs-lcmxo2.v":304:4:304:9|Replicating instance CmdValid (in view: work.RAM2GS(verilog)) with 4 loads 1 time to improve timing.
@N: FX271 :"\\mac\icloud\repos\ram2gs\cpld\ram2gs-lcmxo2.v":163:4:163:9|Replicating instance Ready (in view: work.RAM2GS(verilog)) with 11 loads 1 time to improve timing.
Timing driven replication report
Added 3 Registers via timing driven replication
Added 1 LUTs via timing driven replication

   4		0h:00m:02s		    -1.97ns		 220 /       109


   5		0h:00m:02s		    -1.97ns		 220 /       109

Finished technology timing optimizations and critical path resynthesis (Real Time elapsed 0h:00m:02s; CPU Time elapsed 0h:00m:02s; Memory used current: 197MB peak: 197MB)

@N: FX164 |The option to pack registers in the IOB has not been specified. Please set syn_useioff attribute.  

Finished restoring hierarchy (Real Time elapsed 0h:00m:02s; CPU Time elapsed 0h:00m:02s; Memory used current: 198MB peak: 198MB)


Start Writing Netlists (Real Time elapsed 0h:00m:02s; CPU Time elapsed 0h:00m:02s; Memory used current: 160MB peak: 198MB)

Writing Analyst data base \\Mac\iCloud\Repos\RAM2GS\CPLD\LCMXO2-640HC\impl1\synwork\RAM2GS_LCMXO2_640HC_impl1_m.srm

Finished Writing Netlist Databases (Real Time elapsed 0h:00m:03s; CPU Time elapsed 0h:00m:03s; Memory used current: 198MB peak: 198MB)

Writing EDIF Netlist and constraint files
@N: FX1056 |Writing EDF file: \\Mac\iCloud\Repos\RAM2GS\CPLD\LCMXO2-640HC\impl1\RAM2GS_LCMXO2_640HC_impl1.edi
@N: BW106 |Synplicity Constraint File capacitance units using default value of 1pF 

Finished Writing EDIF Netlist and constraint files (Real Time elapsed 0h:00m:04s; CPU Time elapsed 0h:00m:03s; Memory used current: 203MB peak: 203MB)


Finished Writing Netlists (Real Time elapsed 0h:00m:04s; CPU Time elapsed 0h:00m:04s; Memory used current: 203MB peak: 203MB)


Start final timing analysis (Real Time elapsed 0h:00m:04s; CPU Time elapsed 0h:00m:04s; Memory used current: 201MB peak: 203MB)

@W: MT246 :"\\mac\icloud\repos\ram2gs\cpld\lcmxo2-640hc\refb.v":78:8:78:16|Blackbox EFB is missing a user supplied timing model. This may have a negative effect on timing analysis and optimizations (Quality of Results)
@N: MT615 |Found clock RCLK with period 16.00ns 
@N: MT615 |Found clock PHI2 with period 350.00ns 
@N: MT615 |Found clock nCRAS with period 350.00ns 
@N: MT615 |Found clock nCCAS with period 350.00ns 


##### START OF TIMING REPORT #####[
# Timing report written on Thu Sep 21 05:39:41 2023
#


Top view:               RAM2GS
Requested Frequency:    2.9 MHz
Wire load mode:         top
Paths requested:        5
Constraint File(s):    \\Mac\iCloud\Repos\RAM2GS\CPLD\RAM2GS.sdc
                       
@N: MT320 |This timing report is an estimate of place and route data. For final timing results, use the FPGA vendor place and route report.

@N: MT322 |Clock constraints include only register-to-register paths associated with each individual clock.



Performance Summary
*******************


Worst slack in design: -2.605

                   Requested     Estimated     Requested     Estimated                Clock        Clock           
Starting Clock     Frequency     Frequency     Period        Period        Slack      Type         Group           
-------------------------------------------------------------------------------------------------------------------
PHI2               2.9 MHz       1.0 MHz       350.000       989.870       -1.828     declared     default_clkgroup
RCLK               62.5 MHz      17.3 MHz      16.000        57.686        -0.784     declared     default_clkgroup
nCCAS              2.9 MHz       NA            350.000       NA            NA         declared     default_clkgroup
nCRAS              2.9 MHz       0.8 MHz       350.000       1261.890      -2.605     declared     default_clkgroup
System             100.0 MHz     NA            10.000        NA            12.918     system       system_clkgroup 
===================================================================================================================
Estimated period and frequency reported as NA means no slack depends directly on the clock waveform


@W: MT117 |Paths from clock (RCLK:r) to clock (PHI2:f) are overconstrained because the required time of 1.00 ns is too small.  
@W: MT118 |Paths from clock (nCRAS:f) to clock (RCLK:r) are overconstrained because the required time of 1.00 ns is too small.  
@W: MT118 |Paths from clock (PHI2:f) to clock (RCLK:r) are overconstrained because the required time of 1.00 ns is too small.  
@W: MT116 |Paths from clock (RCLK:r) to clock (PHI2:r) are overconstrained because the required time of 2.00 ns is too small.  
@W: MT117 |Paths from clock (RCLK:r) to clock (nCRAS:f) are overconstrained because the required time of 1.00 ns is too small.  



Clock Relationships
*******************

Clocks            |    rise  to  rise    |    fall  to  fall     |    rise  to  fall     |    fall  to  rise   
---------------------------------------------------------------------------------------------------------------
Starting  Ending  |  constraint  slack   |  constraint  slack    |  constraint  slack    |  constraint  slack  
---------------------------------------------------------------------------------------------------------------
System    RCLK    |  16.000      12.918  |  No paths    -        |  No paths    -        |  No paths    -      
RCLK      System  |  16.000      14.956  |  No paths    -        |  No paths    -        |  No paths    -      
RCLK      RCLK    |  16.000      9.040   |  No paths    -        |  No paths    -        |  No paths    -      
RCLK      PHI2    |  2.000       0.216   |  No paths    -        |  1.000       -0.676   |  No paths    -      
RCLK      nCRAS   |  No paths    -       |  No paths    -        |  1.000       -0.784   |  No paths    -      
PHI2      RCLK    |  No paths    -       |  No paths    -        |  No paths    -        |  1.000       -1.828 
PHI2      PHI2    |  No paths    -       |  350.000     346.603  |  175.000     169.081  |  175.000     173.428
nCRAS     RCLK    |  No paths    -       |  No paths    -        |  No paths    -        |  1.000       -2.605 
===============================================================================================================
 Note: 'No paths' indicates there are no paths in the design for that pair of clock edges.
       'Diff grp' indicates that paths exist but the starting clock and ending clock are in different clock groups.



Interface Information 
*********************

No IO constraint found



====================================
Detailed Report for Clock: PHI2
====================================



Starting Points with Worst Slack
********************************

                  Starting                                             Arrival            
Instance          Reference     Type         Pin     Net               Time        Slack  
                  Clock                                                                   
------------------------------------------------------------------------------------------
CmdUFMShift       PHI2          FD1P3AX      Q       CmdUFMShift       1.044       -1.828 
CmdValid_fast     PHI2          FD1S3AX      Q       CmdValid_fast     0.972       -1.756 
CmdValid          PHI2          FD1S3AX      Q       CmdValid          1.108       -1.725 
CmdLEDEN          PHI2          FD1P3AX      Q       CmdLEDEN          1.044       -1.589 
Cmdn8MEGEN        PHI2          FD1P3AX      Q       Cmdn8MEGEN        1.044       -1.589 
CmdUFMWrite       PHI2          FD1P3AX      Q       CmdUFMWrite       1.044       -0.572 
CmdUFMData        PHI2          FD1P3AX      Q       CmdUFMData        0.972       -0.500 
Bank_0io[0]       PHI2          IFS1P3DX     Q       Bank[0]           0.972       169.081
Bank_0io[1]       PHI2          IFS1P3DX     Q       Bank[1]           0.972       169.081
Bank_0io[2]       PHI2          IFS1P3DX     Q       Bank[2]           0.972       169.081
==========================================================================================


Ending Points with Worst Slack
******************************

               Starting                                               Required           
Instance       Reference     Type        Pin     Net                  Time         Slack 
               Clock                                                                     
-----------------------------------------------------------------------------------------
wb_adr[0]      PHI2          FD1P3AX     SP      un1_wb_rst14_i_0     0.528        -1.828
wb_adr[1]      PHI2          FD1P3AX     SP      un1_wb_rst14_i_0     0.528        -1.828
wb_adr[2]      PHI2          FD1P3AX     SP      un1_wb_rst14_i_0     0.528        -1.828
wb_adr[3]      PHI2          FD1P3AX     SP      un1_wb_rst14_i_0     0.528        -1.828
wb_adr[4]      PHI2          FD1P3AX     SP      un1_wb_rst14_i_0     0.528        -1.828
wb_adr[5]      PHI2          FD1P3AX     SP      un1_wb_rst14_i_0     0.528        -1.828
wb_adr[6]      PHI2          FD1P3AX     SP      un1_wb_rst14_i_0     0.528        -1.828
wb_adr[7]      PHI2          FD1P3AX     SP      un1_wb_rst14_i_0     0.528        -1.828
wb_dati[0]     PHI2          FD1P3AX     SP      un1_wb_rst14_i_0     0.528        -1.828
wb_dati[1]     PHI2          FD1P3AX     SP      un1_wb_rst14_i_0     0.528        -1.828
=========================================================================================



Worst Path Information
***********************


Path information for path number 1: 
      Requested Period:                      1.000
    - Setup time:                            0.472
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         0.528

    - Propagation time:                      2.357
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (non-critical) :                 -1.828

    Number of logic level(s):                1
    Starting point:                          CmdUFMShift / Q
    Ending point:                            wb_adr[0] / SP
    The start point is clocked by            PHI2 [falling] (rise=0.000 fall=175.000 period=350.000) on pin CK
    The end   point is clocked by            RCLK [rising] (rise=0.000 fall=8.000 period=16.000) on pin CK

Instance / Net                          Pin      Pin               Arrival     No. of    
Name                       Type         Name     Dir     Delay     Time        Fan Out(s)
-----------------------------------------------------------------------------------------
CmdUFMShift                FD1P3AX      Q        Out     1.044     1.044 r     -         
CmdUFMShift                Net          -        -       -         -           2         
CmdValid_fast_RNI3K0H1     ORCALUT4     A        In      0.000     1.044 r     -         
CmdValid_fast_RNI3K0H1     ORCALUT4     Z        Out     1.313     2.357 r     -         
un1_wb_rst14_i_0           Net          -        -       -         -           17        
wb_adr[0]                  FD1P3AX      SP       In      0.000     2.357 r     -         
=========================================================================================


Path information for path number 2: 
      Requested Period:                      1.000
    - Setup time:                            0.472
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         0.528

    - Propagation time:                      2.357
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (non-critical) :                 -1.828

    Number of logic level(s):                1
    Starting point:                          CmdUFMShift / Q
    Ending point:                            wb_adr[7] / SP
    The start point is clocked by            PHI2 [falling] (rise=0.000 fall=175.000 period=350.000) on pin CK
    The end   point is clocked by            RCLK [rising] (rise=0.000 fall=8.000 period=16.000) on pin CK

Instance / Net                          Pin      Pin               Arrival     No. of    
Name                       Type         Name     Dir     Delay     Time        Fan Out(s)
-----------------------------------------------------------------------------------------
CmdUFMShift                FD1P3AX      Q        Out     1.044     1.044 r     -         
CmdUFMShift                Net          -        -       -         -           2         
CmdValid_fast_RNI3K0H1     ORCALUT4     A        In      0.000     1.044 r     -         
CmdValid_fast_RNI3K0H1     ORCALUT4     Z        Out     1.313     2.357 r     -         
un1_wb_rst14_i_0           Net          -        -       -         -           17        
wb_adr[7]                  FD1P3AX      SP       In      0.000     2.357 r     -         
=========================================================================================


Path information for path number 3: 
      Requested Period:                      1.000
    - Setup time:                            0.472
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         0.528

    - Propagation time:                      2.357
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (non-critical) :                 -1.828

    Number of logic level(s):                1
    Starting point:                          CmdUFMShift / Q
    Ending point:                            wb_adr[6] / SP
    The start point is clocked by            PHI2 [falling] (rise=0.000 fall=175.000 period=350.000) on pin CK
    The end   point is clocked by            RCLK [rising] (rise=0.000 fall=8.000 period=16.000) on pin CK

Instance / Net                          Pin      Pin               Arrival     No. of    
Name                       Type         Name     Dir     Delay     Time        Fan Out(s)
-----------------------------------------------------------------------------------------
CmdUFMShift                FD1P3AX      Q        Out     1.044     1.044 r     -         
CmdUFMShift                Net          -        -       -         -           2         
CmdValid_fast_RNI3K0H1     ORCALUT4     A        In      0.000     1.044 r     -         
CmdValid_fast_RNI3K0H1     ORCALUT4     Z        Out     1.313     2.357 r     -         
un1_wb_rst14_i_0           Net          -        -       -         -           17        
wb_adr[6]                  FD1P3AX      SP       In      0.000     2.357 r     -         
=========================================================================================


Path information for path number 4: 
      Requested Period:                      1.000
    - Setup time:                            0.472
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         0.528

    - Propagation time:                      2.357
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (non-critical) :                 -1.828

    Number of logic level(s):                1
    Starting point:                          CmdUFMShift / Q
    Ending point:                            wb_adr[5] / SP
    The start point is clocked by            PHI2 [falling] (rise=0.000 fall=175.000 period=350.000) on pin CK
    The end   point is clocked by            RCLK [rising] (rise=0.000 fall=8.000 period=16.000) on pin CK

Instance / Net                          Pin      Pin               Arrival     No. of    
Name                       Type         Name     Dir     Delay     Time        Fan Out(s)
-----------------------------------------------------------------------------------------
CmdUFMShift                FD1P3AX      Q        Out     1.044     1.044 r     -         
CmdUFMShift                Net          -        -       -         -           2         
CmdValid_fast_RNI3K0H1     ORCALUT4     A        In      0.000     1.044 r     -         
CmdValid_fast_RNI3K0H1     ORCALUT4     Z        Out     1.313     2.357 r     -         
un1_wb_rst14_i_0           Net          -        -       -         -           17        
wb_adr[5]                  FD1P3AX      SP       In      0.000     2.357 r     -         
=========================================================================================


Path information for path number 5: 
      Requested Period:                      1.000
    - Setup time:                            0.472
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         0.528

    - Propagation time:                      2.357
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (non-critical) :                 -1.828

    Number of logic level(s):                1
    Starting point:                          CmdUFMShift / Q
    Ending point:                            wb_adr[4] / SP
    The start point is clocked by            PHI2 [falling] (rise=0.000 fall=175.000 period=350.000) on pin CK
    The end   point is clocked by            RCLK [rising] (rise=0.000 fall=8.000 period=16.000) on pin CK

Instance / Net                          Pin      Pin               Arrival     No. of    
Name                       Type         Name     Dir     Delay     Time        Fan Out(s)
-----------------------------------------------------------------------------------------
CmdUFMShift                FD1P3AX      Q        Out     1.044     1.044 r     -         
CmdUFMShift                Net          -        -       -         -           2         
CmdValid_fast_RNI3K0H1     ORCALUT4     A        In      0.000     1.044 r     -         
CmdValid_fast_RNI3K0H1     ORCALUT4     Z        Out     1.313     2.357 r     -         
un1_wb_rst14_i_0           Net          -        -       -         -           17        
wb_adr[4]                  FD1P3AX      SP       In      0.000     2.357 r     -         
=========================================================================================




====================================
Detailed Report for Clock: RCLK
====================================



Starting Points with Worst Slack
********************************

               Starting                                         Arrival           
Instance       Reference     Type        Pin     Net            Time        Slack 
               Clock                                                              
----------------------------------------------------------------------------------
Ready_fast     RCLK          FD1S3AX     Q       Ready_fast     1.256       -0.784
LEDEN          RCLK          FD1S3AX     Q       LEDEN          1.148       -0.676
n8MEGEN        RCLK          FD1S3AX     Q       n8MEGEN        1.108       -0.636
IS[1]          RCLK          FD1P3AX     Q       IS[1]          1.204       9.040 
IS[2]          RCLK          FD1P3AX     Q       IS[2]          1.188       9.056 
IS[3]          RCLK          FD1P3AX     Q       IS[3]          1.148       9.096 
InitReady      RCLK          FD1S3AX     Q       InitReady      1.339       9.228 
FS[15]         RCLK          FD1S3AX     Q       FS[15]         1.228       9.339 
FS[16]         RCLK          FD1S3AX     Q       FS[16]         1.188       9.379 
FS[17]         RCLK          FD1S3AX     Q       FS[17]         1.188       9.379 
==================================================================================


Ending Points with Worst Slack
******************************

               Starting                                          Required           
Instance       Reference     Type         Pin     Net            Time         Slack 
               Clock                                                                
------------------------------------------------------------------------------------
RBA_0io[0]     RCLK          OFS1P3DX     D       RBAd_0[0]      1.089        -0.784
RBA_0io[1]     RCLK          OFS1P3DX     D       RBAd_0[1]      1.089        -0.784
RowA[0]        RCLK          FD1S3AX      D       RowAd_0[0]     1.089        -0.784
RowA[1]        RCLK          FD1S3AX      D       RowAd_0[1]     1.089        -0.784
RowA[2]        RCLK          FD1S3AX      D       RowAd_0[2]     1.089        -0.784
RowA[3]        RCLK          FD1S3AX      D       RowAd_0[3]     1.089        -0.784
RowA[4]        RCLK          FD1S3AX      D       RowAd_0[4]     1.089        -0.784
RowA[5]        RCLK          FD1S3AX      D       RowAd_0[5]     1.089        -0.784
RowA[6]        RCLK          FD1S3AX      D       RowAd_0[6]     1.089        -0.784
RowA[7]        RCLK          FD1S3AX      D       RowAd_0[7]     1.089        -0.784
====================================================================================



Worst Path Information
***********************


Path information for path number 1: 
      Requested Period:                      1.000
    - Setup time:                            -0.089
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         1.089

    - Propagation time:                      1.873
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (non-critical) :                 -0.784

    Number of logic level(s):                1
    Starting point:                          Ready_fast / Q
    Ending point:                            RBA_0io[0] / D
    The start point is clocked by            RCLK [rising] (rise=0.000 fall=8.000 period=16.000) on pin CK
    The end   point is clocked by            nCRAS [falling] (rise=0.000 fall=175.000 period=350.000) on pin SCLK

Instance / Net                  Pin      Pin               Arrival     No. of    
Name               Type         Name     Dir     Delay     Time        Fan Out(s)
---------------------------------------------------------------------------------
Ready_fast         FD1S3AX      Q        Out     1.256     1.256 r     -         
Ready_fast         Net          -        -       -         -           14        
RBAd[0]            ORCALUT4     B        In      0.000     1.256 r     -         
RBAd[0]            ORCALUT4     Z        Out     0.617     1.873 r     -         
RBAd_0[0]          Net          -        -       -         -           1         
RBA_0io[0]         OFS1P3DX     D        In      0.000     1.873 r     -         
=================================================================================


Path information for path number 2: 
      Requested Period:                      1.000
    - Setup time:                            -0.089
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         1.089

    - Propagation time:                      1.873
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (non-critical) :                 -0.784

    Number of logic level(s):                1
    Starting point:                          Ready_fast / Q
    Ending point:                            RowA[9] / D
    The start point is clocked by            RCLK [rising] (rise=0.000 fall=8.000 period=16.000) on pin CK
    The end   point is clocked by            nCRAS [falling] (rise=0.000 fall=175.000 period=350.000) on pin CK

Instance / Net                  Pin      Pin               Arrival     No. of    
Name               Type         Name     Dir     Delay     Time        Fan Out(s)
---------------------------------------------------------------------------------
Ready_fast         FD1S3AX      Q        Out     1.256     1.256 r     -         
Ready_fast         Net          -        -       -         -           14        
RowAd[9]           ORCALUT4     B        In      0.000     1.256 r     -         
RowAd[9]           ORCALUT4     Z        Out     0.617     1.873 f     -         
RowAd_0[9]         Net          -        -       -         -           1         
RowA[9]            FD1S3AX      D        In      0.000     1.873 f     -         
=================================================================================


Path information for path number 3: 
      Requested Period:                      1.000
    - Setup time:                            -0.089
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         1.089

    - Propagation time:                      1.873
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (non-critical) :                 -0.784

    Number of logic level(s):                1
    Starting point:                          Ready_fast / Q
    Ending point:                            RowA[0] / D
    The start point is clocked by            RCLK [rising] (rise=0.000 fall=8.000 period=16.000) on pin CK
    The end   point is clocked by            nCRAS [falling] (rise=0.000 fall=175.000 period=350.000) on pin CK

Instance / Net                  Pin      Pin               Arrival     No. of    
Name               Type         Name     Dir     Delay     Time        Fan Out(s)
---------------------------------------------------------------------------------
Ready_fast         FD1S3AX      Q        Out     1.256     1.256 r     -         
Ready_fast         Net          -        -       -         -           14        
RowAd[0]           ORCALUT4     B        In      0.000     1.256 r     -         
RowAd[0]           ORCALUT4     Z        Out     0.617     1.873 r     -         
RowAd_0[0]         Net          -        -       -         -           1         
RowA[0]            FD1S3AX      D        In      0.000     1.873 r     -         
=================================================================================


Path information for path number 4: 
      Requested Period:                      1.000
    - Setup time:                            -0.089
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         1.089

    - Propagation time:                      1.873
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (non-critical) :                 -0.784

    Number of logic level(s):                1
    Starting point:                          Ready_fast / Q
    Ending point:                            RowA[5] / D
    The start point is clocked by            RCLK [rising] (rise=0.000 fall=8.000 period=16.000) on pin CK
    The end   point is clocked by            nCRAS [falling] (rise=0.000 fall=175.000 period=350.000) on pin CK

Instance / Net                  Pin      Pin               Arrival     No. of    
Name               Type         Name     Dir     Delay     Time        Fan Out(s)
---------------------------------------------------------------------------------
Ready_fast         FD1S3AX      Q        Out     1.256     1.256 r     -         
Ready_fast         Net          -        -       -         -           14        
RowAd[5]           ORCALUT4     B        In      0.000     1.256 r     -         
RowAd[5]           ORCALUT4     Z        Out     0.617     1.873 f     -         
RowAd_0[5]         Net          -        -       -         -           1         
RowA[5]            FD1S3AX      D        In      0.000     1.873 f     -         
=================================================================================


Path information for path number 5: 
      Requested Period:                      1.000
    - Setup time:                            -0.089
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         1.089

    - Propagation time:                      1.873
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (non-critical) :                 -0.784

    Number of logic level(s):                1
    Starting point:                          Ready_fast / Q
    Ending point:                            RowA[8] / D
    The start point is clocked by            RCLK [rising] (rise=0.000 fall=8.000 period=16.000) on pin CK
    The end   point is clocked by            nCRAS [falling] (rise=0.000 fall=175.000 period=350.000) on pin CK

Instance / Net                  Pin      Pin               Arrival     No. of    
Name               Type         Name     Dir     Delay     Time        Fan Out(s)
---------------------------------------------------------------------------------
Ready_fast         FD1S3AX      Q        Out     1.256     1.256 r     -         
Ready_fast         Net          -        -       -         -           14        
RowAd[8]           ORCALUT4     B        In      0.000     1.256 r     -         
RowAd[8]           ORCALUT4     Z        Out     0.617     1.873 r     -         
RowAd_0[8]         Net          -        -       -         -           1         
RowA[8]            FD1S3AX      D        In      0.000     1.873 r     -         
=================================================================================




====================================
Detailed Report for Clock: nCRAS
====================================



Starting Points with Worst Slack
********************************

             Starting                                       Arrival           
Instance     Reference     Type        Pin     Net          Time        Slack 
             Clock                                                            
------------------------------------------------------------------------------
CBR_fast     nCRAS         FD1S3AX     Q       CBR_fast     0.972       -2.605
CBR          nCRAS         FD1S3AX     Q       CBR          1.180       -1.797
FWEr         nCRAS         FD1S3AX     Q       FWEr         1.180       -1.797
==============================================================================


Ending Points with Worst Slack
******************************

               Starting                                                Required           
Instance       Reference     Type         Pin     Net                  Time         Slack 
               Clock                                                                      
------------------------------------------------------------------------------------------
nRCAS_0io      nCRAS         OFS1P3BX     D       N_248_i              1.089        -2.605
nRCS_0io       nCRAS         OFS1P3BX     D       N_247_i              1.089        -1.797
nRWE_0io       nCRAS         OFS1P3BX     D       N_49_i               1.089        -1.797
nRowColSel     nCRAS         FD1S3IX      D       nRowColSel_0_0_0     1.089        -1.797
RCKEEN         nCRAS         FD1S3AX      D       RCKEEN_8             1.089        -1.725
==========================================================================================



Worst Path Information
***********************


Path information for path number 1: 
      Requested Period:                      1.000
    - Setup time:                            -0.089
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         1.089

    - Propagation time:                      3.694
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (critical) :                     -2.605

    Number of logic level(s):                3
    Starting point:                          CBR_fast / Q
    Ending point:                            nRCAS_0io / D
    The start point is clocked by            nCRAS [falling] (rise=0.000 fall=175.000 period=350.000) on pin CK
    The end   point is clocked by            RCLK [rising] (rise=0.000 fall=8.000 period=16.000) on pin SCLK

Instance / Net                     Pin      Pin               Arrival     No. of    
Name                  Type         Name     Dir     Delay     Time        Fan Out(s)
------------------------------------------------------------------------------------
CBR_fast              FD1S3AX      Q        Out     0.972     0.972 r     -         
CBR_fast              Net          -        -       -         -           1         
CBR_fast_RNIQ31K1     ORCALUT4     A        In      0.000     0.972 r     -         
CBR_fast_RNIQ31K1     ORCALUT4     Z        Out     1.089     2.061 r     -         
nRCAS_0_sqmuxa_1      Net          -        -       -         -           2         
nRCAS_0io_RNO_0       ORCALUT4     B        In      0.000     2.061 r     -         
nRCAS_0io_RNO_0       ORCALUT4     Z        Out     1.017     3.077 r     -         
N_248_i_sx            Net          -        -       -         -           1         
nRCAS_0io_RNO         ORCALUT4     D        In      0.000     3.077 r     -         
nRCAS_0io_RNO         ORCALUT4     Z        Out     0.617     3.694 f     -         
N_248_i               Net          -        -       -         -           1         
nRCAS_0io             OFS1P3BX     D        In      0.000     3.694 f     -         
====================================================================================


Path information for path number 2: 
      Requested Period:                      1.000
    - Setup time:                            -0.089
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         1.089

    - Propagation time:                      2.885
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (non-critical) :                 -1.797

    Number of logic level(s):                2
    Starting point:                          CBR / Q
    Ending point:                            nRCS_0io / D
    The start point is clocked by            nCRAS [falling] (rise=0.000 fall=175.000 period=350.000) on pin CK
    The end   point is clocked by            RCLK [rising] (rise=0.000 fall=8.000 period=16.000) on pin SCLK

Instance / Net                       Pin      Pin               Arrival     No. of    
Name                    Type         Name     Dir     Delay     Time        Fan Out(s)
--------------------------------------------------------------------------------------
CBR                     FD1S3AX      Q        Out     1.180     1.180 r     -         
CBR                     Net          -        -       -         -           5         
RCKEEN_8_u_0_0_a2_2     ORCALUT4     A        In      0.000     1.180 r     -         
RCKEEN_8_u_0_0_a2_2     ORCALUT4     Z        Out     1.089     2.269 f     -         
N_590                   Net          -        -       -         -           2         
nRCS_0io_RNO            ORCALUT4     C        In      0.000     2.269 f     -         
nRCS_0io_RNO            ORCALUT4     Z        Out     0.617     2.885 r     -         
N_247_i                 Net          -        -       -         -           1         
nRCS_0io                OFS1P3BX     D        In      0.000     2.885 r     -         
======================================================================================


Path information for path number 3: 
      Requested Period:                      1.000
    - Setup time:                            -0.089
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         1.089

    - Propagation time:                      2.885
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (non-critical) :                 -1.797

    Number of logic level(s):                2
    Starting point:                          FWEr / Q
    Ending point:                            nRCAS_0io / D
    The start point is clocked by            nCRAS [falling] (rise=0.000 fall=175.000 period=350.000) on pin CK
    The end   point is clocked by            RCLK [rising] (rise=0.000 fall=8.000 period=16.000) on pin SCLK

Instance / Net                  Pin      Pin               Arrival     No. of    
Name               Type         Name     Dir     Delay     Time        Fan Out(s)
---------------------------------------------------------------------------------
FWEr               FD1S3AX      Q        Out     1.180     1.180 r     -         
FWEr               Net          -        -       -         -           5         
nRCAS_r_i_0_a2     ORCALUT4     B        In      0.000     1.180 r     -         
nRCAS_r_i_0_a2     ORCALUT4     Z        Out     1.089     2.269 f     -         
N_248_i_1_0        Net          -        -       -         -           2         
nRCAS_0io_RNO      ORCALUT4     C        In      0.000     2.269 f     -         
nRCAS_0io_RNO      ORCALUT4     Z        Out     0.617     2.885 r     -         
N_248_i            Net          -        -       -         -           1         
nRCAS_0io          OFS1P3BX     D        In      0.000     2.885 r     -         
=================================================================================


Path information for path number 4: 
      Requested Period:                      1.000
    - Setup time:                            -0.089
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         1.089

    - Propagation time:                      2.885
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (non-critical) :                 -1.797

    Number of logic level(s):                2
    Starting point:                          CBR / Q
    Ending point:                            nRWE_0io / D
    The start point is clocked by            nCRAS [falling] (rise=0.000 fall=175.000 period=350.000) on pin CK
    The end   point is clocked by            RCLK [rising] (rise=0.000 fall=8.000 period=16.000) on pin SCLK

Instance / Net                       Pin      Pin               Arrival     No. of    
Name                    Type         Name     Dir     Delay     Time        Fan Out(s)
--------------------------------------------------------------------------------------
CBR                     FD1S3AX      Q        Out     1.180     1.180 r     -         
CBR                     Net          -        -       -         -           5         
RCKEEN_8_u_0_0_a2_2     ORCALUT4     A        In      0.000     1.180 r     -         
RCKEEN_8_u_0_0_a2_2     ORCALUT4     Z        Out     1.089     2.269 f     -         
N_590                   Net          -        -       -         -           2         
nRWE_0io_RNO            ORCALUT4     B        In      0.000     2.269 f     -         
nRWE_0io_RNO            ORCALUT4     Z        Out     0.617     2.885 r     -         
N_49_i                  Net          -        -       -         -           1         
nRWE_0io                OFS1P3BX     D        In      0.000     2.885 r     -         
======================================================================================


Path information for path number 5: 
      Requested Period:                      1.000
    - Setup time:                            -0.089
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         1.089

    - Propagation time:                      2.885
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (non-critical) :                 -1.797

    Number of logic level(s):                2
    Starting point:                          FWEr / Q
    Ending point:                            nRCAS_0io / D
    The start point is clocked by            nCRAS [falling] (rise=0.000 fall=175.000 period=350.000) on pin CK
    The end   point is clocked by            RCLK [rising] (rise=0.000 fall=8.000 period=16.000) on pin SCLK

Instance / Net                       Pin      Pin               Arrival     No. of    
Name                    Type         Name     Dir     Delay     Time        Fan Out(s)
--------------------------------------------------------------------------------------
FWEr                    FD1S3AX      Q        Out     1.180     1.180 r     -         
FWEr                    Net          -        -       -         -           5         
nRowColSel_0_0_0_a2     ORCALUT4     B        In      0.000     1.180 r     -         
nRowColSel_0_0_0_a2     ORCALUT4     Z        Out     1.089     2.269 r     -         
N_248_i_1_1             Net          -        -       -         -           2         
nRCAS_0io_RNO           ORCALUT4     B        In      0.000     2.269 r     -         
nRCAS_0io_RNO           ORCALUT4     Z        Out     0.617     2.885 f     -         
N_248_i                 Net          -        -       -         -           1         
nRCAS_0io               OFS1P3BX     D        In      0.000     2.885 f     -         
======================================================================================




====================================
Detailed Report for Clock: System
====================================



Starting Points with Worst Slack
********************************

                     Starting                                          Arrival           
Instance             Reference     Type     Pin         Net            Time        Slack 
                     Clock                                                               
-----------------------------------------------------------------------------------------
ufmefb.EFBInst_0     System        EFB      WBACKO      wb_ack         0.000       12.918
ufmefb.EFBInst_0     System        EFB      WBDATO0     wb_dato[0]     0.000       14.455
ufmefb.EFBInst_0     System        EFB      WBDATO1     wb_dato[1]     0.000       14.455
=========================================================================================


Ending Points with Worst Slack
******************************

               Starting                                         Required           
Instance       Reference     Type        Pin     Net            Time         Slack 
               Clock                                                               
-----------------------------------------------------------------------------------
LEDEN          System        FD1S3AX     D       LEDENe_0       16.089       12.918
n8MEGEN        System        FD1S3AX     D       n8MEGENe_0     16.089       12.918
wb_cyc_stb     System        FD1P3IX     SP      N_178          15.528       14.912
===================================================================================



Worst Path Information
***********************


Path information for path number 1: 
      Requested Period:                      16.000
    - Setup time:                            -0.089
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         16.089

    - Propagation time:                      3.171
    - Clock delay at starting point:         0.000 (ideal)
    - Estimated clock delay at start point:  -0.000
    = Slack (non-critical) :                 12.918

    Number of logic level(s):                4
    Starting point:                          ufmefb.EFBInst_0 / WBACKO
    Ending point:                            LEDEN / D
    The start point is clocked by            System [rising]
    The end   point is clocked by            RCLK [rising] (rise=0.000 fall=8.000 period=16.000) on pin CK

Instance / Net                             Pin        Pin               Arrival     No. of    
Name                          Type         Name       Dir     Delay     Time        Fan Out(s)
----------------------------------------------------------------------------------------------
ufmefb.EFBInst_0              EFB          WBACKO     Out     0.000     0.000 r     -         
wb_ack                        Net          -          -       -         -           2         
ufmefb.EFBInst_0_RNISGNB      ORCALUT4     D          In      0.000     0.000 r     -         
ufmefb.EFBInst_0_RNISGNB      ORCALUT4     Z          Out     1.017     1.017 r     -         
g0_0_a3_2                     Net          -          -       -         -           1         
ufmefb.EFBInst_0_RNISI191     ORCALUT4     C          In      0.000     1.017 r     -         
ufmefb.EFBInst_0_RNISI191     ORCALUT4     Z          Out     0.449     1.466 r     -         
N_4                           Net          -          -       -         -           1         
CmdValid_RNIOOBE2             ORCALUT4     C          In      0.000     1.466 r     -         
CmdValid_RNIOOBE2             ORCALUT4     Z          Out     1.089     2.554 r     -         
CmdValid_RNIOOBE2             Net          -          -       -         -           2         
LEDENe                        ORCALUT4     B          In      0.000     2.554 r     -         
LEDENe                        ORCALUT4     Z          Out     0.617     3.171 r     -         
LEDENe_0                      Net          -          -       -         -           1         
LEDEN                         FD1S3AX      D          In      0.000     3.171 r     -         
==============================================================================================



##### END OF TIMING REPORT #####]

Timing exceptions that could not be applied

Finished final timing analysis (Real Time elapsed 0h:00m:04s; CPU Time elapsed 0h:00m:04s; Memory used current: 202MB peak: 203MB)


Finished timing report (Real Time elapsed 0h:00m:04s; CPU Time elapsed 0h:00m:04s; Memory used current: 202MB peak: 203MB)

---------------------------------------
Resource Usage Report
Part: lcmxo2_640hc-4

Register bits: 109 of 640 (17%)
PIC Latch:       0
I/O cells:       63


Details:
BB:             8
CCU2D:          10
EFB:            1
FD1P3AX:        25
FD1P3IX:        2
FD1S3AX:        53
FD1S3IX:        4
GSR:            1
IB:             25
IFS1P3DX:       9
INV:            7
OB:             30
OFS1P3BX:       4
OFS1P3DX:       11
OFS1P3JX:       1
ORCALUT4:       213
PFUMX:          1
PUR:            1
VHI:            2
VLO:            2
Mapper successful!

At Mapper Exit (Real Time elapsed 0h:00m:04s; CPU Time elapsed 0h:00m:04s; Memory used current: 78MB peak: 203MB)

Process took 0h:00m:04s realtime, 0h:00m:04s cputime
# Thu Sep 21 05:39:42 2023

###########################################################]
