(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")

  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 67)
    (zones 0)
    (modules 3)
    (nets 29)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 A15)
  (net 2 D2)
  (net 3 D1)
  (net 4 D0)
  (net 5 A0)
  (net 6 A1)
  (net 7 A2)
  (net 8 A3)
  (net 9 A4)
  (net 10 A5)
  (net 11 A6)
  (net 12 A7)
  (net 13 A12)
  (net 14 A14)
  (net 15 D3)
  (net 16 D4)
  (net 17 D5)
  (net 18 D6)
  (net 19 D7)
  (net 20 ~CE)
  (net 21 A10)
  (net 22 ~OE)
  (net 23 A11)
  (net 24 A9)
  (net 25 A8)
  (net 26 A13)
  (net 27 ~WE)
  (net 28 VCC)

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net A0)
    (add_net A1)
    (add_net A10)
    (add_net A11)
    (add_net A12)
    (add_net A13)
    (add_net A14)
    (add_net A15)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net A6)
    (add_net A7)
    (add_net A8)
    (add_net A9)
    (add_net D0)
    (add_net D1)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net VCC)
    (add_net ~CE)
    (add_net ~OE)
    (add_net ~WE)
  )

  (module Package_DIP:DIP-32_W15.24mm_Socket (layer F.Cu) (tedit 5A02E8C5) (tstamp 619B97F5)
    (at 78.05 62.9)
    (descr "32-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket")
    (path /61AFB38D)
    (fp_text reference U1 (at 7.62 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SST39SF040 (at 7.62 40.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.255 -1.27) (end 14.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 14.985 -1.27) (end 14.985 39.37) (layer F.Fab) (width 0.1))
    (fp_line (start 14.985 39.37) (end 0.255 39.37) (layer F.Fab) (width 0.1))
    (fp_line (start 0.255 39.37) (end 0.255 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.255 -0.27) (end 1.255 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -1.33) (end -1.27 39.43) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 39.43) (end 16.51 39.43) (layer F.Fab) (width 0.1))
    (fp_line (start 16.51 39.43) (end 16.51 -1.33) (layer F.Fab) (width 0.1))
    (fp_line (start 16.51 -1.33) (end -1.27 -1.33) (layer F.Fab) (width 0.1))
    (fp_line (start 6.62 -1.33) (end 1.16 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 -1.33) (end 1.16 39.43) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 39.43) (end 14.08 39.43) (layer F.SilkS) (width 0.12))
    (fp_line (start 14.08 39.43) (end 14.08 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 14.08 -1.33) (end 8.62 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.39) (end -1.33 39.49) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 39.49) (end 16.57 39.49) (layer F.SilkS) (width 0.12))
    (fp_line (start 16.57 39.49) (end 16.57 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 16.57 -1.39) (end -1.33 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 -1.6) (end -1.55 39.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 39.7) (end 16.8 39.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 16.8 39.7) (end 16.8 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 16.8 -1.6) (end -1.55 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 7.62 19.05) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 7.62 -1.33) (end 6.62 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
    (pad 32 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 VCC))
    (pad 16 thru_hole oval (at 0 38.1) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 A15))
    (pad 31 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 ~WE))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 D2))
    (pad 30 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 A15))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 D1))
    (pad 29 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 A14))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 D0))
    (pad 28 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 A13))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 A0))
    (pad 27 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 A8))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 A1))
    (pad 26 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 A9))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 A2))
    (pad 25 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 A11))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 A3))
    (pad 24 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 ~OE))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 A4))
    (pad 23 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 A10))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 A5))
    (pad 22 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 ~CE))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 A6))
    (pad 21 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 D7))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 A7))
    (pad 20 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 D6))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 A12))
    (pad 19 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 D5))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 A15))
    (pad 18 thru_hole oval (at 15.24 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 D4))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 A15))
    (pad 17 thru_hole oval (at 15.24 38.1) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 D3))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 A15))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-32_W15.24mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x14_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC) (tstamp 619BAAD3)
    (at 89.46 68 180)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (path /61AFD052)
    (fp_text reference J2 (at 0 2.33) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value t-right (at 0 -35.35) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -0.635 1.27) (end 1.27 1.27) (layer B.Fab) (width 0.1))
    (fp_line (start 1.27 1.27) (end 1.27 -34.29) (layer B.Fab) (width 0.1))
    (fp_line (start 1.27 -34.29) (end -1.27 -34.29) (layer B.Fab) (width 0.1))
    (fp_line (start -1.27 -34.29) (end -1.27 0.635) (layer B.Fab) (width 0.1))
    (fp_line (start -1.27 0.635) (end -0.635 1.27) (layer B.Fab) (width 0.1))
    (fp_line (start -1.33 -34.35) (end 1.33 -34.35) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.27) (end -1.33 -34.35) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.33 -1.27) (end 1.33 -34.35) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.27) (end 1.33 -1.27) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 1.33) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.33 1.33) (end 0 1.33) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.8 1.8) (end -1.8 -34.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.8 -34.8) (end 1.8 -34.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.8 -34.8) (end 1.8 1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end -1.8 1.8) (layer B.CrtYd) (width 0.05))
    (fp_text user %R (at 0 -16.51 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (pad 14 thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 D3))
    (pad 13 thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 D4))
    (pad 12 thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 D5))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 D6))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 D7))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 ~CE))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 A10))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 ~OE))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 A11))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 A9))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 A8))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 A13))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 ~WE))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 VCC))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x14_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x14_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC) (tstamp 619BAD22)
    (at 81.85 68 180)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (path /61AFC6D5)
    (fp_text reference J1 (at 0 2.33) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value t-left (at 0 -35.35) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -0.635 1.27) (end 1.27 1.27) (layer B.Fab) (width 0.1))
    (fp_line (start 1.27 1.27) (end 1.27 -34.29) (layer B.Fab) (width 0.1))
    (fp_line (start 1.27 -34.29) (end -1.27 -34.29) (layer B.Fab) (width 0.1))
    (fp_line (start -1.27 -34.29) (end -1.27 0.635) (layer B.Fab) (width 0.1))
    (fp_line (start -1.27 0.635) (end -0.635 1.27) (layer B.Fab) (width 0.1))
    (fp_line (start -1.33 -34.35) (end 1.33 -34.35) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.27) (end -1.33 -34.35) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.33 -1.27) (end 1.33 -34.35) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.27) (end 1.33 -1.27) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 1.33) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.33 1.33) (end 0 1.33) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.8 1.8) (end -1.8 -34.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.8 -34.8) (end 1.8 -34.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.8 -34.8) (end 1.8 1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end -1.8 1.8) (layer B.CrtYd) (width 0.05))
    (fp_text user %R (at 0 -16.51 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (pad 14 thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 A15))
    (pad 13 thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 D2))
    (pad 12 thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 D1))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 D0))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 A0))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 A1))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 A2))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 A3))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 A4))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 A5))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 A6))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 A7))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 A12))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 A14))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x14_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 75 104) (end 75 60) (layer Edge.Cuts) (width 0.05) (tstamp 619B151C))
  (gr_line (start 96 104) (end 75 104) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 96 60) (end 96 104) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 75 60) (end 96 60) (layer Edge.Cuts) (width 0.05))
  (gr_text SST39SF010A (at 85.86 84.57 90) (layer F.SilkS) (tstamp 619BB343)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text Kludge-o-ROM-a (at 85.67 81.87 90) (layer B.SilkS) (tstamp 619BB311)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify mirror))
  )

  (segment (start 78.07 101.02) (end 78.05 101) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 81.85 101.02) (end 78.07 101.02) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 78.05 67.98) (end 78.05 65.44) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 78.05 65.44) (end 78.05 62.9) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 92.134999 66.824999) (end 93.29 67.98) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 79.205001 66.824999) (end 92.134999 66.824999) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 78.05 67.98) (end 79.205001 66.824999) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 76.924999 99.874999) (end 78.05 101) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 76.924999 66.565001) (end 76.924999 99.874999) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 78.05 65.44) (end 76.924999 66.565001) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 81.83 98.46) (end 81.85 98.48) (width 0.25) (layer B.Cu) (net 2))
  (segment (start 78.05 98.46) (end 81.83 98.46) (width 0.25) (layer B.Cu) (net 2))
  (segment (start 81.83 95.92) (end 81.85 95.94) (width 0.25) (layer B.Cu) (net 3))
  (segment (start 78.05 95.92) (end 81.83 95.92) (width 0.25) (layer B.Cu) (net 3))
  (segment (start 81.83 93.38) (end 81.85 93.4) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 78.05 93.38) (end 81.83 93.38) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 81.83 90.84) (end 81.85 90.86) (width 0.25) (layer B.Cu) (net 5))
  (segment (start 78.05 90.84) (end 81.83 90.84) (width 0.25) (layer B.Cu) (net 5))
  (segment (start 81.83 88.3) (end 81.85 88.32) (width 0.25) (layer B.Cu) (net 6))
  (segment (start 78.05 88.3) (end 81.83 88.3) (width 0.25) (layer B.Cu) (net 6))
  (segment (start 81.83 85.76) (end 81.85 85.78) (width 0.25) (layer B.Cu) (net 7))
  (segment (start 78.05 85.76) (end 81.83 85.76) (width 0.25) (layer B.Cu) (net 7))
  (segment (start 81.83 83.22) (end 81.85 83.24) (width 0.25) (layer B.Cu) (net 8))
  (segment (start 78.05 83.22) (end 81.83 83.22) (width 0.25) (layer B.Cu) (net 8))
  (segment (start 81.83 80.68) (end 81.85 80.7) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 78.05 80.68) (end 81.83 80.68) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 81.83 78.14) (end 81.85 78.16) (width 0.25) (layer B.Cu) (net 10))
  (segment (start 78.05 78.14) (end 81.83 78.14) (width 0.25) (layer B.Cu) (net 10))
  (segment (start 81.83 75.6) (end 81.85 75.62) (width 0.25) (layer B.Cu) (net 11))
  (segment (start 78.05 75.6) (end 81.83 75.6) (width 0.25) (layer B.Cu) (net 11))
  (segment (start 81.83 73.06) (end 81.85 73.08) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 78.05 73.06) (end 81.83 73.06) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 78.07 70.54) (end 78.05 70.52) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 81.85 70.54) (end 78.07 70.54) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 88.875001 71.715001) (end 92.094999 71.715001) (width 0.25) (layer B.Cu) (net 14))
  (segment (start 92.094999 71.715001) (end 93.29 70.52) (width 0.25) (layer B.Cu) (net 14))
  (segment (start 85.16 68) (end 88.875001 71.715001) (width 0.25) (layer B.Cu) (net 14))
  (segment (start 81.85 68) (end 85.16 68) (width 0.25) (layer B.Cu) (net 14))
  (segment (start 93.27 101.02) (end 93.29 101) (width 0.25) (layer B.Cu) (net 15))
  (segment (start 89.46 101.02) (end 93.27 101.02) (width 0.25) (layer B.Cu) (net 15))
  (segment (start 93.27 98.48) (end 93.29 98.46) (width 0.25) (layer B.Cu) (net 16))
  (segment (start 89.46 98.48) (end 93.27 98.48) (width 0.25) (layer B.Cu) (net 16))
  (segment (start 93.27 95.94) (end 93.29 95.92) (width 0.25) (layer B.Cu) (net 17))
  (segment (start 89.46 95.94) (end 93.27 95.94) (width 0.25) (layer B.Cu) (net 17))
  (segment (start 93.27 93.4) (end 93.29 93.38) (width 0.25) (layer B.Cu) (net 18))
  (segment (start 89.46 93.4) (end 93.27 93.4) (width 0.25) (layer B.Cu) (net 18))
  (segment (start 93.27 90.86) (end 93.29 90.84) (width 0.25) (layer B.Cu) (net 19))
  (segment (start 89.46 90.86) (end 93.27 90.86) (width 0.25) (layer B.Cu) (net 19))
  (segment (start 93.27 88.32) (end 93.29 88.3) (width 0.25) (layer B.Cu) (net 20))
  (segment (start 89.46 88.32) (end 93.27 88.32) (width 0.25) (layer B.Cu) (net 20))
  (segment (start 93.27 85.78) (end 93.29 85.76) (width 0.25) (layer B.Cu) (net 21))
  (segment (start 89.46 85.78) (end 93.27 85.78) (width 0.25) (layer B.Cu) (net 21))
  (segment (start 93.27 83.24) (end 93.29 83.22) (width 0.25) (layer B.Cu) (net 22))
  (segment (start 89.46 83.24) (end 93.27 83.24) (width 0.25) (layer B.Cu) (net 22))
  (segment (start 93.27 80.7) (end 93.29 80.68) (width 0.25) (layer B.Cu) (net 23))
  (segment (start 89.46 80.7) (end 93.27 80.7) (width 0.25) (layer B.Cu) (net 23))
  (segment (start 93.27 78.16) (end 93.29 78.14) (width 0.25) (layer B.Cu) (net 24))
  (segment (start 89.46 78.16) (end 93.27 78.16) (width 0.25) (layer B.Cu) (net 24))
  (segment (start 93.27 75.62) (end 93.29 75.6) (width 0.25) (layer B.Cu) (net 25))
  (segment (start 89.46 75.62) (end 93.27 75.62) (width 0.25) (layer B.Cu) (net 25))
  (segment (start 89.48 73.06) (end 89.46 73.08) (width 0.25) (layer B.Cu) (net 26))
  (segment (start 93.29 73.06) (end 89.48 73.06) (width 0.25) (layer B.Cu) (net 26))
  (segment (start 92.164999 67.835001) (end 89.46 70.54) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 92.164999 66.565001) (end 92.164999 67.835001) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 93.29 65.44) (end 92.164999 66.565001) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 89.46 66.73) (end 89.46 68) (width 0.25) (layer B.Cu) (net 28))
  (segment (start 93.29 62.9) (end 89.46 66.73) (width 0.25) (layer B.Cu) (net 28))

)
