(module POGOPAD_01x14 (layer F.Cu) (tedit 62916F71)
  (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
  (tags "Through hole pin header THT 1x14 2.54mm single row")
  (fp_text reference J3 (at 0 -2.33 180) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "MKR VIDOR 4000" (at 0 35.35 180) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 16.51 270) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.8 -1.8) (end -1.8 34.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.8 34.8) (end 1.8 34.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.8 34.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
  (pad 1 smd circle (at 0 0) (size 2 2) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd circle (at 0 2.54) (size 2 2) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd circle (at 0 5.08) (size 2 2) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd circle (at 0 7.62) (size 2 2) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd circle (at 0 10.16) (size 2 2) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd circle (at 0 12.7) (size 2 2) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd circle (at 0 15.24) (size 2 2) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd circle (at 0 17.78) (size 2 2) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd circle (at 0 20.32) (size 2 2) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd circle (at 0 22.86) (size 2 2) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd circle (at 0 25.4) (size 2 2) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd circle (at 0 27.94) (size 2 2) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd circle (at 0 30.48) (size 2 2) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd circle (at 0 33.02) (size 2 2) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x14_P2.54mm_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
