<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<text>U1</text>
<text>U2</text>
<text>U3</text>
<text>U4</text>
<text>U5</text>
<text>U6</text>
<text>U7</text>
<text>CON1</text>
<text>D1</text>
<text>R1</text>
<text>J1</text>
<text>J2</text>
<text>J3</text>
<text>J4</text>
<text>MOSI</text>
<text>MISO</text>
<text>SCLK</text>
<text>CS</text>
<text>3V3</text>
<text>TDO</text>
<text>GND</text>
<text>TDI</text>
<text>TCK</text>
<text>TMS</text>
<text>R2</text>
<text>R3</text>
<text>R4</text>
<text>R5</text>
<text>R6</text>
<text>1</text>
<text>25</text>
<text>C13</text>
<text>C8</text>
<text>C14</text>
<text>C15</text>
<text>C9</text>
<text>C16</text>
<text>C10</text>
<text>C17</text>
<text>C11</text>
<text>C18</text>
<text>C12</text>
<text>C1</text>
<text>C2</text>
<text>C3</text>
<text>C4</text>
<text>C5</text>
<text>C6</text>
<text>L1</text>
<text>C20</text>
<text>C19</text>
<text>C7</text>
<text>FPGA DISK CONTROLLER
ORIGINAL DESIGN BY BIG MESS O' WIRES</text>
<text>v1.0</text>
<wire x1="0" y1="7.874" x2="0" y2="77.724" width="0" layer="20"/>
<wire x1="0" y1="77.724" x2="100" y2="77.724" width="0" layer="20"/>
<wire x1="100" y1="77.724" x2="100" y2="7.874" width="0" layer="20"/>
<wire x1="100" y1="7.874" x2="97.79" y2="7.874" width="0" layer="20"/>
<wire x1="97.79" y1="7.874" x2="97.79" y2="0.762" width="0" layer="20"/>
<wire x1="97.79" y1="0.762" x2="97.028" y2="0" width="0" layer="20"/>
<wire x1="97.028" y1="0" x2="32.766" y2="0" width="0" layer="20"/>
<wire x1="32.766" y1="0" x2="32.004" y2="0.762" width="0" layer="20"/>
<wire x1="32.004" y1="0.762" x2="32.004" y2="7.874" width="0" layer="20"/>
<wire x1="32.004" y1="7.874" x2="0" y2="7.874" width="0" layer="20"/>
</plain>
<libraries>
<library name="con-apple2">
<description>&lt;b&gt;Apple ][ Expansion Card Templates&lt;/b&gt;
&lt;br /&gt;
Dimensions are taken from the Apple IIgs Tech Note #28</description>
<packages>
<package name="A2-50PIN-MINI">
</package>
</packages>
</library>
<library name="bmowdisk">
<packages>
<package name="SSOP20">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type SS</description>
</package>
<package name="TQFP100">
</package>
<package name="SOIC08">
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="0805">
</package>
<package name="1X08">
</package>
</packages>
</library>
<library name="v-reg-micrel">
<description>&lt;b&gt;Micrel Voltage Regulator&lt;/b&gt;&lt;p&gt;
Micrel Semiconductor, Inc.&lt;br&gt;
http://www.micrel.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
</packages>
</library>
<library name="retro-usb-2">
<description>Generated from &lt;b&gt;retro-usb.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="MA06-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="MA04-1">
</package>
</packages>
</library>
<library name="big-mess-o-wires">
<packages>
<package name="IDC20">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
series 057 contact pc board low profile headers&lt;p&gt;
straight</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ST1" library="con-apple2" package="A2-50PIN-MINI" value=""/>
<element name="C19" library="SparkFun" package="0805" value="10uF"/>
<element name="U3" library="v-reg-micrel" package="SOT23-5" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="D1" library="led" package="CHIP-LED0805" value=""/>
<element name="R1" library="SparkFun" package="0805" value="390R"/>
<element name="J1" library="retro-usb-2" package="MA06-1" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="U4" library="bmowdisk" package="SSOP20" value="74X245"/>
<element name="R2" library="SparkFun" package="0805" value="390R"/>
<element name="U7" library="bmowdisk" package="SSOP20" value="74X245"/>
<element name="U5" library="bmowdisk" package="SSOP20" value="74X245"/>
<element name="U6" library="bmowdisk" package="SSOP20" value="74X245"/>
<element name="CON1" library="big-mess-o-wires" package="IDC20" value="IDC20"/>
<element name="R5" library="SparkFun" package="0805" value="22K"/>
<element name="R4" library="SparkFun" package="0805" value="22K"/>
<element name="C1" library="SparkFun" package="0805" value="0.1uF"/>
<element name="C2" library="SparkFun" package="0805" value="0.1uF"/>
<element name="C3" library="SparkFun" package="0805" value="0.1uF"/>
<element name="C4" library="SparkFun" package="0805" value="0.1uF"/>
<element name="J4" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="R3" library="SparkFun" package="0805" value="4.7K"/>
<element name="C20" library="SparkFun" package="0805" value="10uF"/>
<element name="C5" library="SparkFun" package="0805" value="0.1uF"/>
<element name="C6" library="SparkFun" package="0805" value="0.1uF"/>
<element name="C14" library="SparkFun" package="0805" value="0.01uF"/>
<element name="C9" library="SparkFun" package="0805" value="0.1uF"/>
<element name="L1" library="SparkFun-Passives" package="0805" value=""/>
<element name="U1" library="bmowdisk" package="TQFP100" value="LCMXO2-1200HC-TQFP100"/>
<element name="J3" library="SparkFun" package="1X08" value="LCD1"/>
<element name="U2" library="bmowdisk" package="SOIC08" value="SPI-FLASH"/>
<element name="J2" library="retro-usb-2" package="MA04-1" value="MA04-1S"/>
<element name="C12" library="SparkFun" package="0805" value="0.1uF"/>
<element name="C13" library="SparkFun" package="0805" value="0.01uF"/>
<element name="C18" library="SparkFun" package="0805" value="0.01uF"/>
<element name="C11" library="SparkFun" package="0805" value="0.1uF"/>
<element name="C8" library="SparkFun" package="0805" value="0.1uF"/>
<element name="C15" library="SparkFun" package="0805" value="0.01uF"/>
<element name="C10" library="SparkFun" package="0805" value="0.1uF"/>
<element name="C16" library="SparkFun" package="0805" value="0.01uF"/>
<element name="C17" library="SparkFun" package="0805" value="0.01uF"/>
<element name="C7" library="SparkFun" package="0805" value="0.1uF"/>
<element name="R6" library="SparkFun" package="0805" value="22K"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U4" pad="10"/>
<contactref element="U3" pad="2"/>
<contactref element="U7" pad="10"/>
<contactref element="U7" pad="1"/>
<contactref element="U5" pad="1"/>
<contactref element="U5" pad="10"/>
<contactref element="U6" pad="1"/>
<contactref element="U6" pad="10"/>
<contactref element="U7" pad="19"/>
<contactref element="U5" pad="19"/>
<contactref element="U6" pad="19"/>
<contactref element="ST1" pad="26"/>
<contactref element="CON1" pad="1"/>
<contactref element="CON1" pad="3"/>
<contactref element="U7" pad="16"/>
<contactref element="U7" pad="17"/>
<contactref element="U7" pad="18"/>
<contactref element="C19" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="J4" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="J1" pad="4"/>
<contactref element="D1" pad="C"/>
<contactref element="U2" pad="4"/>
<contactref element="C17" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="22"/>
<contactref element="U1" pad="33"/>
<contactref element="U1" pad="44"/>
<contactref element="U1" pad="56"/>
<contactref element="U1" pad="72"/>
<contactref element="U1" pad="79"/>
<contactref element="U1" pad="92"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U4" pad="20"/>
<contactref element="U7" pad="20"/>
<contactref element="U5" pad="20"/>
<contactref element="U6" pad="20"/>
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U3" pad="5"/>
<contactref element="C20" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="L1" pad="2"/>
<contactref element="U2" pad="8"/>
<contactref element="U2" pad="3"/>
<contactref element="U2" pad="7"/>
<contactref element="C7" pad="1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R1" pad="2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="P60">
</signal>
<signal name="P59">
</signal>
<signal name="D0">
<contactref element="ST1" pad="49"/>
<contactref element="U4" pad="11"/>
</signal>
<signal name="D1">
<contactref element="ST1" pad="48"/>
<contactref element="U4" pad="12"/>
</signal>
<signal name="D2">
<contactref element="ST1" pad="47"/>
<contactref element="U4" pad="13"/>
</signal>
<signal name="D3">
<contactref element="ST1" pad="46"/>
<contactref element="U4" pad="14"/>
</signal>
<signal name="D4">
<contactref element="ST1" pad="45"/>
<contactref element="U4" pad="15"/>
</signal>
<signal name="D5">
<contactref element="ST1" pad="44"/>
<contactref element="U4" pad="16"/>
</signal>
<signal name="D6">
<contactref element="ST1" pad="43"/>
<contactref element="U4" pad="17"/>
</signal>
<signal name="D7">
<contactref element="ST1" pad="42"/>
<contactref element="U4" pad="18"/>
</signal>
<signal name="D7_33">
<contactref element="U4" pad="2"/>
<contactref element="U1" pad="52"/>
</signal>
<signal name="D6_33">
<contactref element="U4" pad="3"/>
<contactref element="U1" pad="51"/>
</signal>
<signal name="D5_33">
<contactref element="U4" pad="4"/>
<contactref element="U1" pad="47"/>
</signal>
<signal name="D4_33">
<contactref element="U4" pad="5"/>
<contactref element="U1" pad="39"/>
</signal>
<signal name="D3_33">
<contactref element="U4" pad="6"/>
<contactref element="U1" pad="38"/>
</signal>
<signal name="D2_33">
<contactref element="U4" pad="7"/>
<contactref element="U1" pad="37"/>
</signal>
<signal name="D1_33">
<contactref element="U4" pad="8"/>
<contactref element="U1" pad="36"/>
</signal>
<signal name="D0_33">
<contactref element="U4" pad="9"/>
<contactref element="U1" pad="35"/>
</signal>
<signal name="RW">
<contactref element="U4" pad="1"/>
<contactref element="ST1" pad="18"/>
<contactref element="U6" pad="18"/>
</signal>
<signal name="/DEVSEL">
<contactref element="ST1" pad="41"/>
<contactref element="U7" pad="15"/>
</signal>
<signal name="Q3">
<contactref element="ST1" pad="37"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="Q3R">
<contactref element="R2" pad="1"/>
<contactref element="U6" pad="16"/>
</signal>
<signal name="7M">
<contactref element="ST1" pad="36"/>
<contactref element="U6" pad="17"/>
</signal>
<signal name="/RESET">
<contactref element="ST1" pad="31"/>
<contactref element="U7" pad="12"/>
</signal>
<signal name="/IOSTROBE">
<contactref element="ST1" pad="20"/>
<contactref element="U7" pad="11"/>
</signal>
<signal name="/IOSELECT">
<contactref element="ST1" pad="01"/>
<contactref element="U5" pad="11"/>
</signal>
<signal name="A0">
<contactref element="ST1" pad="02"/>
<contactref element="U5" pad="12"/>
</signal>
<signal name="A1">
<contactref element="ST1" pad="03"/>
<contactref element="U5" pad="13"/>
</signal>
<signal name="A2">
<contactref element="ST1" pad="04"/>
<contactref element="U5" pad="14"/>
</signal>
<signal name="A3">
<contactref element="ST1" pad="05"/>
<contactref element="U5" pad="15"/>
</signal>
<signal name="A4">
<contactref element="ST1" pad="06"/>
<contactref element="U5" pad="16"/>
</signal>
<signal name="A5">
<contactref element="ST1" pad="07"/>
<contactref element="U5" pad="17"/>
</signal>
<signal name="A6">
<contactref element="ST1" pad="08"/>
<contactref element="U5" pad="18"/>
</signal>
<signal name="A7">
<contactref element="ST1" pad="09"/>
<contactref element="U6" pad="11"/>
</signal>
<signal name="A8">
<contactref element="ST1" pad="10"/>
<contactref element="U6" pad="12"/>
</signal>
<signal name="A9">
<contactref element="ST1" pad="11"/>
<contactref element="U6" pad="13"/>
</signal>
<signal name="A10">
<contactref element="ST1" pad="12"/>
<contactref element="U6" pad="14"/>
</signal>
<signal name="A11">
<contactref element="ST1" pad="13"/>
<contactref element="U6" pad="15"/>
</signal>
<signal name="N$1">
<contactref element="ST1" pad="27"/>
<contactref element="ST1" pad="24"/>
</signal>
<signal name="N$2">
<contactref element="ST1" pad="28"/>
<contactref element="ST1" pad="23"/>
</signal>
<signal name="5V">
<contactref element="ST1" pad="25"/>
<contactref element="CON1" pad="11"/>
<contactref element="R5" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="U3" pad="1"/>
<contactref element="U3" pad="3"/>
<contactref element="C19" pad="1"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="PH0">
<contactref element="CON1" pad="2"/>
<contactref element="U1" pad="84"/>
</signal>
<signal name="PH1">
<contactref element="CON1" pad="4"/>
<contactref element="U1" pad="85"/>
</signal>
<signal name="PH2">
<contactref element="CON1" pad="6"/>
<contactref element="U1" pad="86"/>
</signal>
<signal name="PH3">
<contactref element="CON1" pad="8"/>
<contactref element="U1" pad="87"/>
</signal>
<signal name="/WREQ">
<contactref element="CON1" pad="10"/>
<contactref element="U1" pad="88"/>
</signal>
<signal name="SEL">
<contactref element="CON1" pad="12"/>
<contactref element="U1" pad="78"/>
</signal>
<signal name="/ENABLE1">
<contactref element="CON1" pad="14"/>
<contactref element="U1" pad="82"/>
</signal>
<signal name="RDDATA">
<contactref element="CON1" pad="16"/>
<contactref element="U7" pad="14"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="WRDATA">
<contactref element="CON1" pad="18"/>
<contactref element="U1" pad="83"/>
</signal>
<signal name="SENSE">
<contactref element="CON1" pad="20"/>
<contactref element="U7" pad="13"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="/EN35">
<contactref element="CON1" pad="7"/>
<contactref element="U1" pad="98"/>
</signal>
<signal name="/ENABLE2">
<contactref element="CON1" pad="5"/>
<contactref element="U1" pad="99"/>
</signal>
<signal name="-12V">
<contactref element="CON1" pad="9"/>
<contactref element="ST1" pad="33"/>
</signal>
<signal name="12V">
<contactref element="CON1" pad="13"/>
<contactref element="CON1" pad="15"/>
<contactref element="ST1" pad="50"/>
</signal>
<signal name="TCK">
<contactref element="J1" pad="2"/>
<contactref element="U1" pad="91"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="TMS">
<contactref element="J1" pad="1"/>
<contactref element="U1" pad="90"/>
</signal>
<signal name="TDI">
<contactref element="J1" pad="3"/>
<contactref element="U1" pad="94"/>
</signal>
<signal name="TDO">
<contactref element="J1" pad="5"/>
<contactref element="U1" pad="95"/>
</signal>
<signal name="VCC_F">
<contactref element="L1" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="11"/>
<contactref element="U1" pad="23"/>
<contactref element="U1" pad="55"/>
<contactref element="U1" pad="73"/>
<contactref element="U1" pad="80"/>
<contactref element="U1" pad="93"/>
<contactref element="U1" pad="100"/>
<contactref element="U1" pad="26"/>
<contactref element="U1" pad="46"/>
<contactref element="U1" pad="50"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="DBG7">
<contactref element="J3" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="25"/>
</signal>
<signal name="DBG6">
<contactref element="J3" pad="2"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="DBG5">
<contactref element="J3" pad="3"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="DBG4">
<contactref element="J3" pad="4"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="DBG3">
<contactref element="J3" pad="5"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="DBG2">
<contactref element="J3" pad="6"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="DBG1">
<contactref element="J3" pad="7"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="DBG0">
<contactref element="J3" pad="8"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="EN245">
<contactref element="U4" pad="19"/>
<contactref element="U1" pad="30"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="U2" pad="5"/>
<contactref element="U1" pad="49"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="SCLK">
<contactref element="U2" pad="6"/>
<contactref element="U1" pad="31"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="U2" pad="2"/>
<contactref element="U1" pad="32"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="MEMCS">
<contactref element="U2" pad="1"/>
<contactref element="U1" pad="27"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="/IOSELECT_33">
<contactref element="U5" pad="9"/>
<contactref element="U1" pad="53"/>
</signal>
<signal name="A0_33">
<contactref element="U5" pad="8"/>
<contactref element="U1" pad="54"/>
</signal>
<signal name="A1_33">
<contactref element="U5" pad="7"/>
<contactref element="U1" pad="57"/>
</signal>
<signal name="A2_33">
<contactref element="U5" pad="6"/>
<contactref element="U1" pad="58"/>
</signal>
<signal name="A4_33">
<contactref element="U5" pad="4"/>
<contactref element="U1" pad="60"/>
</signal>
<signal name="A3_33">
<contactref element="U5" pad="5"/>
<contactref element="U1" pad="59"/>
</signal>
<signal name="A5_33">
<contactref element="U5" pad="3"/>
<contactref element="U1" pad="62"/>
</signal>
<signal name="A6_33">
<contactref element="U5" pad="2"/>
<contactref element="U1" pad="64"/>
</signal>
<signal name="A7_33">
<contactref element="U6" pad="9"/>
<contactref element="U1" pad="65"/>
</signal>
<signal name="A8_33">
<contactref element="U6" pad="8"/>
<contactref element="U1" pad="66"/>
</signal>
<signal name="A9_33">
<contactref element="U6" pad="7"/>
<contactref element="U1" pad="67"/>
</signal>
<signal name="A10_33">
<contactref element="U6" pad="6"/>
<contactref element="U1" pad="68"/>
</signal>
<signal name="A11_33">
<contactref element="U6" pad="5"/>
<contactref element="U1" pad="69"/>
</signal>
<signal name="Q3R_33">
<contactref element="U6" pad="4"/>
<contactref element="U1" pad="70"/>
</signal>
<signal name="7M_33">
<contactref element="U6" pad="3"/>
<contactref element="U1" pad="63"/>
</signal>
<signal name="RW_33">
<contactref element="U6" pad="2"/>
<contactref element="U1" pad="71"/>
</signal>
<signal name="/IOSTROBE_33">
<contactref element="U7" pad="9"/>
<contactref element="U1" pad="74"/>
</signal>
<signal name="/RESET_33">
<contactref element="U7" pad="8"/>
<contactref element="U1" pad="75"/>
</signal>
<signal name="SENSE_33">
<contactref element="U7" pad="7"/>
<contactref element="U1" pad="97"/>
</signal>
<signal name="RDDATA_33">
<contactref element="U7" pad="6"/>
<contactref element="U1" pad="96"/>
</signal>
<signal name="/DEVSEL_33">
<contactref element="U1" pad="34"/>
<contactref element="U7" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
