<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<library>
<description>Generated from &lt;b&gt;bmowdisk.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="1/6W-RES$1">
<description>1/6W Thru-hole Resistor - *UNPROVEN*</description>
</package>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0603-CAP">
</package>
<package name="0603-RES">
</package>
<package name="0805">
</package>
<package name="1206">
</package>
<package name="1210">
</package>
<package name="AXIAL-0.3">
</package>
<package name="AXIAL-0.3-KIT">
</package>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="AXIAL-0.5">
<description>1/2W Resistor, 0.5" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="AXIAL-0.6">
<description>1W Resistor, 0.6" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="AXIAL-0.8">
<description>2W Resistor, 0.8" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="AXIAL-5MM">
</package>
<package name="CAP-PTH-5MM">
</package>
<package name="CAP-PTH-LARGE">
</package>
<package name="CAP-PTH-SMALL">
</package>
<package name="CAP-PTH-SMALL-KIT">
</package>
<package name="CAP-PTH-SMALL2">
</package>
<package name="CTZ3">
<description>CTZ3 Series land pattern for variable capacitor - CTZ3E-50C-W1-PF</description>
</package>
<package name="GRM43D">
</package>
<package name="R2010">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R2512">
</package>
<package name="S4B-PH">
</package>
<package name="USB-A-H">
<description>&lt;b&gt;USB Series A Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-PCB">
</package>
<package name="USB-A-S">
<description>&lt;b&gt;USB Series A Surface Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-S-NOSILK">
</package>
<package name="USB-A-S-NOSILK-FEMALE">
</package>
<package name="USB-A-S-SILK-FEMALE">
</package>
<package name="USB-A-SMT-MALE">
</package>
<package name="USB-B-PTH">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-B-PTH-VERTICAL">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-B-SMT">
<description>USB Series B Surface Mounted</description>
</package>
<package name="USB-MB-H">
<description>&lt;b&gt;USB Series Mini-B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-MICROB">
<description>Micro USB Package</description>
</package>
<package name="USB-MINIB">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="USB-MINIB-NOSTOP">
</package>
<package name="USB-MINIB-OLD">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="IDC20">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
series 057 contact pc board low profile headers&lt;p&gt;
straight</description>
</package>
<package name="SSOP20">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type SS</description>
</package>
<package name="TQFP100">
</package>
<package name="A2-50PIN-MINI">
</package>
<package name="A2-50PIN-SL1-3">
<description>&lt;B&gt;Apple ][ Peripheral Card&lt;/B&gt;
&lt;br /&gt;
Standard 50-pin edge connector for Apple ][ systems
&lt;br /&gt;
Dimensions for slot #1 to #3
&lt;br /&gt;
Dimensions taken from Tech Note #28</description>
</package>
<package name="A2-50PIN-SL4-7">
<description>&lt;B&gt;Apple ][ Peripheral Card&lt;/B&gt;
&lt;br /&gt;
Standard 50-pin edge connector for Apple ][ systems
&lt;br /&gt;
Dimensions for slot #4 to #7
&lt;br /&gt;
Dimensions taken from Tech Note #28</description>
</package>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
<package name="CHIPLED-0603-TTW">
<description>&lt;b&gt;CHIPLED-0603&lt;/b&gt;&lt;p&gt;
Recommended Solder Pad useable for SmartLEDTM and Chipled - Package 0603&lt;br&gt;
Package able to withstand TTW-soldering heat&lt;br&gt;
Package suitable for TTW-soldering&lt;br&gt;
Source: http://www.osram.convergy.de/ ... LO_LS_LY L89K.pdf</description>
</package>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
<package name="IRL80A">
<description>&lt;B&gt;IR LED&lt;/B&gt;&lt;p&gt;
IR transmitter Siemens</description>
</package>
<package name="KA-3528ASYC">
<description>&lt;b&gt;SURFACE MOUNT LED LAMP&lt;/b&gt; 3.5x2.8mm&lt;p&gt;
Source: http://www.kingbright.com/manager/upload/pdf/KA-3528ASYC(Ver1189474662.1)</description>
</package>
<package name="LD260">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, square, Siemens</description>
</package>
<package name="LED2X5">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
2 x 5 mm, rectangle</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
<package name="LED10MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
10 mm, round</description>
</package>
<package name="LSU260">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
1 mm, round, Siemens</description>
</package>
<package name="LUMILED">
<description>&lt;b&gt;Lumileds Lighting. LUXEON®&lt;/b&gt; without cool pad&lt;p&gt;
Source: K2.pdf</description>
</package>
<package name="LUMILED+">
<description>&lt;b&gt;Lumileds Lighting. LUXEON®&lt;/b&gt; with cool pad&lt;p&gt;
Source: K2.pdf</description>
</package>
<package name="LZR181">
<description>&lt;B&gt;LED BLOCK&lt;/B&gt;&lt;p&gt;
1 LED, Siemens</description>
</package>
<package name="MICRO-SIDELED">
<description>&lt;b&gt;Hyper Micro SIDELED®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LS_LY Y876.pdf</description>
</package>
<package name="MINI-TOPLED-SANTANA">
<description>&lt;b&gt;Mini TOPLED Santana®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG M470.pdf</description>
</package>
<package name="OSRAM-MINI-TOP-LED">
<description>&lt;b&gt;BLUE LINETM Hyper Mini TOPLED® Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LB M676.pdf</description>
</package>
<package name="OSRAM-SIDELED">
<description>&lt;b&gt;Super SIDELED® High-Current LED&lt;/b&gt;&lt;p&gt;
LG A672, LP A672 &lt;br&gt;
Source: http://www.osram.convergy.de/ ... LG_LP_A672.pdf (2004.05.13)</description>
</package>
<package name="P-LCC-2">
<description>&lt;b&gt;TOPLED® High-optical Power LED (HOP)&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... ls_t675.pdf</description>
</package>
<package name="P-LCC-2-TOPLED-RG">
<description>&lt;b&gt;Hyper TOPLED® RG Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LS_LY T776.pdf</description>
</package>
<package name="P-LCC-4">
<description>&lt;b&gt;Power TOPLED®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LA_LY E67B.pdf</description>
</package>
<package name="Q62902-B152">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="Q62902-B153">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="Q62902-B155">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="Q62902-B156">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="SFH480">
<description>&lt;B&gt;IR LED&lt;/B&gt;&lt;p&gt;
infrared emitting diode, Infineon
TO-18, lead spacing 2.54 mm, cathode marking&lt;p&gt;
Inifineon</description>
</package>
<package name="SFH482">
<description>&lt;B&gt;IR LED&lt;/B&gt;&lt;p&gt;
infrared emitting diode, Infineon
TO-18, lead spacing 2.54 mm, cathode marking&lt;p&gt;
Inifineon</description>
</package>
<package name="SMART-LED">
<description>&lt;b&gt;SmartLEDTM Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LS_LY L896.pdf</description>
</package>
<package name="SMARTLED-TTW">
<description>&lt;b&gt;SmartLED TTW&lt;/b&gt;&lt;p&gt;
Recommended Solder Pad useable for SmartLEDTM and Chipled - Package 0603&lt;br&gt;
Package able to withstand TTW-soldering heat&lt;br&gt;
Package suitable for TTW-soldering&lt;br&gt;
Source: http://www.osram.convergy.de/ ... LO_LS_LY L89K.pdf</description>
</package>
<package name="U57X32">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
rectangle, 5.7 x 3.2 mm</description>
</package>
<package name="MA04-1">
</package>
<package name="MA04-1-LOCK">
</package>
<package name="MA06-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="MA06-1-LOCK">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="SOIC08">
</package>
</packages>
<symbols>
<symbol name="CAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="RESISTOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="USB">
<pin name="D+"/>
<pin name="D-"/>
<pin name="GND"/>
<pin name="VBUS"/>
</symbol>
<symbol name="244">
<pin name="!OEA" direction="in"/>
<pin name="!OEB" direction="in"/>
<pin name="DA0" direction="in"/>
<pin name="DA1" direction="in"/>
<pin name="DA2" direction="in"/>
<pin name="DA3" direction="in"/>
<pin name="DB0" direction="in"/>
<pin name="DB1" direction="in"/>
<pin name="DB2" direction="in"/>
<pin name="DB3" direction="in"/>
<pin name="OA0" direction="out"/>
<pin name="OA1" direction="out"/>
<pin name="OA2" direction="out"/>
<pin name="OA3" direction="out"/>
<pin name="OB0" direction="out"/>
<pin name="OB1" direction="out"/>
<pin name="OB2" direction="out"/>
<pin name="OB3" direction="out"/>
</symbol>
<symbol name="M10X2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="VCCGND">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="LCMXO2-640HC-4TG100C">
<pin name="CSSPIN/PB4A"/>
<pin name="DONE/PT11D"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="INITN/PT11C"/>
<pin name="JTAGENB/PT10C"/>
<pin name="MCLK/CCLK/PB6A"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="PB4B"/>
<pin name="PB4C"/>
<pin name="PB4D"/>
<pin name="PB6C/PCLKT2_0"/>
<pin name="PB6D/PCLKC2_0"/>
<pin name="PB10A"/>
<pin name="PB10B"/>
<pin name="PB10C/PCLKT2_1"/>
<pin name="PB10D/PCLKC2_0"/>
<pin name="PB12A"/>
<pin name="PB12B"/>
<pin name="PB12C"/>
<pin name="PB12D"/>
<pin name="PB14A"/>
<pin name="PB14B"/>
<pin name="PL2A"/>
<pin name="PL2B"/>
<pin name="PL2C/PCLKT3_2"/>
<pin name="PL2D/PCLKC3_2"/>
<pin name="PL3A"/>
<pin name="PL3B"/>
<pin name="PL3C"/>
<pin name="PL3D"/>
<pin name="PL5A/PCLKT3_1"/>
<pin name="PL5B/PCLKC3_1"/>
<pin name="PL5C"/>
<pin name="PL5D"/>
<pin name="PL6A"/>
<pin name="PL6B"/>
<pin name="PL6C"/>
<pin name="PL6D"/>
<pin name="PL7A/PCLKT3_0"/>
<pin name="PL7B/PCLKC3_0"/>
<pin name="PL7C"/>
<pin name="PL7D"/>
<pin name="PR2A"/>
<pin name="PR2B"/>
<pin name="PR2C"/>
<pin name="PR2D"/>
<pin name="PR3A"/>
<pin name="PR3B"/>
<pin name="PR3C"/>
<pin name="PR3D"/>
<pin name="PR5A"/>
<pin name="PR5B"/>
<pin name="PR5C/PCLKT1_0"/>
<pin name="PR5D/PCLKC1_0"/>
<pin name="PR6A" direction="pwr"/>
<pin name="PR6B" direction="pwr"/>
<pin name="PR6C"/>
<pin name="PR6D"/>
<pin name="PR7A"/>
<pin name="PR7B"/>
<pin name="PR7C"/>
<pin name="PR7D"/>
<pin name="PROGRAMN/PT10D"/>
<pin name="PT6A"/>
<pin name="PT6B"/>
<pin name="PT6C"/>
<pin name="PT6D"/>
<pin name="PT9A/PCLKT0_1"/>
<pin name="PT9B/PCLKC0_1"/>
<pin name="PT10A"/>
<pin name="PT10B"/>
<pin name="PT11A"/>
<pin name="SCL/PCLKT0_0"/>
<pin name="SDA/PCLKC0_0/PT9D"/>
<pin name="SI/SISPI/PB14D"/>
<pin name="SN/PB14C"/>
<pin name="SO/SPISO/PB6B"/>
<pin name="TCK/PT7C"/>
<pin name="TDI/PT7B"/>
<pin name="TDO/PT7A"/>
<pin name="TMS/PT7D"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="VCCIO0@1" direction="pwr"/>
<pin name="VCCIO0@2" direction="pwr"/>
<pin name="VCCIO1@1" direction="pwr"/>
<pin name="VCCIO1@2" direction="pwr"/>
<pin name="VCCIO2@1" direction="pwr"/>
<pin name="VCCIO2@2" direction="pwr"/>
<pin name="VCCIO3@1" direction="pwr"/>
<pin name="VCCIO3@2" direction="pwr"/>
</symbol>
<symbol name="ATPIN">
<pin name="P"/>
</symbol>
<symbol name="LED">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="MA04-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="MA06-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="+3V3">
<pin name="+3V3" direction="sup"/>
</symbol>
<symbol name="+5V">
<pin name="+5V" direction="sup"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="MIC5219B">
<pin name="BYP" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="245">
<pin name="!OE" direction="in"/>
<pin name="DIR" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="B3" direction="out"/>
<pin name="B4" direction="out"/>
<pin name="B5" direction="out"/>
<pin name="B6" direction="out"/>
<pin name="B7" direction="out"/>
<pin name="B8" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="LCMXO2-1200HC-TQFP100">
<pin name="CSSPIN/P27"/>
<pin name="DONE/P76"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="INITN/P77"/>
<pin name="JTAGENB/P82"/>
<pin name="MCLK/CCLK/P31"/>
<pin name="NC" direction="nc"/>
<pin name="VCCIO3@3" direction="pwr"/>
<pin name="NC@2" direction="nc"/>
<pin name="P28"/>
<pin name="P29"/>
<pin name="P30"/>
<pin name="P34/PCLKT2_0"/>
<pin name="P35/PCLKC2_0"/>
<pin name="P36"/>
<pin name="P37"/>
<pin name="P38/PCLKT2_1"/>
<pin name="P39/PCLKC2_0"/>
<pin name="P40"/>
<pin name="P41"/>
<pin name="P42"/>
<pin name="P43"/>
<pin name="P45"/>
<pin name="P47"/>
<pin name="P1"/>
<pin name="P2"/>
<pin name="P3/PCLKT3_2"/>
<pin name="P4/PCLKC3_2"/>
<pin name="P7"/>
<pin name="P8"/>
<pin name="P9"/>
<pin name="P10"/>
<pin name="P12/PCLKT3_1"/>
<pin name="P13/PCLKC3_1"/>
<pin name="P14"/>
<pin name="P15"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="P18"/>
<pin name="P19"/>
<pin name="P20/PCLKT3_0"/>
<pin name="P21/PCLKC3_0"/>
<pin name="P24"/>
<pin name="P25"/>
<pin name="P75"/>
<pin name="P74"/>
<pin name="P71"/>
<pin name="P70"/>
<pin name="P69"/>
<pin name="P68"/>
<pin name="P67"/>
<pin name="P66"/>
<pin name="P65"/>
<pin name="P64"/>
<pin name="P63/PCLKT1_0"/>
<pin name="P62/PCLKC1_0"/>
<pin name="P60"/>
<pin name="P59"/>
<pin name="P58"/>
<pin name="P57"/>
<pin name="P54"/>
<pin name="P53"/>
<pin name="P52"/>
<pin name="P51"/>
<pin name="PROGRAMN/P81"/>
<pin name="P99"/>
<pin name="P98"/>
<pin name="P97"/>
<pin name="P96"/>
<pin name="P88/PCLKT0_1"/>
<pin name="P87/PCLKC0_1"/>
<pin name="P84"/>
<pin name="P83"/>
<pin name="P78"/>
<pin name="SCL/PCLKT0_0/P86"/>
<pin name="SDA/PCLKC0_0/P85"/>
<pin name="SI/SISPI/P49"/>
<pin name="SN/P48"/>
<pin name="SO/SPISO/P32"/>
<pin name="TCK/P91"/>
<pin name="TDI/P94"/>
<pin name="TDO/P95"/>
<pin name="TMS/P90"/>
<pin name="VCCSUPPLY@1" direction="pwr"/>
<pin name="VCCSUPPLY@2" direction="pwr"/>
<pin name="VCCIO0@1" direction="pwr"/>
<pin name="VCCIO0@2" direction="pwr"/>
<pin name="VCCIO1@1" direction="pwr"/>
<pin name="VCCIO1@2" direction="pwr"/>
<pin name="VCCIO2@1" direction="pwr"/>
<pin name="VCCIO2@2" direction="pwr"/>
<pin name="VCCIO3@1" direction="pwr"/>
<pin name="VCCIO3@2" direction="pwr"/>
</symbol>
<symbol name="SPI-FLASH">
<pin name="/WP" direction="pas"/>
<pin name="SO" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="/CS" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="/HOLD" direction="out"/>
<pin name="SCLK" direction="out"/>
<pin name="SI" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CAP" prefix="C" uservalue="yes">
<description>&lt;b&gt;Capacitor&lt;/b&gt;
Standard 0603 ceramic capacitor, and 0.1" leaded capacitor.</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="0402-CAP" package="0402-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603-CAP" package="0603-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1210" package="1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ASMD" package="CTZ3">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KIT" package="CAP-PTH-SMALL-KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="CAP-PTH-SMALL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH1" package="CAP-PTH-5MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH2" package="CAP-PTH-SMALL2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH3" package="CAP-PTH-LARGE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="GRM43D">
<connects>
<connect gate="G$1" pin="1" pad="A"/>
<connect gate="G$1" pin="2" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_" package="AXIAL-5MM">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESISTOR" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor&lt;/b&gt;
Basic schematic elements and footprints for 0603, 1206, and PTH resistors.</description>
<gates>
<gate name="G$1" symbol="RESISTOR"/>
</gates>
<devices>
<device name="0402-RES" package="0402-RES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603-RES" package="0603-RES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805-RES" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2010" package="R2010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2512" package="R2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AXIAL-0.3" package="AXIAL-0.3">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KIT" package="AXIAL-0.3-KIT">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-1/2W" package="AXIAL-0.5">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-1/4W" package="AXIAL-0.4">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-1/6W" package="1/6W-RES$1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-1W" package="AXIAL-0.6">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-2W" package="AXIAL-0.8">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB" prefix="JP">
<description>&lt;b&gt;USB Connectors&lt;/b&gt;
&lt;p&gt;USB-B-PTH is fully proven SKU : PRT-00139/CONN-08278
&lt;p&gt;USB-miniB is fully proven SKU : PRT-00587
&lt;p&gt;USB-A-PCB is untested.
&lt;p&gt;USB-A-H is throughly reviewed, but untested. Spark Fun Electronics SKU : PRT-00437
&lt;p&gt;USB-B-SMT is throughly reviewed, but untested. Needs silkscreen touching up.
&lt;p&gt;USB-A-S has not been used/tested
&lt;p&gt;USB-MB-H has not been used/tested
&lt;P&gt;USB-MICROB has been used. CONN-09505</description>
<gates>
<gate name="G$1" symbol="USB"/>
</gates>
<devices>
<device name="-A-H" package="USB-A-H">
<connects>
<connect gate="G$1" pin="D+" pad="D-"/>
<connect gate="G$1" pin="D-" pad="D+"/>
<connect gate="G$1" pin="GND" pad="VBUS"/>
<connect gate="G$1" pin="VBUS" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-A-S" package="USB-A-S">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-A-SMD" package="USB-A-S-NOSILK-FEMALE">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09520"/>
</technology>
</technologies>
</device>
<device name="-B-S" package="USB-B-SMT">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VUSB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-JST-2MM-SMT" package="S4B-PH">
<connects>
<connect gate="G$1" pin="D+" pad="2"/>
<connect gate="G$1" pin="D-" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VBUS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MB-H" package="USB-MB-H">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MICROB" package="USB-MICROB">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND MT1 MT2"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09505"/>
</technology>
</technologies>
</device>
<device name="-SMD-NS" package="USB-MINIB-NOSTOP">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="A-SMD-MALE" package="USB-A-SMT-MALE">
<connects>
<connect gate="G$1" pin="D+" pad="D+1"/>
<connect gate="G$1" pin="D-" pad="D-1"/>
<connect gate="G$1" pin="GND" pad="GND1"/>
<connect gate="G$1" pin="VBUS" pad="VBUS1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="OLD" package="USB-MINIB-OLD">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PCB" package="USB-A-PCB">
<connects>
<connect gate="G$1" pin="D+" pad="USB_P"/>
<connect gate="G$1" pin="D-" pad="USB_M"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="5V"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="USB-B-PTH">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08278"/>
<attribute name="VALUE" value="USB-B"/>
</technology>
</technologies>
</device>
<device name="PTH-VERTICAL" package="USB-B-PTH-VERTICAL">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="USB-MINIB">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="USB-A-S-NOSILK" package="USB-A-S-NOSILK">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_" package="USB-A-S-SILK-FEMALE">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74X244" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="244"/>
<gate name="P" symbol="VCCGND"/>
</gates>
<devices>
<device name="" package="SSOP20">
<connects>
<connect gate="G$1" pin="!OEA" pad="1"/>
<connect gate="G$1" pin="!OEB" pad="19"/>
<connect gate="G$1" pin="DA0" pad="2"/>
<connect gate="G$1" pin="DA1" pad="4"/>
<connect gate="G$1" pin="DA2" pad="6"/>
<connect gate="G$1" pin="DA3" pad="8"/>
<connect gate="G$1" pin="DB0" pad="17"/>
<connect gate="G$1" pin="DB1" pad="15"/>
<connect gate="G$1" pin="DB2" pad="13"/>
<connect gate="G$1" pin="DB3" pad="11"/>
<connect gate="G$1" pin="OA0" pad="18"/>
<connect gate="G$1" pin="OA1" pad="16"/>
<connect gate="G$1" pin="OA2" pad="14"/>
<connect gate="G$1" pin="OA3" pad="12"/>
<connect gate="G$1" pin="OB0" pad="3"/>
<connect gate="G$1" pin="OB1" pad="5"/>
<connect gate="G$1" pin="OB2" pad="7"/>
<connect gate="G$1" pin="OB3" pad="9"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IDC20">
<gates>
<gate name="G$1" symbol="M10X2"/>
</gates>
<devices>
<device name="" package="IDC20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LCMXO2-640HC-4TG100C">
<gates>
<gate name="G$1" symbol="LCMXO2-640HC-4TG100C"/>
</gates>
<devices>
<device name="" package="TQFP100">
<connects>
<connect gate="G$1" pin="CSSPIN/PB4A" pad="27"/>
<connect gate="G$1" pin="DONE/PT11D" pad="76"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="GND@2" pad="22"/>
<connect gate="G$1" pin="GND@3" pad="33"/>
<connect gate="G$1" pin="GND@4" pad="44"/>
<connect gate="G$1" pin="GND@5" pad="56"/>
<connect gate="G$1" pin="GND@6" pad="72"/>
<connect gate="G$1" pin="GND@7" pad="79"/>
<connect gate="G$1" pin="GND@8" pad="92"/>
<connect gate="G$1" pin="INITN/PT11C" pad="77"/>
<connect gate="G$1" pin="JTAGENB/PT10C" pad="82"/>
<connect gate="G$1" pin="MCLK/CCLK/PB6A" pad="31"/>
<connect gate="G$1" pin="NC" pad="89"/>
<connect gate="G$1" pin="NC@1" pad="11"/>
<connect gate="G$1" pin="NC@2" pad="61"/>
<connect gate="G$1" pin="PB10A" pad="36"/>
<connect gate="G$1" pin="PB10B" pad="37"/>
<connect gate="G$1" pin="PB10C/PCLKT2_1" pad="38"/>
<connect gate="G$1" pin="PB10D/PCLKC2_0" pad="39"/>
<connect gate="G$1" pin="PB12A" pad="40"/>
<connect gate="G$1" pin="PB12B" pad="41"/>
<connect gate="G$1" pin="PB12C" pad="42"/>
<connect gate="G$1" pin="PB12D" pad="43"/>
<connect gate="G$1" pin="PB14A" pad="45"/>
<connect gate="G$1" pin="PB14B" pad="47"/>
<connect gate="G$1" pin="PB4B" pad="28"/>
<connect gate="G$1" pin="PB4C" pad="29"/>
<connect gate="G$1" pin="PB4D" pad="30"/>
<connect gate="G$1" pin="PB6C/PCLKT2_0" pad="34"/>
<connect gate="G$1" pin="PB6D/PCLKC2_0" pad="35"/>
<connect gate="G$1" pin="PL2A" pad="1"/>
<connect gate="G$1" pin="PL2B" pad="2"/>
<connect gate="G$1" pin="PL2C/PCLKT3_2" pad="3"/>
<connect gate="G$1" pin="PL2D/PCLKC3_2" pad="4"/>
<connect gate="G$1" pin="PL3A" pad="7"/>
<connect gate="G$1" pin="PL3B" pad="8"/>
<connect gate="G$1" pin="PL3C" pad="9"/>
<connect gate="G$1" pin="PL3D" pad="10"/>
<connect gate="G$1" pin="PL5A/PCLKT3_1" pad="12"/>
<connect gate="G$1" pin="PL5B/PCLKC3_1" pad="13"/>
<connect gate="G$1" pin="PL5C" pad="14"/>
<connect gate="G$1" pin="PL5D" pad="15"/>
<connect gate="G$1" pin="PL6A" pad="16"/>
<connect gate="G$1" pin="PL6B" pad="17"/>
<connect gate="G$1" pin="PL6C" pad="18"/>
<connect gate="G$1" pin="PL6D" pad="19"/>
<connect gate="G$1" pin="PL7A/PCLKT3_0" pad="20"/>
<connect gate="G$1" pin="PL7B/PCLKC3_0" pad="21"/>
<connect gate="G$1" pin="PL7C" pad="24"/>
<connect gate="G$1" pin="PL7D" pad="25"/>
<connect gate="G$1" pin="PR2A" pad="75"/>
<connect gate="G$1" pin="PR2B" pad="74"/>
<connect gate="G$1" pin="PR2C" pad="71"/>
<connect gate="G$1" pin="PR2D" pad="70"/>
<connect gate="G$1" pin="PR3A" pad="69"/>
<connect gate="G$1" pin="PR3B" pad="68"/>
<connect gate="G$1" pin="PR3C" pad="67"/>
<connect gate="G$1" pin="PR3D" pad="66"/>
<connect gate="G$1" pin="PR5A" pad="65"/>
<connect gate="G$1" pin="PR5B" pad="64"/>
<connect gate="G$1" pin="PR5C/PCLKT1_0" pad="63"/>
<connect gate="G$1" pin="PR5D/PCLKC1_0" pad="62"/>
<connect gate="G$1" pin="PR6A" pad="60"/>
<connect gate="G$1" pin="PR6B" pad="59"/>
<connect gate="G$1" pin="PR6C" pad="58"/>
<connect gate="G$1" pin="PR6D" pad="57"/>
<connect gate="G$1" pin="PR7A" pad="54"/>
<connect gate="G$1" pin="PR7B" pad="53"/>
<connect gate="G$1" pin="PR7C" pad="52"/>
<connect gate="G$1" pin="PR7D" pad="51"/>
<connect gate="G$1" pin="PROGRAMN/PT10D" pad="81"/>
<connect gate="G$1" pin="PT10A" pad="84"/>
<connect gate="G$1" pin="PT10B" pad="83"/>
<connect gate="G$1" pin="PT11A" pad="78"/>
<connect gate="G$1" pin="PT6A" pad="99"/>
<connect gate="G$1" pin="PT6B" pad="98"/>
<connect gate="G$1" pin="PT6C" pad="97"/>
<connect gate="G$1" pin="PT6D" pad="96"/>
<connect gate="G$1" pin="PT9A/PCLKT0_1" pad="88"/>
<connect gate="G$1" pin="PT9B/PCLKC0_1" pad="87"/>
<connect gate="G$1" pin="SCL/PCLKT0_0" pad="86"/>
<connect gate="G$1" pin="SDA/PCLKC0_0/PT9D" pad="85"/>
<connect gate="G$1" pin="SI/SISPI/PB14D" pad="49"/>
<connect gate="G$1" pin="SN/PB14C" pad="48"/>
<connect gate="G$1" pin="SO/SPISO/PB6B" pad="32"/>
<connect gate="G$1" pin="TCK/PT7C" pad="91"/>
<connect gate="G$1" pin="TDI/PT7B" pad="94"/>
<connect gate="G$1" pin="TDO/PT7A" pad="95"/>
<connect gate="G$1" pin="TMS/PT7D" pad="90"/>
<connect gate="G$1" pin="VCC@1" pad="50"/>
<connect gate="G$1" pin="VCC@2" pad="100"/>
<connect gate="G$1" pin="VCCIO0@1" pad="80"/>
<connect gate="G$1" pin="VCCIO0@2" pad="93"/>
<connect gate="G$1" pin="VCCIO1@1" pad="55"/>
<connect gate="G$1" pin="VCCIO1@2" pad="73"/>
<connect gate="G$1" pin="VCCIO2@1" pad="26"/>
<connect gate="G$1" pin="VCCIO2@2" pad="46"/>
<connect gate="G$1" pin="VCCIO3@1" pad="5"/>
<connect gate="G$1" pin="VCCIO3@2" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A2-50PIN" prefix="ST" uservalue="yes">
<description>&lt;B&gt;Apple ][ Peripheral Card Connector&lt;/B&gt;
&lt;br /&gt;
This is the, default, 50-pin connector for slot #1 to #7
&lt;br /&gt;
Pins are laid out as seen from the top of the slot</description>
<gates>
<gate name="_+5V" symbol="ATPIN"/>
<gate name="_+12V" symbol="ATPIN"/>
<gate name="_-5V" symbol="ATPIN"/>
<gate name="_-12V" symbol="ATPIN"/>
<gate name="_00" symbol="ATPIN"/>
<gate name="_01" symbol="ATPIN"/>
<gate name="_7M" symbol="ATPIN"/>
<gate name="_A00" symbol="ATPIN"/>
<gate name="_A01" symbol="ATPIN"/>
<gate name="_A02" symbol="ATPIN"/>
<gate name="_A03" symbol="ATPIN"/>
<gate name="_A04" symbol="ATPIN"/>
<gate name="_A05" symbol="ATPIN"/>
<gate name="_A06" symbol="ATPIN"/>
<gate name="_A07" symbol="ATPIN"/>
<gate name="_A08" symbol="ATPIN"/>
<gate name="_A09" symbol="ATPIN"/>
<gate name="_A10" symbol="ATPIN"/>
<gate name="_A11" symbol="ATPIN"/>
<gate name="_A12" symbol="ATPIN"/>
<gate name="_A13" symbol="ATPIN"/>
<gate name="_A14" symbol="ATPIN"/>
<gate name="_A15" symbol="ATPIN"/>
<gate name="_D0" symbol="ATPIN"/>
<gate name="_D1" symbol="ATPIN"/>
<gate name="_D2" symbol="ATPIN"/>
<gate name="_D3" symbol="ATPIN"/>
<gate name="_D4" symbol="ATPIN"/>
<gate name="_D5" symbol="ATPIN"/>
<gate name="_D6" symbol="ATPIN"/>
<gate name="_D7" symbol="ATPIN"/>
<gate name="_DEVSELECT\" symbol="ATPIN"/>
<gate name="_DMA\" symbol="ATPIN"/>
<gate name="_DMA_IN" symbol="ATPIN"/>
<gate name="_DMA_OUT" symbol="ATPIN"/>
<gate name="_GND" symbol="ATPIN"/>
<gate name="_INH\" symbol="ATPIN"/>
<gate name="_INT_IN" symbol="ATPIN"/>
<gate name="_INT_OUT" symbol="ATPIN"/>
<gate name="_IOSELECT\" symbol="ATPIN"/>
<gate name="_IOSTR\" symbol="ATPIN"/>
<gate name="_IRQ\" symbol="ATPIN"/>
<gate name="_NC@1" symbol="ATPIN"/>
<gate name="_NC@2" symbol="ATPIN"/>
<gate name="_NMI\" symbol="ATPIN"/>
<gate name="_Q3" symbol="ATPIN"/>
<gate name="_RDY" symbol="ATPIN"/>
<gate name="_RES\" symbol="ATPIN"/>
<gate name="_RW" symbol="ATPIN"/>
<gate name="_USER1" symbol="ATPIN"/>
</gates>
<devices>
<device name="MINI" package="A2-50PIN-MINI">
<connects>
<connect gate="_+12V" pin="P" pad="50"/>
<connect gate="_+5V" pin="P" pad="25"/>
<connect gate="_-12V" pin="P" pad="33"/>
<connect gate="_-5V" pin="P" pad="34"/>
<connect gate="_00" pin="P" pad="40"/>
<connect gate="_01" pin="P" pad="38"/>
<connect gate="_7M" pin="P" pad="36"/>
<connect gate="_A00" pin="P" pad="02"/>
<connect gate="_A01" pin="P" pad="03"/>
<connect gate="_A02" pin="P" pad="04"/>
<connect gate="_A03" pin="P" pad="05"/>
<connect gate="_A04" pin="P" pad="06"/>
<connect gate="_A05" pin="P" pad="07"/>
<connect gate="_A06" pin="P" pad="08"/>
<connect gate="_A07" pin="P" pad="09"/>
<connect gate="_A08" pin="P" pad="10"/>
<connect gate="_A09" pin="P" pad="11"/>
<connect gate="_A10" pin="P" pad="12"/>
<connect gate="_A11" pin="P" pad="13"/>
<connect gate="_A12" pin="P" pad="14"/>
<connect gate="_A13" pin="P" pad="15"/>
<connect gate="_A14" pin="P" pad="16"/>
<connect gate="_A15" pin="P" pad="17"/>
<connect gate="_D0" pin="P" pad="49"/>
<connect gate="_D1" pin="P" pad="48"/>
<connect gate="_D2" pin="P" pad="47"/>
<connect gate="_D3" pin="P" pad="46"/>
<connect gate="_D4" pin="P" pad="45"/>
<connect gate="_D5" pin="P" pad="44"/>
<connect gate="_D6" pin="P" pad="43"/>
<connect gate="_D7" pin="P" pad="42"/>
<connect gate="_DEVSELECT\" pin="P" pad="41"/>
<connect gate="_DMA\" pin="P" pad="22"/>
<connect gate="_DMA_IN" pin="P" pad="27"/>
<connect gate="_DMA_OUT" pin="P" pad="24"/>
<connect gate="_GND" pin="P" pad="26"/>
<connect gate="_INH\" pin="P" pad="32"/>
<connect gate="_INT_IN" pin="P" pad="28"/>
<connect gate="_INT_OUT" pin="P" pad="23"/>
<connect gate="_IOSELECT\" pin="P" pad="01"/>
<connect gate="_IOSTR\" pin="P" pad="20"/>
<connect gate="_IRQ\" pin="P" pad="30"/>
<connect gate="_NC@1" pin="P" pad="19"/>
<connect gate="_NC@2" pin="P" pad="35"/>
<connect gate="_NMI\" pin="P" pad="29"/>
<connect gate="_Q3" pin="P" pad="37"/>
<connect gate="_RDY" pin="P" pad="21"/>
<connect gate="_RES\" pin="P" pad="31"/>
<connect gate="_RW" pin="P" pad="18"/>
<connect gate="_USER1" pin="P" pad="39"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SLOT1-3" package="A2-50PIN-SL1-3">
<connects>
<connect gate="_+12V" pin="P" pad="50"/>
<connect gate="_+5V" pin="P" pad="25"/>
<connect gate="_-12V" pin="P" pad="33"/>
<connect gate="_-5V" pin="P" pad="34"/>
<connect gate="_00" pin="P" pad="40"/>
<connect gate="_01" pin="P" pad="38"/>
<connect gate="_7M" pin="P" pad="36"/>
<connect gate="_A00" pin="P" pad="02"/>
<connect gate="_A01" pin="P" pad="03"/>
<connect gate="_A02" pin="P" pad="04"/>
<connect gate="_A03" pin="P" pad="05"/>
<connect gate="_A04" pin="P" pad="06"/>
<connect gate="_A05" pin="P" pad="07"/>
<connect gate="_A06" pin="P" pad="08"/>
<connect gate="_A07" pin="P" pad="09"/>
<connect gate="_A08" pin="P" pad="10"/>
<connect gate="_A09" pin="P" pad="11"/>
<connect gate="_A10" pin="P" pad="12"/>
<connect gate="_A11" pin="P" pad="13"/>
<connect gate="_A12" pin="P" pad="14"/>
<connect gate="_A13" pin="P" pad="15"/>
<connect gate="_A14" pin="P" pad="16"/>
<connect gate="_A15" pin="P" pad="17"/>
<connect gate="_D0" pin="P" pad="49"/>
<connect gate="_D1" pin="P" pad="48"/>
<connect gate="_D2" pin="P" pad="47"/>
<connect gate="_D3" pin="P" pad="46"/>
<connect gate="_D4" pin="P" pad="45"/>
<connect gate="_D5" pin="P" pad="44"/>
<connect gate="_D6" pin="P" pad="43"/>
<connect gate="_D7" pin="P" pad="42"/>
<connect gate="_DEVSELECT\" pin="P" pad="41"/>
<connect gate="_DMA\" pin="P" pad="22"/>
<connect gate="_DMA_IN" pin="P" pad="27"/>
<connect gate="_DMA_OUT" pin="P" pad="24"/>
<connect gate="_GND" pin="P" pad="26"/>
<connect gate="_INH\" pin="P" pad="32"/>
<connect gate="_INT_IN" pin="P" pad="28"/>
<connect gate="_INT_OUT" pin="P" pad="23"/>
<connect gate="_IOSELECT\" pin="P" pad="01"/>
<connect gate="_IOSTR\" pin="P" pad="20"/>
<connect gate="_IRQ\" pin="P" pad="30"/>
<connect gate="_NC@1" pin="P" pad="19"/>
<connect gate="_NC@2" pin="P" pad="35"/>
<connect gate="_NMI\" pin="P" pad="29"/>
<connect gate="_Q3" pin="P" pad="37"/>
<connect gate="_RDY" pin="P" pad="21"/>
<connect gate="_RES\" pin="P" pad="31"/>
<connect gate="_RW" pin="P" pad="18"/>
<connect gate="_USER1" pin="P" pad="39"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SLOT4-7" package="A2-50PIN-SL4-7">
<connects>
<connect gate="_+12V" pin="P" pad="50"/>
<connect gate="_+5V" pin="P" pad="25"/>
<connect gate="_-12V" pin="P" pad="33"/>
<connect gate="_-5V" pin="P" pad="34"/>
<connect gate="_00" pin="P" pad="40"/>
<connect gate="_01" pin="P" pad="38"/>
<connect gate="_7M" pin="P" pad="36"/>
<connect gate="_A00" pin="P" pad="02"/>
<connect gate="_A01" pin="P" pad="03"/>
<connect gate="_A02" pin="P" pad="04"/>
<connect gate="_A03" pin="P" pad="05"/>
<connect gate="_A04" pin="P" pad="06"/>
<connect gate="_A05" pin="P" pad="07"/>
<connect gate="_A06" pin="P" pad="08"/>
<connect gate="_A07" pin="P" pad="09"/>
<connect gate="_A08" pin="P" pad="10"/>
<connect gate="_A09" pin="P" pad="11"/>
<connect gate="_A10" pin="P" pad="12"/>
<connect gate="_A11" pin="P" pad="13"/>
<connect gate="_A12" pin="P" pad="14"/>
<connect gate="_A13" pin="P" pad="15"/>
<connect gate="_A14" pin="P" pad="16"/>
<connect gate="_A15" pin="P" pad="17"/>
<connect gate="_D0" pin="P" pad="49"/>
<connect gate="_D1" pin="P" pad="48"/>
<connect gate="_D2" pin="P" pad="47"/>
<connect gate="_D3" pin="P" pad="46"/>
<connect gate="_D4" pin="P" pad="45"/>
<connect gate="_D5" pin="P" pad="44"/>
<connect gate="_D6" pin="P" pad="43"/>
<connect gate="_D7" pin="P" pad="42"/>
<connect gate="_DEVSELECT\" pin="P" pad="41"/>
<connect gate="_DMA\" pin="P" pad="22"/>
<connect gate="_DMA_IN" pin="P" pad="27"/>
<connect gate="_DMA_OUT" pin="P" pad="24"/>
<connect gate="_GND" pin="P" pad="26"/>
<connect gate="_INH\" pin="P" pad="32"/>
<connect gate="_INT_IN" pin="P" pad="28"/>
<connect gate="_INT_OUT" pin="P" pad="23"/>
<connect gate="_IOSELECT\" pin="P" pad="01"/>
<connect gate="_IOSTR\" pin="P" pad="20"/>
<connect gate="_IRQ\" pin="P" pad="30"/>
<connect gate="_NC@1" pin="P" pad="19"/>
<connect gate="_NC@2" pin="P" pad="35"/>
<connect gate="_NMI\" pin="P" pad="29"/>
<connect gate="_Q3" pin="P" pad="37"/>
<connect gate="_RDY" pin="P" pad="21"/>
<connect gate="_RES\" pin="P" pad="31"/>
<connect gate="_RW" pin="P" pad="18"/>
<connect gate="_USER1" pin="P" pad="39"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED" prefix="LED" uservalue="yes">
<description>&lt;b&gt;LED&lt;/b&gt;&lt;p&gt;
&lt;u&gt;OSRAM&lt;/u&gt;:&lt;br&gt;

- &lt;u&gt;CHIPLED&lt;/u&gt;&lt;br&gt;
LG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971
LH N974, LH R974&lt;br&gt;
LS Q976, LO Q976, LY Q976&lt;br&gt;
LO Q996&lt;br&gt;

- &lt;u&gt;Hyper CHIPLED&lt;/u&gt;&lt;br&gt;
LW Q18S&lt;br&gt;
LB Q993, LB Q99A, LB R99A&lt;br&gt;

- &lt;u&gt;SideLED&lt;/u&gt;&lt;br&gt;
LS A670, LO A670, LY A670, LG A670, LP A670&lt;br&gt;
LB A673, LV A673, LT A673, LW A673&lt;br&gt;
LH A674&lt;br&gt;
LY A675&lt;br&gt;
LS A676, LA A676, LO A676, LY A676, LW A676&lt;br&gt;
LS A679, LY A679, LG A679&lt;br&gt;

-  &lt;u&gt;Hyper Micro SIDELED®&lt;/u&gt;&lt;br&gt;
LS Y876, LA Y876, LO Y876, LY Y876&lt;br&gt;
LT Y87S&lt;br&gt;

- &lt;u&gt;SmartLED&lt;/u&gt;&lt;br&gt;
LW L88C, LW L88S&lt;br&gt;
LB L89C, LB L89S, LG L890&lt;br&gt;
LS L89K, LO L89K, LY L89K&lt;br&gt;
LS L896, LA L896, LO L896, LY L896&lt;br&gt;

- &lt;u&gt;TOPLED&lt;/u&gt;&lt;br&gt;
LS T670, LO T670, LY T670, LG T670, LP T670&lt;br&gt;
LSG T670, LSP T670, LSY T670, LOP T670, LYG T670&lt;br&gt;
LG T671, LOG T671, LSG T671&lt;br&gt;
LB T673, LV T673, LT T673, LW T673&lt;br&gt;
LH T674&lt;br&gt;
LS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676&lt;br&gt;
LB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C&lt;br&gt;
LS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C&lt;br&gt;
LW T67C&lt;br&gt;
LS T679, LY T679, LG T679&lt;br&gt;
LS T770, LO T770, LY T770, LG T770, LP T770&lt;br&gt;
LB T773, LV T773, LT T773, LW T773&lt;br&gt;
LH T774&lt;br&gt;
LS E675, LA E675, LY E675, LS T675&lt;br&gt;
LS T776, LA T776, LO T776, LY T776, LB T776&lt;br&gt;
LHGB T686&lt;br&gt;
LT T68C, LB T68C&lt;br&gt;

- &lt;u&gt;Hyper Mini TOPLED®&lt;/u&gt;&lt;br&gt;
LB M676&lt;br&gt;

- &lt;u&gt;Mini TOPLED Santana®&lt;/u&gt;&lt;br&gt;
LG M470&lt;br&gt;
LS M47K, LO M47K, LY M47K
&lt;p&gt;
Source: http://www.osram.convergy.de&lt;p&gt;

&lt;u&gt;LUXEON:&lt;/u&gt;&lt;br&gt;
- &lt;u&gt;LUMILED®&lt;/u&gt;&lt;br&gt;
LXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00&lt;br&gt;
LXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00&lt;br&gt;
LXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00&lt;br&gt;
LXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00&lt;br&gt;
LXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00&lt;br&gt;
LXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00&lt;br&gt;
LXK2-PH12-R00, LXK2-PH12-S00&lt;br&gt;
LXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00
&lt;p&gt;
Source: www.luxeon.com&lt;p&gt;

&lt;u&gt;KINGBRIGHT:&lt;/U&gt;&lt;p&gt;
KA-3528ASYC&lt;br&gt;
Source: www.kingbright.com</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="SMARTLED-TTW">
<connects>
<connect gate="G$1" pin="A" pad="A@1"/>
<connect gate="G$1" pin="C" pad="C@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-LUMILED" package="LUMILED">
<connects>
<connect gate="G$1" pin="A" pad="2+"/>
<connect gate="G$1" pin="C" pad="4-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-LUMILED+" package="LUMILED+">
<connects>
<connect gate="G$1" pin="A" pad="2+"/>
<connect gate="G$1" pin="C" pad="4-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3MM" package="LED3MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="LED5MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="10MM" package="LED10MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B152" package="Q62902-B152">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B153" package="Q62902-B153">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B155" package="Q62902-B155">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B156" package="Q62902-B156">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIP-LED0603" package="CHIP-LED0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIP-LED0805" package="CHIP-LED0805">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED-0603-TTW" package="CHIPLED-0603-TTW">
<connects>
<connect gate="G$1" pin="A" pad="A@1"/>
<connect gate="G$1" pin="C" pad="C@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED_0603" package="CHIPLED_0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED_0805" package="CHIPLED_0805">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED_1206" package="CHIPLED_1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="IRL80A" package="IRL80A">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KA-3528ASYC" package="KA-3528ASYC">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LD260" package="LD260">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LSU260" package="LSU260">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LZR181" package="LZR181">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MICRO-SIDELED" package="MICRO-SIDELED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MINI-TOP" package="OSRAM-MINI-TOP-LED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P-LCC-2" package="P-LCC-2">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P-LCC-2-BACK" package="P-LCC-2-TOPLED-RG">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P-LCC-4" package="P-LCC-4">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C@4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SFH480" package="SFH480">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SFH482" package="SFH482">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SIDELED" package="OSRAM-SIDELED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMART-LED" package="SMART-LED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMT1206" package="1206">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SQR2X5" package="LED2X5">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SQR5.7X3.2" package="U57X32">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TOPLED-SANTANA" package="MINI-TOPLED-SANTANA">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MA04-1">
<gates>
<gate name="G$1" symbol="MA04-1"/>
</gates>
<devices>
<device name="LOCK" package="MA04-1-LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="MA04-1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MA06-1" prefix="SV" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="MA06-1"/>
</gates>
<devices>
<device name="LOCK" package="MA06-1-LOCK">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="1" pin="3" pad="3"/>
<connect gate="1" pin="4" pad="4"/>
<connect gate="1" pin="5" pad="5"/>
<connect gate="1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NORMAL" package="MA06-1">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="1" pin="3" pad="3"/>
<connect gate="1" pin="4" pad="4"/>
<connect gate="1" pin="5" pad="5"/>
<connect gate="1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="+3V3" prefix="+3V3">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="+3V3"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="+5V" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="+5V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MIC5219XX" prefix="IC" uservalue="yes">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G1" symbol="MIC5219B"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G1" pin="BYP" pad="4"/>
<connect gate="G1" pin="EN" pad="3"/>
<connect gate="G1" pin="GND" pad="2"/>
<connect gate="G1" pin="IN" pad="1"/>
<connect gate="G1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74X245">
<gates>
<gate name="G1" symbol="245"/>
</gates>
<devices>
<device name="" package="SSOP20">
<connects>
<connect gate="G1" pin="!OE" pad="19"/>
<connect gate="G1" pin="A0" pad="2"/>
<connect gate="G1" pin="A1" pad="3"/>
<connect gate="G1" pin="A2" pad="4"/>
<connect gate="G1" pin="A3" pad="5"/>
<connect gate="G1" pin="A4" pad="6"/>
<connect gate="G1" pin="A5" pad="7"/>
<connect gate="G1" pin="A6" pad="8"/>
<connect gate="G1" pin="A7" pad="9"/>
<connect gate="G1" pin="B1" pad="18"/>
<connect gate="G1" pin="B2" pad="17"/>
<connect gate="G1" pin="B3" pad="16"/>
<connect gate="G1" pin="B4" pad="15"/>
<connect gate="G1" pin="B5" pad="14"/>
<connect gate="G1" pin="B6" pad="13"/>
<connect gate="G1" pin="B7" pad="12"/>
<connect gate="G1" pin="B8" pad="11"/>
<connect gate="G1" pin="DIR" pad="1"/>
<connect gate="G1" pin="GND" pad="10"/>
<connect gate="G1" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LCMXO2-1200HC-TQFP100">
<gates>
<gate name="G$1" symbol="LCMXO2-1200HC-TQFP100"/>
</gates>
<devices>
<device name="" package="TQFP100">
<connects>
<connect gate="G$1" pin="CSSPIN/P27" pad="27"/>
<connect gate="G$1" pin="DONE/P76" pad="76"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="GND@2" pad="22"/>
<connect gate="G$1" pin="GND@3" pad="33"/>
<connect gate="G$1" pin="GND@4" pad="44"/>
<connect gate="G$1" pin="GND@5" pad="56"/>
<connect gate="G$1" pin="GND@6" pad="72"/>
<connect gate="G$1" pin="GND@7" pad="79"/>
<connect gate="G$1" pin="GND@8" pad="92"/>
<connect gate="G$1" pin="INITN/P77" pad="77"/>
<connect gate="G$1" pin="JTAGENB/P82" pad="82"/>
<connect gate="G$1" pin="MCLK/CCLK/P31" pad="31"/>
<connect gate="G$1" pin="NC" pad="89"/>
<connect gate="G$1" pin="NC@2" pad="61"/>
<connect gate="G$1" pin="P1" pad="1"/>
<connect gate="G$1" pin="P10" pad="10"/>
<connect gate="G$1" pin="P12/PCLKT3_1" pad="12"/>
<connect gate="G$1" pin="P13/PCLKC3_1" pad="13"/>
<connect gate="G$1" pin="P14" pad="14"/>
<connect gate="G$1" pin="P15" pad="15"/>
<connect gate="G$1" pin="P16" pad="16"/>
<connect gate="G$1" pin="P17" pad="17"/>
<connect gate="G$1" pin="P18" pad="18"/>
<connect gate="G$1" pin="P19" pad="19"/>
<connect gate="G$1" pin="P2" pad="2"/>
<connect gate="G$1" pin="P20/PCLKT3_0" pad="20"/>
<connect gate="G$1" pin="P21/PCLKC3_0" pad="21"/>
<connect gate="G$1" pin="P24" pad="24"/>
<connect gate="G$1" pin="P25" pad="25"/>
<connect gate="G$1" pin="P28" pad="28"/>
<connect gate="G$1" pin="P29" pad="29"/>
<connect gate="G$1" pin="P3/PCLKT3_2" pad="3"/>
<connect gate="G$1" pin="P30" pad="30"/>
<connect gate="G$1" pin="P34/PCLKT2_0" pad="34"/>
<connect gate="G$1" pin="P35/PCLKC2_0" pad="35"/>
<connect gate="G$1" pin="P36" pad="36"/>
<connect gate="G$1" pin="P37" pad="37"/>
<connect gate="G$1" pin="P38/PCLKT2_1" pad="38"/>
<connect gate="G$1" pin="P39/PCLKC2_0" pad="39"/>
<connect gate="G$1" pin="P4/PCLKC3_2" pad="4"/>
<connect gate="G$1" pin="P40" pad="40"/>
<connect gate="G$1" pin="P41" pad="41"/>
<connect gate="G$1" pin="P42" pad="42"/>
<connect gate="G$1" pin="P43" pad="43"/>
<connect gate="G$1" pin="P45" pad="45"/>
<connect gate="G$1" pin="P47" pad="47"/>
<connect gate="G$1" pin="P51" pad="51"/>
<connect gate="G$1" pin="P52" pad="52"/>
<connect gate="G$1" pin="P53" pad="53"/>
<connect gate="G$1" pin="P54" pad="54"/>
<connect gate="G$1" pin="P57" pad="57"/>
<connect gate="G$1" pin="P58" pad="58"/>
<connect gate="G$1" pin="P59" pad="59"/>
<connect gate="G$1" pin="P60" pad="60"/>
<connect gate="G$1" pin="P62/PCLKC1_0" pad="62"/>
<connect gate="G$1" pin="P63/PCLKT1_0" pad="63"/>
<connect gate="G$1" pin="P64" pad="64"/>
<connect gate="G$1" pin="P65" pad="65"/>
<connect gate="G$1" pin="P66" pad="66"/>
<connect gate="G$1" pin="P67" pad="67"/>
<connect gate="G$1" pin="P68" pad="68"/>
<connect gate="G$1" pin="P69" pad="69"/>
<connect gate="G$1" pin="P7" pad="7"/>
<connect gate="G$1" pin="P70" pad="70"/>
<connect gate="G$1" pin="P71" pad="71"/>
<connect gate="G$1" pin="P74" pad="74"/>
<connect gate="G$1" pin="P75" pad="75"/>
<connect gate="G$1" pin="P78" pad="78"/>
<connect gate="G$1" pin="P8" pad="8"/>
<connect gate="G$1" pin="P83" pad="83"/>
<connect gate="G$1" pin="P84" pad="84"/>
<connect gate="G$1" pin="P87/PCLKC0_1" pad="87"/>
<connect gate="G$1" pin="P88/PCLKT0_1" pad="88"/>
<connect gate="G$1" pin="P9" pad="9"/>
<connect gate="G$1" pin="P96" pad="96"/>
<connect gate="G$1" pin="P97" pad="97"/>
<connect gate="G$1" pin="P98" pad="98"/>
<connect gate="G$1" pin="P99" pad="99"/>
<connect gate="G$1" pin="PROGRAMN/P81" pad="81"/>
<connect gate="G$1" pin="SCL/PCLKT0_0/P86" pad="86"/>
<connect gate="G$1" pin="SDA/PCLKC0_0/P85" pad="85"/>
<connect gate="G$1" pin="SI/SISPI/P49" pad="49"/>
<connect gate="G$1" pin="SN/P48" pad="48"/>
<connect gate="G$1" pin="SO/SPISO/P32" pad="32"/>
<connect gate="G$1" pin="TCK/P91" pad="91"/>
<connect gate="G$1" pin="TDI/P94" pad="94"/>
<connect gate="G$1" pin="TDO/P95" pad="95"/>
<connect gate="G$1" pin="TMS/P90" pad="90"/>
<connect gate="G$1" pin="VCCIO0@1" pad="80"/>
<connect gate="G$1" pin="VCCIO0@2" pad="93"/>
<connect gate="G$1" pin="VCCIO1@1" pad="55"/>
<connect gate="G$1" pin="VCCIO1@2" pad="73"/>
<connect gate="G$1" pin="VCCIO2@1" pad="26"/>
<connect gate="G$1" pin="VCCIO2@2" pad="46"/>
<connect gate="G$1" pin="VCCIO3@1" pad="5"/>
<connect gate="G$1" pin="VCCIO3@2" pad="23"/>
<connect gate="G$1" pin="VCCIO3@3" pad="11"/>
<connect gate="G$1" pin="VCCSUPPLY@1" pad="50"/>
<connect gate="G$1" pin="VCCSUPPLY@2" pad="100"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPI-FLASH">
<gates>
<gate name="G$1" symbol="SPI-FLASH"/>
</gates>
<devices>
<device name="" package="SOIC08">
<connects>
<connect gate="G$1" pin="/CS" pad="1"/>
<connect gate="G$1" pin="/HOLD" pad="7"/>
<connect gate="G$1" pin="/WP" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCLK" pad="6"/>
<connect gate="G$1" pin="SI" pad="5"/>
<connect gate="G$1" pin="SO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
