(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "74LS166" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -7.62 21.59 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LS166" (at -7.62 -21.59 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_fp_filters" "DIP?16*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LS166_1_0"
      (pin input line (at -12.7 17.78 0) (length 5.08)
        (name "Ds" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 5.08 180) (length 5.08)
        (name "D3" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 2.54 180) (length 5.08)
        (name "D2" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 0 180) (length 5.08)
        (name "D1" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -12.7 7.62 0) (length 5.08)
        (name "Qh" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -2.54 180) (length 5.08)
        (name "D0" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 2.54 0) (length 5.08)
        (name "SH_~{LD}" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 25.4 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 15.24 180) (length 5.08)
        (name "D7" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 12.7 180) (length 5.08)
        (name "D6" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 10.16 180) (length 5.08)
        (name "D5" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 7.62 180) (length 5.08)
        (name "D4" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -12.7 0) (length 5.08)
        (name "CK_INH" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input clock (at -12.7 -2.54 0) (length 5.08)
        (name "CLK" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -25.4 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -12.7 15.24 0) (length 5.08)
        (name "Clr" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LS166_1_1"
      (rectangle (start -7.62 20.32) (end 7.62 -20.32)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
  )
  (symbol "74LS192" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -7.62 13.97 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LS192" (at 5.08 13.97 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74ls193.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "TTL CNT CNT4" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Synchronous 4-bit Up/Down (2 clk) counter" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm* DIP*W7.62mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LS192_1_0"
      (pin input line (at -12.7 -2.54 0) (length 5.08)
        (name "B" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 5.08)
        (name "C" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -5.08 180) (length 5.08)
        (name "~{LOAD}" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 -10.16 180) (length 5.08)
        (name "~{CO}" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 -12.7 180) (length 5.08)
        (name "~{BO}" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -12.7 0) (length 5.08)
        (name "CLR" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 0 0) (length 5.08)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 17.78 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 7.62 180) (length 5.08)
        (name "QB" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 10.16 180) (length 5.08)
        (name "QA" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input clock (at -12.7 7.62 0) (length 5.08)
        (name "DOWN" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input clock (at -12.7 10.16 0) (length 5.08)
        (name "UP" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 5.08 180) (length 5.08)
        (name "QC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 2.54 180) (length 5.08)
        (name "QD" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -20.32 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -7.62 0) (length 5.08)
        (name "D" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LS192_1_1"
      (rectangle (start -7.62 12.7) (end 7.62 -15.24)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
  )
  (symbol "74LS193" (extends "74LS192")
    (property "Reference" "U" (at -7.62 13.97 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LS193" (at 5.08 13.97 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74ls193.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "TTL CNT CNT4" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Synchronous 4-bit Up/Down (2 clk) counter" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm* DIP*W7.62mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "74LS240" (pin_names (offset 0.002)) (in_bom yes) (on_board yes)
    (property "Reference" "U**" (at 0.635 2.54 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "Standard Template" (at -43.18 -76.708 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Footprint" "Package_DIP:DIP-20_W7.62mm" (at -44.45 -73.66 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74ls244.pdf" (at -41.402 -71.374 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Component Value" "74LS240" (at 9.144 4.826 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Tolerance" "n/a" (at -37.338 -81.534 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer" "Texas Instrument" (at -41.402 -60.198 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer Link" "https://www.ti.com/product/SN74LS240?keyMatch=SN74LS240&tisearch=search-everything&usecase=GPN-ALT" (at -38.608 -66.802 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "RoHS Document Link" "https://4donline.ihs.com/images/VipMasterIC/IC/TXII/TXII-E-A0013673131/TXII-E-A0013673131-1.pdf?hkey=6D0214268300F1406B835FE51CB13195" (at -23.114 -64.77 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer PN" "SN74LS240N " (at -39.116 -63.754 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "RoHS" "Yes" (at -26.416 -61.976 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Allow Substitution" "Yes" (at -26.67 -67.818 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Fitted" "Yes" (at -25.654 -72.644 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Tracking" "No" (at -26.162 -70.104 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "BOM Comment" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Component Type" "(Resistor / Capacitor / Bipolar Transistor, etc.)" (at -19.812 -78.74 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Package Type" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Package Variant" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Number of Pins" "If applicable" (at -37.338 -84.074 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Storage)" "If applicable" (at -37.338 -86.106 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Operating)" "If applicable" (at -37.084 -88.646 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Soldering)" "If applicable" (at -37.084 -91.44 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp Coeff." "If applicable" (at -37.084 -93.98 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Power Rating" "If applicable" (at -37.084 -96.52 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Material" "If applicable" (at -37.084 -98.806 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Class" "If applicable" (at -37.084 -101.092 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Standards Version" "1.1" (at -25.654 -75.692 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "ttl buffer octal tristateU" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Octal 3-state bidirectional buffer" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "C_*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LS240_1_0"
      (polyline
        (pts
          (xy 1.016 0)
          (xy -1.524 1.27)
          (xy -1.524 -1.27)
          (xy 1.016 0)
        )
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (circle (center 1.397 0) (radius 0.254)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (pin input inverted (at -12.7 -10.16 0) (length 5.08)
        (name "1OE" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -20.32 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 5.08)
        (name "2A3" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -12.7 -2.54 0) (length 5.08)
        (name "1Y3" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 0 0) (length 5.08)
        (name "2A2" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -12.7 2.54 0) (length 5.08)
        (name "1Y2" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 5.08)
        (name "2A1" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -12.7 7.62 0) (length 5.08)
        (name "1Y1" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 10.16 0) (length 5.08)
        (name "2A0" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -12.7 12.7 0) (length 5.08)
        (name "1Y0" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -12.7 -12.7 0) (length 5.08)
        (name "2OE" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -2.54 180) (length 5.08)
        (name "1A0" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 20.32 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 12.7 12.7 180) (length 5.08)
        (name "2Y0" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -5.08 180) (length 5.08)
        (name "1A1" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 12.7 10.16 180) (length 5.08)
        (name "2Y1" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -7.62 180) (length 5.08)
        (name "1A2" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 12.7 7.62 180) (length 5.08)
        (name "2Y2" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -10.16 180) (length 5.08)
        (name "1A3" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 12.7 5.08 180) (length 5.08)
        (name "2Y3" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LS240_1_1"
      (rectangle (start -7.62 15.24) (end 7.62 -15.24)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
  )
  (symbol "ATmega1284P-P" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -12.7 49.53 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "ATmega1284P-P" (at 2.54 -49.53 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "Package_DIP:DIP-40_W15.24mm" (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "20MHz, 128kB Flash, 16kB SRAM, 4kB EEPROM, JTAG, DIP-40" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP*W15.24mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ATmega1284P-P_0_1"
      (rectangle (start -12.7 -48.26) (end 12.7 48.26)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "ATmega1284P-P_1_1"
      (pin bidirectional line (at -15.24 13.97 0) (length 2.54)
        (name "PB0" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 50.8 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -50.8 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -12.7 36.83 0) (length 2.54)
        (name "XTAL2" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 41.91 0) (length 2.54)
        (name "XTAL1" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -19.05 0) (length 2.54)
        (name "PD0/RXD0" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -21.59 0) (length 2.54)
        (name "PD1/TXD0" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -24.13 0) (length 2.54)
        (name "PD2/RXD1" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -26.67 0) (length 2.54)
        (name "PD3/TXD1" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -29.21 0) (length 2.54)
        (name "PD4" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -31.75 0) (length 2.54)
        (name "PD5" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 11.43 0) (length 2.54)
        (name "PB1" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -34.29 0) (length 2.54)
        (name "PD6" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -36.83 0) (length 2.54)
        (name "PD7" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -2.54 180) (length 2.54)
        (name "PC0" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -5.08 180) (length 2.54)
        (name "PC1" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -7.62 180) (length 2.54)
        (name "PC2" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -10.16 180) (length 2.54)
        (name "PC3" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -12.7 180) (length 2.54)
        (name "PC4" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -15.24 180) (length 2.54)
        (name "PC5" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -17.78 180) (length 2.54)
        (name "PC6" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -20.32 180) (length 2.54)
        (name "PC7" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 8.89 0) (length 2.54)
        (name "PB2" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 50.8 270) (length 2.54)
        (name "AVCC" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -50.8 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -15.24 27.94 0) (length 2.54)
        (name "AREF" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 25.4 180) (length 2.54)
        (name "PA7" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 27.94 180) (length 2.54)
        (name "PA6" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 30.48 180) (length 2.54)
        (name "PA5" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 33.02 180) (length 2.54)
        (name "PA4" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 35.56 180) (length 2.54)
        (name "PA3" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 38.1 180) (length 2.54)
        (name "PA2" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 40.64 180) (length 2.54)
        (name "PA1" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 6.35 0) (length 2.54)
        (name "PB3" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 43.18 180) (length 2.54)
        (name "PA0" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 3.81 0) (length 2.54)
        (name "PB4" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 1.27 0) (length 2.54)
        (name "PB5/MOSI" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -1.27 0) (length 2.54)
        (name "PB6/MISO" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -3.81 0) (length 2.54)
        (name "PB7/SCK" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 31.75 0) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ATmega2560-16AU" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 1.27 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "ATmega256-16AU" (at 0 -1.27 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm" (at 0 13.97 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ATmega2560-16AU_0_1"
      (rectangle (start -16.51 -85.09) (end 16.51 69.85)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "ATmega2560-16AU_1_1"
      (pin bidirectional line (at 20.32 -53.34 180) (length 3.81)
        (name "PG5" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 73.66 270) (length 3.81)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 7.62 73.66 270) (length 3.81)
        (name "AVCC" (effects (font (size 1.27 1.27))))
        (number "100" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 -88.9 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -55.88 0) (length 3.81)
        (name "PH0" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -58.42 0) (length 3.81)
        (name "PH1" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -60.96 0) (length 3.81)
        (name "PH2" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -63.5 0) (length 3.81)
        (name "PH3" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -66.04 0) (length 3.81)
        (name "PH4" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -68.58 0) (length 3.81)
        (name "PH5" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -71.12 0) (length 3.81)
        (name "PH6" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 0 0) (length 3.81)
        (name "PB0" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -25.4 0) (length 3.81)
        (name "RXD0/PE0" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -2.54 0) (length 3.81)
        (name "SCK/PB1" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -5.08 0) (length 3.81)
        (name "MOSI/PB2" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -7.62 0) (length 3.81)
        (name "MISO/PB3" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -10.16 0) (length 3.81)
        (name "PB4" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -12.7 0) (length 3.81)
        (name "PB5" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -15.24 0) (length 3.81)
        (name "PB6" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -17.78 0) (length 3.81)
        (name "PB7" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -73.66 0) (length 3.81)
        (name "PH7" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -48.26 180) (length 3.81)
        (name "PG3" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -50.8 180) (length 3.81)
        (name "PG4" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -27.94 0) (length 3.81)
        (name "TXD0/PE1" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 55.88 0) (length 3.81)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 73.66 270) (length 3.81)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -88.9 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -20.32 60.96 0) (length 3.81)
        (name "XTAL2" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 66.04 0) (length 3.81)
        (name "XTAL1" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -15.24 180) (length 3.81)
        (name "PL0" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -17.78 180) (length 3.81)
        (name "PL1" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -20.32 180) (length 3.81)
        (name "PL2" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -22.86 180) (length 3.81)
        (name "PL3" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -25.4 180) (length 3.81)
        (name "PL4" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -30.48 0) (length 3.81)
        (name "PE2" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -27.94 180) (length 3.81)
        (name "PL5" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -30.48 180) (length 3.81)
        (name "PL6" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -33.02 180) (length 3.81)
        (name "PL7" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -58.42 180) (length 3.81)
        (name "PD0" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -60.96 180) (length 3.81)
        (name "PD1" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -63.5 180) (length 3.81)
        (name "PD2" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -66.04 180) (length 3.81)
        (name "PD3" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -68.58 180) (length 3.81)
        (name "PD4" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -71.12 180) (length 3.81)
        (name "PD5" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -73.66 180) (length 3.81)
        (name "PD6" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -33.02 0) (length 3.81)
        (name "PE3" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -76.2 180) (length 3.81)
        (name "PD7" (effects (font (size 1.27 1.27))))
        (number "50" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -40.64 180) (length 3.81)
        (name "PG0" (effects (font (size 1.27 1.27))))
        (number "51" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -43.18 180) (length 3.81)
        (name "PG1" (effects (font (size 1.27 1.27))))
        (number "52" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 60.96 180) (length 3.81)
        (name "PC0" (effects (font (size 1.27 1.27))))
        (number "53" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 58.42 180) (length 3.81)
        (name "PC1" (effects (font (size 1.27 1.27))))
        (number "54" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 55.88 180) (length 3.81)
        (name "PC2" (effects (font (size 1.27 1.27))))
        (number "55" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 53.34 180) (length 3.81)
        (name "PC3" (effects (font (size 1.27 1.27))))
        (number "56" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 50.8 180) (length 3.81)
        (name "PC4" (effects (font (size 1.27 1.27))))
        (number "57" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 48.26 180) (length 3.81)
        (name "PC5" (effects (font (size 1.27 1.27))))
        (number "58" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 45.72 180) (length 3.81)
        (name "PC6" (effects (font (size 1.27 1.27))))
        (number "59" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -35.56 0) (length 3.81)
        (name "PE4" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 43.18 180) (length 3.81)
        (name "PC7" (effects (font (size 1.27 1.27))))
        (number "60" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 73.66 270) (length 3.81)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "61" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -88.9 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "62" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 35.56 180) (length 3.81)
        (name "PJ0" (effects (font (size 1.27 1.27))))
        (number "63" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 33.02 180) (length 3.81)
        (name "PJ1" (effects (font (size 1.27 1.27))))
        (number "64" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 30.48 180) (length 3.81)
        (name "PJ2" (effects (font (size 1.27 1.27))))
        (number "65" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 27.94 180) (length 3.81)
        (name "PJ3" (effects (font (size 1.27 1.27))))
        (number "66" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 25.4 180) (length 3.81)
        (name "PJ4" (effects (font (size 1.27 1.27))))
        (number "67" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 22.86 180) (length 3.81)
        (name "PJ5" (effects (font (size 1.27 1.27))))
        (number "68" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 20.32 180) (length 3.81)
        (name "PJ6" (effects (font (size 1.27 1.27))))
        (number "69" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -38.1 0) (length 3.81)
        (name "PE5" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -45.72 180) (length 3.81)
        (name "PG2" (effects (font (size 1.27 1.27))))
        (number "70" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -7.62 180) (length 3.81)
        (name "PA7" (effects (font (size 1.27 1.27))))
        (number "71" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -5.08 180) (length 3.81)
        (name "PA6" (effects (font (size 1.27 1.27))))
        (number "72" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -2.54 180) (length 3.81)
        (name "PA5" (effects (font (size 1.27 1.27))))
        (number "73" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 0 180) (length 3.81)
        (name "PA4" (effects (font (size 1.27 1.27))))
        (number "74" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 2.54 180) (length 3.81)
        (name "PA3" (effects (font (size 1.27 1.27))))
        (number "75" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 5.08 180) (length 3.81)
        (name "PA2" (effects (font (size 1.27 1.27))))
        (number "76" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 7.62 180) (length 3.81)
        (name "PA1" (effects (font (size 1.27 1.27))))
        (number "77" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 10.16 180) (length 3.81)
        (name "PA0" (effects (font (size 1.27 1.27))))
        (number "78" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 17.78 180) (length 3.81)
        (name "PJ7" (effects (font (size 1.27 1.27))))
        (number "79" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -40.64 0) (length 3.81)
        (name "PE6" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 73.66 270) (length 3.81)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "80" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -88.9 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "81" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 5.08 0) (length 3.81)
        (name "PK7" (effects (font (size 1.27 1.27))))
        (number "82" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 7.62 0) (length 3.81)
        (name "PK6" (effects (font (size 1.27 1.27))))
        (number "83" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 10.16 0) (length 3.81)
        (name "PK5" (effects (font (size 1.27 1.27))))
        (number "84" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 12.7 0) (length 3.81)
        (name "PK4" (effects (font (size 1.27 1.27))))
        (number "85" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 15.24 0) (length 3.81)
        (name "PK3" (effects (font (size 1.27 1.27))))
        (number "86" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 17.78 0) (length 3.81)
        (name "PK2" (effects (font (size 1.27 1.27))))
        (number "87" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 20.32 0) (length 3.81)
        (name "PK1" (effects (font (size 1.27 1.27))))
        (number "88" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 22.86 0) (length 3.81)
        (name "PK0" (effects (font (size 1.27 1.27))))
        (number "89" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -43.18 0) (length 3.81)
        (name "PE7" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 27.94 0) (length 3.81)
        (name "PF7/TDI" (effects (font (size 1.27 1.27))))
        (number "90" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 30.48 0) (length 3.81)
        (name "PF6/TDO" (effects (font (size 1.27 1.27))))
        (number "91" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 33.02 0) (length 3.81)
        (name "PF5/TMS" (effects (font (size 1.27 1.27))))
        (number "92" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 35.56 0) (length 3.81)
        (name "PF4/TCK" (effects (font (size 1.27 1.27))))
        (number "93" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 38.1 0) (length 3.81)
        (name "PF3" (effects (font (size 1.27 1.27))))
        (number "94" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 40.64 0) (length 3.81)
        (name "PF2" (effects (font (size 1.27 1.27))))
        (number "95" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 43.18 0) (length 3.81)
        (name "PF1" (effects (font (size 1.27 1.27))))
        (number "96" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 45.72 0) (length 3.81)
        (name "PF0" (effects (font (size 1.27 1.27))))
        (number "97" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -20.32 50.8 0) (length 3.81)
        (name "AREF" (effects (font (size 1.27 1.27))))
        (number "98" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -88.9 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "99" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ATmega328P-PU-MCU_Microchip_ATmega" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -12.7 36.83 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "ATmega328P-PU-MCU_Microchip_ATmega" (at 2.54 -36.83 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "Package_DIP:DIP-28_W7.62mm" (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP*W7.62mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ATmega328P-PU-MCU_Microchip_ATmega_0_1"
      (rectangle (start -12.7 -35.56) (end 12.7 35.56)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "ATmega328P-PU-MCU_Microchip_ATmega_1_1"
      (pin tri_state line (at 15.24 -7.62 180) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 12.7 180) (length 2.54)
        (name "PB7" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 -25.4 180) (length 2.54)
        (name "PD5" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 -27.94 180) (length 2.54)
        (name "PD6" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 -30.48 180) (length 2.54)
        (name "PD7" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 30.48 180) (length 2.54)
        (name "PB0" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 27.94 180) (length 2.54)
        (name "PB1" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 25.4 180) (length 2.54)
        (name "PB2" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 22.86 180) (length 2.54)
        (name "MOSI" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 20.32 180) (length 2.54)
        (name "MISO/PB4" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 17.78 180) (length 2.54)
        (name "SCK/PB5" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 -12.7 180) (length 2.54)
        (name "PD0" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 38.1 270) (length 2.54)
        (name "AVCC" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -15.24 30.48 0) (length 2.54)
        (name "AREF" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -38.1 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 7.62 180) (length 2.54)
        (name "PC0" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 5.08 180) (length 2.54)
        (name "PC1" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 2.54 180) (length 2.54)
        (name "PC2" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 0 180) (length 2.54)
        (name "PC3" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 -2.54 180) (length 2.54)
        (name "PC4" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 -5.08 180) (length 2.54)
        (name "PC5" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 -15.24 180) (length 2.54)
        (name "PD1" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 -17.78 180) (length 2.54)
        (name "PD2" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 -20.32 180) (length 2.54)
        (name "PD3" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 -22.86 180) (length 2.54)
        (name "PD4" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 38.1 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -38.1 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 15.24 180) (length 2.54)
        (name "PB6" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ATmega328P-PU-MCU_Microchip_ATmega_encoder" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -12.7 36.83 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "ATmega328P-PU-MCU_Microchip_ATmega_encoder" (at 2.54 -36.83 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "Package_DIP:DIP-28_W7.62mm" (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP*W7.62mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ATmega328P-PU-MCU_Microchip_ATmega_encoder_0_1"
      (rectangle (start -12.7 -35.56) (end 12.7 35.56)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "ATmega328P-PU-MCU_Microchip_ATmega_encoder_1_1"
      (pin tri_state line (at 15.24 -7.62 180) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 12.7 180) (length 2.54)
        (name "PB7" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 -25.4 180) (length 2.54)
        (name "PD5" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 -27.94 180) (length 2.54)
        (name "PD6" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 -30.48 180) (length 2.54)
        (name "PD7" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 15.24 30.48 180) (length 2.54)
        (name "PB0" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 15.24 27.94 180) (length 2.54)
        (name "PB1" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 15.24 25.4 180) (length 2.54)
        (name "PB2" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 15.24 22.86 180) (length 2.54)
        (name "MOSI" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 15.24 20.32 180) (length 2.54)
        (name "MISO/PB4" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 15.24 17.78 180) (length 2.54)
        (name "SCK/PB5" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 -12.7 180) (length 2.54)
        (name "PD0" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 38.1 270) (length 2.54)
        (name "AVCC" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -15.24 30.48 0) (length 2.54)
        (name "AREF" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -38.1 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 7.62 180) (length 2.54)
        (name "PC0" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 5.08 180) (length 2.54)
        (name "PC1" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 2.54 180) (length 2.54)
        (name "PC2" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 0 180) (length 2.54)
        (name "PC3" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 -2.54 180) (length 2.54)
        (name "PC4" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 -5.08 180) (length 2.54)
        (name "PC5" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 -15.24 180) (length 2.54)
        (name "PD1" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 -17.78 180) (length 2.54)
        (name "PD2" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 -20.32 180) (length 2.54)
        (name "PD3" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 -22.86 180) (length 2.54)
        (name "PD4" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 38.1 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -38.1 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 15.24 15.24 180) (length 2.54)
        (name "PB6" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "IC TTL 74LS240 Octal buffer, inverting, active low enables, DIP" (pin_names (offset 0.002)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0.635 2.54 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "74LS240" (at -50.8 -47.498 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Footprint" "Package_DIP:DIP-20_W7.62mm_LongPads" (at -53.34 -43.18 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74s244.pdf" (at -49.022 -42.164 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Component Value" "74LS240" (at 7.62 17.78 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Tolerance" "If applicable" (at -44.958 -52.324 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer" "Texas Instruments" (at -49.022 -30.988 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer Link" "https://www.ti.com/product/SN74LS240?keyMatch=SN74LS240&tisearch=search-everything&usecase=GPN-ALT" (at -46.228 -37.592 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "RoHS Document Link" "RoHs Linkhttps://4donline.ihs.com/images/VipMasterIC/IC/TXII/TXII-E-A0013673131/TXII-E-A0013673131-1.pdf?hkey=6D0214268300F1406B835FE51CB13195" (at -45.974 -77.47 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer PN" "74LS240N" (at -46.736 -34.544 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "RoHS" "Yes" (at -49.276 -74.676 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Allow Substitution" "Yes" (at -49.53 -80.518 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Fitted" "Yes" (at -48.514 -85.344 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Tracking" "No" (at -49.022 -82.804 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "BOM Comment" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Component Type" "IC" (at -4.572 -36.83 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Package Type" "DIP" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Package Variant" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Number of Pins" "20" (at -44.958 -54.864 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Storage)" "-65C/120C" (at -44.958 -56.896 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Operating)" "0C/70C" (at -44.704 -59.436 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Soldering)" "If applicable" (at -44.704 -62.23 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp Coeff." "If applicable" (at -44.704 -64.77 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Power Rating" "If applicable" (at -44.704 -67.31 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Material" "If applicable" (at -44.704 -69.596 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Class" "If applicable" (at -44.704 -71.882 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Standards Version" "1.1" (at -48.514 -88.392 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "TTL octal buffer inverting" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "74LS240 Octal buffer, inverting, active low enables, DIP" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "C_*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "IC TTL 74LS240 Octal buffer, inverting, active low enables, DIP_1_0"
      (polyline
        (pts
          (xy 1.016 0)
          (xy -1.524 1.27)
          (xy -1.524 -1.27)
          (xy 1.016 0)
        )
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (circle (center 1.397 0) (radius 0.254)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (pin input inverted (at -12.7 -10.16 0) (length 5.08)
        (name "1OE" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -20.32 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 5.08)
        (name "2A3" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -12.7 -2.54 0) (length 5.08)
        (name "1Y3" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 0 0) (length 5.08)
        (name "2A2" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -12.7 2.54 0) (length 5.08)
        (name "1Y2" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 5.08)
        (name "2A1" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -12.7 7.62 0) (length 5.08)
        (name "1Y1" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 10.16 0) (length 5.08)
        (name "2A0" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -12.7 12.7 0) (length 5.08)
        (name "1Y0" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -12.7 -12.7 0) (length 5.08)
        (name "2OE" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -2.54 180) (length 5.08)
        (name "1A0" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 20.32 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 12.7 12.7 180) (length 5.08)
        (name "2Y0" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -5.08 180) (length 5.08)
        (name "1A1" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 12.7 10.16 180) (length 5.08)
        (name "2Y1" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -7.62 180) (length 5.08)
        (name "1A2" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 12.7 7.62 180) (length 5.08)
        (name "2Y2" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -10.16 180) (length 5.08)
        (name "1A3" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 12.7 5.08 180) (length 5.08)
        (name "2Y3" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "IC TTL 74LS240 Octal buffer, inverting, active low enables, DIP_1_1"
      (rectangle (start -7.62 15.24) (end 7.62 -15.24)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
  )
  (symbol "RES 1k ohm 1% MLCC 0805 Yageo" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "R" (at 0.635 2.54 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "1k" (at -27.94 -34.798 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (at 0.9652 -3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-RC_Group_51_RoHS_L_12.pdf" (at 29.972 -28.956 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Component Value" "1k" (at 9.144 4.826 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Tolerance" "1%" (at -22.098 -39.624 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer" "Yageo" (at -24.384 -18.034 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer Link" "https://www.yageo.com/en/Home" (at -9.398 -24.892 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "RoHS Document Link" "https://www.mouser.com/catalog/additional/Yageo_6012_R_Chip_RoHS_Certificate.pdf" (at 14.478 -68.834 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer PN" " RC0805FR-071KP" (at -17.78 -21.59 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "RoHS" "Yes" (at -26.416 -65.786 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Allow Substitution" "Yes" (at -25.908 -71.628 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Fitted" "Yes" (at -25.654 -76.454 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Tracking" "No" (at -26.162 -73.914 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "BOM Comment" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Component Type" "Resistor" (at -4.572 -36.83 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Package Type" "SMT 0805" (at -22.606 -60.198 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Package Variant" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Number of Pins" "2" (at -22.098 -42.164 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Storage)" "If applicable" (at -22.098 -44.196 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Operating)" "-55C / +155C" (at -21.844 -46.736 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Soldering)" "If applicable" (at -21.844 -49.53 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp Coeff." "+50ppm/C" (at -21.844 -52.07 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Power Rating" "125 mW" (at -23.114 -54.61 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Material" "Thin Film" (at -21.844 -56.896 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Class" "" (at -21.844 -62.992 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Standards Version" "1.1" (at -25.654 -79.502 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "template" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Resistor, 1k 1% metal film, through-hole" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "C_*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "RES 1k ohm 1% MLCC 0805 Yageo_0_1"
      (polyline
        (pts
          (xy -2.286 0)
          (xy -2.54 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.286 0)
          (xy 2.54 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.762 0)
          (xy -1.143 -1.016)
          (xy -1.524 0)
          (xy -1.905 1.016)
          (xy -2.286 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.762 0)
          (xy 0.381 -1.016)
          (xy 0 0)
          (xy -0.381 1.016)
          (xy -0.762 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.286 0)
          (xy 1.905 -1.016)
          (xy 1.524 0)
          (xy 1.143 1.016)
          (xy 0.762 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "RES 1k ohm 1% MLCC 0805 Yageo_1_1"
      (pin passive line (at 3.81 0 180) (length 1.27)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -3.81 0 0) (length 1.27)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "RES 1k ohm 1% metal film.Yageo" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "R" (at 0.635 2.54 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "1k" (at -27.94 -34.798 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (at -3.81 -15.24 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/lr/YAGEO%20MFR_datasheet_2022v2.pdf" (at -26.162 -29.464 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Component Value" "1k" (at 9.144 4.826 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Tolerance" "1%" (at -22.098 -39.624 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer" "Yageo" (at -26.162 -18.288 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer Link" "https://yageo.com" (at -23.368 -24.892 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "RoHS Document Link" "https://4donline.ihs.com/images/VipMasterIC/IC/YAGO/YAGO-E-A0009164361/YAGO-E-A0009164361-1.pdf?hkey=6D0214268300F1406B835FE51CB13195" (at -23.114 -68.58 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer PN" "MFR-25FTE52-330R" (at -23.876 -21.844 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "RoHS" "yes" (at -26.416 -65.786 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Allow Substitution" "Yes" (at -26.67 -71.628 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Fitted" "Yes" (at -25.654 -76.454 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Tracking" "No" (at -26.162 -73.914 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "BOM Comment" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Component Type" "Resistor" (at -4.572 -36.83 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Package Type" "Through hole axial" (at -25.4 -15.24 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Package Variant" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Number of Pins" "2" (at -22.098 -42.164 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Storage)" "If applicable" (at -22.098 -44.196 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Operating)" "-55C/155C" (at -21.844 -46.736 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Soldering)" "If applicable" (at -21.844 -49.53 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp Coeff." "50 ppm / C" (at -21.844 -52.07 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Power Rating" "1/4 W" (at -21.844 -54.61 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Material" "metal film" (at -21.844 -56.896 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Class" "If applicable" (at -21.844 -62.992 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Standards Version" "1.1" (at -25.654 -79.502 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "template" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Resistor, 1K 1% metal film, through-hole" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "C_*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "RES 1k ohm 1% metal film.Yageo_0_1"
      (polyline
        (pts
          (xy -2.286 0)
          (xy -2.54 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.286 0)
          (xy 2.54 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.762 0)
          (xy -1.143 -1.016)
          (xy -1.524 0)
          (xy -1.905 1.016)
          (xy -2.286 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.762 0)
          (xy 0.381 -1.016)
          (xy 0 0)
          (xy -0.381 1.016)
          (xy -0.762 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.286 0)
          (xy 1.905 -1.016)
          (xy 1.524 0)
          (xy 1.143 1.016)
          (xy 0.762 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "RES 1k ohm 1% metal film.Yageo_1_1"
      (pin passive line (at 3.81 0 180) (length 1.27)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -3.81 0 0) (length 1.27)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "RES 330 ohm 1% MLCC 0805 Yageo" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "R" (at 0.635 2.54 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "RES 330 ohm 1% MLCC 0805 Yageo" (at -27.94 -34.798 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (at 0.9652 -3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-RC_Group_51_RoHS_L_12.pdf" (at 29.972 -28.956 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Component Value" "330 ohm" (at 9.144 4.826 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Tolerance" "1%" (at -22.098 -39.624 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer" "Yageo" (at -24.384 -18.034 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer Link" "https://www.yageo.com/en/Home" (at -9.398 -24.892 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "RoHS Document Link" "https://www.mouser.com/catalog/additional/Yageo_6012_R_Chip_RoHS_Certificate.pdf" (at 14.478 -68.834 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer PN" " RC0805FR-07330RL" (at -17.78 -21.59 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "RoHS" "Yes" (at -26.416 -65.786 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Allow Substitution" "Yes" (at -25.908 -71.628 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Fitted" "Yes" (at -25.654 -76.454 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Tracking" "No" (at -26.162 -73.914 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "BOM Comment" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Component Type" "Resistor" (at -4.572 -36.83 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Package Type" "SMT 0805" (at -22.606 -60.198 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Package Variant" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Number of Pins" "2" (at -22.098 -42.164 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Storage)" "If applicable" (at -22.098 -44.196 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Operating)" "-55C / +155C" (at -21.844 -46.736 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Soldering)" "If applicable" (at -21.844 -49.53 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp Coeff." "+50ppm/C" (at -21.844 -52.07 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Power Rating" "125 mW" (at -23.114 -54.61 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Material" "Thin Film" (at -21.844 -56.896 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Class" "" (at -21.844 -62.992 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Standards Version" "1.1" (at -25.654 -79.502 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "template" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Standard Component Template" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "C_*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "RES 330 ohm 1% MLCC 0805 Yageo_0_1"
      (polyline
        (pts
          (xy -2.286 0)
          (xy -2.54 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.286 0)
          (xy 2.54 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.762 0)
          (xy -1.143 -1.016)
          (xy -1.524 0)
          (xy -1.905 1.016)
          (xy -2.286 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.762 0)
          (xy 0.381 -1.016)
          (xy 0 0)
          (xy -0.381 1.016)
          (xy -0.762 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.286 0)
          (xy 1.905 -1.016)
          (xy 1.524 0)
          (xy 1.143 1.016)
          (xy 0.762 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "RES 330 ohm 1% MLCC 0805 Yageo_1_1"
      (pin passive line (at 3.81 0 180) (length 1.27)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -3.81 0 0) (length 1.27)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "RES 330 ohm 1% metal film.Yageo" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "R" (at 0.635 2.54 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "330 ohms" (at -27.94 -34.798 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (at -3.81 -15.24 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/lr/YAGEO%20MFR_datasheet_2022v2.pdf" (at -26.162 -29.464 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Component Value" "330 ohm" (at 9.144 4.826 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Tolerance" "1%" (at -22.098 -39.624 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer" "Yageo" (at -26.162 -18.288 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer Link" "https://yageo.com" (at -23.368 -24.892 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "RoHS Document Link" "https://4donline.ihs.com/images/VipMasterIC/IC/YAGO/YAGO-E-A0009164361/YAGO-E-A0009164361-1.pdf?hkey=6D0214268300F1406B835FE51CB13195" (at -23.114 -68.58 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer PN" "MFR-25FTE52-330R" (at -23.876 -21.844 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "RoHS" "yes" (at -26.416 -65.786 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Allow Substitution" "Yes" (at -26.67 -71.628 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Fitted" "Yes" (at -25.654 -76.454 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Tracking" "No" (at -26.162 -73.914 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "BOM Comment" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Component Type" "Resistor" (at -4.572 -36.83 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Package Type" "Through hole axial" (at -25.4 -15.24 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Package Variant" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Number of Pins" "2" (at -22.098 -42.164 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Storage)" "If applicable" (at -22.098 -44.196 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Operating)" "-55C/155C" (at -21.844 -46.736 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Soldering)" "If applicable" (at -21.844 -49.53 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp Coeff." "50 ppm / C" (at -21.844 -52.07 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Power Rating" "1/4 W" (at -21.844 -54.61 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Material" "metal film" (at -21.844 -56.896 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Class" "If applicable" (at -21.844 -62.992 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Standards Version" "1.1" (at -25.654 -79.502 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "template" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Standard Component Template" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "C_*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "RES 330 ohm 1% metal film.Yageo_0_1"
      (polyline
        (pts
          (xy -2.286 0)
          (xy -2.54 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.286 0)
          (xy 2.54 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.762 0)
          (xy -1.143 -1.016)
          (xy -1.524 0)
          (xy -1.905 1.016)
          (xy -2.286 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.762 0)
          (xy 0.381 -1.016)
          (xy 0 0)
          (xy -0.381 1.016)
          (xy -0.762 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.286 0)
          (xy 1.905 -1.016)
          (xy 1.524 0)
          (xy 1.143 1.016)
          (xy 0.762 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "RES 330 ohm 1% metal film.Yageo_1_1"
      (pin passive line (at 3.81 0 180) (length 1.27)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -3.81 0 0) (length 1.27)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "RES100 ohm 1% thin film 0603, Yageo" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "R" (at 0.635 2.54 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "RES100 ohm 1% thin film 0603, Yageo" (at -27.94 -34.798 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (at 0.9652 -3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-RT_1-to-0.01_RoHS_L_12.pdf" (at 29.972 -28.956 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Component Value" "100 ohm" (at 9.144 4.826 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Tolerance" "1%" (at -22.098 -39.624 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer" "Yageo" (at -24.384 -18.034 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer Link" "https://www.yageo.com/en/Home" (at -9.398 -24.892 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "RoHS Document Link" "https://www.mouser.com/catalog/additional/Yageo_6012_R_Chip_RoHS_Certificate.pdf" (at 14.478 -68.834 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer PN" "RT0603FRE07100RL" (at -17.78 -21.59 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "RoHS" "Yes" (at -26.416 -65.786 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Allow Substitution" "Yes" (at -25.908 -71.628 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Fitted" "Yes" (at -25.654 -76.454 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Tracking" "No" (at -26.162 -73.914 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "BOM Comment" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Component Type" "(Resistor / Capacitor / Bipolar Transistor, etc.)" (at -4.572 -36.83 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Package Type" "SMT 0603" (at -22.606 -60.198 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Package Variant" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Number of Pins" "" (at -22.098 -42.164 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Storage)" "If applicable" (at -22.098 -44.196 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Operating)" "-55C / +155C" (at -21.844 -46.736 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Soldering)" "If applicable" (at -21.844 -49.53 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp Coeff." "+50ppm/C" (at -21.844 -52.07 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Power Rating" "1/10 W" (at -23.114 -54.61 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Material" "Thin Film" (at -21.844 -56.896 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Class" "" (at -21.844 -62.992 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Standards Version" "1.1" (at -25.654 -79.502 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "template" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Standard Component Template" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "C_*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "RES100 ohm 1% thin film 0603, Yageo_0_1"
      (polyline
        (pts
          (xy -2.286 0)
          (xy -2.54 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.286 0)
          (xy 2.54 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.762 0)
          (xy -1.143 -1.016)
          (xy -1.524 0)
          (xy -1.905 1.016)
          (xy -2.286 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.762 0)
          (xy 0.381 -1.016)
          (xy 0 0)
          (xy -0.381 1.016)
          (xy -0.762 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.286 0)
          (xy 1.905 -1.016)
          (xy 1.524 0)
          (xy 1.143 1.016)
          (xy 0.762 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "RES100 ohm 1% thin film 0603, Yageo_1_1"
      (pin passive line (at 3.81 0 180) (length 1.27)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -3.81 0 0) (length 1.27)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "SW Cherry MX/Futaba 1U Style B" (pin_numbers hide) (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
    (property "Reference" "SW" (at 0.635 2.54 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "Key" (at -27.94 -34.798 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "unikbd:Key_MX" (at 6.0452 -3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.mouser.com/datasheet/2/71/chcp_s_a0002957244_1-2263075.pdf" (at -26.162 -29.464 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Component Value" "Key" (at 9.144 4.826 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Tolerance" "If applicable" (at -22.098 -39.624 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer" "Cherry" (at -26.162 -18.288 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer Link" "https://www.cherrymx.de/en/cherry-mx/mx-original/mx-black.html" (at -23.368 -24.892 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "RoHS Document Link" "https://www.mouser.com/catalog/additional/Cherry_Electrical_Products_5409_RoHS_Certificate.pdf" (at -23.114 -64.77 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer PN" "MX1A-11NN" (at -23.876 -21.844 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "RoHS" "Yes" (at -26.416 -61.976 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Allow Substitution" "Yes" (at -26.67 -67.818 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Fitted" "Yes" (at -25.654 -72.644 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Tracking" "No" (at -26.162 -70.104 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "BOM Comment" "" (at 5.08 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Component Type" "Switch" (at -4.572 -36.83 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Package Type" "" (at 5.08 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Package Variant" "" (at 5.08 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Number of Pins" "2" (at -22.098 -42.164 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Storage)" "" (at -22.098 -44.196 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Operating)" "-40C/+170C" (at -21.844 -46.736 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Soldering)" "If applicable" (at -21.844 -49.53 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp Coeff." "If applicable" (at -21.844 -52.07 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Power Rating" "10 mA" (at -21.844 -54.61 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Material" "If applicable" (at -21.844 -56.896 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Class" "If applicable" (at -21.844 -59.182 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Standards Version" "1.1" (at -25.654 -75.692 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "switch futaba cherry mx 1U" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Combined Cherry MX / Futaba 1U" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "C_*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SW Cherry MX/Futaba 1U Style B_1_1"
      (polyline
        (pts
          (xy 1.27 -2.54)
          (xy 0.8636 -2.54)
        )
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 0)
          (xy 0.8636 0)
        )
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 0.8636 -2.413) (end 0 -2.667)
        (stroke (width 0.1524) (type default))
        (fill (type outline))
      )
      (rectangle (start 0.8636 0.127) (end 0 -0.127)
        (stroke (width 0.1524) (type default))
        (fill (type outline))
      )
      (pin passive line (at 5.08 0 180) (length 3.81)
        (name "Pin_1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 5.08 -2.54 180) (length 3.81)
        (name "Pin_2" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "SW Cherry MX/Futaba 2U Style B" (pin_numbers hide) (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
    (property "Reference" "SW" (at 5.715 2.54 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "Key" (at -22.86 -34.798 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "unikbd:Key_MX_2u" (at -35.56 -17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.mouser.com/datasheet/2/71/chcp_s_a0002957244_1-2263075.pdf" (at -21.082 -29.464 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Component Value" "Key" (at 14.224 4.826 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Tolerance" "If applicable" (at -17.018 -39.624 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer" "Cherry" (at -21.082 -18.288 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer Link" "https://www.cherrymx.de/en/cherry-mx/mx-original/mx-black.html" (at -18.288 -24.892 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "RoHS Document Link" "https://www.mouser.com/catalog/additional/Cherry_Electrical_Products_5409_RoHS_Certificate.pdf" (at -18.034 -64.77 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer PN" "MX1A-11NN" (at -18.796 -21.844 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "RoHS" "Yes" (at -21.336 -61.976 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Allow Substitution" "Yes" (at -21.59 -67.818 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Fitted" "Yes" (at -20.574 -72.644 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Tracking" "No" (at -21.082 -70.104 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "BOM Comment" "" (at 5.08 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Component Type" "Switch" (at 0.508 -36.83 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Package Type" "" (at 5.08 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Package Variant" "" (at 5.08 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Number of Pins" "2" (at -17.018 -42.164 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Storage)" "" (at -17.018 -44.196 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Operating)" "-40C/+170C" (at -16.764 -46.736 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Soldering)" "If applicable" (at -16.764 -49.53 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp Coeff." "If applicable" (at -16.764 -52.07 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Power Rating" "10 mA" (at -16.764 -54.61 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Material" "If applicable" (at -16.764 -56.896 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Class" "If applicable" (at -16.764 -59.182 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Standards Version" "1.1" (at -20.574 -75.692 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "switch futaba cherry mx 2U" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Combined Cherry MX / Futaba 2U" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "C_*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SW Cherry MX/Futaba 2U Style B_1_1"
      (polyline
        (pts
          (xy 1.27 -2.54)
          (xy 0.8636 -2.54)
        )
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 0)
          (xy 0.8636 0)
        )
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 0.8636 -2.413) (end 0 -2.667)
        (stroke (width 0.1524) (type default))
        (fill (type outline))
      )
      (rectangle (start 0.8636 0.127) (end 0 -0.127)
        (stroke (width 0.1524) (type default))
        (fill (type outline))
      )
      (pin passive line (at 5.08 0 180) (length 3.81)
        (name "Pin_1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 5.08 -2.54 180) (length 3.81)
        (name "Pin_2" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "SW Cherry MX/Futaba 8U Spacebar Style B" (pin_numbers hide) (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
    (property "Reference" "SW" (at 0.635 2.54 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "Key" (at -27.94 -34.798 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "unikbd:Key_MX_Spacebar_5.25" (at -10.16 -12.7 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.mouser.com/datasheet/2/71/chcp_s_a0002957244_1-2263075.pdf" (at -26.162 -29.464 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Component Value" "Key" (at 9.144 4.826 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Tolerance" "If applicable" (at -22.098 -39.624 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer" "Cherry" (at -26.162 -18.288 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer Link" "https://www.cherrymx.de/en/cherry-mx/mx-original/mx-black.html" (at -23.368 -24.892 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "RoHS Document Link" "https://www.mouser.com/catalog/additional/Cherry_Electrical_Products_5409_RoHS_Certificate.pdf" (at -23.114 -64.77 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer PN" "MX1A-11NN" (at -23.876 -21.844 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "RoHS" "Yes" (at -26.416 -61.976 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Allow Substitution" "Yes" (at -26.67 -67.818 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Fitted" "Yes" (at -25.654 -72.644 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Tracking" "No" (at -26.162 -70.104 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "BOM Comment" "" (at 5.08 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Component Type" "Switch" (at -4.572 -36.83 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Package Type" "" (at 5.08 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Package Variant" "" (at 5.08 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Number of Pins" "2" (at -22.098 -42.164 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Storage)" "" (at -22.098 -44.196 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Operating)" "-40C/+170C" (at -21.844 -46.736 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Soldering)" "If applicable" (at -21.844 -49.53 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp Coeff." "If applicable" (at -21.844 -52.07 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Power Rating" "10 mA" (at -21.844 -54.61 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Material" "If applicable" (at -21.844 -56.896 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Class" "If applicable" (at -21.844 -59.182 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Standards Version" "1.1" (at -25.654 -75.692 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "switch futaba cherry mx 8U spacebar" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Combined Cherry MX / Futaba 8U Spacebar" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "C_*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SW Cherry MX/Futaba 8U Spacebar Style B_1_1"
      (polyline
        (pts
          (xy 1.27 -2.54)
          (xy 0.8636 -2.54)
        )
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 0)
          (xy 0.8636 0)
        )
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 0.8636 -2.413) (end 0 -2.667)
        (stroke (width 0.1524) (type default))
        (fill (type outline))
      )
      (rectangle (start 0.8636 0.127) (end 0 -0.127)
        (stroke (width 0.1524) (type default))
        (fill (type outline))
      )
      (pin passive line (at 5.08 0 180) (length 3.81)
        (name "Pin_1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 5.08 -2.54 180) (length 3.81)
        (name "Pin_2" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "SW_Push_LED" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
    (property "Reference" "SW" (at -0.635 5.715 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "SW_Push_LED" (at 0 -3.175 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 7.62 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (at 0 7.62 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "switch normally-open pushbutton push-button LED" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Push button switch with LED, generic" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SW_Push_LED_0_0"
      (polyline
        (pts
          (xy 0.635 1.27)
          (xy 0.635 -1.27)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.54 -1.905)
          (xy 1.27 -0.635)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.54 0)
          (xy -2.54 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 -1.905)
          (xy 2.54 -0.635)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.54 -1.27)
          (xy 2.54 -1.905)
          (xy 1.905 -1.905)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 -1.27)
          (xy 3.81 -1.905)
          (xy 3.175 -1.905)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.635 0)
          (xy -1.27 1.27)
          (xy -1.27 -1.27)
          (xy 0.635 0)
        )
        (stroke (width 0) (type default))
        (fill (type outline))
      )
    )
    (symbol "SW_Push_LED_0_1"
      (circle (center -2.032 2.54) (radius 0.508)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 3.81)
          (xy 2.54 3.81)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 3.81)
          (xy 0 5.588)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (circle (center 2.032 2.54) (radius 0.508)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (pin passive line (at 5.08 2.54 180) (length 2.54)
        (name "1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 2.54 0) (length 2.54)
        (name "2" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 0 0) (length 2.54)
        (name "3" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 5.08 0 180) (length 2.54)
        (name "4" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Standard Template" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "R**" (at 0.635 2.54 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "Standard Template" (at -27.94 -34.798 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Footprint" "" (at 0.9652 -3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (at -26.162 -29.464 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Component Value" "Comp. Value" (at 9.144 4.826 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Tolerance" "If applicable" (at -22.098 -39.624 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer" "Mfg" (at -26.162 -18.288 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer Link" "Mfg Link" (at -23.368 -24.892 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "RoHS Document Link" "RoHs Link" (at -23.114 -64.77 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Manufacturer PN" "MFG PN" (at -23.876 -21.844 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "RoHS" "Yes" (at -26.416 -61.976 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Allow Substitution" "No" (at -26.67 -67.818 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Fitted" "Yes" (at -25.654 -72.644 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Tracking" "No" (at -26.162 -70.104 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "BOM Comment" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Component Type" "(Resistor / Capacitor / Bipolar Transistor, etc.)" (at -4.572 -36.83 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Package Type" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Package Variant" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Number of Pins" "If applicable" (at -22.098 -42.164 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Storage)" "If applicable" (at -22.098 -44.196 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Operating)" "If applicable" (at -21.844 -46.736 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp (Soldering)" "If applicable" (at -21.844 -49.53 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Temp Coeff." "If applicable" (at -21.844 -52.07 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Power Rating" "If applicable" (at -21.844 -54.61 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Material" "If applicable" (at -21.844 -56.896 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Class" "If applicable" (at -21.844 -59.182 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Standards Version" "1.1" (at -25.654 -75.692 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "template" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Standard Component Template" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "C_*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Standard Template_0_1"
      (polyline
        (pts
          (xy -2.032 -0.254)
          (xy -2.286 -0.254)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.54 -0.254)
          (xy 2.794 -0.254)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.508 -0.254)
          (xy -0.889 -1.27)
          (xy -1.27 -0.254)
          (xy -1.651 0.762)
          (xy -2.032 -0.254)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.016 -0.254)
          (xy 0.635 -1.27)
          (xy 0.254 -0.254)
          (xy -0.127 0.762)
          (xy -0.508 -0.254)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.54 -0.254)
          (xy 2.159 -1.27)
          (xy 1.778 -0.254)
          (xy 1.397 0.762)
          (xy 1.016 -0.254)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "Standard Template_1_1"
      (pin passive line (at 4.064 -0.254 180) (length 1.27)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -3.556 -0.254 0) (length 1.27)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "diode-combined" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
    (property "Reference" "D" (at 0 2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "diode-combined" (at 0 -2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "unikbd:diode-combined" (at -20.32 -22.86 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf" (at -7.62 -20.32 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "diode" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "100V 0.15A standard switching diode, DO-35" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "D*DO?35*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "diode-combined_0_1"
      (polyline
        (pts
          (xy -1.27 1.27)
          (xy -1.27 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 0)
          (xy -1.27 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 1.27)
          (xy 1.27 -1.27)
          (xy -1.27 0)
          (xy 1.27 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
    )
    (symbol "diode-combined_1_1"
      (pin passive line (at -3.81 0 0) (length 2.54)
        (name "K" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 3.81 0 180) (length 2.54)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "diode-jumpered" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
    (property "Reference" "D" (at 0 2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "diode-jumpered" (at 0 -2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "unikbd:D_DO-35_SOD27_P7.62mm_Horizontal_bypassed" (at -20.32 -22.86 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf" (at -7.62 -20.32 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "net tie jumpered diode" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "100V 0.15A standard switching diode, DO-35" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "D*DO?35*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "diode-jumpered_0_1"
      (polyline
        (pts
          (xy -1.27 1.27)
          (xy -1.27 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 0)
          (xy -1.27 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 1.27)
          (xy 1.27 -1.27)
          (xy -1.27 0)
          (xy 1.27 1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
    )
    (symbol "diode-jumpered_1_1"
      (pin passive line (at -3.81 0 0) (length 2.54)
        (name "K" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 3.81 0 180) (length 2.54)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
