(module diode-combined (layer F.Cu) (tedit 5F23BF4D)
  (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
  (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
  (attr smd)
  (fp_text reference REF** (at 1.3462 3.9742) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (fp_text value D_DO-35_SOD27_P7.62mm_Horizontal (at -2.921 -16.4474) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -0.76 -1.58) (end 0.7 -1.58) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.7 1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
  (fp_line (start 0.7 1.52) (end -0.7 1.52) (layer F.Fab) (width 0.1))
  (fp_line (start -0.76 1.58) (end 1.4 1.58) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.7 -1.52) (end -0.7 -1.52) (layer F.Fab) (width 0.1))
  (fp_line (start -0.7 1.52) (end -0.7 -1.52) (layer F.Fab) (width 0.1))
  (fp_line (start -0.76 1.58) (end -0.76 0.65) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.76 -1.58) (end -0.76 -0.65) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.15 0.65) (end -0.15 0.25) (layer F.Fab) (width 0.1))
  (fp_line (start -0.15 0.45) (end -0.4 0.45) (layer F.Fab) (width 0.1))
  (fp_line (start -0.15 0.45) (end 0.15 0.65) (layer F.Fab) (width 0.1))
  (fp_line (start 0.15 0.65) (end 0.15 0.25) (layer F.Fab) (width 0.1))
  (fp_line (start 0.15 0.25) (end -0.15 0.45) (layer F.Fab) (width 0.1))
  (fp_line (start 0.15 0.45) (end 0.4 0.45) (layer F.Fab) (width 0.1))
  (fp_line (start -1.746 1) (end -1.746 -1) (layer B.Fab) (width 0.1))
  (fp_line (start -1.746 -1) (end 2.254 -1) (layer B.Fab) (width 0.1))
  (fp_line (start 2.254 -1) (end 2.254 1) (layer B.Fab) (width 0.1))
  (fp_line (start 2.254 1) (end -1.746 1) (layer B.Fab) (width 0.1))
  (fp_line (start -3.556 0) (end -1.746 0) (layer B.Fab) (width 0.1))
  (fp_line (start 4.064 0) (end 2.254 0) (layer B.Fab) (width 0.1))
  (fp_line (start -1.146 1) (end -1.146 -1) (layer B.Fab) (width 0.1))
  (fp_line (start -1.046 1) (end -1.046 -1) (layer B.Fab) (width 0.1))
  (fp_line (start -1.246 1) (end -1.246 -1) (layer B.Fab) (width 0.1))
  (fp_line (start -1.866 1.12) (end -1.866 -1.12) (layer B.SilkS) (width 0.12))
  (fp_line (start -1.866 -1.12) (end 2.374 -1.12) (layer B.SilkS) (width 0.12))
  (fp_line (start 2.374 -1.12) (end 2.374 1.12) (layer B.SilkS) (width 0.12))
  (fp_line (start 2.374 1.12) (end -1.866 1.12) (layer B.SilkS) (width 0.12))
  (fp_line (start -2.516 0) (end -1.866 0) (layer B.SilkS) (width 0.12))
  (fp_line (start 3.024 0) (end 2.374 0) (layer B.SilkS) (width 0.12))
  (fp_line (start -1.146 1.12) (end -1.146 -1.12) (layer B.SilkS) (width 0.12))
  (fp_line (start -1.026 1.12) (end -1.026 -1.12) (layer B.SilkS) (width 0.12))
  (fp_line (start -1.266 1.12) (end -1.266 -1.12) (layer B.SilkS) (width 0.12))
  (fp_line (start -4.606 1.25) (end -4.606 -1.25) (layer B.CrtYd) (width 0.05))
  (fp_line (start -4.606 -1.25) (end 5.114 -1.25) (layer B.CrtYd) (width 0.05))
  (fp_line (start 5.114 -1.25) (end 5.114 1.25) (layer B.CrtYd) (width 0.05))
  (fp_line (start 5.114 1.25) (end -4.606 1.25) (layer B.CrtYd) (width 0.05))
  (fp_poly (pts (xy 4.1656 0.5334) (xy 4.0132 0.5334) (xy 4.0132 0.9906) (xy 1.2192 0.9906)
    (xy 1.2192 1.143) (xy 4.1656 1.143)) (layer F.Cu) (width 0.1))
  (fp_poly (pts (xy -1.2192 -0.0762) (xy -3.048 -0.0762) (xy -3.048 0.0762) (xy -1.2192 0.0762)) (layer F.Cu) (width 0.1))
  (fp_text user %R (at -1.8288 3.8862) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.12)))
  )
  (pad 3 smd rect (at 1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
  (pad "" smd rect (at 1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 1 thru_hole rect (at -3.556 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 4.064 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
    (offset (xyz -3.556 0 -1.4986))
    (scale (xyz 1 1 1))
    (rotate (xyz 180 0 0))
  )
  (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOT-23.wrl
    (offset (xyz 0 0.0762 0.0508))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 180))
  )
)
