(footprint "diode-combined" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
  (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
  (attr smd)
  (fp_text reference "REF**" (at 7.4168 0.381) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    (tstamp 9a5031ed-ec12-4b1a-ae77-88564238f6fa)
  )
  (fp_text value "D_DO-35_SOD27_P7.62mm_Horizontal" (at -2.921 -16.4474) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a3d628b6-e450-4e14-a382-ea42b01e5e46)
  )
  (fp_text user "${REFERENCE}" (at 5.9944 -1.524) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.12)))
    (tstamp 91433c11-a5d3-4c05-b727-fdf95e7fa55a)
  )
  (fp_line (start -2.516 0) (end -1.866 0)
    (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 2ebfa4c0-52f6-477d-84ae-fde44362e12d))
  (fp_line (start -1.866 -1.12) (end 2.374 -1.12)
    (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp acd118ef-5003-4a76-b509-9118820b4c3a))
  (fp_line (start -1.866 1.12) (end -1.866 -1.12)
    (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp b46bc59c-2358-4b59-a25d-fbb3cb16df2e))
  (fp_line (start -1.266 1.12) (end -1.266 -1.12)
    (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 9cfee364-0a36-4168-9a03-9e2b8aa1532c))
  (fp_line (start -1.146 1.12) (end -1.146 -1.12)
    (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 65d199a4-3f39-4027-92d8-8b96a11565c3))
  (fp_line (start -1.026 1.12) (end -1.026 -1.12)
    (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp ffc7539d-4080-44cf-b011-f3b2023c7bdd))
  (fp_line (start 2.374 -1.12) (end 2.374 1.12)
    (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 57f9526e-4c99-4072-97b8-066d0a57bbfa))
  (fp_line (start 2.374 1.12) (end -1.866 1.12)
    (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp f31b7a91-9d17-405c-9333-5c2c7b64a125))
  (fp_line (start 3.024 0) (end 2.374 0)
    (stroke (width 0.12) (type solid)) (layer "B.SilkS") (tstamp 319a4a95-c418-4326-a8b7-8a6c7430ffaf))
  (fp_line (start -0.76 -1.58) (end -0.76 -0.65)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 400aa8b9-525e-4b74-8431-08f160c18c9a))
  (fp_line (start -0.76 -1.58) (end 0.7 -1.58)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d79dc885-3d55-4139-9cfe-95a99b1b887f))
  (fp_line (start -0.76 1.58) (end -0.76 0.65)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 82c6902a-689e-4107-a05f-01e99ead1a0a))
  (fp_line (start -0.76 1.58) (end 1.4 1.58)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7dc4b7e6-40cd-4d0c-af62-f4afd387d198))
  (fp_line (start -4.606 -1.25) (end 5.114 -1.25)
    (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 6bacd9ba-ac8c-4654-85ad-a3b2e6b1883b))
  (fp_line (start -4.606 1.25) (end -4.606 -1.25)
    (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 4cbd7873-db33-4daf-831f-89f5cb785cd7))
  (fp_line (start 5.114 -1.25) (end 5.114 1.25)
    (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp fbd02659-b43a-4653-ac5b-34a3e6ec113e))
  (fp_line (start 5.114 1.25) (end -4.606 1.25)
    (stroke (width 0.05) (type solid)) (layer "B.CrtYd") (tstamp 8a2ceddd-9c30-4506-a364-2858aefa41cd))
  (fp_line (start -1.7 -1.75) (end 1.7 -1.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 854b32ac-58cf-4638-9cec-37e2c2e892fb))
  (fp_line (start -1.7 1.75) (end -1.7 -1.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a4a5cb02-dc58-40a9-82b8-82ddeefd8d40))
  (fp_line (start 1.7 -1.75) (end 1.7 1.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5b422957-e485-42a4-b147-9fbfb29d049b))
  (fp_line (start 1.7 1.75) (end -1.7 1.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b649cec8-89c4-4cab-b1cc-6d9e01037f63))
  (fp_line (start -3.556 0) (end -1.746 0)
    (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 6e580d05-e9c9-4854-8b1a-75c75f6abc9e))
  (fp_line (start -1.746 -1) (end 2.254 -1)
    (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp a6cf9898-6005-45e9-96bb-3732f4d4f5bf))
  (fp_line (start -1.746 1) (end -1.746 -1)
    (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp ea82f956-26e9-49c2-b514-26649aff04be))
  (fp_line (start -1.246 1) (end -1.246 -1)
    (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 50603d47-6d27-4c8b-9d77-0efd2aebd9ac))
  (fp_line (start -1.146 1) (end -1.146 -1)
    (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 4be72ddf-e3fd-435f-9c6b-1ab5d5e469a6))
  (fp_line (start -1.046 1) (end -1.046 -1)
    (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp b327189d-ef01-441d-9738-e90f2400c9ef))
  (fp_line (start 2.254 -1) (end 2.254 1)
    (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp 0146e898-aeba-4624-b172-4002d1b7e289))
  (fp_line (start 2.254 1) (end -1.746 1)
    (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp f776b4a5-601c-4dd0-a822-65b1a7ca85ea))
  (fp_line (start 4.064 0) (end 2.254 0)
    (stroke (width 0.1) (type solid)) (layer "B.Fab") (tstamp e105655b-06c9-4456-981a-9fb7f072f2f6))
  (fp_line (start -0.7 1.52) (end -0.7 -1.52)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b88b8d93-4be3-48cb-af37-0763f35118ac))
  (fp_line (start -0.15 0.45) (end -0.4 0.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 85ec75d8-d66b-4275-b3ab-be08ddca07df))
  (fp_line (start -0.15 0.45) (end 0.15 0.65)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 43d7e843-b9cb-4123-8cac-3b3a3f192e82))
  (fp_line (start -0.15 0.65) (end -0.15 0.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 261fd709-b119-45e9-aff5-04154ebd9314))
  (fp_line (start 0.15 0.25) (end -0.15 0.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 110b6b8b-3d9a-49d9-a651-062dc12fd279))
  (fp_line (start 0.15 0.45) (end 0.4 0.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 389cedd3-c41f-4b55-b21a-f799d09847f4))
  (fp_line (start 0.15 0.65) (end 0.15 0.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 100d5a18-682a-4558-93e2-5a8dd299ab9d))
  (fp_line (start 0.7 -1.52) (end -0.7 -1.52)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f13bbe1d-3f04-49c6-8270-639b62b4252f))
  (fp_line (start 0.7 1.52) (end -0.7 1.52)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3b026976-d908-4912-bba2-893c5a17c51c))
  (fp_line (start 0.7 1.52) (end 0.7 -1.52)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0538aa2a-99c5-43eb-83e9-ea71514cd641))
  (pad "1" thru_hole rect (at -3.556 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp 025dd152-58ec-477d-aeeb-143880b94e0e))
  (pad "1" smd custom (at -1 0 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly
        (pts
          (xy 0.2192 0.0762)
          (xy 2.048 0.0762)
          (xy 2.048 -0.0762)
          (xy 0.2192 -0.0762)
        )
        (width 0.1) (fill yes))
    ) (tstamp 4425e3e4-bfde-49cd-b6d0-87896ea0174a))
  (pad "2" smd custom (at 1 0.95 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly
        (pts
          (xy -3.1656 0.4166)
          (xy -3.0132 0.4166)
          (xy -3.0132 -0.0406)
          (xy -0.2192 -0.0406)
          (xy -0.2192 -0.193)
          (xy -3.1656 -0.193)
        )
        (width 0.1) (fill yes))
    ) (tstamp 32524cff-711f-4252-b868-dbe08915a525))
  (pad "2" thru_hole oval (at 4.064 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp ffd110d8-3669-49c3-9fc9-32a7868c2705))
  (pad "NC" smd rect (at 1 -0.95 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp ba3a84a4-76f0-4b7f-a7e3-771a7ac6e6a5))
  (model "${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
    (offset (xyz -3.556 0 -1.4986))
    (scale (xyz 1 1 1))
    (rotate (xyz 180 0 0))
  )
  (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOT-23.wrl"
    (offset (xyz 0 0.0762 0.0508))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 180))
  )
)
