NEW
  AUTO 3,1
*--------------------------------------
*      SEARCH TEXT BUFFER FOR LINE
*
*      LINE NUMBER TO BE FOUND IS AT 0,X AND 1,X
*
*      IF FOUND, RETURN CARRY SET
*                (LINE.START) = ADDRESS OF LINE
*                (LINE.END  ) = ADDRESS OF NEXT LINE
*
*      IF NOT FOUND, RETURN CARRY CLEAR
*                (LINE.START) = ADDRESS OF NEXT LINE
*                (LINE.END  ) = ADDRESS OF NEXT LINE
*
*--------------------------------
SERTXT LDA PP       START AT BEGINNING OF TEXT BUFFER
       STA LINE.END
       LDA PP+1
       STA LINE.END+1
SERNXT LDA LINE.END+1      CONTINUE SEARCH WITH NEXT LINE
       STA LINE.START+1
       LDA LINE.END
       STA LINE.START
       CMP HI.MEM
       LDA LINE.START+1      SEE IF AT END YET
       SBC HI.MEM+1
       BCS .3       YES, DID NOT FIND
       LDY #0       POINT AT LINE LENGTH
       LDA (LINE.START),Y  GET LINE LENGTH
       ADC LINE.END      POINT TO NEXT LINE
       STA LINE.END
       BCC .1
       INC LINE.END+1
.1     INY          POINT AT LINE NUMBER
       LDA (LINE.START),Y  COMPARE TO DESRIRED LINE NUMBER
       CMP 0,X
       INY
       LDA (LINE.START),Y
       SBC 1,X
       BCC SERNXT   NOT THERE YET
       BNE .2       PASSED IT UP
       DEY          CHECK LOW BYTE AGAIN
       LDA (LINE.START),Y
       CMP 0,X
       BEQ .4       FOUND IT!
.2     LDA LINE.START      PASSED IT UP
       STA LINE.END      MAKE BOTH POINT AT SAME LINE
       LDA LINE.START+1
       STA LINE.END+1
.3     CLC          RETURN CARRY CLEAR
.4     RTS
*--------------------------------
*      DELETE LINES
*--------------------------------
DELETE
       JSR GNNB     GET NEXT NON-BLANK CHAR
       CMP #'/'
       BEQ .1       ...PATHNAME

       JSR CHECK.LETTER
       BCC .2       ...NOT LETTER, PROBABLY LINES

.1     JMP PASS.CMD.TO.PRODOS

.2     JSR BACKUP.CHAR.PNTR
       JSR PARSE.LINE.RANGE
       BCS SYNX.3   ...NO NUMBERS, SYNTAX ERROR

DELETE.LINES
       LDX #-1
       SEC
.2     LDA SRCP+1,X SEE IF RANGE EMPTY OR CROSSED
       STA LINE.START+1,X
       LDA ENDP+1,X
       STA A4L+1,X
       SBC LINE.START+1,X
       STA MOVE.DISTANCE+1,X
       INX
       BEQ .2
       TAX          TEST HI-BYTE OF MOVE.DISTANCE
       BPL MOVE.TEXT.UP  ...POSITIVE, RANGE GOOD
SYNX.3 JMP SYNX
*--------------------------------
*      MOVE TEXT FROM <PP> THRU <LINE.START>
*      UP <MOVE.DISTANCE> BYTES TO <A4L,A4H>
*--------------------------------
MOVE.TEXT.UP
       JSR COMPUTE.BLOCK.SIZE
       CLC
       LDA PP
       ADC MOVE.DISTANCE
       STA PP
       LDA PP+1
       ADC MOVE.DISTANCE+1
       STA PP+1
       LDY #0
       BEQ .3       ...ALWAYS
*---MOVE A WHOLE BLOCK-----------
.1     LDA (LINE.START),Y  MOVE BYTES 255 THRU 1 IN BLOCK
       STA (A4L),Y
.2     DEY
       BNE .1
       LDA (LINE.START),Y  MOVE LOWEST BYTE IN BLOCK
       STA (A4L),Y
.3     DEC LINE.START+1      PRIOR BLOCK
       DEC A4H
       DEX          ANY MORE BLOCKS?
       BNE .2       YES
*---MOVE SHORT BLOCK IF ANY------
       LDX BLKSIZ   PARTIAL BLOCK SIZE
       BEQ .5       NONE LEFT
.4     DEY
       LDA (LINE.START),Y
       STA (A4L),Y
       DEX
       BNE .4
.5     RTS
*--------------------------------
*      COPY L1,L2,L3
*          L1 = FIRST LINE OF RANGE TO COPY
*          L2 = LAST LINE OF RANGE TO COPY
*          L3 = LINE NUMBER BEFORE WHICH TO INSERT
*                   THE COPIED LINES
*--------------------------------
ERR1   JMP SYNX
ERR2   .EQ ERR1
ERR3   JMP MFER
ERR4   .EQ ERR1
*--------------------------------
COPY
       JSR PARSE.LINE.RANGE
       JSR GNNB     look for a comma
       CMP #','
       BNE ERR1     ...no comma
       SEC          SAVE POINTER AND COMPUTE LENGTH
       LDA SRCP     REALLY -(LENGTH)
       SBC ENDP
       STA MOVE.DISTANCE
       LDA SRCP+1
       SBC ENDP+1
       STA MOVE.DISTANCE+1
       BPL ERR2     RANGE BACKWARD OR EMPTY
*--------------------------------
       CLC
       LDA PP       COMPUTE NEW PP POINTER
       ADC MOVE.DISTANCE
       STA A4L
       LDA PP+1
       ADC MOVE.DISTANCE+1
       STA A4H
*--------------------------------
       LDA A4L      SEE IF ROOM FOR THIS
       CMP LO.MEM
       LDA A4L+1
       SBC LO.MEM+1
       BCC ERR3     MEM FULL ERR
*---Get Target Line Number-------
       JSR GNNB     pick up first digit of target line number
       JSR SCAN.LINE.NUMBER   (or it might be ".")
       BCS ERR1     ...not a line number of "."
       LDA 0,X      copy line number to A0L,H
       STA A0L
       LDA 1,X
       STA A0H
*---Verify valid target line-----
       LDA SRCP     BE SURE NOT INSIDE SOURCE BLOCK
       CMP LINE.START
       LDA SRCP+1
       SBC LINE.START+1
       BCS .1       BELOW SOURCE BLOCK
       LDA LINE.START
       CMP ENDP
       LDA LINE.START+1
       SBC ENDP+1
       BCC ERR4     INSIDE SOURCE BLOCK
*--------------------------------
*   TARGET IS ABOVE SOURCE BLOCK, SO WE HAVE TO
*   ADJUST SOURCE BLOCK POINTERS.
*--------------------------------
       CLC
       LDA SRCP
       ADC MOVE.DISTANCE
       STA SRCP
       LDA SRCP+1
       ADC MOVE.DISTANCE+1
       STA SRCP+1
       CLC
       LDA ENDP
       ADC MOVE.DISTANCE
       STA ENDP
       LDA ENDP+1
       ADC MOVE.DISTANCE+1
       STA ENDP+1
*--------------------------------
.1     JSR MOVE.TEXT.DOWN  MAKE THE HOLE
*--------------------------------
       LDA SRCP     SAVE SRCP AT A1
       STA A1L      (POINTS TO BLOCK TO BE COPIED)
       LDA SRCP+1
       STA A1H
.2     CLC          ADD (Y) TO A4
       TYA
       ADC A4L      POINTS TO BEGINNING OF NEXT 
       STA A4L      LINE IN HOLE
       BCC .3
       INC A4H
.3     LDY #0
       LDA (A1L),Y  COPY LINE LENGTH
       STA (A4L),Y
       INY          INSERT LINE #
       LDA A0L      OF TARGET LINE
       STA (A4L),Y
       INY          INSERT LINE #
       LDA A0H      OF TARGET LINE
       STA (A4L),Y
.4     INY          COPY REST OF LINE
       LDA (A1L),Y
       STA (A4L),Y
       BNE .4       UNTIL <EOL> TOKEN
       INY
       CLC
       TYA
       ADC A1L      POINT TO NEXT SOURCE LINE
       STA A1L
       BCC .5
       INC A1H
.5     CMP ENDP
       LDA A1H
       SBC ENDP+1
       BCC .2
       LDY #QDELOR
       JSR YES.OR.NO
       BNE .6
       JSR DELETE.LINES
.6     RTS
*--------------------------------
*      MOVE TEXT FROM <PP> THRU <LINE.START>
*      DOWN -<MOVE.DISTANCE> BYTES TO <A4L,A4H>
*--------------------------------
MOVE.TEXT.DOWN
       JSR COMPUTE.BLOCK.SIZE
       LDA PP
       STA A2L
       LDA PP+1
       STA A2H
       LDA A4L
       STA PP
       LDA A4H
       STA PP+1
       LDY #0
       BEQ .2       ...ALWAYS
.1     LDA (A2L),Y  YES, MOVE 256 BYTES
       STA (A4L),Y
       INY
       BNE .1
       INC A2H      POINT AT NEXT BLOCK
       INC A4H
.2     DEX          ANY WHOLE BLOCKS LEFT?
       BNE .1       YES
*---MOVE PARTIAL BLOCK-----------
       LDX BLKSIZ   SIZE OF PARTIAL BLOCK
       BEQ .4       EMPTY
.3     LDA (A2L),Y
       STA (A4L),Y
       INY
       DEX
       BNE .3
.4     RTS
*--------------------------------
*      COMPUTE SIZE OF TEXT BLOCK
*      FROM <PP> TO <LINE.START>
*
*      RETURN # WHOLE BLOCKS OF 256 BYTES +1 IN X
*      RETURN # BYTES IN PARTIAL BLOCK IN <BLKSIZ>
*--------------------------------
COMPUTE.BLOCK.SIZE
       SEC          COMPUTE # OF BYTES TO BE MOVED
       LDA LINE.START      CURRENT TOP POINTER
       SBC PP       CURRENT BOTTOM POINTER
       STA BLKSIZ   SAVE PARTIAL PAGE AMOUNT
       LDA LINE.START+1
       SBC PP+1
       TAX          # OF WHOLE PAGES IN X
       INX
       RTS
*--------------------------------------
MAN
SAVE usr/src/scmasm.31/scmasm.s.tsrch
LOAD usr/src/scmasm.31/scmasm.s
ASM
