NEW
  AUTO 3,1
				.LIST OFF	
				.OP	65C02
				.OR	$2000
				.TF drv/lancegs.drv
*--------------------------------------
				.INB inc/macros.i
				.INB inc/a2osx.i
				.INB inc/mli.e.i
				.INB inc/nic.i
				.INB inc/nic.91c96.i
				.INB inc/eth.i
*--------------------------------------
ZPArgPtr		.EQ ZPBIN
DEVSLOT0x		.EQ ZPBIN+2
*--------------------------------------
*			File Header (16 Bytes)
*--------------------------------------
CS.START		cld
				jmp Dev.Detect			cld,jmp abs=DRV
				.DA #$61				6502,Level 1 (65c02)
				.DA #1					DRV Layout Version 1
				.DA 0
				.DA CS.END-CS.START			Code Length
				.DA 0
				.DA 0
				.DA 0
*--------------------------------------
* Relocation Table
*--------------------------------------
L.MSG.DETECT	.DA MSG.DETECT
L.MSG.DETECT.OK	.DA MSG.DETECT.OK
L.MSG.DETECT.KO	.DA MSG.DETECT.KO
L.DRV.CS.START	.DA DRV.CS.START
L.FD.DEV		.DA FD.DEV
L.FD.DEV.NAME	.DA FD.DEV.NAME
L.SSCANF.MAC	.DA SSCANF.MAC
L.MAC0			.DA DCB+S.DCB.NIC.MAC
L.MAC1			.DA DCB+S.DCB.NIC.MAC+1
L.MAC2			.DA DCB+S.DCB.NIC.MAC+2
L.MAC3			.DA DCB+S.DCB.NIC.MAC+3
L.MAC4			.DA DCB+S.DCB.NIC.MAC+4
L.MAC5			.DA DCB+S.DCB.NIC.MAC+5
				.DA 0					End Of Reloc Table
*--------------------------------------
Dev.Detect		>STYA ZPArgPtr

				>LDYA L.MSG.DETECT
				>SYSCALL PutS
				ldx #$70
				ldy #7

.1				lda A2osX.S,y		IO based detection, avoid scanning in Disk Controller IO!!!!
				bne .2

				lda L91C96.BSR+1,x
				cmp #L91C96.DEVID
				beq .3
	
.2				dec FD.DEV.NAME+3
				txa
				sec
				sbc #$10
				tax
				dey
				bne .1
	
				>LDYA L.MSG.DETECT.KO
				>SYSCALL PutS

				lda #MLI.E.NODEV
				sec
				rts

.3				stx DEVSLOTx0
				sty DEVSLOT0x

				jsr Dev.ParseArgs
				bcs .99

.8				>PUSHW L.MSG.DETECT.OK
				>PUSHW L.FD.DEV.NAME
				>PUSHBI 2
				>SYSCALL PrintF

				>PUSHWI DRV.END
				>PUSHWI DRV.CS.END-DRV.CS.START
				>PUSHWI DRV.CS.START
				>LDYA L.DRV.CS.START
				>SYSCALL InsDrv
.99				bcs .9

				>STYA FD.DEV+S.FD.DEV.DRVPTR

				>PUSHW L.FD.DEV
				>PUSHW L.FD.DEV.NAME
				>SYSCALL MKDev
				bcs .9

				ldx DEVSLOT0x
				lda #A2osX.S.NIC
				sta A2osX.S,x
*				clc			
.9				rts
*--------------------------------------
Dev.ParseArgs	lda (ZPArgPtr)
				bne .1

				lda A2osX.RANDOM16
				eor A2osX.TIMER16
				sta DCB+S.DCB.NIC.MAC+3
				eor A2osX.RANDOM16+1
				sta DCB+S.DCB.NIC.MAC+4
				eor A2osX.TIMER16+1
				sta DCB+S.DCB.NIC.MAC+5
				clc
				rts

.1				>PUSHW ZPArgPtr
				>PUSHW L.SSCANF.MAC
				
				ldx #0

.2				>PUSHW L.MAC0,x
				inx
				inx
				cpx #12
				bne .2

				>PUSHBI 12				6 x byte PTRs
				>SYSCALL SScanF
				bcc .8

				lda #E.SYN
				sec
.8				rts
*--------------------------------------
CS.END
MSG.DETECT		.CZ "LanCeGS/SMSC91C96 Driver."
MSG.DETECT.OK	.CZ "LanCeGS/SMSC91C96 Installed As Device : %s\r\n"
MSG.DETECT.KO	.CZ "Hardware Not Found."
SSCANF.MAC		.CZ "%h:%h:%h:%h:%h:%h"
*--------------------------------------
FD.DEV			.DA #S.FD.T.CDEV
				.DA #0					HANDLER
				.DA #0					BUSID
				.DA #0					DEVID
				.DA 0					BUSPTR
				.BS 2					DRVPTR
				.DA 0					DCBPTR
				.DA 0					BUFPTR
FD.DEV.NAME		.AZ "eth7"
*--------------------------------------
*			Driver Code
*--------------------------------------
ZPIOCTL			.EQ ZPDRV
ZPBufPtr		.EQ ZPDRV+2
Size			.EQ ZPDRV+4
Counter			.EQ ZPDRV+6
*--------------------------------------
DRV.CS.START	cld
				jmp (.1,x)
.1				.DA STATUS
				.DA A2osX.BADCALL
				.DA A2osX.BADCALL
				.DA A2osX.BADCALL
				.DA A2osX.BADCALL
				.DA A2osX.BADCALL
				.DA OPEN
				.DA CLOSE
				.DA READ
				.DA WRITE
				.DA 0					end or relocation
*--------------------------------------
STATUS			>STYA ZPIOCTL

				ldy #S.IOCTL.S
				lda (ZPIOCTL),y
				beq .1
				cmp #S.IOCTL.S.GETDIB
				bne STATUS.DCB

				ldx #S.DIB-1
				.HS 2C					bit abs
.1				ldx #3

				ldy #S.IOCTL.BUFPTR
				lda (ZPIOCTL),y
				sta .3+1
				iny
				lda (ZPIOCTL),y
				sta .3+2

.2				lda DIB,x

.3				sta $ffff,x				SELF MODIFIED
				dex
				bpl .2

				clc
				rts

STATUS.DCB		cmp #S.IOCTL.S.GETDCB
				bne STATUS.9

				stz DCB+S.DCB.NIC.LINK

				ldx DEVSLOTx0

				stz L91C96.BSR,x
				lda L91C96.0.EPHSR,x
				lda L91C96.0.EPHSR+1,x
				and /L91C96.0.EPHSR.LINK
				beq .1
				lda #S.DCB.NIC.LINK.OK
				tsb DCB+S.DCB.NIC.LINK
	
				lda L91C96.0.TCR,x
				lda L91C96.0.TCR+1,x
				and /L91C96.0.TCR.FDSE
				beq .1

				lda #S.DCB.NIC.LINK.FD
				tsb DCB+S.DCB.NIC.LINK

.1				ldy #S.IOCTL.BUFPTR
				lda (ZPIOCTL),y
				sta .4+1
				iny
				lda (ZPIOCTL),y
				sta .4+2

				ldx #S.DCB.NIC-1

.3				lda DCB,x
.4				sta $ffff,x				SELF MODIFIED
				dex
				bpl .3

				clc
				rts

STATUS.9		lda #MLI.E.BADCTL
				sec
				rts
*--------------------------------------
OPEN			lda #S.DIB.S.OPENED
				bit DIB+S.DIB.S
				bne .9

				jsr CLOSE

*				ldx DEVSLOTx0			Done by CLOSE

				lda #L91C96.0.TCR.FDSE+L91C96.0.TCR.FUDPLX+L91C96.0.TCR.PADEN+L91C96.0.TCR.TXENA
				sta L91C96.0.TCR,x
				lda /L91C96.0.TCR.FDSE+L91C96.0.TCR.FUDPLX+L91C96.0.TCR.PADEN+L91C96.0.TCR.TXENA
				sta L91C96.0.TCR+1,x
				lda #L91C96.0.RCR.NOCRC+L91C96.0.RCR.RXENA+L91C96.0.RCR.ALLMUL
				sta L91C96.0.RCR,x
				lda /L91C96.0.RCR.NOCRC+L91C96.0.RCR.RXENA+L91C96.0.RCR.ALLMUL
				sta L91C96.0.RCR+1,x

				lda #1
				sta L91C96.BSR,x

				lda #L91C96.1.CR.NOWAIT
				sta L91C96.1.CR,x
				lda /L91C96.1.CR.NOWAIT
				sta L91C96.1.CR+1,x

				ldy #0

.2				lda DCB+S.DCB.NIC.MAC,y
				sta L91C96.1.IAR,x
				inx
				iny
				cpy #6
				bne .2

.3				ldx DEVSLOTx0

				lda #L91C96.1.CTR.DEFAULT+L91C96.1.CTR.AUTOREL
				sta L91C96.1.CTR,x
				lda /L91C96.1.CTR.DEFAULT+L91C96.1.CTR.AUTOREL
				sta L91C96.1.CTR+1,x
				clc
				rts

.9				lda #MLI.E.OPEN
				sec
				rts
*--------------------------------------
CLOSE			ldx DEVSLOTx0

				stz L91C96.BSR,x

				lda #L91C96.0.RCR.RESET
				sta L91C96.0.RCR,x
				lda /L91C96.0.RCR.RESET
				sta L91C96.0.RCR+1,x

				lda $C019				we can use VBL as we are not on //c

.1				eor $C019
				bpl .1

.2				eor $C019
				bpl .2

				stz L91C96.0.RCR,x
				stz L91C96.0.RCR+1,x
				clc
				rts
*--------------------------------------
READ			php
				sei

				>STYA ZPIOCTL

				ldx DEVSLOTx0

				lda #2
				sta L91C96.BSR,x

				lda L91C96.2.IST,x
				and #L91C96.2.IST.RCV
				beq READWRITE.9

.1				lda #L91C96.2.PTR.RCVD+L91C96.2.PTR.AUTOI+L91C96.2.PTR.READ
				sta L91C96.2.PTR,x
				lda /L91C96.2.PTR.RCVD+L91C96.2.PTR.AUTOI+L91C96.2.PTR.READ
				sta L91C96.2.PTR+1,x 

				lda L91C96.2.DATA,x		Get Frame Status Word (lo)
				lda L91C96.2.DATA,x		Get Frame Status Word (HI)
				asl
				asl
				asl 					#$10 = odd?
				asl						if odd, CS
				lda L91C96.2.DATA,x		get lo byte count
				sbc	#5					compute Size
				pha

				ldy #S.IOCTL.BYTECNT
				sta (ZPIOCTL),y
				eor #$ff
				sta Counter

				lda L91C96.2.DATA,x		get hi byte count
				sbc #0
				iny
				sta (ZPIOCTL),y
				eor #$ff
				sta Counter+1
				eor #$ff

				ply						Y,A = Size

				>SYSCALL2 GetMem
				bcs READWRITE.99

				>STYA ZPBufPtr

				phx

				phy

				ldy #S.IOCTL.BUFPTR+1
				sta (ZPIOCTL),y
				dey
				pla
				sta (ZPIOCTL),y
				ldx DEVSLOTx0

				ldy #0
				
.2				inc Counter
				bne .3
				inc Counter+1
				beq .4

.3				lda L91C96.2.DATA,x
				sta (ZPBufPtr),y
				iny
				bne .2

				inc ZPBufPtr+1
				bra .2

.4				lda #L91C96.2.MMUCR.REMREL
				sta L91C96.2.MMUCR,x

.8				pla						hMem

				plp
				clc
				rts
*--------------------------------------
READWRITE.9		lda #E.NODATA

READWRITE.99	plp
				sec
				rts
*--------------------------------------
WRITE			php
				sei
				>STYA ZPIOCTL

				ldx DEVSLOTx0

				lda #2
				sta L91C96.BSR,x
			
				ldy #S.IOCTL.BYTECNT
				lda (ZPIOCTL),y
				sta Size
				eor #$ff
				sta Counter
				eor #$ff
				clc
				adc #6					3 WORDs more Status, len & Control

				bne .10

				clc						LO byte is 0, no need for an extra empty page

.10				iny
				lda (ZPIOCTL),y
				sta Size+1
				eor #$ff
				sta Counter+1
				eor #$ff

				adc #0

.1				ora #L91C96.2.MMUCR.ALLOC
				sta L91C96.2.MMUCR,x

				ldy #0

.2				lda L91C96.2.IST,x
				and #L91C96.2.IST.ALLOC
				bne .3

				dey
				bne .2

				bra READWRITE.9

.3				lda L91C96.2.AAR,x
				sta L91C96.2.PNR,x
				lda #L91C96.2.PTR.AUTOI
				sta L91C96.2.PTR,x
				lda /L91C96.2.PTR.AUTOI
				sta L91C96.2.PTR+1,x
				ldy #S.IOCTL.BUFPTR
				lda (ZPIOCTL),y
				sta ZPBufPtr
				iny
				lda (ZPIOCTL),y
				sta ZPBufPtr+1

				ldy #S.ETH.SRCMAC+5		Add Src MAC Address
				ldx #5

.4				lda DCB+S.DCB.NIC.MAC,x
				sta (ZPBufPtr),y
				dey
				dex
				bpl .4

				ldx DEVSLOTx0

				stz L91C96.2.DATA,x		write fake status word
				stz L91C96.2.DATA,x

				lda Size
				pha
				eor #$01
				lsr
				pla

				adc #$05				add 5 if odd, 6 if even
				sta L91C96.2.DATA,x

				lda Size+1
				adc #$00
				sta L91C96.2.DATA,x

				ldy #0

.5				inc Counter
				bne .51
				inc Counter+1
				beq .70

.51				lda (ZPBufPtr),y
				iny
				bne .6

				inc ZPBufPtr+1

.6				inc Counter
				bne .61

				inc Counter+1
				beq .71

.61				sta L91C96.2.DATA,x
				lda (ZPBufPtr),y
				sta L91C96.2.DATA,x
				iny
				bne .5

				inc ZPBufPtr+1
				bra .5

.70				lda #0
				sta L91C96.2.DATA,x
				sta L91C96.2.DATA,x
				bra .8

.71				sta L91C96.2.DATA,x
				lda #%00100000			signal an extra (odd) byte
				sta L91C96.2.DATA,x

.8				lda #L91C96.2.MMUCR.NQPKT
				sta L91C96.2.MMUCR,x

				plp
				clc
				rts
*--------------------------------------	
DRV.CS.END
DEVSLOTx0		.BS 1
*--------------------------------------
DIB				.DA #0
				.DA #0,#0,#0			size
				.PS "LanCEGS/L91C96"
				.BS 2
				.DA #S.DIB.T.NIC
				.BS 1					Subtype
				.BS 2					Version
*--------------------------------------
DCB				.DA #S.DCB.T.NIC
				.BS 1					FLAGS
				.BS 1					LINK
				.DA #S.DCB.NIC.SPEED.10
				.HS 000E3A123456		MAC
				.BS 12					IP/MASK/GW
*--------------------------------------
DRV.END
MAN
SAVE usr/src/drv/lancegs.drv.s
ASM
