NEW
  AUTO 3,1
*--------------------------------------
* 'detree' deallocates blocks from tree files. it is assumed that the device has
* been pre-selected and the 'gbuf' may be used.
*
* on entry:
*  stortype = storage type in upper nibble, lower nibble is undisturbed.
*  firstbl & firstbh = first block of file (index or data).
*  deblock = 0
*  dtree = ptr to 1st block with data to be deallocated at tree level.
*  dsap = ptr to 1st block at sapling level.
*  dseed = byte (0-511) position to be zeroed from (inclusive).
*
* on exit:
*  stortype = modified result of storage type (if applicable).
*  firstbl & h = modified if storage type changed.
*  deblock = total number of blocks freed at all levels.
*  dtree, dsap, deseed unchanged.
*
* to trim a tree to a seed file, both dtree and dsap must be zero.
* to go from tree to sapling, dtree alone must be zero.
*--------------------------------------
detree			lda stortyp				which kind of tree ?
				cmp #$20			 	is it a 'seed' ?
				bcc L4C46			  	if yes.

				cmp #$30			 	a sapling ?
				bcc L4C51			  	if yes.

				cmp #$40			 	is it at least a 'tree' ?
				bcc L4C59			  	branch if it is.

				lda #$0C			 	block allocation error.
				jsr GP.SysDeath			P8 system death vector

* seedling file type - make sure first desirable block is the only
* block available in a seedling file.

L4C46  			lda dsap
				ora dtree
				bne L4CC2

				jmp seedel0

* sapling file type - make sure first desirable block is within the range of
* blocks available in a sapling file

L4C51  			lda dtree				can't have any blocks in this range
				bne L4CC2			  	if so then done

				jmp sapdel0				else go deallocate

L4C59			lda #$80
				sta topdest				for tree top start at end, work backwards.

L4C5E  			jsr drdfrst				read specified first block into gbuf.
				bcs L4CC2			  	return errors.

				ldy topdest				get current pointer to top indexes.
				cpy dtree			  	have enough sapling indexes been
				beq L4CC3			  	deallocated? yes, now deallocate blocks

				ldx #$07				buffer up to 8 sapling index block

L4C6D  			lda gbuf,y				addresses. fetch low block address
				sta dealbufl,x			and save it.
				ora gbuf+$100,y			is it a real block that is allocated?
				beq L4C81			  	branch if phantom block.

				lda gbuf+$100,y			fetch high block address
				sta dealbufh,x			and save it.
				dex		 				decrement and test for dealc buf filled.
				bmi L4C93				branch if 8 addresses fetched.

L4C81  			dey		 				look for end of deallocation limit.
				cpy dtree			  	is this the last position on tree level?
				bne L4C6D			  	if not.

				iny

L4C8A  			stz dealbufl,x		 	fill rest of dealc buffer with null addresses.
				stz dealbufh,x
				dex
				bpl L4C8A

L4C93  			dey		 				decrement to prepare for next time.
				sty topdest				save index.

				ldx #$07

L4C99  			stx dtmpx			  	save index to dealc buf.
				lda dealbufl,x
				sta bloknml
				ora dealbufh,x			finished ?
				beq L4C5E			  	branch if done with this level.

				lda dealbufh,x			complete address with high byte,
				sta bloknml+1
				jsr XDOS.ReadGBuf		read sapling level into gbuf.
				bcs L4CC2			  	return errors.

				jsr dealblk				go free all data indexes in this block
				bcs L4CC2

				jsr XDOS.WriteGBuf		write the flipped index block
				bcs L4CC2

				ldx dtmpx			  	restore index to dealc buff.
				dex		 				are there more to free?
				bpl L4C99			  	branch if so.

				bmi L4C5E			  	branch always to get up to 8 more

L4CC2  			rts		 				sapling block numbers.

L4CC3  			ldy dtree			  	deallocate all sapling blocks greater
				iny		 				than specified block.
				jsr dalblk1				(master index in gbuf)
				bcs L4CC2			  	if errors.

				jsr XDOS.WriteGBuf		write updated master index back to disk.
				bcs L4CC2

				ldy dtree				figure out if tree can become sapling.
				beq L4CEB			  	branch if it can.

				lda gbuf,y			 	otherwise, continue with partial, deallocation of last sapling index.
				ora gbuf+$100,y			is there such a sapling index block ?
				beq L4CC2			  	all done if not.

				lda gbuf,y
				ldx gbuf+$100,y			read in sapling level to be modified.

				jsr XDOS.ReadGBufAX	 	read highest sapling index into gbuf.
				bcc L4CF5

				rts

L4CEB  			jsr shrink				shrink tree to sapling
				bcs L4CC2

sapdel0			jsr drdfrst				read specified sapling level index
				bcs L4CC2			  	into gbuf. branch if error.

L4CF5  			ldy dsap				pointer to last of desirable indexes.
				iny		 				inc to 1st undesirable.
				beq L4D05			  	branch if all are desirable.

				jsr dalblk1				deallocate all indexes above specified.
				bcs L4CC2

				jsr XDOS.WriteGBuf		write out the index block
				bcs L4CC2

L4D05  			ldy dsap			 	prepare to clean up last data block.
				beq L4D1F			  	branch if possibility of making a seed.

L4D0A  			lda gbuf,y			 	fetch low order data block address.
				ora gbuf+$100,y			is it a real block ?
				beq L4CC2			  	if not, then done.

				lda gbuf,y
				ldx gbuf+$100,y

				jsr XDOS.ReadGBufAX	 	go read data block into gbuf.
				bcc L4D2E			  	branch if good read

L4D1E			rts		 				or return error.

L4D1F  			lda dtree			  	are both tree and sap levels zero ?
				bne L4D0A			  	if not.

				jsr shrink				reduce this sap to a seed.
				bcs L4D1E			  	if error.

seedel0			jsr drdfrst				go read data block.
				bcs L4D1E			  	if error.

L4D2E  			ldy dseed+1				check high byte for no deletion.
				beq L4D39			  	branch if all of 2nd page to be deleted.

				dey						if dseed > $200 then all were done.
				bne L4D1E			  	branch if that is the case.

				ldy dseed			  	clear only bytes >= dseed.

L4D39  			lda #$00

L4D3B  			sta gbuf+$100,y			zero out unwanted data
				iny
				bne L4D3B

				ldy dseed+1				is that all ?
				bne L4D4F			  	yes.

				ldy dseed

L4D49  			sta gbuf,y
				iny
				bne L4D49

L4D4F  			jmp XDOS.WriteGBuf		update data block to disk.

L4D52  			rts		 				return error status.

drdfrst			lda firstbl				read specified 1st block into gbuf
				ldx firstbh
				jmp XDOS.ReadGBufAX		go read it

* beware that dealloc may bring in a new bitmap block and may destroy
* locations 46 and 47 which are used to point to the current index block.

shrink			ldx firstbh				first deallocate top index block
				phx
				lda firstbl
				pha		 				save block address of this index block.
				jsr XDOS.DeallocAX		free it from the bitmap
				pla
				sta bloknml				set master of sapling
				pla						index block address.
				sta bloknml+1
				bcs L4D1E			  	report errors.

				lda gbuf			 	get # of new 1st block from old index.
				sta firstbl
				lda gbuf+$100
				sta firstbh
				ldy #$00
				jsr swapme				flip that one entry in old top index.
				sec		 				now change file type,
				lda stortyp				from tree to sapling,
				sbc #$10			 	or from sapling to seed.
				sta stortyp
				jmp XDOS.WriteGBuf		write the (deallocated) old top index.

dealblk			ldy #$00			 	start at beginning.
dalblk1			lda bloknml				save disk address of gbuf's data.
				pha
				lda bloknml+1
				pha

L4D96  			sty saptr			  	save current index.
				lda gbuf,y			 	get low address of block to deallocate.
				cmp #$01			 	test for null block into carry.
				ldx gbuf+$100,y			get remainder of block address.
				bne L4DA5			  	branch if not null.

				bcc L4DB0			  	was the low part null too ?

L4DA5  			jsr XDOS.DeallocAX		free it up on volume bitmap.
				bcs L4DB4			  	return any error.

				ldy saptr			  	get index to sapling level index block.

				jsr swapme

L4DB0  			iny		 				next block address.
				bne L4D96			  	if more to deallocate or test.

				clc		 				no error.

L4DB4  			tax		 				save error code, if any.
				pla		 				restore blocknm (16 bit)
				sta bloknml+1
				pla
				sta bloknml
				txa		 				restore return code
				rts

swapme			lda delflag				swapping or zeroing ?
				bne L4DC5			  	skip if swapping.

				tax		 				make x = 0.
				beq L4DCB			  	zero the index (always taken).

L4DC5  			ldx gbuf+$100,y		   	index high
				lda gbuf,y			 	index low
L4DCB  			sta gbuf+$100,y		   	save index high
				txa
				sta gbuf,y			 	save index low
				rts						done.
*--------------------------------------
* MEMMGR memory manager
*
* allocate buffer in memory tables
*--------------------------------------
alcbuffr 		ldy #$04				index to user specified buffer.
alcbufr1 		lda (A3L),y				this buffer must be on a page boundary.
				tax		 				save for validation.
				cmp #$08
				bcc L4E1E			  	cannot be lower than video !

				cmp #$BC				nor greater than $BB00
				bcs L4E1E			  	since it would wipe out globals...

				sta datptr+1
				dey
				lda (A3L),y				low address should be zero !
				sta datptr
				bne L4E1E			  	error if not page boundary.

				inx		 				add 4 pages for 1k buffer.
				inx
				inx
				inx

L4DED			dex		 				test for conflicts.
				jsr cmembit				test for free buffer space
				and MEMTABL,y			P8 memory bitmap
				bne L4E1E			  	report memory conflict, if any.

				cpx datptr+1			test all 4 pages.
				bne L4DED

				inx		 				add 4 pages again for allocation.
				inx
				inx
				inx

L4DFE  			dex		 				set proper bits to 1
				jsr cmembit
				ora MEMTABL,y			to mark it's allocation.
				sta MEMTABL,y
				cpx datptr+1			set all 4 pages
				bne L4DFE

				ldy fcbptr			 	calculate buffer number
				lda FCBs,y
				asl			  			buffer number = (entnum) * 2.
				sta FCBs+FCB.BUFID,y	save it in fcb.
				tax		 				use entnum * 2 as index to global
				lda datptr+1			buffer addr tables. get addr already
				sta buftbl-1,x			validated as good. store hi addr

				clc		 				(entnums start at 1, not 0)
				rts

L4E1E  			lda #MLI.E.BADBUF	 	buffer is in use or not legal
				sec
				rts
*--------------------------------------
relbuffr 		tax						index into global buffer table.
				lda buftbl-2,x
				sta bufaddrl
				lda buftbl-1,x
				sta bufaddrh
				beq relbuffr.8		 	branch if unallocated buffer space.

				stz buftbl-1,x			take address out of buffer list.
				stz buftbl-2,x			(x was set up by getbufadr)

freebuf			ldx bufaddrh			get hi buffer address
				inx		 				add 4 pages to account for 1k space.
				inx
				inx
				inx

.1  			dex		 				drop to next lower page.
				jsr cmembit				get bit and position to memtable of
				eor #$FF			 	this page. invert mask.
				and MEMTABL,y			mark address as free space.
				sta MEMTABL,y
				cpx bufaddrh			all pages freed ?
				bne .1				  	no.

relbuffr.8 		clc		 				no error.
				rts
*--------------------------------------
* calculate memory allocation bit position.
* on entry: x = high address of buffer, low address assumed zero.
* on exit: acc = allocation bit mask, x = unchanged, y = pointer to memtabl byte
*--------------------------------------
cmembit			txa						page address
				and #$07			 	which page in any 2k set ?
				tay		 				use as index to determine
				lda whichbit,y			bit position representation.
				pha		 				save bit position mask for now.
				txa		 				page address.
				lsr
				lsr			  			determine 2k set
				lsr
				tay		 				return it in y.
				pla		 				restore bit mask. return bit position
				rts		 				in a & y, pointer to memtabl in x.
*--------------------------------------
valdbuf			lda usrbuf+1			high address of user's buffer
				cmp #$02			 	must be greater than page 2.
				bcc L4E1E			  	report bad buffer

				ldx cbytes+1
				lda cbytes			 	get cbytes-1 value.
				sbc #$01			 	(carry is set)
				bcs L4E76

				dex

L4E76  			clc
				adc usrbuf			 	calculate end of request address.
				txa		 				do high address.
				adc usrbuf+1			the final address
				tax		 				must be less than $BFnn (globals)
				cpx #$BF
				bcs L4E1E			  	report bad buffer.

				inx		 				loop thru all affected pages.

vldbuf1			dex		 				check next lower page.
				jsr cmembit
				and MEMTABL,y			if 0 then no conflict.
				bne L4E1E			  	branch if conflict.

				cpx usrbuf+1			was that the last (lowest) page ?
				bne vldbuf1			 	if not.

				clc		 				all pages ok.
				rts
*--------------------------------------
XDOS.GetBuf		ldy #$02			 	give user address of file buffer referenced by refnum.
				lda bufaddrl
				sta (A3L),y
				iny
				lda bufaddrh
				sta (A3L),y
				clc		 				no errors possible
				rts
*--------------------------------------
XDOS.SetBuf		ldy #$03
				jsr alcbufr1			allocate new buffer address over old one
				bcs L4EC7				report any errors immediately

				lda bufaddrh
				sta usrbuf+1
				lda bufaddrl
				sta usrbuf
				jsr freebuf				free address space of old buffer

				ldy #$00
				ldx #$03

.1  			lda (usrbuf),y			move all 4 pages of the buffer to
				sta (datptr),y			new location.
				iny
				bne .1

				inc datptr+1
				inc usrbuf+1
				dex
				bpl .1
XDOS.SetBuf.CLCRTS
				clc		 				no errors
L4EC7  			rts
*--------------------------------------
XDOS.IsValidChar
				cmp #'0'
				bcc XDOS.IsValidFirstChar
				cmp #'9'+1
				bcc XDOS.IsValidFirstChar.RTS
XDOS.IsValidFirstChar
				.DO ENHFILENAME=1
				cmp #'.'
				beq XDOS.SetBuf.CLCRTS
				cmp #'_'
				beq XDOS.SetBuf.CLCRTS
				.FIN
				cmp #'A'
				bcc XDOS.IsValidFirstChar.SEC
				cmp #'Z'+1
				.DO LOWERCASE=1
				bcc XDOS.IsValidFirstChar.RTS
				cmp #'a'
				bcc XDOS.IsValidFirstChar.SEC
				cmp #'z'+1
				.FIN
XDOS.IsValidFirstChar.RTS
				rts

XDOS.IsValidFirstChar.SEC
				sec
				rts
*--------------------------------------
* move 3 pages of dispatcher from 'displc2' to 'dispadr'
* this move routine must be resident above $E000 at all times
*--------------------------------------
calldisp 		lda RRAMWRAMBNK2		read/write RAM bank 2
				lda RRAMWRAMBNK2

				stz A1L
				lda #$D1
				sta A1L+1

				stz A2L
				lda #$10
				sta A2L+1

				ldy #$00
				ldx #$03				3 pages to move.

.1  			lda (A1L),y
				sta (A2L),y
				iny
				bne .1

				inc	A1L+1			  	pointers to next page
				inc	A2L+1
				dex		 				move all pages needed
				bne .1

				lda RRAMWRAMBNK1		read/write RAM bank 1
				lda RRAMWRAMBNK1		swap mli space back in

				stz mliact			 	MLI active flag

				stz softev
				lda #$10				point RESET to dispatch entry
				sta softev+1
				eor #$A5
				sta pwredup				power up byte

				jmp $1000
*--------------------------------------
XDOS.SPREMAP	ldx #$03				assume 3 parameters.
				lda A4L			  		command number
				sta cmdnum
				bne .1					taken if not status call

				ldy #XDOS.SPStatus		set up memory for the status list buffer
				sty buf					fake up the prodos parameters
				ldy /XDOS.SPStatus
				sty buf+1
				stz bloknml				set statcode = 0 for simple status call

.1  			cmp #$03			 	format command ?
				bne .2				  	no.

				ldx #$01			 	format has only 1 parameter.

.2  			stx XDOS.SPParams		set # of parms.

				lda unitnum				DSSS0000
				lsr			  			turn unit number into an index
				lsr
				lsr
				lsr
				tax						range = 1-15

				lda XDOS.SPUnit-1,x		get the smartport unit number and
				sta XDOS.SPParams.U		store into smartport parm list.
				lda XDOS.SPVectLo-1,x
				sta sp_vector+1			copy smartport entry address
				lda XDOS.SPVectHi-1,x
				sta sp_vector+2

				ldx #$04				copy buffer pointer and block #

.3  			lda buf-1,x				from prodos parameters
				sta XDOS.SPParams.B-1,x		to smartport parameter block
				dex
				bne .3

sp_vector 		jsr $0000				smartport call (entry address gets modified)
cmdnum			.HS 00					command #
				.DA XDOS.SPParams
				bcs	.9

				ldx cmdnum				status call ?
				bne .9				  	no...

				ldx XDOS.SPStatus+1		else get the block count
				ldy XDOS.SPStatus+2
				lda	XDOS.SPStatus		get the returned status.
				bit #$10			 	is there a disk present ?
				beq .8

				and #$44			 	mask all but write allowed and write
				eor #$40			 	protected bits. if allowed and not
*				clc
				beq .9				  	protected, exit with carry clear

				lda #MLI.E.WRTPROT	 	else return write protected error.
				.HS 2C					BIT ABS
.8				lda #MLI.E.OFFLINE		return offline error.
				sec
.9  			rts
*--------------------------------------
XDOS.SPParams	.HS 03					# of parms (always 3 except format)
XDOS.SPParams.U	.HS 00			  		unit number
XDOS.SPParams.B	.HS 0000				data buffer
				.HS 000000				block number (3 bytes)
*--------------------------------------
XDOS.TBX		jmp (.1,x)

.1				.DA XDOS.TBX.MemReset
				.DA XDOS.TBX.EnumBlk
				.DA XDOS.TBX.EnumNext
*--------------------------------------
XDOS.TBX.MemReset
				ldx #$17

.1  			stz MEMTABL,x			P8 memory bitmap
				dex
				bne .1

				inc MEMTABL+$17			protect global page
				lda #$CF				protect zero page, stack and page 1
				sta MEMTABL
				rts
*--------------------------------------
XDOS.TBX.EnumBlk
				jsr XDOS.ZPT.InitA

				ldx h_maxent

				lda (zpt)
				cmp #$E0
				bcc .2

				ldy #$1F+3
				ldx #3

.1				lda (zpt),y
				sta h_entln,x
				dey
				dex
				bpl .1

				jsr XDOS.ZPT.Next		skip header

				ldx h_maxent
				dex						skip header

.2				stx cntent

XDOS.TBX.CheckFCnt
				lda h_fcnt
				ora h_fcnt+1
				beq XDOS.TBX.SECRTS
*				clc
				rts
*--------------------------------------
XDOS.TBX.EnumNext
				sty	sos
				sta sos+1
				
				jsr XDOS.TBX.CheckFCnt
				bcs .9

.1				dec cntent
				bmi XDOS.TBX.SECRTS

				lda (zpt)
				and #$0F
				beq .7

				sta (sos)

				pha

				jsr XDOS.ZPT.Unpack

				ply

.2				lda (zpt),y
				sta (sos),y
				dey
				bne .2

				ldy #16					FileType
				lda (zpt),y

				pha
				jsr XDOS.ZPT.Next
				
				lda h_fcnt+1
				bne .3
				
				dec h_fcnt+1

.3				dec h_fcnt				
				
				pla
*				clc
.9				rts

.7				jsr XDOS.ZPT.Next
				bra .1
*--------------------------------------
XDOS.TBX.SECRTS	sec
				rts
*--------------------------------------				
XDOS.ZPT.InitGBuf
				lda /gbuf

XDOS.ZPT.InitA	sta zpt+1
				lda #4
				sta zpt

				rts
*--------------------------------------
XDOS.ZPT.Unpack	ldy #$1D				MIN_VERSION
				lda (zpt),y
				bpl .6					no lowercase information

				lda (zpt)
				and #$0F
				beq .6					length=0

				tay

.2				cpy #8					CS if MIN_VERSION to use
				phy

				bcs .3

				ldy #$1D				MIN_VERSION
				lda (zpt),y

				ply
				and whichbit,y
				beq .5

				bra .4

.3				ldy #$1C				VERSION
				lda (zpt),y

				ply
				and whichbit-8,y
				beq .5

.4				lda (zpt),y
				eor #$20				to lowercase
				sta (zpt),y

.5				dey
				bne .2

.6				rts
*--------------------------------------
XDOS.ZPT.Next	lda h_entln

XDOS.ZPT.NextA	clc
				adc zpt
				sta zpt
				bcc .8

				inc zpt+1
				clc

.8				rts
*--------------------------------------
* data tables
*--------------------------------------
XDOS.CmdNums	.HS D3D4D5D6			table of valid mli command numbers.
				.HS 40410000
				.HS 808182
				.HS 65
				.HS C0C1C2C3C4C5C6C7C8C9CACBCCCDCECF
				.HS 00
				.HS D0D1D2

XDOS.ParamCnt	.HS 02020202			parameter counts for the calls
				.HS 0201FFFF
				.HS 030300
				.HS 04
				.HS 070102070A0201010303040401010202
				.HS FF
				.HS 020202

XDOS.CmdFlags	.HS A0A1A2
				.HS A384
				.HS 050607
				.HS 88494A4B
				.HS 2C2D
				.HS 4E4F
				.HS 50515253
				.HS 94959697

cmdtable 		.DA XDOS.Create
				.DA XDOS.Destroy
				.DA XDOS.Rename
				.DA XDOS.SetFileInfo

				.DA XDOS.GetFileInfo
				.DA XDOS.Online
				.DA XDOS.SetPrefix
				.DA XDOS.GetPrefix

				.DA XDOS.Open
				.DA XDOS.NewLine
				.DA XDOS.Read
				.DA XDOS.Write

				.DA XDOS.Close
				.DA XDOS.Flush
				.DA XDOS.SetMark
				.DA XDOS.GetMark

				.DA XDOS.SetEOF
				.DA XDOS.GetEOF
				.DA XDOS.SetBuf
				.DA XDOS.GetBuf

				.DA XDOS.SetFileInfoEx
				.DA XDOS.GetFileInfoEx
				.DA XDOS.ACL

dinctbl			.HS 0100000200			table to increment directory usage/eof counts
				.DO LOWERCASE=1
XDOS.VolHdrDef	.HS C3270D
XDOS.VolHdrDef.Cnt	.EQ *-XDOS.VolHdrDef
				.ELSE
pass			.HS 75
xdosver			.HS 00
compat			.HS 00
				.HS C3270D000000
				.FIN
rootstuf 		.HS 0F02000400000800
whichbit 		.HS 8040201008040201
ofcbtbl			.HS 0C0D1819151617
inftabl			.HS 1E101F2080939421
				.HS 22232418191A1B
deathmsg		.AS -"SYS ERR-$0"
deathmsg.LEN	.EQ *-deathmsg
*--------------------------------------
XDOS.DATA		.DUMMY
*--------------------------------------
own_blk			.HS 0000
own_ent			.HS 00
own_len			.HS 00
*--------------------------------------
				.DO ACL=1
h_acl			.BS 8
				.FIN
h_credt			.HS 0000				directory creation date
				.HS 0000				directory creation time
				.HS 00			 	 	version under which this dir created
				.HS 00			 	 	earliest version that it's compatible
h_attr			.HS 00				 	attributes (protect bit, etc.)
h_entln			.HS 00				 	length of each entry in this directory
h_maxent 		.HS 00				 	maximum number of entries per block
h_fcnt			.HS 0000			 	current # of files in this directory
h_bmap			.HS 0000			 	address of first allocation bitmap
h_tblk			.HS 0000			 	total number of blocks on this unit
*--------------------------------------
d_dev			.HS 00				 	device number of this directory entry
d_head			.HS 0000			 	address of <sub> directory header
d_entblk 		.HS 0000				address of block which contains entry
d_entnum 		.HS 00				 	entry number within block
d_stor			.BS 16				  	file name
d_filid			.HS 00				 	user's identification byte
d_frst			.HS 0000			 	first block of file
d_usage			.HS 0000			 	# of blocks allocated to this file
d_eof			.HS 000000			 	current end of file marker
d_credt			.HS 0000				file creation date
				.HS 0000				file creation time
d_sosver 		.HS 00					sos version that created this file
d_comp			.HS 00				 	backward version compatibility
d_attr			.HS 00				 	attributes (protect, r/w, enable, etc.)
d_auxid			.HS 0000			 	user auxilliary identification
d_moddt			.HS 0000				file's last modification date
				.HS 0000				file's last modification time
d_dhdr			.HS 0000			 	file directory header block address
*--------------------------------------
scrtch			.HS 00000000			scratch area for allocation address conversion.
oldeof			.HS 000000				temp used in r/w
oldmark			.HS 000000
xvcbptr			.HS 00				 	used in 'cmpvcb' as a temp
vcbptr			.HS 00
fcbptr			.HS 00
fcbflg			.HS 00
reql			.HS 00
reqh			.HS 00
levels			.HS 00
totent			.HS 00
entcntl			.HS 00
entcnth			.HS 00
cntent			.HS 00
nofree			.HS 00
bmcnt			.HS 00
saptr			.HS 00
pathcnt			.HS 00
p_dev			.HS 00
p_blok			.HS 0000
bmptr			.HS 00
basval			.HS 00
half			.HS 00

* bitmap info tables

bmastat			.HS 00
bmadev			.HS 00
bmadadr			.HS 0000
bmacmap			.HS 00
tposll			.HS 00
tposlh			.HS 00
tposhi			.HS 00
rwreql			.HS 00
rwreqh			.HS 00
nlchar			.HS 00
nlmask			.HS 00
ioaccess 		.HS 00			 		has a call been made to disk device handler ?
cmdtemp			.HS 00
bkbitflg		.HS 00					used to set or clear backup bit
duplflag 		.HS 00
vcbentry 		.HS 00

* xdos temporary variables

namcnt			.HS 00
rnptr			.HS 00
namptr			.HS 00
vnptr			.HS 00
prfxflg			.HS 00
cferr			.HS 00

* deallocation temporary variables

firstbl			.HS 00
firstbh			.HS 00
stortyp			.HS 00
deblock			.HS 0000
dtree			.HS 00
dsap			.HS 00
dseed			.HS 0000
topdest			.HS 00
dtmpx			.HS 00
loklst			.EQ	*					look list of recognized device numbers
dealbufl 		.HS 0000000000000000
dealbufh 		.HS 0000000000000000
cbytes			.HS 0000
				.HS 00					cbytes+2 must = 0
bufaddrl		.HS 00
bufaddrh 		.HS 00
delflag			.HS 00			  		used by 'detree' to know if called from delete (destroy).
*--------------------------------------
* variables used by SP remap & XRW Disk ][ to store last track used
*--------------------------------------
XRW.D2Trk		.EQ *
XDOS.SPUnit		.HS 00000000000000		14+1 for S0D2
				.HS	00
				.HS 00000000000000

XRW.D2VolNum	.EQ *
XDOS.SPVectLo	.HS 00000000000000  	storage for low byte of smartport entry.
				.HS 00
				.HS 00000000000000

XRW.D2SeekTime	.EQ *
XDOS.SPVectHi	.HS 00000000000000  	storage for high byte of smartport entry.
				.HS 00
				.HS 00000000000000

XDOS.SPStatus	.HS 00000000

				.LIST ON
XDOS.DATA.LEN	.EQ *-XDOS.DATA
				.LIST OFF
				.ED
*--------------------------------------
* zero fill to page boundary - 3 ($FEFD). so that cortland flag stays within page boundary.
				.LIST ON
XDOS.FREE	.EQ $FEFD-*-XDOS.DATA.LEN	(2.0.3 = $0C)
				.LIST OFF
cortdisp		.EQ $FEFD
cortflag 		.EQ $FEFF			  		cortland flag. 1 = Cortland system (must stay within page boundary)
*--------------------------------------
XDOS.LEN		.EQ *-XDOS
MAN
SAVE usr/src/prodos.fx/prodos.s.xdos.f
LOAD usr/src/prodos.fx/prodos.s
ASM
