40COL
%c%RAPL

* Running Average Power Limit

* Part of an infrastructure to allow
  setting custom  per-package hardware
  enforced power limits

* User Accessible Energy/Power 
  readings are a bonus feature
  of the interface
