Passport by 4am               2021-04-28
                                        
 ______________________________________ 
                                        
                                        
                                        
Reading from S6,D1                      
T00,S00 Found DOS 3.3 bootloader        
Using disk's own RWTS                   
Writing to S6,D2                        
T00,S09 Switching to built-in RWTS      
T00,S02 RWTS requires timing bits after 
the data prologue by jumping to $B660   
T00,S02,$F6: 4C60B6 -> BD8CC0           
T00,S0B,$08: 4C20B74C0EA9 -> BD8CC020B8B
8                                       
Crack complete. Press any key `         
                                        
                                        
                                        
                                        
                                        
                                        
                                        
