# @(#)gettytab	3.1	(ULTRIX)	4/20/90
#	Based on 4.2bsd labelled: 4.7 (Berkeley) 85/02/05
#
# $Id: gtab,v 1.1 1998/04/22 05:29:03 gdr-ftp Exp $
#
# Most of the table entries here are just copies of the
# old getty table, it is by no means certain, or even likely,
# then any of them are optimal for any purpose whatever.
# Nor is it likely that more than a couple are even correct
#

#
# The default gettytab entry, used to set defaults for all other
# entries, and in cases where getty is called with no table name
#
default:\
	:ap:fd#1000:\
	:im=\r\n\r\n\
GNO v2.0.6 \
(%h - %t)\r\n\r\r\n\r:\
	:sp#9600:er=\0177:

#
# Fixed speed entries
#
#	The "std.NNN" names are known to the special case
#	portselector code in getty, however they can
#	be assigned to any table desired.
#	The "NNN-baud" names are known to the special case
#	autobaud code in getty, and likewise can
#	be assigned to any table desired (hopefully the same speed).
#
a|std.110|110-baud:\
	:nd#1:cd#1:uc:sp#110:
b|std.134|134.5-baud:\
	:ep:nd#1:cd#2:ff#1:td#1:sp#134:ht:nl:
1|std.150|150-baud:\
	:ep:nd#1:cd#2:td#1:fd#1:sp#150:ht:nl:lm=\E\72\6\6\17login\72 :
c|std.300|300-baud:\
	:nd#1:cd#1:sp#300:pd:
d|std.600|600-baud:\
	:nd#1:cd#1:sp#600:pd:
f|std.1200|1200-baud:\
	:fd#1:sp#1200:pd:
6|std.2400|2400-baud:\
	:sp#2400:ht:pd:
7|std.4800|4800-baud:\
	:sp#4800:ht:pd:
2|std.9600|9600-baud:\
	:sp#9600:pd:
H|std.19200|19200-baud:\
	:sp#19200:pd:
#
# Setup terminal with full 8-bit support.
#
8bit.300|300-baud-8bit:\
	:nd#1:cd#1:sp#300:p8:
8bit.600|600-baud-8bit:\
	:nd#1:cd#1:sp#600:p8:
8bit.1200|1200-baud-8bit:\
	:fd#1:sp#1200:p8:
8bit.2400|2400-baud-8bit:\
	:sp#2400:p8:
8bit.4800|4800-baud-8bit:\
	:sp#4800:p8:
P|8bit.9600|9600-baud-8bit|8bit:\
	:sp#9600:p8:tt=vt100:
8bit.19200|19200-baud-8bit:\
	:sp#19200:p8:tt=vt100:

#
# Dial in rotary tables, speed selection via 'break'
#
0|d300|Dial-300:\
	:nx=d1200:cd#2:sp#300:
d1200|Dial-1200:\
	:nx=d150:fd#1:sp#1200:
d150|Dial-150:\
	:nx=d110:lm@:tc=150-baud:
d110|Dial-110:\
	:nx=d300:tc=300-baud:

#
# Odd special case terminals
#
-|tty33|asr33|Pity the poor user of this beast:\
	:tc=110-baud:

4|Console|Console Decwriter II:\
	:nd@:cd@:rw:tc=300-baud:

e|Console-1200|Console Decwriter III:\
	:fd@:nd@:cd@:rw:tc=1200-baud:

i|Interdata console:\
	:uc:sp#0:

l|lsi chess terminal:\
	:sp#300:

v|xterm|Xwindow|Vs100|X window system:\
	:fd@:nd@:cd@:rw:sp#9600:pd:

#
# Fast dialup terminals, 1200/300 rotary (can start either way)
#
3|D1200|Fast-Dial-1200:\
	:nx=D300:tc=std.1200:
5|D300|Fast-Dial-300:\
	:nx=D1200:tc=std.300:
#
# Faster dialup terminals, 2400/1200 rotary (can start either way)
#
g|H1200|High-Dial-1200:\
	:nx=H2400:tc=std.1200:
h|H2400|High-Dial-2400:\
	:nx=H1200:tc=std.2400:
#
# Faster dialup terminals, 2400/1200/300 rotary (can start any way)
#
m|S300|Triple-Dial-300:\
	:nx=S1200:tc=std.300:
n|S1200|Triple-Dial-1200:\
	:nx=S2400:tc=std.1200:
o|S2400|Triple-Dial-2400:\
	:nx=S300:tc=std.2400:

#
# Wierdo special case for fast crt's with hardcopy devices
#
8|T9600|CRT with hardcopy:\
	:nx=T300:tc=std.9600:
9|T300|CRT with hardcopy (300):\
	:nx=T9600:tc=std.300:

#
# Plugboard, and misc other terminals
#
p|P9600|Plugboard-9600:\
	:nx=P300:tc=std.9600:
q|P300|Plugboard-300:\
	:nx=P1200:tc=std.300:
r|P1200|Plugboard-1200:\
	:nx=P9600:tc=std.1200:

#
# XXXX Port selector
#
s|Port Selector:\
	:ps:sp#1200:

#
# Auto-baud speed detect entry for Micom 600.
# Special code in getty will switch this out
# to one of the NNN-baud entries.
#
A|Auto-baud:\
	:ab:sp#2400:f0#040:
