(module QSOP-20_3.9x8.7mm_P0.635mm_Renesas (layer F.Cu) (tedit 5A02F25C)
  (descr "20-Lead Plastic Shrink Small Outline Narrow Body (http://www.analog.com/media/en/technical-documentation/data-sheets/ADuM7640_7641_7642_7643.pdf)")
  (tags "QSOP 0.635")
  (attr smd)
  (fp_text reference U9 (at -3 -5.1) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value 74FCT245ATQG (at 0 5.3) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.075 3.3) (end -2.075 4.475) (layer F.SilkS) (width 0.12))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 0.8 0.8) (thickness 0.08)))
  )
  (fp_line (start -0.95 -4.35) (end 1.95 -4.35) (layer F.Fab) (width 0.1))
  (fp_line (start 1.95 -4.35) (end 1.95 4.35) (layer F.Fab) (width 0.1))
  (fp_line (start 1.95 4.35) (end -1.95 4.35) (layer F.Fab) (width 0.1))
  (fp_line (start -1.95 4.35) (end -1.95 -3.35) (layer F.Fab) (width 0.1))
  (fp_line (start -1.95 -3.35) (end -0.95 -4.35) (layer F.Fab) (width 0.1))
  (fp_line (start -3.71 -4.6) (end -3.71 4.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.7 -4.6) (end 3.7 4.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.71 -4.6) (end 3.7 -4.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.71 4.6) (end 3.7 4.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.075 4.475) (end 2.075 4.475) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.075 -4.475) (end 2.075 -4.475) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.5 -3.3) (end -2.075 -3.3) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.075 3.3) (end 2.075 4.475) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.075 -3.3) (end -2.075 -4.475) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.075 -3.3) (end 2.075 -4.475) (layer F.SilkS) (width 0.12))
  (pad 14 smd rect (at 2.6943 0.9525) (size 1.68 0.41) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at 2.6943 0.3175) (size 1.68 0.41) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -2.6943 0.9525) (size 1.68 0.41) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -2.6943 0.3175) (size 1.68 0.41) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at 2.6943 -0.9525) (size 1.68 0.41) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at 2.6943 -0.3175) (size 1.68 0.41) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -2.6943 -0.3175) (size 1.68 0.41) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -2.6943 -0.9525) (size 1.68 0.41) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -2.6943 -2.8575) (size 1.68 0.41) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -2.6943 -2.2225) (size 1.68 0.41) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -2.6943 -1.5875) (size 1.68 0.41) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -2.6943 1.5875) (size 1.68 0.41) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -2.6943 2.2225) (size 1.68 0.41) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -2.6943 2.8575) (size 1.68 0.41) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 2.6943 2.8575) (size 1.68 0.41) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at 2.6943 2.2225) (size 1.68 0.41) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at 2.6943 1.5875) (size 1.68 0.41) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at 2.6943 -1.5875) (size 1.68 0.41) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at 2.6943 -2.2225) (size 1.68 0.41) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at 2.6943 -2.8575) (size 1.68 0.41) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Package_SO.3dshapes/QSOP-20_3.9x8.7mm_P0.635mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
