(module RJ45_UDE_RB1-125B8G1A (layer F.Cu) (tedit 5F6F3CF6)
  (descr "1 Port RJ45 Connector Through Hole 10/100/1000 Base-T, https://datasheet.lcsc.com/szlcsc/1901091107_UDE-Corp-RB1-125B8G1A_C363353.pdf#page=3")
  (tags "RJ45 ethernet")
  (fp_text reference REF** (at 6 -3.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value RJ45_UDE_RB1-125B8G1A (at 5.5 21) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -0.6 -2) (end -2.16 -2) (layer F.Fab) (width 0.1))
  (fp_line (start 0 -1.4) (end 0.6 -2) (layer F.Fab) (width 0.1))
  (fp_line (start 0 -1.4) (end -0.6 -2) (layer F.Fab) (width 0.1))
  (fp_line (start 10.83 9.09) (end 12.03 9.09) (layer Dwgs.User) (width 0.12))
  (fp_line (start 12.03 9.09) (end 12.03 3.69) (layer Dwgs.User) (width 0.12))
  (fp_line (start 12.03 3.69) (end 10.83 3.69) (layer Dwgs.User) (width 0.12))
  (fp_line (start 10.83 3.69) (end 10.83 9.09) (layer Dwgs.User) (width 0.12))
  (fp_line (start 10.83 9.09) (end 12.03 7.89) (layer Dwgs.User) (width 0.12))
  (fp_line (start 10.83 8.09) (end 12.03 6.89) (layer Dwgs.User) (width 0.12))
  (fp_line (start 10.83 7.09) (end 12.03 5.89) (layer Dwgs.User) (width 0.12))
  (fp_line (start 10.83 6.09) (end 12.03 4.89) (layer Dwgs.User) (width 0.12))
  (fp_line (start 10.83 5.09) (end 12.03 3.89) (layer Dwgs.User) (width 0.12))
  (fp_line (start 10.83 4.09) (end 11.23 3.69) (layer Dwgs.User) (width 0.12))
  (fp_line (start -0.6 6.09) (end 0.6 4.89) (layer Dwgs.User) (width 0.12))
  (fp_line (start -0.6 9.09) (end 0.6 9.09) (layer Dwgs.User) (width 0.12))
  (fp_line (start 0.6 9.09) (end 0.6 3.69) (layer Dwgs.User) (width 0.12))
  (fp_line (start -0.6 9.09) (end 0.6 7.89) (layer Dwgs.User) (width 0.12))
  (fp_line (start -0.6 8.09) (end 0.6 6.89) (layer Dwgs.User) (width 0.12))
  (fp_line (start -0.6 3.69) (end -0.6 9.09) (layer Dwgs.User) (width 0.12))
  (fp_line (start -0.6 5.09) (end 0.6 3.89) (layer Dwgs.User) (width 0.12))
  (fp_line (start -0.6 7.09) (end 0.6 5.89) (layer Dwgs.User) (width 0.12))
  (fp_line (start -0.6 4.09) (end -0.2 3.69) (layer Dwgs.User) (width 0.12))
  (fp_line (start 0.6 3.69) (end -0.6 3.69) (layer Dwgs.User) (width 0.12))
  (fp_line (start 13.59 -2) (end 13.59 19.78) (layer F.Fab) (width 0.1))
  (fp_line (start 0.6 -2) (end 13.59 -2) (layer F.Fab) (width 0.1))
  (fp_line (start 13.59 19.78) (end -2.16 19.78) (layer F.Fab) (width 0.1))
  (fp_line (start -2.66 4.09) (end -2.66 -2.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 14.09 20.28) (end -2.66 20.28) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.66 -2.5) (end 14.09 -2.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 14.09 -2.5) (end 14.09 4.09) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.36 19.98) (end -2.36 7.58) (layer F.SilkS) (width 0.12))
  (fp_line (start 13.79 4.08) (end 13.79 -2.2) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.36 -2.2) (end 13.79 -2.2) (layer F.SilkS) (width 0.12))
  (fp_line (start 13.79 19.98) (end 13.79 7.58) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.36 4.08) (end -2.36 -2.2) (layer F.SilkS) (width 0.12))
  (fp_line (start 13.79 19.98) (end -2.36 19.98) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.16 19.78) (end -2.16 15.78) (layer Dwgs.User) (width 0.12))
  (fp_line (start -2.16 15.78) (end 4.21 15.78) (layer Dwgs.User) (width 0.12))
  (fp_line (start 4.21 15.78) (end 4.21 14.28) (layer Dwgs.User) (width 0.12))
  (fp_line (start 4.21 14.28) (end 7.22 14.28) (layer Dwgs.User) (width 0.12))
  (fp_line (start 7.22 14.28) (end 7.22 15.78) (layer Dwgs.User) (width 0.12))
  (fp_line (start 7.22 15.78) (end 13.59 15.78) (layer Dwgs.User) (width 0.12))
  (fp_line (start 13.59 15.78) (end 13.59 19.78) (layer Dwgs.User) (width 0.12))
  (fp_line (start 13.59 19.78) (end -2.16 19.78) (layer Dwgs.User) (width 0.12))
  (fp_line (start -2.16 19.78) (end 1.84 15.78) (layer Dwgs.User) (width 0.12))
  (fp_line (start -2.16 18.78) (end 0.84 15.78) (layer Dwgs.User) (width 0.12))
  (fp_line (start -2.16 17.78) (end -0.16 15.78) (layer Dwgs.User) (width 0.12))
  (fp_line (start -2.16 16.78) (end -1.16 15.78) (layer Dwgs.User) (width 0.12))
  (fp_line (start -1.16 19.78) (end 2.84 15.78) (layer Dwgs.User) (width 0.12))
  (fp_line (start -0.16 19.78) (end 3.84 15.78) (layer Dwgs.User) (width 0.12))
  (fp_line (start 3.84 19.78) (end 7.84 15.78) (layer Dwgs.User) (width 0.12))
  (fp_line (start 4.84 19.78) (end 8.84 15.78) (layer Dwgs.User) (width 0.12))
  (fp_line (start 5.84 19.78) (end 9.84 15.78) (layer Dwgs.User) (width 0.12))
  (fp_line (start 6.84 19.78) (end 10.84 15.78) (layer Dwgs.User) (width 0.12))
  (fp_line (start 7.84 19.78) (end 11.84 15.78) (layer Dwgs.User) (width 0.12))
  (fp_line (start 8.84 19.78) (end 12.84 15.78) (layer Dwgs.User) (width 0.12))
  (fp_line (start 1.84 19.78) (end 7.22 14.4) (layer Dwgs.User) (width 0.12))
  (fp_line (start 0.84 19.77) (end 6.33 14.28) (layer Dwgs.User) (width 0.12))
  (fp_line (start 2.84 19.77) (end 7.22 15.39) (layer Dwgs.User) (width 0.12))
  (fp_line (start 9.84 19.78) (end 13.59 16.03) (layer Dwgs.User) (width 0.12))
  (fp_line (start 10.84 19.77) (end 13.59 17.02) (layer Dwgs.User) (width 0.12))
  (fp_line (start 11.84 19.77) (end 13.59 18.02) (layer Dwgs.User) (width 0.12))
  (fp_line (start 12.84 19.77) (end 13.59 19.02) (layer Dwgs.User) (width 0.12))
  (fp_line (start 4.21 15.41) (end 5.34 14.29) (layer Dwgs.User) (width 0.12))
  (fp_text user %R (at 6 6) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.66 4.09) (end -3.81 4.09) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.81 4.09) (end -3.81 7.59) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.81 7.59) (end -2.66 7.59) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.16 19.78) (end -2.16 -2) (layer F.Fab) (width 0.1))
  (fp_line (start -2.66 7.59) (end -2.66 20.28) (layer F.CrtYd) (width 0.05))
  (fp_line (start 14.09 4.09) (end 15.24 4.09) (layer F.CrtYd) (width 0.05))
  (fp_line (start 15.24 4.09) (end 15.24 7.59) (layer F.CrtYd) (width 0.05))
  (fp_line (start 15.24 7.59) (end 14.09 7.59) (layer F.CrtYd) (width 0.05))
  (fp_line (start 14.09 7.59) (end 14.09 20.28) (layer F.CrtYd) (width 0.05))
  (pad R1 thru_hole rect (at 0 0) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask))
  (pad R2 thru_hole circle (at 1.27 2.54) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask))
  (pad R3 thru_hole circle (at 2.54 0) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask))
  (pad R4 thru_hole circle (at 3.81 2.54) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask))
  (pad R5 thru_hole circle (at 5.08 0) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask))
  (pad R6 thru_hole circle (at 6.35 2.54) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask))
  (pad R7 thru_hole circle (at 7.62 0) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask))
  (pad R8 thru_hole circle (at 8.89 2.54) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask))
  (pad L1 thru_hole circle (at 12.04 12.27) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask))
  (pad L2 thru_hole circle (at 9.5 13.79) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask))
  (pad L3 thru_hole circle (at 1.93 12.27) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask))
  (pad L4 thru_hole circle (at -0.61 13.79) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask))
  (pad SH thru_hole circle (at -2.06 5.84) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask))
  (pad SH thru_hole circle (at 13.49 5.84) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 0 8.89) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 11.43 8.89) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
  (pad R9 thru_hole circle (at 10.16 0) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask))
  (pad R10 thru_hole circle (at 11.43 2.54) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_RJ.3dshapes/RJ45_UDE_RB1-125B8G1A.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
