(module HDMI_A_Amphenol_10029449-111 (layer F.Cu) (tedit 5E1BB628)
  (descr "HDMI, Type A, 10029449-111RLF, https://www.amphenol-icc.com/hdmi-10029449111rlf.html")
  (tags "HDMI type a connector")
  (attr smd)
  (fp_text reference REF** (at 0 -4.8) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value HDMI_A_Amphenol_10029449-111 (at 0 8.45) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -8.2 1.7) (end -8.2 -1.3) (layer F.SilkS) (width 0.12))
  (fp_line (start -8.2 -3.4) (end -5 -3.4) (layer F.SilkS) (width 0.12))
  (fp_line (start -8.2 4.2) (end -8.2 5.2) (layer F.SilkS) (width 0.12))
  (fp_line (start 8.2 5.2) (end 8.2 4.2) (layer F.SilkS) (width 0.12))
  (fp_line (start 8.2 -3.4) (end 8.2 -2.8) (layer F.SilkS) (width 0.12))
  (fp_line (start 8.2 -3.4) (end 5.5 -3.4) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.5 -3.4) (end 5.5 -4.05) (layer F.SilkS) (width 0.12))
  (fp_line (start 8.1 -3.3) (end 8.1 6.42) (layer F.Fab) (width 0.1))
  (fp_line (start 8.1 6.42) (end -8.1 6.42) (layer F.Fab) (width 0.1))
  (fp_line (start -8.1 6.42) (end -8.1 -3.3) (layer F.Fab) (width 0.1))
  (fp_line (start -8.1 -3.3) (end 8.1 -3.3) (layer F.Fab) (width 0.1))
  (fp_text user %R (at 0 1.45) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -9 -4.4) (end 9 -4.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9 -4.4) (end 9 6.92) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9 6.92) (end -9 6.92) (layer F.CrtYd) (width 0.05))
  (fp_line (start -9 6.92) (end -9 -4.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.75 -1.8) (end 4.5 -1.3) (layer F.Fab) (width 0.1))
  (fp_line (start 4.5 -1.3) (end 5 -1.3) (layer F.Fab) (width 0.1))
  (fp_line (start 5 -1.3) (end 4.75 -1.8) (layer F.Fab) (width 0.1))
  (fp_line (start -3 5.45) (end 3 5.45) (layer Dwgs.User) (width 0.1))
  (fp_text user "PCB Edge" (at 0 4.7) (layer Dwgs.User)
    (effects (font (size 0.5 0.5) (thickness 0.1)))
  )
  (fp_line (start -8.2 -3.4) (end -8.2 -2.8) (layer F.SilkS) (width 0.12))
  (fp_line (start 8.2 1.7) (end 8.2 -1.3) (layer F.SilkS) (width 0.12))
  (pad 1 smd rect (at 4.75 -2.95) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 4.25 -2.95) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 3.75 -2.95) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 3.25 -2.95) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 2.75 -2.95) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 2.25 -2.95) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 1.75 -2.95) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 1.25 -2.95) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 0.75 -2.95) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 0.25 -2.95) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -0.25 -2.95) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at -0.75 -2.95) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at -1.25 -2.95) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at -1.75 -2.95) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at -2.25 -2.95) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at -2.75 -2.95) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at -3.25 -2.95) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at -3.75 -2.95) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at -4.25 -2.95) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask))
  (pad SH thru_hole circle (at 7.25 -2.05) (size 2 2) (drill 1.3) (layers *.Cu *.Mask))
  (pad SH thru_hole circle (at -7.25 -2.05) (size 2 2) (drill 1.3) (layers *.Cu *.Mask))
  (pad SH thru_hole circle (at 7.85 2.9) (size 2 2) (drill 1.3) (layers *.Cu *.Mask))
  (pad SH thru_hole circle (at -7.85 2.9) (size 2 2) (drill 1.3) (layers *.Cu *.Mask))
  (model 10029449-111RLF.stp
    (offset (xyz 0 0.3 3.5))
    (scale (xyz 1 1 1))
    (rotate (xyz 180 0 0))
  )
)
