(module SolderJumper-3_P1.3mm_Bridged12_NoSilkscreen (layer F.Cu) (tedit 61B802DF)
  (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
  (tags "solder jumper open")
  (attr virtual)
  (fp_text reference JP1 (at 3.556 0) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SolderJumper_3_Bridged12 (at 0 1.9 -180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.3 -1.25) (end 2.3 -1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.3 -1.25) (end -2.3 1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.3 1.25) (end 2.3 -1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.3 1.25) (end -2.3 1.25) (layer F.CrtYd) (width 0.05))
  (fp_poly (pts (xy -0.9 -0.3) (xy -0.4 -0.3) (xy -0.4 0.3) (xy -0.9 0.3)) (layer F.Cu) (width 0))
  (pad 1 smd custom (at -1.3 0) (size 1 0.5) (layers F.Cu F.Mask)
    (zone_connect 2)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
      (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
      (gr_poly (pts
         (xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)) (width 0))
    ))
  (pad 2 smd rect (at 0 0) (size 1 1.5) (layers F.Cu F.Mask))
  (pad 3 smd custom (at 1.3 0) (size 1 0.5) (layers F.Cu F.Mask)
    (zone_connect 2)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
      (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
      (gr_poly (pts
         (xy -0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy -0.55 0.75)) (width 0))
    ))
)
