14759294537252
mousebites
0.9_and_1.3_in_OLED_Footprint
Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x04 2.54mm single row
0
8
5
mousebites
0.9_in_OLED_Footprint
Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x04 2.54mm single row
0
8
5
mousebites
1.3_in_OLED_Footprint
Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x04 2.54mm single row
0
8
5
mousebites
Breakaway_Mousebite


0
0
0
mousebites
PinSocket_1x04_P2.54mm_Vertical
Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x04 2.54mm single row
0
8
5
mousebites
SolderJumper-3_P1.3mm_Bridged12_NoSilkscreen
SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip
solder jumper open
0
3
3
mousebites
dogcow


0
0
0
mousebites
mac_happy_small


0
0
0
mousebites
pi_logo


0
0
0
