(module PinSocket_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 61B6B096)
  (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
  (tags "Through hole socket strip THT 1x04 2.54mm single row")
  (fp_text reference J2 (at 0 10.39) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "OLED Connector" (at 0 10.3265 -180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center 0 15.61) (end 1.5 15.61) (layer F.SilkS) (width 0.12))
  (fp_circle (center 23.2 15.61) (end 24.7 15.61) (layer F.SilkS) (width 0.12))
  (fp_circle (center 23.2 -7.94) (end 24.7 -7.94) (layer F.SilkS) (width 0.12))
  (fp_circle (center 0 -7.94) (end 1.5 -7.94) (layer F.SilkS) (width 0.12))
  (fp_line (start 24.7 17.56) (end -1.524 17.56) (layer F.SilkS) (width 0.12))
  (fp_line (start 25.2 -9.4615) (end 25.2 17.06) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.5 -9.94) (end 24.7015 -9.94) (layer F.SilkS) (width 0.12))
  (fp_line (start -2 -9.4615) (end -2 17.06) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.8 -1.78) (end 1.8 9.42) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.75 -1.78) (end 1.8 -1.78) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.75 9.42) (end -1.75 -1.78) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.8 9.42) (end -1.75 9.42) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0 8.95) (end -1.33 8.95) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.33 8.95) (end -1.33 7.62) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.33 6.35) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.33 -1.33) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.33 6.35) (end 1.33 -1.33) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.33 6.35) (end -1.33 6.35) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.27 -1.27) (end 1.27 8.89) (layer F.Fab) (width 0.1))
  (fp_line (start -1.27 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
  (fp_line (start -1.27 8.255) (end -1.27 -1.27) (layer F.Fab) (width 0.1))
  (fp_line (start -0.635 8.89) (end -1.27 8.255) (layer F.Fab) (width 0.1))
  (fp_line (start 1.27 8.89) (end -0.635 8.89) (layer F.Fab) (width 0.1))
  (fp_text user %R (at 0 3.81 -270) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user SDA (at 2.7305 0) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)))
  )
  (fp_text user SCL (at 2.711453 2.582333) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)))
  )
  (fp_text user VCC (at 2.749548 5.164666) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)))
  )
  (fp_text user GND (at 2.825738 7.747) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)))
  )
  (fp_arc (start 24.7 17.06) (end 24.7 17.56) (angle -90) (layer F.SilkS) (width 0.12))
  (fp_arc (start 24.7 -9.44) (end 25.2 -9.44) (angle -90) (layer F.SilkS) (width 0.12))
  (fp_arc (start -1.5 -9.44) (end -1.5 -9.94) (angle -90) (layer F.SilkS) (width 0.12))
  (fp_arc (start -1.5 17.06) (end -2 17.06) (angle -90) (layer F.SilkS) (width 0.12))
  (pad 4 thru_hole oval (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 0 -7.94) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 0 15.61) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 23.2 -7.94) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 23.2 15.61) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
