(module 1.3_in_OLED_Footprint (layer F.Cu) (tedit 61C34F4A)
  (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
  (tags "Through hole socket strip THT 1x04 2.54mm single row")
  (fp_text reference REF** (at 1.025 -6.425) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "OLED Connector" (at 0 6.4915 -180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.775 5.585) (end -1.775 -5.615) (layer B.CrtYd) (width 0.05))
  (fp_line (start 1.775 -5.59) (end 1.775 5.61) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.775 -5.615) (end 1.775 -5.615) (layer B.CrtYd) (width 0.05))
  (fp_line (start 1.775 5.61) (end -1.775 5.61) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 0.5 -15.2) (end 2.75 -15.2) (layer B.CrtYd) (width 0.12))
  (fp_circle (center 0.5 15.175) (end 2.75 15.175) (layer B.CrtYd) (width 0.12))
  (fp_circle (center 29 15.2) (end 31.25 15.2) (layer B.CrtYd) (width 0.12))
  (fp_circle (center 28.990284 -15.2) (end 30.925 -15.2) (layer B.CrtYd) (width 0.12))
  (fp_circle (center 0.5 15.2) (end 2.75 15.2) (layer F.CrtYd) (width 0.12))
  (fp_circle (center 29 15.2) (end 31.25 15.2) (layer F.CrtYd) (width 0.12))
  (fp_circle (center 29 -15.2) (end 30.934716 -15.2) (layer F.CrtYd) (width 0.12))
  (fp_circle (center 0.5 -15.2) (end 2.75 -15.2) (layer F.CrtYd) (width 0.12))
  (fp_line (start 1.27 5.08) (end -0.635 5.08) (layer F.Fab) (width 0.1))
  (fp_line (start -0.635 5.08) (end -1.27 4.445) (layer F.Fab) (width 0.1))
  (fp_line (start -1.27 4.445) (end -1.27 -5.08) (layer F.Fab) (width 0.1))
  (fp_line (start -1.27 -5.08) (end 1.27 -5.08) (layer F.Fab) (width 0.1))
  (fp_line (start 1.27 -5.08) (end 1.27 5.08) (layer F.Fab) (width 0.1))
  (fp_line (start 1.33 2.54) (end -1.33 2.54) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.33 2.54) (end 1.33 -5.14) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.33 -5.14) (end -1.33 -5.14) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.33 2.54) (end -1.33 -5.14) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.33 5.14) (end -1.33 3.81) (layer F.SilkS) (width 0.12))
  (fp_line (start 0 5.14) (end -1.33 5.14) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.8 5.61) (end -1.75 5.61) (layer B.CrtYd) (width 0.05))
  (fp_line (start -1.775 5.61) (end -1.775 -5.59) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.775 -5.59) (end 1.775 -5.59) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.8 -5.59) (end 1.8 5.61) (layer B.CrtYd) (width 0.05))
  (fp_line (start -2 17.2) (end -2 -17.2) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.5 -17.7) (end 31 -17.7) (layer F.SilkS) (width 0.12))
  (fp_line (start 31.5 17.2) (end 31.5 -17.2) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.5 17.7) (end 31 17.7) (layer F.SilkS) (width 0.12))
  (fp_circle (center 0.5 -15.2) (end 2 -15.2) (layer F.SilkS) (width 0.12))
  (fp_circle (center 29 -15.2) (end 30.5 -15.2) (layer F.SilkS) (width 0.12))
  (fp_circle (center 29 15.2) (end 30.5 15.2) (layer F.SilkS) (width 0.12))
  (fp_circle (center 0.5 15.2) (end 2 15.2) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.35 -14.71) (end 20.05 -14.71) (layer F.SilkS) (width 0.12))
  (fp_line (start 20.05 -14.71) (end 20.05 14.71) (layer F.SilkS) (width 0.12))
  (fp_line (start 20.05 14.71) (end 5.35 14.71) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.35 14.71) (end 5.35 -14.71) (layer F.SilkS) (width 0.12))
  (fp_line (start 4 -17) (end 27 -17) (layer F.SilkS) (width 0.12))
  (fp_line (start 27 -17) (end 27 17) (layer F.SilkS) (width 0.12))
  (fp_line (start 27 17) (end 4 17) (layer F.SilkS) (width 0.12))
  (fp_line (start 4 17) (end 4 -17) (layer F.SilkS) (width 0.12))
  (fp_arc (start -1.5 17.2) (end -2 17.2) (angle -90) (layer F.SilkS) (width 0.12))
  (fp_arc (start -1.5 -17.2) (end -1.5 -17.7) (angle -90) (layer F.SilkS) (width 0.12))
  (fp_arc (start 31 -17.2) (end 31.5 -17.2) (angle -90) (layer F.SilkS) (width 0.12))
  (fp_arc (start 31 17.2) (end 31 17.7) (angle -90) (layer F.SilkS) (width 0.12))
  (fp_text user GND (at 2.725738 3.987) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)))
  )
  (fp_text user VCC (at 2.649548 1.404666) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)))
  )
  (fp_text user SCL (at 2.611453 -1.177667) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)))
  )
  (fp_text user SDA (at 2.6305 -3.76) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)))
  )
  (fp_text user %R (at 0 0 -270) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 5 thru_hole circle (at 29 15.2) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 29 -15.2) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 0.5 15.2) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 0.5 -15.2) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 3.81 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 0 1.27 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 0 -1.27 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 0 -3.81 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl
    (offset (xyz 0 3.81 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
