(footprint "0.9_and_1.3_in_OLED_Footprint" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 61DE2661)
  (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
  (tags "Through hole socket strip THT 1x04 2.54mm single row")
  (attr through_hole)
  (fp_text reference "J2" (at 0 6.58) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4d770cf5-2570-44ce-82d7-01b22dd0dfa9)
  )
  (fp_text value "OLED Connector" (at 0 6.5165 -180) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 7ee5ae77-ad6f-4554-84d3-ed4b63e95639)
  )
  (fp_text user "GND" (at -1.9 4 90) (layer "B.SilkS")
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify mirror))
    (tstamp 13d8bfa6-d7d2-43b6-8fd6-aa77f4d342d5)
  )
  (fp_text user "VCC" (at -1.7 1.5 90) (layer "B.SilkS")
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify mirror))
    (tstamp 2bd88b42-a583-4824-8baf-4ecac716152a)
  )
  (fp_text user "SCL" (at -1.8 -1 90) (layer "B.SilkS")
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify mirror))
    (tstamp 2d14feb1-4575-47c1-9b52-3c7fb892f819)
  )
  (fp_text user "SDA" (at -1.8 -3.7 90) (layer "B.SilkS")
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify mirror))
    (tstamp c9c437a5-3127-4e17-93f1-fcd6223b2daf)
  )
  (fp_text user "SCL" (at -1.8 -1.1 90) (layer "F.SilkS")
    (effects (font (size 0.8 0.8) (thickness 0.1)))
    (tstamp 5a4b792d-7daf-49f9-a003-f77559fa2efd)
  )
  (fp_text user "SDA" (at -1.8 -3.7 90) (layer "F.SilkS")
    (effects (font (size 0.8 0.8) (thickness 0.1)))
    (tstamp 86ab502a-b4f3-439d-b0ba-23f8fc09431b)
  )
  (fp_text user "GND" (at -1.9 4 90) (layer "F.SilkS")
    (effects (font (size 0.8 0.8) (thickness 0.1)))
    (tstamp cc55bf8f-d3a8-4da6-a5f8-64c109c81511)
  )
  (fp_text user "VCC" (at -1.8 1.5 90) (layer "F.SilkS")
    (effects (font (size 0.8 0.8) (thickness 0.1)))
    (tstamp da5e2eb9-cffc-4a6d-876e-eb7dcbbad407)
  )
  (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp abaed4f7-8b9b-42fb-b7e6-2364a8a9edf3)
  )
  (fp_line (start -1.33 2.54) (end -1.33 -5.14) (layer "F.SilkS") (width 0.12) (tstamp 0c3f101c-5d7c-4f8f-abf0-4066322fab6b))
  (fp_line (start 1.33 2.54) (end -1.33 2.54) (layer "F.SilkS") (width 0.12) (tstamp 21329ce4-f53b-4757-a186-68e3ce22792c))
  (fp_line (start 1.33 -5.14) (end -1.33 -5.14) (layer "F.SilkS") (width 0.12) (tstamp 5ac9e4bc-322c-4ce1-942d-8bdf6f2db28f))
  (fp_line (start 0 5.14) (end -1.33 5.14) (layer "F.SilkS") (width 0.12) (tstamp c17611e7-b006-48aa-88a5-0a087d80bf70))
  (fp_line (start -1.33 5.14) (end -1.33 3.81) (layer "F.SilkS") (width 0.12) (tstamp d2463a16-5ee1-4ea5-b724-3f5c6b12b298))
  (fp_line (start 1.33 2.54) (end 1.33 -5.14) (layer "F.SilkS") (width 0.12) (tstamp f621dca6-2e8a-4ab7-8a4b-480d0a1e895d))
  (fp_rect (start -2 -13.75) (end 25.2 13.85) (layer "Dwgs.User") (width 0.12) (fill none) (tstamp 25891a7d-5ca8-485e-8d76-29a8b6e1dae0))
  (fp_rect (start -3 -17.6) (end 31.4 17.5) (layer "Dwgs.User") (width 0.12) (fill none) (tstamp 72e32a2d-6d54-4c08-8135-8a9c14a6b016))
  (fp_line (start -1.75 5.61) (end -1.75 -5.59) (layer "F.CrtYd") (width 0.05) (tstamp 05e7bc89-2182-401c-803d-ae34796e9841))
  (fp_line (start 1.8 -5.59) (end 1.8 5.61) (layer "F.CrtYd") (width 0.05) (tstamp b428b46e-6bb2-4218-88bb-f65b402ba084))
  (fp_line (start 1.8 5.61) (end -1.75 5.61) (layer "F.CrtYd") (width 0.05) (tstamp d3197f7f-9a98-4fbd-957b-d629a634d50a))
  (fp_line (start -1.75 -5.59) (end 1.8 -5.59) (layer "F.CrtYd") (width 0.05) (tstamp ff965ae9-0de4-48fa-a1a6-d1580e191547))
  (fp_line (start 1.27 -5.08) (end 1.27 5.08) (layer "F.Fab") (width 0.1) (tstamp afd0b185-caaf-4f93-99db-f0b618dfdb0d))
  (fp_line (start -1.27 4.445) (end -1.27 -5.08) (layer "F.Fab") (width 0.1) (tstamp c9fd13d8-34fc-4eff-b8ce-cde6d5a9c87a))
  (fp_line (start -1.27 -5.08) (end 1.27 -5.08) (layer "F.Fab") (width 0.1) (tstamp f2571a4c-3e67-4916-9c0e-b0974b924c84))
  (fp_line (start -0.635 5.08) (end -1.27 4.445) (layer "F.Fab") (width 0.1) (tstamp f9bb99c7-ccda-4b6c-a116-fa3715af7191))
  (fp_line (start 1.27 5.08) (end -0.635 5.08) (layer "F.Fab") (width 0.1) (tstamp faad28a2-09fa-4ce9-a367-71b6860b94ed))
  (pad "1" thru_hole rect (at 0 3.81 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 91aeb66b-3414-4567-889a-6c6508c65350))
  (pad "2" thru_hole oval (at 0 1.27 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 05fa7b1a-8ed3-4b32-82c0-6b7ad7df3417))
  (pad "3" thru_hole oval (at 0 -1.27 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 7807b0c6-5091-4f3d-9363-0b79274786b0))
  (pad "4" thru_hole oval (at 0 -3.81 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 086cae51-9891-41f4-b716-2063551784ef))
  (pad "5" thru_hole oval (at 24 -11) (size 2.5 6.5) (drill oval 2 6) (layers *.Cu *.Mask) (tstamp 047e0d1e-484a-4d10-b086-6b188a78c581))
  (pad "5" thru_hole oval (at 0.5 -12.5) (size 2.5 8.5) (drill oval 2 8) (layers *.Cu *.Mask) (tstamp 1cd3d1b4-e18e-4851-9980-bde55fb0c52d))
  (pad "5" thru_hole oval (at 0.5 12.5) (size 2.5 8.5) (drill oval 2 8) (layers *.Cu *.Mask) (tstamp 2a884ec1-8b99-4278-96d4-ba229cbf2441))
  (pad "5" thru_hole oval (at 24 11) (size 2.5 6.5) (drill oval 2 6) (layers *.Cu *.Mask) (tstamp d646c145-0888-4122-a9ee-c80c4050d447))
  (model "${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl"
    (offset (xyz 0 3.81 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
