# Timing report for WarpSE
Author: Copyright (c) 1995-2013 Xilinx, Inc. All rights reserved.

# Timing Report

Need help reading this report?

Design Name | WarpSE
Device, Speed (SpeedFile Version) | XC95144XL, -10 (3.0)
Date Created | Sat Apr 08 05:49:36 2023
Created By | Timing Report Generator: version P.20131013
Copyright | Copyright (c) 1995-2013 Xilinx, Inc. All rights reserved.

## Summary

Notes and Warnings
Note: This design contains no timing constraints.
Note: A default set of constraints using a delay of 0.000ns will be used for analysis.

Performance Summary
Min. Clock Period | 12.200 ns.
Max. Clock Frequency (fSYSTEM) | 81.967 MHz.
Limited by Cycle Time for FCLK
Clock to Setup (tCYC) | 12.200 ns.
Pad to Pad Delay (tPD) | 11.000 ns.
Setup to Clock at the Pad (tSU) | 8.700 ns.
Clock Pad to Output Pad Delay (tCO) | 14.500 ns.

## Timing Constraints

Constraint Name | Requirement (ns) | Delay (ns) | Paths | Paths Failing
--- | --- | --- | --- | ---
TS1000 | 0.0 | 0.0 | 0 | 0
TS1001 | 0.0 | 0.0 | 0 | 0
TS1002 | 0.0 | 0.0 | 0 | 0
AUTO_TS_F2F | 0.0 | 12.2 | 551 | 551
AUTO_TS_P2P | 0.0 | 14.5 | 84 | 84
AUTO_TS_P2F | 0.0 | 10.5 | 247 | 247
AUTO_TS_F2P | 0.0 | 12.7 | 43 | 43

### Constraint: TS1000

Description: PERIOD:PERIOD_FCLK:0.000 nS
Path | Requirement (ns) | Delay (ns) | Slack (ns)
--- | --- | --- | ---

### Constraint: TS1001

Description: PERIOD:PERIOD_C16M:0.000 nS
Path | Requirement (ns) | Delay (ns) | Slack (ns)
--- | --- | --- | ---

### Constraint: TS1002

Description: PERIOD:PERIOD_C8M:0.000 nS
Path | Requirement (ns) | Delay (ns) | Slack (ns)
--- | --- | --- | ---

### Constraint: AUTO_TS_F2F

Description: MAXDELAY:FROM:FFS(*):TO:FFS(*):0.000 nS
Path | Requirement (ns) | Delay (ns) | Slack (ns)
--- | --- | --- | ---
iobs/TS_FSM_FFd2.Q to IOWRREQ.D | 0.000 | 12.200 | -12.200
nADoutLE1.Q to IOWRREQ.D | 0.000 | 12.200 | -12.200
cnt/IS_FSM_FFd1.Q to cnt/LTimer<0>.D | 0.000 | 11.400 | -11.400

### Constraint: AUTO_TS_P2P

Description: MAXDELAY:FROM:PADS(*):TO:PADS(*):0.000 nS
Path | Requirement (ns) | Delay (ns) | Slack (ns)
--- | --- | --- | ---
FCLK to RA<11> | 0.000 | 14.500 | -14.500
FCLK to RA<4> | 0.000 | 14.500 | -14.500
FCLK to RA<5> | 0.000 | 14.500 | -14.500

### Constraint: AUTO_TS_P2F

Description: MAXDELAY:FROM:PADS(*):TO:FFS(*):0.000 nS
Path | Requirement (ns) | Delay (ns) | Slack (ns)
--- | --- | --- | ---
A_FSB<10> to IOWRREQ.D | 0.000 | 10.500 | -10.500
A_FSB<11> to IOWRREQ.D | 0.000 | 10.500 | -10.500
A_FSB<12> to IOWRREQ.D | 0.000 | 10.500 | -10.500

### Constraint: AUTO_TS_F2P

Description: MAXDELAY:FROM:FFS(*):TO:PADS(*):0.000 nS
Path | Requirement (ns) | Delay (ns) | Slack (ns)
--- | --- | --- | ---
cs/nOverlay.Q to nRAS | 0.000 | 12.700 | -12.700
nAoutOE.Q to nAS_IOB | 0.000 | 12.700 | -12.700
nAoutOE.Q to nLDS_IOB | 0.000 | 12.700 | -12.700

Number of constraints not met: 4

## Data Sheet Report

### Maximum External Clock Speeds

Clock | fEXT (MHz) | Reason
--- | --- | ---
FCLK | 81.967 | Limited by Cycle Time for FCLK
C16M | 90.909 | Limited by Cycle Time for C16M
C8M | 100.000 | Limited by Cycle Time for C8M

### Setup/Hold Times for Clocks

Setup/Hold Times for Clock FCLK
Source Pad | Setup to clk (edge) | Hold to clk (edge)
--- | --- | ---
A_FSB<10> | 8.700 | 0.000
A_FSB<11> | 8.700 | 0.000
A_FSB<12> | 8.700 | 0.000
A_FSB<13> | 8.700 | 0.000
A_FSB<14> | 8.700 | 0.000
A_FSB<15> | 8.700 | 0.000
A_FSB<16> | 7.500 | 0.000
A_FSB<17> | 7.900 | 0.000
A_FSB<18> | 7.900 | 0.000
A_FSB<19> | 7.900 | 0.000
A_FSB<20> | 7.900 | 0.000
A_FSB<21> | 7.900 | 0.000
A_FSB<22> | 8.700 | 0.000
A_FSB<23> | 8.700 | 0.000
A_FSB<8> | 8.700 | 0.000
A_FSB<9> | 8.700 | 0.000
E | 6.500 | 0.000
nAS_FSB | 7.900 | 0.000
nIPL2 | 6.500 | 0.000
nLDS_FSB | 6.500 | 0.000
nRES | 6.500 | 0.000
nUDS_FSB | 6.500 | 0.000
nWE_FSB | 7.500 | 0.000

Setup/Hold Times for Clock C16M
Source Pad | Setup to clk (edge) | Hold to clk (edge)
--- | --- | ---
C8M | 6.500 | 0.000

Setup/Hold Times for Clock C8M
Source Pad | Setup to clk (edge) | Hold to clk (edge)
--- | --- | ---
E | 6.500 | 0.000
nBERR_IOB | 6.500 | 0.000
nDTACK_IOB | 6.500 | 0.000
nRES | 6.500 | 0.000
nVPA_IOB | 6.500 | 0.000

### Clock to Pad Timing

Clock FCLK to Pad
Destination Pad | Clock (edge) to Pad
--- | ---
RA<11> | 14.500
RA<4> | 14.500
RA<5> | 14.500
nAS_IOB | 14.500
nLDS_IOB | 14.500
nRAS | 14.500
nRES | 14.500
nUDS_IOB | 14.500
nVMA_IOB | 14.500
RA<0> | 13.500
RA<10> | 13.500
RA<1> | 13.500
RA<2> | 13.500
RA<3> | 13.500
RA<6> | 13.500
RA<7> | 13.500
RA<8> | 13.500
RA<9> | 13.500
nADoutLE0 | 13.500
nDoutOE | 13.500
nRAMLWE | 13.500
nRAMUWE | 13.500
nROMCS | 13.500
nADoutLE1 | 5.800
nAoutOE | 5.800
nBERR_FSB | 5.800
nBR_IOB | 5.800
nCAS | 5.800
nDTACK_FSB | 5.800
nVPA_FSB | 5.800

Clock C16M to Pad
Destination Pad | Clock (edge) to Pad
--- | ---
nADoutLE0 | 13.500
nDoutOE | 13.500
nAS_IOB | 5.800
nDinLE | 5.800
nLDS_IOB | 5.800
nUDS_IOB | 5.800

Clock C8M to Pad
Destination Pad | Clock (edge) to Pad
--- | ---
nVMA_IOB | 5.800

### Clock to Setup Times for Clocks

Clock to Setup for clock FCLK
Source | Destination | Delay
--- | --- | ---
iobs/TS_FSM_FFd2.Q | IOWRREQ.D | 12.200
nADoutLE1.Q | IOWRREQ.D | 12.200
cnt/IS_FSM_FFd1.Q | cnt/LTimer<0>.D | 11.400
cnt/IS_FSM_FFd2.Q | cnt/LTimer<0>.D | 11.400
cnt/LTimer<0>.Q | cnt/LTimer<0>.D | 11.400
cnt/LTimer<10>.Q | cnt/LTimer<0>.D | 11.400
cnt/LTimer<11>.Q | cnt/LTimer<0>.D | 11.400
cnt/LTimer<12>.Q | cnt/LTimer<0>.D | 11.400
cnt/LTimer<1>.Q | cnt/LTimer<0>.D | 11.400
cnt/LTimer<2>.Q | cnt/LTimer<0>.D | 11.400
cnt/LTimer<3>.Q | cnt/LTimer<0>.D | 11.400
cnt/LTimer<4>.Q | cnt/LTimer<0>.D | 11.400
cnt/LTimer<5>.Q | cnt/LTimer<0>.D | 11.400
cnt/LTimer<6>.Q | cnt/LTimer<0>.D | 11.400
cnt/LTimer<7>.Q | cnt/LTimer<0>.D | 11.400
cnt/LTimer<8>.Q | cnt/LTimer<0>.D | 11.400
cnt/LTimer<9>.Q | cnt/LTimer<0>.D | 11.400
cs/nOverlay.Q | IOWRREQ.D | 11.400
fsb/ASrf.Q | cnt/LTimer<0>.D | 11.400
iobs/IORW1.Q | iobs/IORW1.D | 11.400
iobs/Sent.Q | iobs/Sent.D | 11.400
iobs/TS_FSM_FFd2.Q | IOL0.D | 11.400
iobs/TS_FSM_FFd2.Q | IOU0.D | 11.400
iobs/TS_FSM_FFd2.Q | iobs/TS_FSM_FFd2.D | 11.400
nADoutLE1.Q | IOL0.D | 11.400
nADoutLE1.Q | IOU0.D | 11.400
nADoutLE1.Q | iobs/TS_FSM_FFd2.D | 11.400
IOL0.Q | IOL0.D | 11.000
IONPReady.Q | IONPReady.D | 11.000
IOU0.Q | IOU0.D | 11.000
RefReq.Q | ram/CAS.D | 11.000
RefReq.Q | ram/RAMEN.D | 11.000
RefReq.Q | ram/RS_FSM_FFd6.D | 11.000
RefReq.Q | ram/RS_FSM_FFd8.D | 11.000
RefUrg.Q | cnt/Timer<1>.D | 11.000
RefUrg.Q | cnt/Timer<2>.D | 11.000
RefUrg.Q | cnt/Timer<3>.D | 11.000
RefUrg.Q | ram/RAMEN.D | 11.000
RefUrg.Q | ram/RS_FSM_FFd4.D | 11.000
cnt/Er<0>.Q | cnt/Timer<1>.D | 11.000
cnt/Er<0>.Q | cnt/Timer<2>.D | 11.000
cnt/Er<0>.Q | cnt/Timer<3>.D | 11.000
cnt/Er<1>.Q | cnt/Timer<1>.D | 11.000
cnt/Er<1>.Q | cnt/Timer<2>.D | 11.000
cnt/Er<1>.Q | cnt/Timer<3>.D | 11.000
cnt/IS_FSM_FFd1.Q | nAoutOE.D | 11.000
cnt/IS_FSM_FFd2.Q | nAoutOE.D | 11.000
cnt/Timer<0>.Q | cnt/Timer<2>.D | 11.000
cnt/Timer<0>.Q | cnt/Timer<3>.D | 11.000
cnt/Timer<1>.Q | cnt/Timer<2>.D | 11.000
cnt/Timer<1>.Q | cnt/Timer<3>.D | 11.000
cnt/Timer<2>.Q | cnt/Timer<2>.D | 11.000
cnt/Timer<2>.Q | cnt/Timer<3>.D | 11.000
cnt/Timer<3>.Q | cnt/Timer<3>.D | 11.000
cs/nOverlay.Q | IOL0.D | 11.000
cs/nOverlay.Q | IORDREQ.D | 11.000
cs/nOverlay.Q | IOU0.D | 11.000
cs/nOverlay.Q | iobs/Sent.D | 11.000
cs/nOverlay.Q | iobs/TS_FSM_FFd2.D | 11.000
cs/nOverlay.Q | ram/CAS.D | 11.000
cs/nOverlay.Q | ram/RAMEN.D | 11.000
cs/nOverlay.Q | ram/RASEL.D | 11.000
cs/nOverlay.Q | ram/RS_FSM_FFd6.D | 11.000
cs/nOverlay.Q | ram/RS_FSM_FFd8.D | 11.000
fsb/ASrf.Q | IOL0.D | 11.000
fsb/ASrf.Q | IORDREQ.D | 11.000
fsb/ASrf.Q | IOU0.D | 11.000
fsb/ASrf.Q | IOWRREQ.D | 11.000
fsb/ASrf.Q | iobs/IORW1.D | 11.000
fsb/ASrf.Q | iobs/Load1.D | 11.000
fsb/ASrf.Q | ram/CAS.D | 11.000
fsb/ASrf.Q | ram/RAMEN.D | 11.000
fsb/ASrf.Q | ram/RASEL.D | 11.000
fsb/ASrf.Q | ram/RS_FSM_FFd6.D | 11.000
fsb/ASrf.Q | ram/RS_FSM_FFd8.D | 11.000
iobs/IOL1.Q | IOL0.D | 11.000
iobs/IORW1.Q | IORDREQ.D | 11.000
iobs/IORW1.Q | IOWRREQ.D | 11.000
iobs/IOU1.Q | IOU0.D | 11.000
iobs/Sent.Q | IOWRREQ.D | 11.000
iobs/Sent.Q | iobs/IORW1.D | 11.000
iobs/Sent.Q | iobs/Load1.D | 11.000
iobs/TS_FSM_FFd1.Q | iobs/IORW1.D | 11.000
iobs/TS_FSM_FFd1.Q | iobs/Load1.D | 11.000
iobs/TS_FSM_FFd2.Q | ALE0S.D | 11.000
iobs/TS_FSM_FFd2.Q | IORDREQ.D | 11.000
iobs/TS_FSM_FFd2.Q | iobs/IORW1.D | 11.000
iobs/TS_FSM_FFd2.Q | iobs/Load1.D | 11.000
iobs/TS_FSM_FFd2.Q | iobs/Sent.D | 11.000
nADoutLE1.Q | IORDREQ.D | 11.000
nADoutLE1.Q | iobs/IORW1.D | 11.000
nADoutLE1.Q | iobs/Load1.D | 11.000
nAoutOE.Q | nAoutOE.D | 11.000
ram/BACTr.Q | ram/CAS.D | 11.000
ram/BACTr.Q | ram/RAMEN.D | 11.000
ram/BACTr.Q | ram/RS_FSM_FFd6.D | 11.000
ram/BACTr.Q | ram/RS_FSM_FFd8.D | 11.000
ram/RAMEN.Q | ram/CAS.D | 11.000
ram/RAMEN.Q | ram/RASEL.D | 11.000
ram/RS_FSM_FFd1.Q | ram/RS_FSM_FFd4.D | 11.000
ram/RS_FSM_FFd4.Q | ram/RS_FSM_FFd8.D | 11.000
ram/RS_FSM_FFd5.Q | ram/RS_FSM_FFd4.D | 11.000
ram/RS_FSM_FFd7.Q | ram/RASEL.D | 11.000
ram/RS_FSM_FFd8.Q | ram/CAS.D | 11.000
ram/RS_FSM_FFd8.Q | ram/RAMEN.D | 11.000
ram/RS_FSM_FFd8.Q | ram/RASEL.D | 11.000
ram/RS_FSM_FFd8.Q | ram/RS_FSM_FFd6.D | 11.000
ram/RefDone.Q | ram/CAS.D | 11.000
ram/RefDone.Q | ram/RAMEN.D | 11.000
ram/RefDone.Q | ram/RS_FSM_FFd4.D | 11.000
ram/RefDone.Q | ram/RS_FSM_FFd6.D | 11.000
ram/RefDone.Q | ram/RS_FSM_FFd8.D | 11.000
IONPReady.Q | nDTACK_FSB.D | 10.000
IONPReady.Q | nVPA_FSB.D | 10.000
IORDREQ.Q | IORDREQ.D | 10.000
IOWRREQ.Q | IOWRREQ.D | 10.000
QoSReady.Q | QoSReady.D | 10.000
QoSReady.Q | nDTACK_FSB.D | 10.000
QoSReady.Q | nVPA_FSB.D | 10.000
RefReq.Q | ram/RefDone.D | 10.000
RefUrg.Q | cnt/IS_FSM_FFd1.D | 10.000
RefUrg.Q | cnt/IS_FSM_FFd2.D | 10.000
RefUrg.Q | cnt/LTimer<0>.CE | 10.000
RefUrg.Q | cnt/LTimer<10>.CE | 10.000
RefUrg.Q | cnt/LTimer<11>.CE | 10.000
RefUrg.Q | cnt/LTimer<12>.CE | 10.000
RefUrg.Q | cnt/LTimer<1>.CE | 10.000
RefUrg.Q | cnt/LTimer<2>.CE | 10.000
RefUrg.Q | cnt/LTimer<3>.CE | 10.000
RefUrg.Q | cnt/LTimer<4>.CE | 10.000
RefUrg.Q | cnt/LTimer<5>.CE | 10.000
RefUrg.Q | cnt/LTimer<6>.CE | 10.000
RefUrg.Q | cnt/LTimer<7>.CE | 10.000
RefUrg.Q | cnt/LTimer<8>.CE | 10.000
RefUrg.Q | cnt/LTimer<9>.CE | 10.000
RefUrg.Q | cnt/LTimerTC.CE | 10.000
RefUrg.Q | cnt/Timer<0>.D | 10.000
RefUrg.Q | ram/CAS.D | 10.000
RefUrg.Q | ram/RS_FSM_FFd6.D | 10.000
RefUrg.Q | ram/RS_FSM_FFd8.D | 10.000
RefUrg.Q | ram/RefDone.D | 10.000
cnt/Er<0>.Q | RefReq.CE | 10.000
cnt/Er<0>.Q | RefUrg.CE | 10.000
cnt/Er<0>.Q | cnt/Er<1>.D | 10.000
cnt/Er<0>.Q | cnt/IS_FSM_FFd1.D | 10.000
cnt/Er<0>.Q | cnt/IS_FSM_FFd2.D | 10.000
cnt/Er<0>.Q | cnt/LTimer<0>.CE | 10.000
cnt/Er<0>.Q | cnt/LTimer<10>.CE | 10.000
cnt/Er<0>.Q | cnt/LTimer<11>.CE | 10.000
cnt/Er<0>.Q | cnt/LTimer<12>.CE | 10.000
cnt/Er<0>.Q | cnt/LTimer<1>.CE | 10.000
cnt/Er<0>.Q | cnt/LTimer<2>.CE | 10.000
cnt/Er<0>.Q | cnt/LTimer<3>.CE | 10.000
cnt/Er<0>.Q | cnt/LTimer<4>.CE | 10.000
cnt/Er<0>.Q | cnt/LTimer<5>.CE | 10.000
cnt/Er<0>.Q | cnt/LTimer<6>.CE | 10.000
cnt/Er<0>.Q | cnt/LTimer<7>.CE | 10.000
cnt/Er<0>.Q | cnt/LTimer<8>.CE | 10.000
cnt/Er<0>.Q | cnt/LTimer<9>.CE | 10.000
cnt/Er<0>.Q | cnt/LTimerTC.CE | 10.000
cnt/Er<0>.Q | cnt/Timer<0>.CE | 10.000
cnt/Er<0>.Q | cnt/Timer<0>.D | 10.000
cnt/Er<0>.Q | cnt/Timer<1>.CE | 10.000
cnt/Er<0>.Q | cnt/Timer<2>.CE | 10.000
cnt/Er<0>.Q | cnt/Timer<3>.CE | 10.000
cnt/Er<1>.Q | RefReq.CE | 10.000
cnt/Er<1>.Q | RefUrg.CE | 10.000
cnt/Er<1>.Q | cnt/IS_FSM_FFd1.D | 10.000
cnt/Er<1>.Q | cnt/IS_FSM_FFd2.D | 10.000
cnt/Er<1>.Q | cnt/LTimer<0>.CE | 10.000
cnt/Er<1>.Q | cnt/LTimer<10>.CE | 10.000
cnt/Er<1>.Q | cnt/LTimer<11>.CE | 10.000
cnt/Er<1>.Q | cnt/LTimer<12>.CE | 10.000
cnt/Er<1>.Q | cnt/LTimer<1>.CE | 10.000
cnt/Er<1>.Q | cnt/LTimer<2>.CE | 10.000
cnt/Er<1>.Q | cnt/LTimer<3>.CE | 10.000
cnt/Er<1>.Q | cnt/LTimer<4>.CE | 10.000
cnt/Er<1>.Q | cnt/LTimer<5>.CE | 10.000
cnt/Er<1>.Q | cnt/LTimer<6>.CE | 10.000
cnt/Er<1>.Q | cnt/LTimer<7>.CE | 10.000
cnt/Er<1>.Q | cnt/LTimer<8>.CE | 10.000
cnt/Er<1>.Q | cnt/LTimer<9>.CE | 10.000
cnt/Er<1>.Q | cnt/LTimerTC.CE | 10.000
cnt/Er<1>.Q | cnt/Timer<0>.CE | 10.000
cnt/Er<1>.Q | cnt/Timer<0>.D | 10.000
cnt/Er<1>.Q | cnt/Timer<1>.CE | 10.000
cnt/Er<1>.Q | cnt/Timer<2>.CE | 10.000
cnt/Er<1>.Q | cnt/Timer<3>.CE | 10.000
cnt/IS_FSM_FFd1.Q | cnt/IS_FSM_FFd1.D | 10.000
cnt/IS_FSM_FFd1.Q | cnt/IS_FSM_FFd2.D | 10.000
cnt/IS_FSM_FFd1.Q | cnt/LTimer<10>.D | 10.000
cnt/IS_FSM_FFd1.Q | cnt/LTimer<11>.D | 10.000
cnt/IS_FSM_FFd1.Q | cnt/LTimer<12>.D | 10.000
cnt/IS_FSM_FFd1.Q | nBR_IOB.D | 10.000
cnt/IS_FSM_FFd1.Q | nRESout.D | 10.000
cnt/IS_FSM_FFd2.Q | cnt/IS_FSM_FFd1.D | 10.000
cnt/IS_FSM_FFd2.Q | cnt/IS_FSM_FFd2.D | 10.000
cnt/IS_FSM_FFd2.Q | cnt/LTimer<10>.D | 10.000
cnt/IS_FSM_FFd2.Q | cnt/LTimer<11>.D | 10.000
cnt/IS_FSM_FFd2.Q | cnt/LTimer<12>.D | 10.000
cnt/IS_FSM_FFd2.Q | nBR_IOB.D | 10.000
cnt/IS_FSM_FFd2.Q | nRESout.D | 10.000
cnt/LTimer<0>.Q | QoSReady.D | 10.000
cnt/LTimer<0>.Q | cnt/LTimer<10>.D | 10.000
cnt/LTimer<0>.Q | cnt/LTimer<11>.D | 10.000
cnt/LTimer<0>.Q | cnt/LTimer<12>.D | 10.000
cnt/LTimer<0>.Q | cnt/LTimer<1>.D | 10.000
cnt/LTimer<0>.Q | cnt/LTimer<2>.D | 10.000
cnt/LTimer<0>.Q | cnt/LTimer<3>.D | 10.000
cnt/LTimer<0>.Q | cnt/LTimer<4>.D | 10.000
cnt/LTimer<0>.Q | cnt/LTimer<5>.D | 10.000
cnt/LTimer<0>.Q | cnt/LTimer<6>.D | 10.000
cnt/LTimer<0>.Q | cnt/LTimer<7>.D | 10.000
cnt/LTimer<0>.Q | cnt/LTimer<8>.D | 10.000
cnt/LTimer<0>.Q | cnt/LTimer<9>.D | 10.000
cnt/LTimer<0>.Q | cnt/LTimerTC.D | 10.000
cnt/LTimer<10>.Q | QoSReady.D | 10.000
cnt/LTimer<10>.Q | cnt/LTimer<10>.D | 10.000
cnt/LTimer<10>.Q | cnt/LTimer<11>.D | 10.000
cnt/LTimer<10>.Q | cnt/LTimer<12>.D | 10.000
cnt/LTimer<10>.Q | cnt/LTimerTC.D | 10.000
cnt/LTimer<11>.Q | QoSReady.D | 10.000
cnt/LTimer<11>.Q | cnt/LTimer<11>.D | 10.000
cnt/LTimer<11>.Q | cnt/LTimer<12>.D | 10.000
cnt/LTimer<11>.Q | cnt/LTimerTC.D | 10.000
cnt/LTimer<12>.Q | QoSReady.D | 10.000
cnt/LTimer<12>.Q | cnt/LTimer<12>.D | 10.000
cnt/LTimer<12>.Q | cnt/LTimerTC.D | 10.000
cnt/LTimer<1>.Q | QoSReady.D | 10.000
cnt/LTimer<1>.Q | cnt/LTimer<10>.D | 10.000
cnt/LTimer<1>.Q | cnt/LTimer<11>.D | 10.000
cnt/LTimer<1>.Q | cnt/LTimer<12>.D | 10.000
cnt/LTimer<1>.Q | cnt/LTimer<2>.D | 10.000
cnt/LTimer<1>.Q | cnt/LTimer<3>.D | 10.000
cnt/LTimer<1>.Q | cnt/LTimer<4>.D | 10.000
cnt/LTimer<1>.Q | cnt/LTimer<5>.D | 10.000
cnt/LTimer<1>.Q | cnt/LTimer<6>.D | 10.000
cnt/LTimer<1>.Q | cnt/LTimer<7>.D | 10.000
cnt/LTimer<1>.Q | cnt/LTimer<8>.D | 10.000
cnt/LTimer<1>.Q | cnt/LTimer<9>.D | 10.000
cnt/LTimer<1>.Q | cnt/LTimerTC.D | 10.000
cnt/LTimer<2>.Q | QoSReady.D | 10.000
cnt/LTimer<2>.Q | cnt/LTimer<10>.D | 10.000
cnt/LTimer<2>.Q | cnt/LTimer<11>.D | 10.000
cnt/LTimer<2>.Q | cnt/LTimer<12>.D | 10.000
cnt/LTimer<2>.Q | cnt/LTimer<3>.D | 10.000
cnt/LTimer<2>.Q | cnt/LTimer<4>.D | 10.000
cnt/LTimer<2>.Q | cnt/LTimer<5>.D | 10.000
cnt/LTimer<2>.Q | cnt/LTimer<6>.D | 10.000
cnt/LTimer<2>.Q | cnt/LTimer<7>.D | 10.000
cnt/LTimer<2>.Q | cnt/LTimer<8>.D | 10.000
cnt/LTimer<2>.Q | cnt/LTimer<9>.D | 10.000
cnt/LTimer<2>.Q | cnt/LTimerTC.D | 10.000
cnt/LTimer<3>.Q | QoSReady.D | 10.000
cnt/LTimer<3>.Q | cnt/LTimer<10>.D | 10.000
cnt/LTimer<3>.Q | cnt/LTimer<11>.D | 10.000
cnt/LTimer<3>.Q | cnt/LTimer<12>.D | 10.000
cnt/LTimer<3>.Q | cnt/LTimer<4>.D | 10.000
cnt/LTimer<3>.Q | cnt/LTimer<5>.D | 10.000
cnt/LTimer<3>.Q | cnt/LTimer<6>.D | 10.000
cnt/LTimer<3>.Q | cnt/LTimer<7>.D | 10.000
cnt/LTimer<3>.Q | cnt/LTimer<8>.D | 10.000
cnt/LTimer<3>.Q | cnt/LTimer<9>.D | 10.000
cnt/LTimer<3>.Q | cnt/LTimerTC.D | 10.000
cnt/LTimer<4>.Q | QoSReady.D | 10.000
cnt/LTimer<4>.Q | cnt/LTimer<10>.D | 10.000
cnt/LTimer<4>.Q | cnt/LTimer<11>.D | 10.000
cnt/LTimer<4>.Q | cnt/LTimer<12>.D | 10.000
cnt/LTimer<4>.Q | cnt/LTimer<5>.D | 10.000
cnt/LTimer<4>.Q | cnt/LTimer<6>.D | 10.000
cnt/LTimer<4>.Q | cnt/LTimer<7>.D | 10.000
cnt/LTimer<4>.Q | cnt/LTimer<8>.D | 10.000
cnt/LTimer<4>.Q | cnt/LTimer<9>.D | 10.000
cnt/LTimer<4>.Q | cnt/LTimerTC.D | 10.000
cnt/LTimer<5>.Q | QoSReady.D | 10.000
cnt/LTimer<5>.Q | cnt/LTimer<10>.D | 10.000
cnt/LTimer<5>.Q | cnt/LTimer<11>.D | 10.000
cnt/LTimer<5>.Q | cnt/LTimer<12>.D | 10.000
cnt/LTimer<5>.Q | cnt/LTimer<6>.D | 10.000
cnt/LTimer<5>.Q | cnt/LTimer<7>.D | 10.000
cnt/LTimer<5>.Q | cnt/LTimer<8>.D | 10.000
cnt/LTimer<5>.Q | cnt/LTimer<9>.D | 10.000
cnt/LTimer<5>.Q | cnt/LTimerTC.D | 10.000
cnt/LTimer<6>.Q | QoSReady.D | 10.000
cnt/LTimer<6>.Q | cnt/LTimer<10>.D | 10.000
cnt/LTimer<6>.Q | cnt/LTimer<11>.D | 10.000
cnt/LTimer<6>.Q | cnt/LTimer<12>.D | 10.000
cnt/LTimer<6>.Q | cnt/LTimer<7>.D | 10.000
cnt/LTimer<6>.Q | cnt/LTimer<8>.D | 10.000
cnt/LTimer<6>.Q | cnt/LTimer<9>.D | 10.000
cnt/LTimer<6>.Q | cnt/LTimerTC.D | 10.000
cnt/LTimer<7>.Q | QoSReady.D | 10.000
cnt/LTimer<7>.Q | cnt/LTimer<10>.D | 10.000
cnt/LTimer<7>.Q | cnt/LTimer<11>.D | 10.000
cnt/LTimer<7>.Q | cnt/LTimer<12>.D | 10.000
cnt/LTimer<7>.Q | cnt/LTimer<8>.D | 10.000
cnt/LTimer<7>.Q | cnt/LTimer<9>.D | 10.000
cnt/LTimer<7>.Q | cnt/LTimerTC.D | 10.000
cnt/LTimer<8>.Q | QoSReady.D | 10.000
cnt/LTimer<8>.Q | cnt/LTimer<10>.D | 10.000
cnt/LTimer<8>.Q | cnt/LTimer<11>.D | 10.000
cnt/LTimer<8>.Q | cnt/LTimer<12>.D | 10.000
cnt/LTimer<8>.Q | cnt/LTimer<9>.D | 10.000
cnt/LTimer<8>.Q | cnt/LTimerTC.D | 10.000
cnt/LTimer<9>.Q | QoSReady.D | 10.000
cnt/LTimer<9>.Q | cnt/LTimer<10>.D | 10.000
cnt/LTimer<9>.Q | cnt/LTimer<11>.D | 10.000
cnt/LTimer<9>.Q | cnt/LTimer<12>.D | 10.000
cnt/LTimer<9>.Q | cnt/LTimerTC.D | 10.000
cnt/LTimerTC.Q | cnt/IS_FSM_FFd1.D | 10.000
cnt/LTimerTC.Q | cnt/IS_FSM_FFd2.D | 10.000
cnt/Timer<0>.Q | RefReq.D | 10.000
cnt/Timer<0>.Q | RefUrg.D | 10.000
cnt/Timer<0>.Q | cnt/Timer<0>.D | 10.000
cnt/Timer<0>.Q | cnt/Timer<1>.D | 10.000
cnt/Timer<1>.Q | RefReq.D | 10.000
cnt/Timer<1>.Q | RefUrg.D | 10.000
cnt/Timer<1>.Q | cnt/Timer<1>.D | 10.000
cnt/Timer<2>.Q | RefReq.D | 10.000
cnt/Timer<2>.Q | RefUrg.D | 10.000
cnt/Timer<3>.Q | RefReq.D | 10.000
cnt/Timer<3>.Q | RefUrg.D | 10.000
cnt/WS<0>.Q | QoSReady.D | 10.000
cnt/WS<0>.Q | cnt/WS<0>.D | 10.000
cnt/WS<0>.Q | cnt/WS<1>.D | 10.000
cnt/WS<0>.Q | cnt/WS<2>.D | 10.000
cnt/WS<0>.Q | cnt/WS<3>.D | 10.000
cnt/WS<1>.Q | QoSReady.D | 10.000
cnt/WS<1>.Q | cnt/WS<1>.D | 10.000
cnt/WS<1>.Q | cnt/WS<2>.D | 10.000
cnt/WS<1>.Q | cnt/WS<3>.D | 10.000
cnt/WS<2>.Q | QoSReady.D | 10.000
cnt/WS<2>.Q | cnt/WS<2>.D | 10.000
cnt/WS<2>.Q | cnt/WS<3>.D | 10.000
cnt/WS<3>.Q | QoSReady.D | 10.000
cnt/WS<3>.Q | cnt/WS<3>.D | 10.000
cnt/nIPL2r.Q | cnt/IS_FSM_FFd1.D | 10.000
cnt/nIPL2r.Q | nBR_IOB.D | 10.000
cs/ODCSr.Q | cs/nOverlay.D | 10.000
cs/nOverlay.Q | cs/nOverlay.D | 10.000
cs/nOverlay.Q | ram/Once.D | 10.000
cs/nOverlay.Q | ram/RASrr.D | 10.000
cs/nOverlay.Q | ram/RS_FSM_FFd7.D | 10.000
fsb/ASrf.Q | IONPReady.D | 10.000
fsb/ASrf.Q | QoSReady.D | 10.000
fsb/ASrf.Q | cnt/WS<0>.D | 10.000
fsb/ASrf.Q | cnt/WS<1>.D | 10.000
fsb/ASrf.Q | cnt/WS<2>.D | 10.000
fsb/ASrf.Q | cnt/WS<3>.D | 10.000
fsb/ASrf.Q | cs/ODCSr.D | 10.000
fsb/ASrf.Q | cs/nOverlay.D | 10.000
fsb/ASrf.Q | iobs/Sent.D | 10.000
fsb/ASrf.Q | iobs/TS_FSM_FFd2.D | 10.000
fsb/ASrf.Q | nBERR_FSB.D | 10.000
fsb/ASrf.Q | nDTACK_FSB.D | 10.000
fsb/ASrf.Q | nVPA_FSB.D | 10.000
fsb/ASrf.Q | ram/BACTr.D | 10.000
fsb/ASrf.Q | ram/Once.D | 10.000
fsb/ASrf.Q | ram/RASrr.D | 10.000
fsb/ASrf.Q | ram/RS_FSM_FFd7.D | 10.000
iobs/Clear1.Q | nADoutLE1.D | 10.000
iobs/IOACTr.Q | IORDREQ.D | 10.000
iobs/IOACTr.Q | IOWRREQ.D | 10.000
iobs/IOACTr.Q | iobs/TS_FSM_FFd1.D | 10.000
iobs/IOACTr.Q | iobs/TS_FSM_FFd2.D | 10.000
iobs/IODONEr.Q | IONPReady.D | 10.000
iobs/Load1.Q | iobs/IOL1.CE | 10.000
iobs/Load1.Q | iobs/IOU1.CE | 10.000
iobs/Load1.Q | nADoutLE1.D | 10.000
iobs/Sent.Q | IOL0.D | 10.000
iobs/Sent.Q | IONPReady.D | 10.000
iobs/Sent.Q | IORDREQ.D | 10.000
iobs/Sent.Q | IOU0.D | 10.000
iobs/Sent.Q | iobs/TS_FSM_FFd2.D | 10.000
iobs/Sent.Q | nBERR_FSB.D | 10.000
iobs/TS_FSM_FFd1.Q | IOL0.D | 10.000
iobs/TS_FSM_FFd1.Q | IORDREQ.D | 10.000
iobs/TS_FSM_FFd1.Q | IOU0.D | 10.000
iobs/TS_FSM_FFd1.Q | IOWRREQ.D | 10.000
iobs/TS_FSM_FFd1.Q | iobs/Clear1.D | 10.000
iobs/TS_FSM_FFd1.Q | iobs/Sent.D | 10.000
iobs/TS_FSM_FFd1.Q | iobs/TS_FSM_FFd1.D | 10.000
iobs/TS_FSM_FFd1.Q | iobs/TS_FSM_FFd2.D | 10.000
iobs/TS_FSM_FFd2.Q | iobs/Clear1.D | 10.000
iobs/TS_FSM_FFd2.Q | iobs/TS_FSM_FFd1.D | 10.000
nADoutLE1.Q | iobs/Sent.D | 10.000
nADoutLE1.Q | nADoutLE1.D | 10.000
nBERR_FSB.Q | nBERR_FSB.D | 10.000
nBR_IOB.Q | nAoutOE.D | 10.000
nBR_IOB.Q | nBR_IOB.D | 10.000
ram/CAS.Q | nCAS.D | 10.000
ram/Once.Q | ram/Once.D | 10.000
ram/Once.Q | ram/RAMEN.D | 10.000
ram/RAMEN.Q | ram/Once.D | 10.000
ram/RAMEN.Q | ram/RAMEN.D | 10.000
ram/RAMEN.Q | ram/RASrr.D | 10.000
ram/RAMEN.Q | ram/RS_FSM_FFd6.D | 10.000
ram/RAMEN.Q | ram/RS_FSM_FFd7.D | 10.000
ram/RAMEN.Q | ram/RS_FSM_FFd8.D | 10.000
ram/RS_FSM_FFd2.Q | ram/RS_FSM_FFd1.D | 10.000
ram/RS_FSM_FFd2.Q | ram/RefDone.D | 10.000
ram/RS_FSM_FFd3.Q | ram/RASrr.D | 10.000
ram/RS_FSM_FFd3.Q | ram/RS_FSM_FFd2.D | 10.000
ram/RS_FSM_FFd3.Q | ram/RefDone.D | 10.000
ram/RS_FSM_FFd4.Q | ram/RAMEN.D | 10.000
ram/RS_FSM_FFd5.Q | ram/CAS.D | 10.000
ram/RS_FSM_FFd5.Q | ram/RS_FSM_FFd6.D | 10.000
ram/RS_FSM_FFd6.Q | ram/CAS.D | 10.000
ram/RS_FSM_FFd6.Q | ram/RASrr.D | 10.000
ram/RS_FSM_FFd6.Q | ram/RS_FSM_FFd3.D | 10.000
ram/RS_FSM_FFd7.Q | ram/CAS.D | 10.000
ram/RS_FSM_FFd7.Q | ram/RAMEN.D | 10.000
ram/RS_FSM_FFd7.Q | ram/RASrf.D | 10.000
ram/RS_FSM_FFd7.Q | ram/RS_FSM_FFd5.D | 10.000
ram/RS_FSM_FFd8.Q | ram/Once.D | 10.000
ram/RS_FSM_FFd8.Q | ram/RASrr.D | 10.000
ram/RS_FSM_FFd8.Q | ram/RS_FSM_FFd7.D | 10.000
ram/RS_FSM_FFd8.Q | ram/RS_FSM_FFd8.D | 10.000
ram/RefDone.Q | ram/RefDone.D | 10.000

Clock to Setup for clock C16M
Source | Destination | Delay
--- | --- | ---
IOACT.Q | IOACT.D | 11.000
iobm/C8Mr.Q | nLDS_IOB.D | 11.000
iobm/C8Mr.Q | nUDS_IOB.D | 11.000
iobm/IORDREQr.Q | nLDS_IOB.D | 11.000
iobm/IORDREQr.Q | nUDS_IOB.D | 11.000
iobm/IOS_FSM_FFd1.Q | IOACT.D | 11.000
iobm/IOS_FSM_FFd2.Q | IOACT.D | 11.000
iobm/IOS_FSM_FFd3.Q | IOACT.D | 11.000
iobm/IOS_FSM_FFd7.Q | IOACT.D | 11.000
iobm/IOS_FSM_FFd7.Q | nLDS_IOB.D | 11.000
iobm/IOS_FSM_FFd7.Q | nUDS_IOB.D | 11.000
iobm/IOWRREQr.Q | IOACT.D | 11.000
ALE0M.Q | ALE0M.D | 10.000
iobm/C8Mr.Q | IOACT.D | 10.000
iobm/C8Mr.Q | iobm/DoutOE.D | 10.000
iobm/C8Mr.Q | iobm/IOS0.D | 10.000
iobm/C8Mr.Q | iobm/IOS_FSM_FFd2.D | 10.000
iobm/C8Mr.Q | iobm/IOS_FSM_FFd3.D | 10.000
iobm/C8Mr.Q | iobm/IOS_FSM_FFd6.D | 10.000
iobm/C8Mr.Q | iobm/IOS_FSM_FFd7.D | 10.000
iobm/C8Mr.Q | nAS_IOB.D | 10.000
iobm/DoutOE.Q | iobm/DoutOE.D | 10.000
iobm/IORDREQr.Q | ALE0M.D | 10.000
iobm/IORDREQr.Q | IOACT.D | 10.000
iobm/IORDREQr.Q | iobm/IOS0.D | 10.000
iobm/IORDREQr.Q | iobm/IOS_FSM_FFd6.D | 10.000
iobm/IORDREQr.Q | iobm/IOS_FSM_FFd7.D | 10.000
iobm/IORDREQr.Q | nAS_IOB.D | 10.000
iobm/IOS0.Q | iobm/IOS0.D | 10.000
iobm/IOS_FSM_FFd1.Q | ALE0M.D | 10.000
iobm/IOS_FSM_FFd1.Q | iobm/IOS0.D | 10.000
iobm/IOS_FSM_FFd1.Q | iobm/IOS_FSM_FFd7.D | 10.000
iobm/IOS_FSM_FFd2.Q | ALE0M.D | 10.000
iobm/IOS_FSM_FFd2.Q | iobm/IOS0.D | 10.000
iobm/IOS_FSM_FFd2.Q | iobm/IOS_FSM_FFd1.D | 10.000
iobm/IOS_FSM_FFd3.Q | ALE0M.D | 10.000
iobm/IOS_FSM_FFd3.Q | iobm/DoutOE.D | 10.000
iobm/IOS_FSM_FFd3.Q | iobm/IOS0.D | 10.000
iobm/IOS_FSM_FFd3.Q | iobm/IOS_FSM_FFd2.D | 10.000
iobm/IOS_FSM_FFd3.Q | iobm/IOS_FSM_FFd3.D | 10.000
iobm/IOS_FSM_FFd3.Q | nAS_IOB.D | 10.000
iobm/IOS_FSM_FFd3.Q | nDinLE.D | 10.000
iobm/IOS_FSM_FFd3.Q | nLDS_IOB.D | 10.000
iobm/IOS_FSM_FFd3.Q | nUDS_IOB.D | 10.000
iobm/IOS_FSM_FFd4.Q | ALE0M.D | 10.000
iobm/IOS_FSM_FFd4.Q | IOACT.D | 10.000
iobm/IOS_FSM_FFd4.Q | iobm/DoutOE.D | 10.000
iobm/IOS_FSM_FFd4.Q | iobm/IOS0.D | 10.000
iobm/IOS_FSM_FFd4.Q | iobm/IOS_FSM_FFd3.D | 10.000
iobm/IOS_FSM_FFd4.Q | nAS_IOB.D | 10.000
iobm/IOS_FSM_FFd4.Q | nDinLE.D | 10.000
iobm/IOS_FSM_FFd4.Q | nLDS_IOB.D | 10.000
iobm/IOS_FSM_FFd4.Q | nUDS_IOB.D | 10.000
iobm/IOS_FSM_FFd5.Q | ALE0M.D | 10.000
iobm/IOS_FSM_FFd5.Q | IOACT.D | 10.000
iobm/IOS_FSM_FFd5.Q | iobm/DoutOE.D | 10.000
iobm/IOS_FSM_FFd5.Q | iobm/IOS0.D | 10.000
iobm/IOS_FSM_FFd5.Q | iobm/IOS_FSM_FFd4.D | 10.000
iobm/IOS_FSM_FFd5.Q | nAS_IOB.D | 10.000
iobm/IOS_FSM_FFd5.Q | nLDS_IOB.D | 10.000
iobm/IOS_FSM_FFd5.Q | nUDS_IOB.D | 10.000
iobm/IOS_FSM_FFd6.Q | ALE0M.D | 10.000
iobm/IOS_FSM_FFd6.Q | IOACT.D | 10.000
iobm/IOS_FSM_FFd6.Q | iobm/DoutOE.D | 10.000
iobm/IOS_FSM_FFd6.Q | iobm/IOS0.D | 10.000
iobm/IOS_FSM_FFd6.Q | iobm/IOS_FSM_FFd5.D | 10.000
iobm/IOS_FSM_FFd6.Q | nAS_IOB.D | 10.000
iobm/IOS_FSM_FFd6.Q | nLDS_IOB.D | 10.000
iobm/IOS_FSM_FFd6.Q | nUDS_IOB.D | 10.000
iobm/IOS_FSM_FFd7.Q | ALE0M.D | 10.000
iobm/IOS_FSM_FFd7.Q | iobm/DoutOE.D | 10.000
iobm/IOS_FSM_FFd7.Q | iobm/IOS0.D | 10.000
iobm/IOS_FSM_FFd7.Q | iobm/IOS_FSM_FFd6.D | 10.000
iobm/IOS_FSM_FFd7.Q | iobm/IOS_FSM_FFd7.D | 10.000
iobm/IOS_FSM_FFd7.Q | nAS_IOB.D | 10.000
iobm/IOWRREQr.Q | ALE0M.D | 10.000
iobm/IOWRREQr.Q | iobm/DoutOE.D | 10.000
iobm/IOWRREQr.Q | iobm/IOS0.D | 10.000
iobm/IOWRREQr.Q | iobm/IOS_FSM_FFd6.D | 10.000
iobm/IOWRREQr.Q | iobm/IOS_FSM_FFd7.D | 10.000
iobm/IOWRREQr.Q | nAS_IOB.D | 10.000
nLDS_IOB.Q | nLDS_IOB.D | 10.000
nUDS_IOB.Q | nUDS_IOB.D | 10.000

Clock to Setup for clock C8M
Source | Destination | Delay
--- | --- | ---
iobm/ES<0>.Q | IODONE.D | 10.000
iobm/ES<0>.Q | iobm/ES<0>.D | 10.000
iobm/ES<0>.Q | iobm/ES<1>.D | 10.000
iobm/ES<0>.Q | iobm/ES<2>.D | 10.000
iobm/ES<0>.Q | iobm/ES<3>.D | 10.000
iobm/ES<0>.Q | nVMA_IOB.D | 10.000
iobm/ES<1>.Q | IODONE.D | 10.000
iobm/ES<1>.Q | iobm/ES<0>.D | 10.000
iobm/ES<1>.Q | iobm/ES<1>.D | 10.000
iobm/ES<1>.Q | iobm/ES<2>.D | 10.000
iobm/ES<1>.Q | iobm/ES<3>.D | 10.000
iobm/ES<1>.Q | nVMA_IOB.D | 10.000
iobm/ES<2>.Q | IODONE.D | 10.000
iobm/ES<2>.Q | iobm/ES<0>.D | 10.000
iobm/ES<2>.Q | iobm/ES<1>.D | 10.000
iobm/ES<2>.Q | iobm/ES<2>.D | 10.000
iobm/ES<2>.Q | iobm/ES<3>.D | 10.000
iobm/ES<2>.Q | nVMA_IOB.D | 10.000
iobm/ES<3>.Q | IODONE.D | 10.000
iobm/ES<3>.Q | iobm/ES<0>.D | 10.000
iobm/ES<3>.Q | iobm/ES<1>.D | 10.000
iobm/ES<3>.Q | iobm/ES<3>.D | 10.000
iobm/ES<3>.Q | nVMA_IOB.D | 10.000
iobm/Er.Q | iobm/ES<0>.D | 10.000
iobm/Er.Q | iobm/ES<1>.D | 10.000
iobm/Er.Q | iobm/ES<2>.D | 10.000
iobm/Er.Q | iobm/ES<3>.D | 10.000
iobm/VPAr.Q | nVMA_IOB.D | 10.000
nVMA_IOB.Q | IODONE.D | 10.000
nVMA_IOB.Q | nVMA_IOB.D | 10.000

### Pad to Pad List

Source Pad | Destination Pad | Delay
--- | --- | ---
A_FSB<11> | RA<4> | 11.000
A_FSB<12> | RA<5> | 11.000
A_FSB<20> | RA<11> | 11.000
A_FSB<22> | nRAS | 11.000
A_FSB<23> | nRAS | 11.000
A_FSB<3> | RA<4> | 11.000
A_FSB<4> | RA<5> | 11.000
nAS_FSB | nOE | 11.000
nAS_FSB | nRAS | 11.000
nAS_FSB | nROMWE | 11.000
nWE_FSB | nOE | 11.000
nWE_FSB | nROMWE | 11.000
A_FSB<10> | RA<1> | 10.000
A_FSB<13> | RA<6> | 10.000
A_FSB<14> | RA<7> | 10.000
A_FSB<15> | RA<9> | 10.000
A_FSB<16> | RA<2> | 10.000
A_FSB<17> | RA<10> | 10.000
A_FSB<18> | RA<8> | 10.000
A_FSB<19> | RA<11> | 10.000
A_FSB<19> | RA<3> | 10.000
A_FSB<1> | RA<0> | 10.000
A_FSB<20> | RA<3> | 10.000
A_FSB<20> | nDinOE | 10.000
A_FSB<20> | nROMCS | 10.000
A_FSB<21> | RA<8> | 10.000
A_FSB<21> | nDinOE | 10.000
A_FSB<21> | nROMCS | 10.000
A_FSB<22> | nDinOE | 10.000
A_FSB<22> | nROMCS | 10.000
A_FSB<23> | nDinOE | 10.000
A_FSB<23> | nROMCS | 10.000
A_FSB<2> | RA<1> | 10.000
A_FSB<5> | RA<6> | 10.000
A_FSB<6> | RA<7> | 10.000
A_FSB<7> | RA<10> | 10.000
A_FSB<7> | RA<2> | 10.000
A_FSB<8> | RA<9> | 10.000
A_FSB<9> | RA<0> | 10.000
nAS_FSB | nDinOE | 10.000
nAS_FSB | nRAMLWE | 10.000
nAS_FSB | nRAMUWE | 10.000
nLDS_FSB | nRAMLWE | 10.000
nUDS_FSB | nRAMUWE | 10.000
nWE_FSB | nDinOE | 10.000
nWE_FSB | nRAMLWE | 10.000
nWE_FSB | nRAMUWE | 10.000

Number of paths analyzed: 925
Number of Timing errors: 925
Analysis Completed: Sat Apr 08 05:49:36 2023