 
cpldfit:  version P.20131013                        Xilinx Inc.
                                  Fitter Report
Design Name: WarpSE                              Date:  4- 9-2023,  4:14AM
Device Used: XC95144XL-10-TQ100
Fitting Status: Successful

*************************  Mapped Resource Summary  **************************

Macrocells     Product Terms    Function Block   Registers      Pins           
Used/Tot       Used/Tot         Inps Used/Tot    Used/Tot       Used/Tot       
125/144 ( 87%) 438 /720  ( 61%) 285/432 ( 66%)   100/144 ( 69%) 70 /81  ( 86%)

** Function Block Resources **

Function    Mcells      FB Inps     Pterms      IO          
Block       Used/Tot    Used/Tot    Used/Tot    Used/Tot    
FB1          18/18*      28/54       40/90      11/11*
FB2          15/18       16/54       16/90       8/10
FB3          16/18       39/54       81/90      10/10*
FB4          17/18       42/54       62/90      10/10*
FB5          11/18       42/54       38/90       8/10
FB6          18/18*      36/54       68/90      10/10*
FB7          18/18*      41/54       52/90       7/10
FB8          12/18       41/54       81/90       6/10
             -----       -----       -----      -----    
            125/144     285/432     438/720     70/81 

* - Resource is exhausted

** Global Control Resources **

Signal 'C16M' mapped onto global clock net GCK1.
Signal 'C8M' mapped onto global clock net GCK2.
Signal 'FCLK' mapped onto global clock net GCK3.
Global output enable net(s) unused.
Global set/reset net(s) unused.

** Pin Resources **

Signal Type    Required     Mapped  |  Pin Type            Used    Total 
------------------------------------|------------------------------------
Input         :   32          32    |  I/O              :    64      73
Output        :   34          34    |  GCK/IO           :     3       3
Bidirectional :    1           1    |  GTS/IO           :     3       4
GCK           :    3           3    |  GSR/IO           :     0       1
GTS           :    0           0    |
GSR           :    0           0    |
                 ----        ----
        Total     70          70

** Power Data **

There are 125 macrocells in high performance mode (MCHP).
There are 0 macrocells in low power mode (MCLP).
End of Mapped Resource Summary
**************************  Errors and Warnings  ***************************

WARNING:Cpld - Unable to retrieve the path to the iSE Project Repository. Will
   use the default filename of 'WarpSE.ise'.
INFO:Cpld - Inferring BUFG constraint for signal 'C16M' based upon the LOC
   constraint 'P22'. It is recommended that you declare this BUFG explicitedly
   in your design. Note that for certain device families the output of a BUFG
   constraint can not drive a gated clock, and the BUFG constraint will be
   ignored.
INFO:Cpld - Inferring BUFG constraint for signal 'C8M' based upon the LOC
   constraint 'P23'. It is recommended that you declare this BUFG explicitedly
   in your design. Note that for certain device families the output of a BUFG
   constraint can not drive a gated clock, and the BUFG constraint will be
   ignored.
INFO:Cpld - Inferring BUFG constraint for signal 'FCLK' based upon the LOC
   constraint 'P27'. It is recommended that you declare this BUFG explicitedly
   in your design. Note that for certain device families the output of a BUFG
   constraint can not drive a gated clock, and the BUFG constraint will be
   ignored.
WARNING:Cpld:1007 - Removing unused input(s) 'C20MEN'.  The input(s) are unused
   after optimization. Please verify functionality via simulation.
WARNING:Cpld:1007 - Removing unused input(s) 'SW<1>'.  The input(s) are unused
   after optimization. Please verify functionality via simulation.
WARNING:Cpld:1007 - Removing unused input(s) 'SW<2>'.  The input(s) are unused
   after optimization. Please verify functionality via simulation.
WARNING:Cpld:1007 - Removing unused input(s) 'SW<3>'.  The input(s) are unused
   after optimization. Please verify functionality via simulation.
WARNING:Cpld:1007 - Removing unused input(s) 'nBG_IOB'.  The input(s) are unused
   after optimization. Please verify functionality via simulation.
*************************  Summary of Mapped Logic  ************************

** 35 Outputs **

Signal                                        Total Total Loc     Pin  Pin     Pin     Pwr  Slew Reg Init
Name                                          Pts   Inps          No.  Type    Use     Mode Rate State
nDTACK_FSB                                    9     17    FB3_9   28   I/O     O       STD  FAST RESET
nROMWE                                        1     2     FB3_17  34   I/O     O       STD  FAST 
nAoutOE                                       2     4     FB4_2   87   I/O     O       STD  FAST SET
nDoutOE                                       2     5     FB4_5   89   I/O     O       STD  FAST 
nDinOE                                        3     6     FB4_6   90   I/O     O       STD  FAST 
nRES                                          1     1     FB4_8   91   I/O     I/O     STD  FAST 
nVPA_FSB                                      3     12    FB4_11  93   I/O     O       STD  FAST RESET
nROMCS                                        2     5     FB5_2   35   I/O     O       STD  FAST 
nCAS                                          1     1     FB5_5   36   I/O     O       STD  FAST RESET
nOE                                           1     2     FB5_6   37   I/O     O       STD  FAST 
RA<4>                                         2     3     FB5_9   40   I/O     O       STD  FAST 
RA<3>                                         2     3     FB5_11  41   I/O     O       STD  FAST 
RA<5>                                         2     3     FB5_12  42   I/O     O       STD  FAST 
RA<2>                                         2     3     FB5_14  43   I/O     O       STD  FAST 
RA<6>                                         2     3     FB5_15  46   I/O     O       STD  FAST 
nVMA_IOB                                      3     8     FB6_2   74   I/O     O       STD  FAST RESET
nLDS_IOB                                      6     10    FB6_9   79   I/O     O       STD  FAST RESET
nUDS_IOB                                      6     10    FB6_11  80   I/O     O       STD  FAST RESET
nAS_IOB                                       4     9     FB6_12  81   I/O     O       STD  FAST RESET
nADoutLE1                                     2     3     FB6_14  82   I/O     O       STD  FAST SET
nADoutLE0                                     1     2     FB6_15  85   I/O     O       STD  FAST 
nDinLE                                        1     2     FB6_17  86   I/O     O       STD  FAST RESET
RA<1>                                         2     3     FB7_2   50   I/O     O       STD  FAST 
RA<7>                                         2     3     FB7_5   52   I/O     O       STD  FAST 
RA<0>                                         2     3     FB7_6   53   I/O     O       STD  FAST 
RA<8>                                         2     3     FB7_8   54   I/O     O       STD  FAST 
RA<10>                                        2     3     FB7_9   55   I/O     O       STD  FAST 
RA<9>                                         2     3     FB7_11  56   I/O     O       STD  FAST 
C25MEN                                        0     0     FB7_12  58   I/O     O       STD  FAST 
RA<11>                                        2     3     FB8_2   63   I/O     O       STD  FAST 
nRAS                                          3     7     FB8_5   64   I/O     O       STD  FAST 
nRAMLWE                                       1     4     FB8_6   65   I/O     O       STD  FAST 
nRAMUWE                                       1     4     FB8_8   66   I/O     O       STD  FAST 
nBERR_FSB                                     3     5     FB8_12  70   I/O     O       STD  FAST RESET
nBR_IOB                                       2     4     FB8_15  72   I/O     O       STD  FAST RESET

** 90 Buried Nodes **

Signal                                        Total Total Loc     Pwr  Reg Init
Name                                          Pts   Inps          Mode State
iobs/Clear1                                   1     2     FB1_1   STD  RESET
iobm/Er                                       1     1     FB1_2   STD  RESET
cnt/nIPL2r                                    1     1     FB1_3   STD  RESET
cnt/Er<1>                                     1     1     FB1_4   STD  RESET
cnt/Er<0>                                     1     1     FB1_5   STD  RESET
ram/RS_FSM_FFd4                               2     4     FB1_6   STD  RESET
iobs/TS_FSM_FFd1                              2     3     FB1_7   STD  RESET
iobs/IOU1                                     2     2     FB1_8   STD  RESET
cnt/Timer<0>                                  2     4     FB1_9   STD  RESET
cnt/IS_FSM_FFd2                               2     6     FB1_10  STD  RESET
RefUrg                                        2     6     FB1_11  STD  RESET
RefReq                                        2     6     FB1_12  STD  RESET
IOPWReady                                     2     3     FB1_13  STD  RESET
IOBERR                                        2     2     FB1_14  STD  RESET
iobm/ES<2>                                    3     5     FB1_15  STD  RESET
cnt/Timer<1>                                  4     5     FB1_16  STD  RESET
cnt/Timer<3>                                  5     7     FB1_17  STD  RESET
cnt/Timer<2>                                  5     6     FB1_18  STD  RESET
ram/RS_FSM_FFd5                               1     1     FB2_4   STD  RESET
ram/RS_FSM_FFd3                               1     1     FB2_5   STD  RESET
ram/RS_FSM_FFd2                               1     1     FB2_6   STD  RESET
ram/RS_FSM_FFd1                               1     1     FB2_7   STD  RESET
ram/RASrf                                     1     1     FB2_8   STD  RESET
iobs/IODONEr                                  1     1     FB2_9   STD  RESET
iobs/IOACTr                                   1     1     FB2_10  STD  RESET
iobm/VPAr                                     1     1     FB2_11  STD  RESET
iobm/IOWRREQr                                 1     1     FB2_12  STD  RESET
iobm/IOS_FSM_FFd5                             1     1     FB2_13  STD  RESET
iobm/IOS_FSM_FFd4                             1     1     FB2_14  STD  RESET
iobm/IOS_FSM_FFd1                             1     1     FB2_15  STD  RESET
iobm/IORDREQr                                 1     1     FB2_16  STD  RESET
iobm/C8Mr                                     1     1     FB2_17  STD  RESET
iobm/IOS_FSM_FFd2                             2     4     FB2_18  STD  RESET
iobs/Sent                                     13    18    FB3_1   STD  RESET
ram/RefDone                                   2     5     FB3_2   STD  RESET
ram/RS_FSM_FFd7                               2     7     FB3_3   STD  RESET
cs/nOverlay                                   2     5     FB3_4   STD  RESET
ram/RS_FSM_FFd6                               3     7     FB3_5   STD  RESET
ram/RASrr                                     4     9     FB3_6   STD  RESET
ram/RASEL                                     3     8     FB3_7   STD  RESET

Signal                                        Total Total Loc     Pwr  Reg Init
Name                                          Pts   Inps          Mode State
ram/Once                                      3     8     FB3_8   STD  RESET
RAMReady                                      4     8     FB3_10  STD  RESET
ram/RS_FSM_FFd8                               5     11    FB3_11  STD  SET
ram/RAMEN                                     6     10    FB3_12  STD  RESET
ram/CAS                                       7     13    FB3_14  STD  RESET
iobs/Load1                                    8     17    FB3_15  STD  RESET
IORDREQ                                       9     15    FB3_16  STD  RESET
QoSReady                                      18    25    FB4_1   STD  RESET
fsb/ASrf                                      1     1     FB4_3   STD  RESET
cnt/WS<0>                                     1     3     FB4_4   STD  RESET
$OpTx$$OpTx$FX_DC$354_INV$541                 1     2     FB4_7   STD  
iobs/IOL1                                     2     2     FB4_9   STD  RESET
cs/ODCSr                                      2     6     FB4_10  STD  RESET
cnt/WS<2>                                     3     5     FB4_12  STD  RESET
cnt/WS<1>                                     3     4     FB4_13  STD  RESET
IONPReady                                     5     16    FB4_14  STD  RESET
cnt/LTimer<1>                                 11    24    FB4_15  STD  RESET
cnt/WS<3>                                     3     6     FB4_16  STD  RESET
nRESout                                       1     2     FB4_17  STD  RESET
cnt/LTimerTC                                  1     12    FB5_13  STD  RESET
ALE0S                                         1     1     FB5_16  STD  RESET
cnt/LTimer<0>                                 22    34    FB5_18  STD  RESET
iobm/IOS_FSM_FFd6                             2     5     FB6_1   STD  RESET
iobm/IOS_FSM_FFd7                             3     6     FB6_3   STD  SET
iobm/IOS_FSM_FFd3                             3     5     FB6_4   STD  RESET
iobm/ES<0>                                    3     6     FB6_5   STD  RESET
iobm/ES<3>                                    4     6     FB6_6   STD  RESET
iobm/ES<1>                                    4     6     FB6_7   STD  RESET
iobm/DoutOE                                   4     8     FB6_8   STD  RESET
IODONE                                        4     8     FB6_10  STD  RESET
iobm/IOS0                                     5     12    FB6_13  STD  RESET
ALE0M                                         5     11    FB6_16  STD  RESET
IOACT                                         8     14    FB6_18  STD  RESET
cnt/LTimer<9>                                 3     15    FB7_1   STD  RESET
cnt/LTimer<8>                                 3     14    FB7_3   STD  RESET
cnt/LTimer<7>                                 3     13    FB7_4   STD  RESET
cnt/LTimer<6>                                 3     12    FB7_7   STD  RESET
cnt/LTimer<5>                                 3     11    FB7_10  STD  RESET
cnt/LTimer<4>                                 3     10    FB7_13  STD  RESET
cnt/LTimer<3>                                 3     9     FB7_14  STD  RESET

Signal                                        Total Total Loc     Pwr  Reg Init
Name                                          Pts   Inps          Mode State
cnt/LTimer<2>                                 3     8     FB7_15  STD  RESET
cnt/LTimer<11>                                3     17    FB7_16  STD  RESET
cnt/LTimer<10>                                3     16    FB7_17  STD  RESET
cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2  10    36    FB7_18  STD  
IOL0                                          16    21    FB8_1   STD  RESET
iobs/TS_FSM_FFd2                              13    19    FB8_3   STD  RESET
IOWRREQ                                       15    21    FB8_9   STD  RESET
IOU0                                          16    21    FB8_14  STD  RESET
cnt/IS_FSM_FFd1                               1     7     FB8_16  STD  RESET
iobs/IORW1                                    8     18    FB8_17  STD  RESET

** 35 Inputs **

Signal                                        Loc     Pin  Pin     Pin     
Name                                                  No.  Type    Use     
A_FSB<13>                                     FB1_2   11   I/O     I
A_FSB<14>                                     FB1_3   12   I/O     I
A_FSB<15>                                     FB1_5   13   I/O     I
A_FSB<16>                                     FB1_6   14   I/O     I
A_FSB<17>                                     FB1_8   15   I/O     I
A_FSB<18>                                     FB1_9   16   I/O     I
A_FSB<19>                                     FB1_11  17   I/O     I
A_FSB<20>                                     FB1_12  18   I/O     I
A_FSB<21>                                     FB1_14  19   I/O     I
A_FSB<22>                                     FB1_15  20   I/O     I
C16M                                          FB1_17  22   GCK/I/O GCK
A_FSB<5>                                      FB2_6   2    GTS/I/O I
A_FSB<6>                                      FB2_8   3    GTS/I/O I
A_FSB<7>                                      FB2_9   4    GTS/I/O I
A_FSB<8>                                      FB2_11  6    I/O     I
A_FSB<9>                                      FB2_12  7    I/O     I
A_FSB<10>                                     FB2_14  8    I/O     I
A_FSB<11>                                     FB2_15  9    I/O     I
A_FSB<12>                                     FB2_17  10   I/O     I
C8M                                           FB3_2   23   GCK/I/O GCK/I
A_FSB<23>                                     FB3_5   24   I/O     I
E                                             FB3_6   25   I/O     I
FCLK                                          FB3_8   27   GCK/I/O GCK
nWE_FSB                                       FB3_11  29   I/O     I
nLDS_FSB                                      FB3_12  30   I/O     I
nAS_FSB                                       FB3_14  32   I/O     I
nUDS_FSB                                      FB3_15  33   I/O     I
nIPL2                                         FB4_9   92   I/O     I
A_FSB<1>                                      FB4_12  94   I/O     I
A_FSB<2>                                      FB4_14  95   I/O     I
A_FSB<3>                                      FB4_15  96   I/O     I
A_FSB<4>                                      FB4_17  97   I/O     I
nBERR_IOB                                     FB6_5   76   I/O     I
nVPA_IOB                                      FB6_6   77   I/O     I
nDTACK_IOB                                    FB6_8   78   I/O     I

Legend:
Pin No. - ~ - User Assigned
**************************  Function Block Details  ************************
Legend:
Total Pt     - Total product terms used by the macrocell signal
Imp Pt       - Product terms imported from other macrocells
Exp Pt       - Product terms exported to other macrocells
               in direction shown
Unused Pt    - Unused local product terms remaining in macrocell
Loc          - Location where logic was mapped in device
Pin Type/Use - I  - Input             GCK - Global Clock
               O  - Output            GTS - Global Output Enable
              (b) - Buried macrocell  GSR - Global Set/Reset
X            - Signal used as input to the macrocell logic.
Pin No.      - ~  - User Assigned
*********************************** FB1  ***********************************
Number of function block inputs used/remaining:               28/26
Number of signals used by logic mapping into function block:  28
Signal              Total   Imp   Exp Unused  Loc     Pin   Pin     Pin
Name                Pt      Pt    Pt  Pt               #    Type    Use
iobs/Clear1           1       0     0   4     FB1_1         (b)     (b)
iobm/Er               1       0     0   4     FB1_2   11    I/O     I
cnt/nIPL2r            1       0     0   4     FB1_3   12    I/O     I
cnt/Er<1>             1       0     0   4     FB1_4         (b)     (b)
cnt/Er<0>             1       0     0   4     FB1_5   13    I/O     I
ram/RS_FSM_FFd4       2       0     0   3     FB1_6   14    I/O     I
iobs/TS_FSM_FFd1      2       0     0   3     FB1_7         (b)     (b)
iobs/IOU1             2       0     0   3     FB1_8   15    I/O     I
cnt/Timer<0>          2       0     0   3     FB1_9   16    I/O     I
cnt/IS_FSM_FFd2       2       0     0   3     FB1_10        (b)     (b)
RefUrg                2       0     0   3     FB1_11  17    I/O     I
RefReq                2       0     0   3     FB1_12  18    I/O     I
IOPWReady             2       0     0   3     FB1_13        (b)     (b)
IOBERR                2       0     0   3     FB1_14  19    I/O     I
iobm/ES<2>            3       0     0   2     FB1_15  20    I/O     I
cnt/Timer<1>          4       0     0   1     FB1_16        (b)     (b)
cnt/Timer<3>          5       0     0   0     FB1_17  22    GCK/I/O GCK
cnt/Timer<2>          5       0     0   0     FB1_18        (b)     (b)

Signals Used by Logic in Function Block
  1: E                 11: cnt/Timer<3>      20: iobs/TS_FSM_FFd2 
  2: RefUrg            12: iobm/ES<0>        21: nADoutLE1 
  3: cnt/Er<0>         13: iobm/ES<1>        22: nAS_IOB 
  4: cnt/Er<1>         14: iobm/ES<2>        23: nBERR_IOB 
  5: cnt/IS_FSM_FFd1   15: iobm/Er           24: nIPL2 
  6: cnt/IS_FSM_FFd2   16: iobs/Clear1       25: nUDS_FSB 
  7: cnt/LTimerTC      17: iobs/IOACTr       26: ram/RS_FSM_FFd1 
  8: cnt/Timer<0>      18: iobs/Load1        27: ram/RS_FSM_FFd5 
  9: cnt/Timer<1>      19: iobs/TS_FSM_FFd1  28: ram/RefDone 
 10: cnt/Timer<2>     

Signal                        1         2         3         4 FB
Name                0----+----0----+----0----+----0----+----0 Inputs
iobs/Clear1          ..................XX.................... 2
iobm/Er              X....................................... 1
cnt/nIPL2r           .......................X................ 1
cnt/Er<1>            ..X..................................... 1
cnt/Er<0>            X....................................... 1
ram/RS_FSM_FFd4      .X.......................XXX............ 4
iobs/TS_FSM_FFd1     ................X.XX.................... 3
iobs/IOU1            .................X......X............... 2
cnt/Timer<0>         .XXX...X................................ 4
cnt/IS_FSM_FFd2      .XXXXXX................................. 6
RefUrg               ..XX...XXXX............................. 6
RefReq               ..XX...XXXX............................. 6
IOPWReady            ...............X.X..X................... 3
IOBERR               .....................XX................. 2
iobm/ES<2>           X..........XXXX......................... 5
cnt/Timer<1>         .XXX...XX............................... 5
cnt/Timer<3>         .XXX...XXXX............................. 7
cnt/Timer<2>         .XXX...XXX.............................. 6
                    0----+----1----+----2----+----3----+----4
                              0         0         0         0
*********************************** FB2  ***********************************
Number of function block inputs used/remaining:               16/38
Number of signals used by logic mapping into function block:  16
Signal              Total   Imp   Exp Unused  Loc     Pin   Pin     Pin
Name                Pt      Pt    Pt  Pt               #    Type    Use
(unused)              0       0     0   5     FB2_1         (b)     
(unused)              0       0     0   5     FB2_2   99    GSR/I/O 
(unused)              0       0     0   5     FB2_3         (b)     
ram/RS_FSM_FFd5       1       0     0   4     FB2_4         (b)     (b)
ram/RS_FSM_FFd3       1       0     0   4     FB2_5   1     GTS/I/O (b)
ram/RS_FSM_FFd2       1       0     0   4     FB2_6   2     GTS/I/O I
ram/RS_FSM_FFd1       1       0     0   4     FB2_7         (b)     (b)
ram/RASrf             1       0     0   4     FB2_8   3     GTS/I/O I
iobs/IODONEr          1       0     0   4     FB2_9   4     GTS/I/O I
iobs/IOACTr           1       0     0   4     FB2_10        (b)     (b)
iobm/VPAr             1       0     0   4     FB2_11  6     I/O     I
iobm/IOWRREQr         1       0     0   4     FB2_12  7     I/O     I
iobm/IOS_FSM_FFd5     1       0     0   4     FB2_13        (b)     (b)
iobm/IOS_FSM_FFd4     1       0     0   4     FB2_14  8     I/O     I
iobm/IOS_FSM_FFd1     1       0     0   4     FB2_15  9     I/O     I
iobm/IORDREQr         1       0     0   4     FB2_16        (b)     (b)
iobm/C8Mr             1       0     0   4     FB2_17  10    I/O     I
iobm/IOS_FSM_FFd2     2       0     0   3     FB2_18        (b)     (b)

Signals Used by Logic in Function Block
  1: C8M                7: iobm/C8Mr          12: nVPA_IOB 
  2: IOACT              8: iobm/IOS_FSM_FFd2  13: ram/RS_FSM_FFd2 
  3: IOBERR             9: iobm/IOS_FSM_FFd3  14: ram/RS_FSM_FFd3 
  4: IODONE            10: iobm/IOS_FSM_FFd5  15: ram/RS_FSM_FFd6 
  5: IORDREQ           11: iobm/IOS_FSM_FFd6  16: ram/RS_FSM_FFd7 
  6: IOWRREQ          

Signal                        1         2         3         4 FB
Name                0----+----0----+----0----+----0----+----0 Inputs
ram/RS_FSM_FFd5      ...............X........................ 1
ram/RS_FSM_FFd3      ..............X......................... 1
ram/RS_FSM_FFd2      .............X.......................... 1
ram/RS_FSM_FFd1      ............X........................... 1
ram/RASrf            ...............X........................ 1
iobs/IODONEr         ...X.................................... 1
iobs/IOACTr          .X...................................... 1
iobm/VPAr            ...........X............................ 1
iobm/IOWRREQr        .....X.................................. 1
iobm/IOS_FSM_FFd5    ..........X............................. 1
iobm/IOS_FSM_FFd4    .........X.............................. 1
iobm/IOS_FSM_FFd1    .......X................................ 1
iobm/IORDREQr        ....X................................... 1
iobm/C8Mr            X....................................... 1
iobm/IOS_FSM_FFd2    ..XX..X.X............................... 4
                    0----+----1----+----2----+----3----+----4
                              0         0         0         0
*********************************** FB3  ***********************************
Number of function block inputs used/remaining:               39/15
Number of signals used by logic mapping into function block:  39
Signal              Total   Imp   Exp Unused  Loc     Pin   Pin     Pin
Name                Pt      Pt    Pt  Pt               #    Type    Use
iobs/Sent            13       8<-   0   0     FB3_1         (b)     (b)
ram/RefDone           2       0   /\3   0     FB3_2   23    GCK/I/O GCK/I
ram/RS_FSM_FFd7       2       0     0   3     FB3_3         (b)     (b)
cs/nOverlay           2       0     0   3     FB3_4         (b)     (b)
ram/RS_FSM_FFd6       3       0     0   2     FB3_5   24    I/O     I
ram/RASrr             4       0     0   1     FB3_6   25    I/O     I
ram/RASEL             3       0   \/2   0     FB3_7         (b)     (b)
ram/Once              3       2<- \/4   0     FB3_8   27    GCK/I/O GCK
nDTACK_FSB            9       4<-   0   0     FB3_9   28    I/O     O
RAMReady              4       0   \/1   0     FB3_10        (b)     (b)
ram/RS_FSM_FFd8       5       1<- \/1   0     FB3_11  29    I/O     I
ram/RAMEN             6       1<-   0   0     FB3_12  30    I/O     I
(unused)              0       0   \/5   0     FB3_13        (b)     (b)
ram/CAS               7       5<- \/3   0     FB3_14  32    I/O     I
iobs/Load1            8       3<-   0   0     FB3_15  33    I/O     I
IORDREQ               9       4<-   0   0     FB3_16        (b)     (b)
nROMWE                1       0   /\4   0     FB3_17  34    I/O     O
(unused)              0       0   \/5   0     FB3_18        (b)     (b)

Signals Used by Logic in Function Block
  1: A_FSB<13>         14: nRES.PIN          27: nADoutLE1 
  2: A_FSB<14>         15: QoSReady          28: nAS_FSB 
  3: A_FSB<16>         16: RAMReady          29: nWE_FSB 
  4: A_FSB<17>         17: RefReq            30: ram/Once 
  5: A_FSB<18>         18: RefUrg            31: ram/RAMEN 
  6: A_FSB<19>         19: cs/ODCSr          32: ram/RS_FSM_FFd2 
  7: A_FSB<20>         20: cs/nOverlay       33: ram/RS_FSM_FFd3 
  8: A_FSB<21>         21: fsb/ASrf          34: ram/RS_FSM_FFd4 
  9: A_FSB<22>         22: iobs/IOACTr       35: ram/RS_FSM_FFd5 
 10: A_FSB<23>         23: iobs/IORW1        36: ram/RS_FSM_FFd6 
 11: IONPReady         24: iobs/Sent         37: ram/RS_FSM_FFd7 
 12: IOPWReady         25: iobs/TS_FSM_FFd1  38: ram/RS_FSM_FFd8 
 13: IORDREQ           26: iobs/TS_FSM_FFd2  39: ram/RefDone 

Signal                        1         2         3         4 FB
Name                0----+----0----+----0----+----0----+----0 Inputs
iobs/Sent            XXXXXXXXXX.........XX..XXXXXX........... 18
ram/RefDone          ................XX.............XX.....X. 5
ram/RS_FSM_FFd7      ........XX.........XX......X..X......X.. 7
cs/nOverlay          .............X....XXX......X............ 5
ram/RS_FSM_FFd6      ................XX..X......X......X..XX. 7
ram/RASrr            ........XX.........XX......X..X.X..X.X.. 9
ram/RASEL            ........XX.........XX......X..X.....XX.. 8
ram/Once             ........XX.........XX......X.XX......X.. 8
nDTACK_FSB           XXXXXXXXXXXX..XX....X......XX........... 17
RAMReady             ...............XXX..X......X.....X...XX. 8
ram/RS_FSM_FFd8      ........XX......XX.XX......X..X..X...XX. 11
ram/RAMEN            ................XX..X......X.XX..X..XXX. 10
ram/CAS              ........XX......XX.XX......X..X...XXXXX. 13
iobs/Load1           XXXXXXXXXX..........X..XXXXXX........... 17
IORDREQ              ......XXXX..X......XXXXXXXXXX........... 15
nROMWE               ...........................XX........... 2
                    0----+----1----+----2----+----3----+----4
                              0         0         0         0
*********************************** FB4  ***********************************
Number of function block inputs used/remaining:               42/12
Number of signals used by logic mapping into function block:  42
Signal              Total   Imp   Exp Unused  Loc     Pin   Pin     Pin
Name                Pt      Pt    Pt  Pt               #    Type    Use
QoSReady             18      13<-   0   0     FB4_1         (b)     (b)
nAoutOE               2       2<- /\5   0     FB4_2   87    I/O     O
fsb/ASrf              1       0   /\2   2     FB4_3         (b)     (b)
cnt/WS<0>             1       0     0   4     FB4_4         (b)     (b)
nDoutOE               2       0     0   3     FB4_5   89    I/O     O
nDinOE                3       0     0   2     FB4_6   90    I/O     O
$OpTx$$OpTx$FX_DC$354_INV$541
                      1       0     0   4     FB4_7         (b)     (b)
nRES                  1       0     0   4     FB4_8   91    I/O     I/O
iobs/IOL1             2       0     0   3     FB4_9   92    I/O     I
cs/ODCSr              2       0     0   3     FB4_10        (b)     (b)
nVPA_FSB              3       0     0   2     FB4_11  93    I/O     O
cnt/WS<2>             3       0   \/2   0     FB4_12  94    I/O     I
cnt/WS<1>             3       2<- \/4   0     FB4_13        (b)     (b)
IONPReady             5       4<- \/4   0     FB4_14  95    I/O     I
cnt/LTimer<1>        11       6<-   0   0     FB4_15  96    I/O     I
cnt/WS<3>             3       0   /\2   0     FB4_16        (b)     (b)
nRESout               1       0   \/3   1     FB4_17  97    I/O     I
(unused)              0       0   \/5   0     FB4_18        (b)     (b)

Signals Used by Logic in Function Block
  1: $OpTx$$OpTx$FX_DC$354_INV$541  15: A_FSB<23>                                     29: fsb/ASrf 
  2: A_FSB<10>                      16: A_FSB<8>                                      30: iobm/DoutOE 
  3: A_FSB<11>                      17: A_FSB<9>                                      31: iobm/IORDREQr 
  4: A_FSB<12>                      18: IONPReady                                     32: iobm/IOS0 
  5: A_FSB<13>                      19: QoSReady                                      33: iobm/IOWRREQr 
  6: A_FSB<14>                      20: cnt/IS_FSM_FFd1                               34: iobs/IODONEr 
  7: A_FSB<15>                      21: cnt/IS_FSM_FFd2                               35: iobs/Load1 
  8: A_FSB<16>                      22: cnt/LTimer<0>                                 36: iobs/Sent 
  9: A_FSB<17>                      23: cnt/LTimer<1>                                 37: nAS_FSB 
 10: A_FSB<18>                      24: cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2  38: nAoutOE 
 11: A_FSB<19>                      25: cnt/WS<0>                                     39: nBR_IOB 
 12: A_FSB<20>                      26: cnt/WS<1>                                     40: nLDS_FSB 
 13: A_FSB<21>                      27: cnt/WS<2>                                     41: nRESout 
 14: A_FSB<22>                      28: cnt/WS<3>                                     42: nWE_FSB 

Signal                        1         2         3         4         5 FB
Name                0----+----0----+----0----+----0----+----0----+----0 Inputs
QoSReady             XXXXXXXXXXXXXXXXX.X..XX.XXXX.............X........ 25
nAoutOE              ...................XX................XX........... 4
fsb/ASrf             ....................................X............. 1
cnt/WS<0>            ........................X...X.......X............. 3
nDoutOE              .............................XXXX....X............ 5
nDinOE               ...........XXXX.....................X....X........ 6
$OpTx$$OpTx$FX_DC$354_INV$541 
                     ............................X.......X............. 2
nRES                 ........................................X......... 1
iobs/IOL1            ..................................X....X.......... 2
cs/ODCSr             ...........XXXX.............X.......X............. 6
nVPA_FSB             .......XXXXXXXX..XX.........X.......X............. 12
cnt/WS<2>            ........................XXX.X.......X............. 5
cnt/WS<1>            ........................XX..X.......X............. 4
IONPReady            ....XX.XXXXXXXX..X..........X....X.XX....X........ 16
cnt/LTimer<1>        .XXXXXXXXXXXXXXXX..XXXXX....X.......X....X........ 24
cnt/WS<3>            ........................XXXXX.......X............. 6
nRESout              ...................XX............................. 2
                    0----+----1----+----2----+----3----+----4----+----5
                              0         0         0         0         0
*********************************** FB5  ***********************************
Number of function block inputs used/remaining:               42/12
Number of signals used by logic mapping into function block:  42
Signal              Total   Imp   Exp Unused  Loc     Pin   Pin     Pin
Name                Pt      Pt    Pt  Pt               #    Type    Use
(unused)              0       0   /\5   0     FB5_1         (b)     (b)
nROMCS                2       0   /\3   0     FB5_2   35    I/O     O
(unused)              0       0     0   5     FB5_3         (b)     
(unused)              0       0     0   5     FB5_4         (b)     
nCAS                  1       0     0   4     FB5_5   36    I/O     O
nOE                   1       0     0   4     FB5_6   37    I/O     O
(unused)              0       0     0   5     FB5_7         (b)     
(unused)              0       0     0   5     FB5_8   39    I/O     
RA<4>                 2       0     0   3     FB5_9   40    I/O     O
(unused)              0       0     0   5     FB5_10        (b)     
RA<3>                 2       0     0   3     FB5_11  41    I/O     O
RA<5>                 2       0     0   3     FB5_12  42    I/O     O
cnt/LTimerTC          1       0     0   4     FB5_13        (b)     (b)
RA<2>                 2       0     0   3     FB5_14  43    I/O     O
RA<6>                 2       0     0   3     FB5_15  46    I/O     O
ALE0S                 1       0   \/4   0     FB5_16        (b)     (b)
(unused)              0       0   \/5   0     FB5_17  49    I/O     (b)
cnt/LTimer<0>        22      17<-   0   0     FB5_18        (b)     (b)

Signals Used by Logic in Function Block
  1: A_FSB<10>         15: A_FSB<3>          29: cnt/LTimer<4> 
  2: A_FSB<11>         16: A_FSB<4>          30: cnt/LTimer<5> 
  3: A_FSB<12>         17: A_FSB<5>          31: cnt/LTimer<6> 
  4: A_FSB<13>         18: A_FSB<7>          32: cnt/LTimer<7> 
  5: A_FSB<14>         19: A_FSB<8>          33: cnt/LTimer<8> 
  6: A_FSB<15>         20: A_FSB<9>          34: cnt/LTimer<9> 
  7: A_FSB<16>         21: cnt/IS_FSM_FFd1   35: cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2 
  8: A_FSB<17>         22: cnt/IS_FSM_FFd2   36: cs/nOverlay 
  9: A_FSB<18>         23: cnt/LTimer<0>     37: fsb/ASrf 
 10: A_FSB<19>         24: cnt/LTimer<10>    38: iobs/TS_FSM_FFd2 
 11: A_FSB<20>         25: cnt/LTimer<11>    39: nAS_FSB 
 12: A_FSB<21>         26: cnt/LTimer<1>     40: nWE_FSB 
 13: A_FSB<22>         27: cnt/LTimer<2>     41: ram/CAS 
 14: A_FSB<23>         28: cnt/LTimer<3>     42: ram/RASEL 

Signal                        1         2         3         4         5 FB
Name                0----+----0----+----0----+----0----+----0----+----0 Inputs
nROMCS               ..........XXXX.....................X.............. 5
nCAS                 ........................................X......... 1
nOE                  ......................................XX.......... 2
RA<4>                .X............X..........................X........ 3
RA<3>                .........XX..............................X........ 3
RA<5>                ..X............X.........................X........ 3
cnt/LTimerTC         ......................XXXXXXXXXXXX................ 12
RA<2>                ......X..........X.......................X........ 3
RA<6>                ...X............X........................X........ 3
ALE0S                .....................................X............ 1
cnt/LTimer<0>        XXXXXXXXXXXXXX....XXXXXXXXXXXXXXXXX.X.XX.......... 34
                    0----+----1----+----2----+----3----+----4----+----5
                              0         0         0         0         0
*********************************** FB6  ***********************************
Number of function block inputs used/remaining:               36/18
Number of signals used by logic mapping into function block:  36
Signal              Total   Imp   Exp Unused  Loc     Pin   Pin     Pin
Name                Pt      Pt    Pt  Pt               #    Type    Use
iobm/IOS_FSM_FFd6     2       0     0   3     FB6_1         (b)     (b)
nVMA_IOB              3       0     0   2     FB6_2   74    I/O     O
iobm/IOS_FSM_FFd7     3       0     0   2     FB6_3         (b)     (b)
iobm/IOS_FSM_FFd3     3       0     0   2     FB6_4         (b)     (b)
iobm/ES<0>            3       0     0   2     FB6_5   76    I/O     I
iobm/ES<3>            4       0     0   1     FB6_6   77    I/O     I
iobm/ES<1>            4       0     0   1     FB6_7         (b)     (b)
iobm/DoutOE           4       0   \/1   0     FB6_8   78    I/O     I
nLDS_IOB              6       1<-   0   0     FB6_9   79    I/O     O
IODONE                4       0   \/1   0     FB6_10        (b)     (b)
nUDS_IOB              6       1<-   0   0     FB6_11  80    I/O     O
nAS_IOB               4       0     0   1     FB6_12  81    I/O     O
iobm/IOS0             5       0     0   0     FB6_13        (b)     (b)
nADoutLE1             2       0     0   3     FB6_14  82    I/O     O
nADoutLE0             1       0     0   4     FB6_15  85    I/O     O
ALE0M                 5       0     0   0     FB6_16        (b)     (b)
nDinLE                1       0   \/3   1     FB6_17  86    I/O     O
IOACT                 8       3<-   0   0     FB6_18        (b)     (b)

Signals Used by Logic in Function Block
  1: ALE0M             13: iobm/ES<1>         25: iobm/IOS_FSM_FFd7 
  2: ALE0S             14: iobm/ES<2>         26: iobm/IOWRREQr 
  3: E                 15: iobm/ES<3>         27: iobm/VPAr 
  4: IOACT             16: iobm/Er            28: iobs/Clear1 
  5: IOBERR            17: iobm/IORDREQr      29: iobs/Load1 
  6: IODONE            18: iobm/IOS0          30: nADoutLE1 
  7: IOL0              19: iobm/IOS_FSM_FFd1  31: nAS_IOB 
  8: IOU0              20: iobm/IOS_FSM_FFd2  32: nAoutOE 
  9: nRES.PIN          21: iobm/IOS_FSM_FFd3  33: nDTACK_IOB 
 10: iobm/C8Mr         22: iobm/IOS_FSM_FFd4  34: nLDS_IOB 
 11: iobm/DoutOE       23: iobm/IOS_FSM_FFd5  35: nUDS_IOB 
 12: iobm/ES<0>        24: iobm/IOS_FSM_FFd6  36: nVMA_IOB 

Signal                        1         2         3         4 FB
Name                0----+----0----+----0----+----0----+----0 Inputs
iobm/IOS_FSM_FFd6    .........X......X.......XX.....X........ 5
nVMA_IOB             ...X.......XXXX...........X....X...X.... 8
iobm/IOS_FSM_FFd7    .........X......X.X.....XX.....X........ 6
iobm/IOS_FSM_FFd3    ....XX...X..........XX.................. 5
iobm/ES<0>           ..X........XXXXX........................ 6
iobm/ES<3>           ..X........XXXXX........................ 6
iobm/ES<1>           ..X........XXXXX........................ 6
iobm/DoutOE          .........XX.........XXXXXX.............. 8
nLDS_IOB             ......X..X......X...XXXXX......X.X...... 10
IODONE               ........X..XXXX...............X.X..X.... 8
nUDS_IOB             .......X.X......X...XXXXX......X..X..... 10
nAS_IOB              .........X......X...XXXXXX.....X........ 9
iobm/IOS0            .........X......XXXXXXXXXX.....X........ 12
nADoutLE1            ...........................XXX.......... 3
nADoutLE0            XX...................................... 2
ALE0M                X...............X.XXXXXXXX.....X........ 11
nDinLE               ....................XX.................. 2
IOACT                ...XXX...X......X.XXXXXXXX.....X........ 14
                    0----+----1----+----2----+----3----+----4
                              0         0         0         0
*********************************** FB7  ***********************************
Number of function block inputs used/remaining:               41/13
Number of signals used by logic mapping into function block:  41
Signal              Total   Imp   Exp Unused  Loc     Pin   Pin     Pin
Name                Pt      Pt    Pt  Pt               #    Type    Use
cnt/LTimer<9>         3       1<- /\3   0     FB7_1         (b)     (b)
RA<1>                 2       0   /\1   2     FB7_2   50    I/O     O
cnt/LTimer<8>         3       0     0   2     FB7_3         (b)     (b)
cnt/LTimer<7>         3       0     0   2     FB7_4         (b)     (b)
RA<7>                 2       0     0   3     FB7_5   52    I/O     O
RA<0>                 2       0     0   3     FB7_6   53    I/O     O
cnt/LTimer<6>         3       0     0   2     FB7_7         (b)     (b)
RA<8>                 2       0     0   3     FB7_8   54    I/O     O
RA<10>                2       0     0   3     FB7_9   55    I/O     O
cnt/LTimer<5>         3       0     0   2     FB7_10        (b)     (b)
RA<9>                 2       0     0   3     FB7_11  56    I/O     O
C25MEN                0       0     0   5     FB7_12  58    I/O     O
cnt/LTimer<4>         3       0     0   2     FB7_13        (b)     (b)
cnt/LTimer<3>         3       0     0   2     FB7_14  59    I/O     (b)
cnt/LTimer<2>         3       0     0   2     FB7_15  60    I/O     (b)
cnt/LTimer<11>        3       0     0   2     FB7_16        (b)     (b)
cnt/LTimer<10>        3       0   \/2   0     FB7_17  61    I/O     (b)
cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2
                     10       5<-   0   0     FB7_18        (b)     (b)

Signals Used by Logic in Function Block
  1: A_FSB<10>         15: A_FSB<23>         29: cnt/LTimer<1> 
  2: A_FSB<11>         16: A_FSB<2>          30: cnt/LTimer<2> 
  3: A_FSB<12>         17: A_FSB<6>          31: cnt/LTimer<3> 
  4: A_FSB<13>         18: A_FSB<7>          32: cnt/LTimer<4> 
  5: A_FSB<14>         19: A_FSB<8>          33: cnt/LTimer<5> 
  6: A_FSB<15>         20: A_FSB<9>          34: cnt/LTimer<6> 
  7: A_FSB<16>         21: RefUrg            35: cnt/LTimer<7> 
  8: A_FSB<17>         22: cnt/Er<0>         36: cnt/LTimer<8> 
  9: A_FSB<18>         23: cnt/Er<1>         37: cnt/LTimer<9> 
 10: A_FSB<19>         24: cnt/IS_FSM_FFd1   38: fsb/ASrf 
 11: A_FSB<1>          25: cnt/IS_FSM_FFd2   39: nAS_FSB 
 12: A_FSB<20>         26: cnt/LTimer<0>     40: nWE_FSB 
 13: A_FSB<21>         27: cnt/LTimer<10>    41: ram/RASEL 
 14: A_FSB<22>         28: cnt/LTimer<11>   

Signal                        1         2         3         4         5 FB
Name                0----+----0----+----0----+----0----+----0----+----0 Inputs
cnt/LTimer<9>        ....................XXXXXX..XXXXXXXXX............. 15
RA<1>                X..............X........................X......... 3
cnt/LTimer<8>        ....................XXXXXX..XXXXXXXX.............. 14
cnt/LTimer<7>        ....................XXXXXX..XXXXXXX............... 13
RA<7>                ....X...........X.......................X......... 3
RA<0>                ..........X........X....................X......... 3
cnt/LTimer<6>        ....................XXXXXX..XXXXXX................ 12
RA<8>                ........X...X...........................X......... 3
RA<10>               .......X.........X......................X......... 3
cnt/LTimer<5>        ....................XXXXXX..XXXXX................. 11
RA<9>                .....X............X.....................X......... 3
C25MEN               .................................................. 0
cnt/LTimer<4>        ....................XXXXXX..XXXX.................. 10
cnt/LTimer<3>        ....................XXXXXX..XXX................... 9
cnt/LTimer<2>        ....................XXXXXX..XX.................... 8
cnt/LTimer<11>       ....................XXXXXXXXXXXXXXXXX............. 17
cnt/LTimer<10>       ....................XXXXXXX.XXXXXXXXX............. 16
cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2 
                     XXXXXXXXXX.XXXX...XXXXXXXXXXXXXXXXXXXXXX.......... 36
                    0----+----1----+----2----+----3----+----4----+----5
                              0         0         0         0         0
*********************************** FB8  ***********************************
Number of function block inputs used/remaining:               41/13
Number of signals used by logic mapping into function block:  41
Signal              Total   Imp   Exp Unused  Loc     Pin   Pin     Pin
Name                Pt      Pt    Pt  Pt               #    Type    Use
IOL0                 16      11<-   0   0     FB8_1         (b)     (b)
RA<11>                2       2<- /\5   0     FB8_2   63    I/O     O
iobs/TS_FSM_FFd2     13      10<- /\2   0     FB8_3         (b)     (b)
(unused)              0       0   /\5   0     FB8_4         (b)     (b)
nRAS                  3       3<- /\5   0     FB8_5   64    I/O     O
nRAMLWE               1       0   /\3   1     FB8_6   65    I/O     O
(unused)              0       0   \/1   4     FB8_7         (b)     (b)
nRAMUWE               1       1<- \/5   0     FB8_8   66    I/O     O
IOWRREQ              15      10<-   0   0     FB8_9   67    I/O     (b)
(unused)              0       0   /\5   0     FB8_10        (b)     (b)
(unused)              0       0   \/1   4     FB8_11  68    I/O     (b)
nBERR_FSB             3       1<- \/3   0     FB8_12  70    I/O     O
(unused)              0       0   \/5   0     FB8_13        (b)     (b)
IOU0                 16      11<-   0   0     FB8_14  71    I/O     (b)
nBR_IOB               2       0   /\3   0     FB8_15  72    I/O     O
cnt/IS_FSM_FFd1       1       0   \/4   0     FB8_16        (b)     (b)
iobs/IORW1            8       4<- \/1   0     FB8_17  73    I/O     (b)
(unused)              0       0   \/5   0     FB8_18        (b)     (b)

Signals Used by Logic in Function Block
  1: A_FSB<13>         15: RefUrg            29: iobs/TS_FSM_FFd1 
  2: A_FSB<14>         16: cnt/Er<0>         30: iobs/TS_FSM_FFd2 
  3: A_FSB<16>         17: cnt/Er<1>         31: nADoutLE1 
  4: A_FSB<17>         18: cnt/IS_FSM_FFd1   32: nAS_FSB 
  5: A_FSB<18>         19: cnt/IS_FSM_FFd2   33: nBERR_FSB 
  6: A_FSB<19>         20: cnt/LTimerTC      34: nBR_IOB 
  7: A_FSB<20>         21: cnt/nIPL2r        35: nLDS_FSB 
  8: A_FSB<21>         22: cs/nOverlay       36: nUDS_FSB 
  9: A_FSB<22>         23: fsb/ASrf          37: nWE_FSB 
 10: A_FSB<23>         24: iobs/IOACTr       38: ram/RAMEN 
 11: IOBERR            25: iobs/IOL1         39: ram/RASEL 
 12: IOL0              26: iobs/IORW1        40: ram/RASrf 
 13: IOU0              27: iobs/IOU1         41: ram/RASrr 
 14: IOWRREQ           28: iobs/Sent        

Signal                        1         2         3         4         5 FB
Name                0----+----0----+----0----+----0----+----0----+----0 Inputs
IOL0                 XXXXXXXXXX.X.........XX.X..XXXXX..X.X............. 21
RA<11>               .....XX...............................X........... 3
iobs/TS_FSM_FFd2     XXXXXXXXXX...........XXX...XXXXX....X............. 19
nRAS                 ........XX...........X.........X.....X.XX......... 7
nRAMLWE              ...............................X..X.XX............ 4
nRAMUWE              ...............................X...XXX............ 4
IOWRREQ              XXXXXXXXXX...X.......XXX.X.XXXXX....X............. 21
nBERR_FSB            ..........X...........X....X...XX................. 5
IOU0                 XXXXXXXXXX..X........XX...XXXXXX...XX............. 21
nBR_IOB              .................XX.X............X................ 4
cnt/IS_FSM_FFd1      ..............XXXXXXX............................. 7
iobs/IORW1           XXXXXXXXXX............X..X.XXXXX....X............. 18
                    0----+----1----+----2----+----3----+----4----+----5
                              0         0         0         0         0
*******************************  Equations  ********************************

********** Mapped Logic **********


$OpTx$$OpTx$FX_DC$354_INV$541 <= (nAS_FSB AND NOT fsb/ASrf);

FDCPE_ALE0M: FDCPE port map (ALE0M,ALE0M_D,C16M,'0','0');
ALE0M_D <= ((iobm/IOS_FSM_FFd7 AND NOT iobm/IOS_FSM_FFd3 AND 
	NOT iobm/IOS_FSM_FFd4 AND NOT iobm/IOS_FSM_FFd5 AND NOT iobm/IOS_FSM_FFd6 AND nAoutOE)
	OR (NOT iobm/IOS_FSM_FFd7 AND NOT iobm/IOS_FSM_FFd3 AND 
	NOT iobm/IOS_FSM_FFd4 AND NOT iobm/IOS_FSM_FFd5 AND NOT iobm/IOS_FSM_FFd6 AND 
	iobm/IOS_FSM_FFd1)
	OR (NOT iobm/IOS_FSM_FFd7 AND NOT iobm/IOS_FSM_FFd3 AND 
	NOT iobm/IOS_FSM_FFd4 AND NOT iobm/IOS_FSM_FFd5 AND NOT iobm/IOS_FSM_FFd6 AND 
	iobm/IOS_FSM_FFd2)
	OR (NOT iobm/IOS_FSM_FFd7 AND NOT iobm/IOS_FSM_FFd3 AND 
	NOT iobm/IOS_FSM_FFd4 AND NOT iobm/IOS_FSM_FFd5 AND NOT iobm/IOS_FSM_FFd6 AND NOT ALE0M)
	OR (iobm/IOS_FSM_FFd7 AND NOT iobm/IOS_FSM_FFd3 AND 
	NOT iobm/IOS_FSM_FFd4 AND NOT iobm/IOS_FSM_FFd5 AND NOT iobm/IOS_FSM_FFd6 AND 
	NOT iobm/IORDREQr AND NOT iobm/IOWRREQr));

FDCPE_ALE0S: FDCPE port map (ALE0S,iobs/TS_FSM_FFd2,FCLK,'0','0');


C25MEN <= '1';























FDCPE_IOACT: FDCPE port map (IOACT,IOACT_D,C16M,'0','0');
IOACT_D <= ((iobm/IOS_FSM_FFd4)
	OR (iobm/IOS_FSM_FFd5)
	OR (iobm/IOS_FSM_FFd6)
	OR (NOT IOBERR AND NOT IODONE AND iobm/IOS_FSM_FFd3)
	OR (iobm/IOS_FSM_FFd7 AND iobm/IOWRREQr AND NOT nAoutOE)
	OR (NOT iobm/IOS_FSM_FFd7 AND NOT iobm/IOS_FSM_FFd3 AND IOACT AND 
	NOT iobm/IOS_FSM_FFd1 AND NOT iobm/IOS_FSM_FFd2)
	OR (iobm/IOS_FSM_FFd3 AND iobm/C8Mr)
	OR (iobm/IOS_FSM_FFd7 AND iobm/IORDREQr AND NOT nAoutOE));

FDCPE_IOBERR: FDCPE port map (IOBERR,NOT nBERR_IOB,NOT C8M,nAS_IOB,'0');

FDCPE_IODONE: FDCPE port map (IODONE,IODONE_D,NOT C8M,nAS_IOB,'0');
IODONE_D <= ((NOT nRES.PIN)
	OR (NOT nDTACK_IOB)
	OR (NOT nVMA_IOB AND NOT iobm/ES(0) AND NOT iobm/ES(2) AND NOT iobm/ES(1) AND 
	iobm/ES(3)));

FTCPE_IOL0: FTCPE port map (IOL0,IOL0_T,FCLK,'0','0');
IOL0_T <= ((iobs/TS_FSM_FFd1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT A_FSB(19) AND 
	NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT A_FSB(18) AND 
	NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT A_FSB(17) AND 
	NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT A_FSB(16) AND 
	NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(21) AND NOT A_FSB(20) AND cs/nOverlay AND 
	NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (iobs/IORW1.EXP)
	OR (NOT iobs/IOL1 AND NOT IOL0 AND NOT nADoutLE1)
	OR (nAS_FSB AND NOT iobs/TS_FSM_FFd2 AND NOT fsb/ASrf AND 
	nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT A_FSB(21) AND 
	NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT A_FSB(20) AND 
	NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND nWE_FSB AND 
	NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (iobs/Sent AND NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (nLDS_FSB AND NOT IOL0 AND nADoutLE1)
	OR (NOT nLDS_FSB AND IOL0 AND nADoutLE1)
	OR (iobs/IOL1 AND IOL0 AND NOT nADoutLE1));

FDCPE_IONPReady: FDCPE port map (IONPReady,IONPReady_D,FCLK,'0','0');
IONPReady_D <= ((NOT iobs/Sent AND NOT IONPReady)
	OR (NOT IONPReady AND NOT iobs/IODONEr)
	OR (nAS_FSB AND NOT fsb/ASrf)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(13) AND 
	NOT nWE_FSB AND NOT IONPReady)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(14) AND 
	NOT nWE_FSB AND NOT IONPReady));

FDCPE_IOPWReady: FDCPE port map (IOPWReady,IOPWReady_D,FCLK,'0','0');
IOPWReady_D <= ((iobs/Clear1)
	OR (NOT iobs/Load1 AND nADoutLE1));

FDCPE_IORDREQ: FDCPE port map (IORDREQ,IORDREQ_D,FCLK,'0','0');
IORDREQ_D <= ((NOT iobs/IORW1 AND NOT iobs/TS_FSM_FFd2 AND NOT nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT iobs/TS_FSM_FFd2 AND 
	nADoutLE1)
	OR (nAS_FSB AND NOT iobs/TS_FSM_FFd2 AND NOT fsb/ASrf AND 
	nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(21) AND NOT A_FSB(20) AND cs/nOverlay AND 
	NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (iobs/TS_FSM_FFd1 AND NOT iobs/TS_FSM_FFd2)
	OR (iobs/TS_FSM_FFd1 AND iobs/IOACTr)
	OR (iobs/TS_FSM_FFd2 AND NOT IORDREQ)
	OR (iobs/Sent AND NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (NOT nWE_FSB AND NOT iobs/TS_FSM_FFd2 AND nADoutLE1));

FTCPE_IOU0: FTCPE port map (IOU0,IOU0_T,FCLK,'0','0');
IOU0_T <= ((iobs/TS_FSM_FFd1)
	OR (nBERR_FSB_OBUF.EXP)
	OR (NOT iobs/IOU1 AND NOT IOU0 AND NOT nADoutLE1)
	OR (nAS_FSB AND NOT iobs/TS_FSM_FFd2 AND NOT fsb/ASrf AND 
	nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT A_FSB(21) AND 
	NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT A_FSB(20) AND 
	NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND nWE_FSB AND 
	NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT A_FSB(18) AND 
	NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT A_FSB(17) AND 
	NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT A_FSB(16) AND 
	NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (iobs/Sent AND NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (nUDS_FSB AND NOT IOU0 AND nADoutLE1)
	OR (NOT nUDS_FSB AND IOU0 AND nADoutLE1)
	OR (iobs/IOU1 AND IOU0 AND NOT nADoutLE1));

FDCPE_IOWRREQ: FDCPE port map (IOWRREQ,IOWRREQ_D,FCLK,'0','0');
IOWRREQ_D <= ((A_FSB(22) AND A_FSB(21) AND NOT iobs/Sent AND NOT nWE_FSB AND 
	NOT nAS_FSB AND NOT iobs/TS_FSM_FFd1 AND NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (A_FSB(22) AND A_FSB(21) AND NOT iobs/Sent AND NOT nWE_FSB AND 
	NOT iobs/TS_FSM_FFd1 AND NOT iobs/TS_FSM_FFd2 AND fsb/ASrf AND nADoutLE1)
	OR (A_FSB(22) AND A_FSB(20) AND NOT iobs/Sent AND NOT nWE_FSB AND 
	NOT nAS_FSB AND NOT iobs/TS_FSM_FFd1 AND NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (A_FSB(22) AND A_FSB(20) AND NOT iobs/Sent AND NOT nWE_FSB AND 
	NOT iobs/TS_FSM_FFd1 AND NOT iobs/TS_FSM_FFd2 AND fsb/ASrf AND nADoutLE1)
	OR (A_FSB(22) AND NOT iobs/Sent AND NOT cs/nOverlay AND NOT nWE_FSB AND 
	NOT nAS_FSB AND NOT iobs/TS_FSM_FFd1 AND NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (A_FSB(22) AND NOT iobs/Sent AND NOT cs/nOverlay AND NOT nWE_FSB AND 
	NOT iobs/TS_FSM_FFd1 AND NOT iobs/TS_FSM_FFd2 AND fsb/ASrf AND nADoutLE1)
	OR (A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND A_FSB(18) AND 
	A_FSB(17) AND A_FSB(16) AND A_FSB(13) AND NOT iobs/Sent AND NOT nWE_FSB AND 
	NOT nAS_FSB AND NOT iobs/TS_FSM_FFd1 AND NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND A_FSB(18) AND 
	A_FSB(17) AND A_FSB(16) AND A_FSB(13) AND NOT iobs/Sent AND NOT nWE_FSB AND 
	NOT iobs/TS_FSM_FFd1 AND NOT iobs/TS_FSM_FFd2 AND fsb/ASrf AND nADoutLE1)
	OR (A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND A_FSB(18) AND 
	A_FSB(17) AND A_FSB(16) AND A_FSB(14) AND NOT iobs/Sent AND NOT nWE_FSB AND 
	NOT nAS_FSB AND NOT iobs/TS_FSM_FFd1 AND NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND A_FSB(18) AND 
	A_FSB(17) AND A_FSB(16) AND A_FSB(14) AND NOT iobs/Sent AND NOT nWE_FSB AND 
	NOT iobs/TS_FSM_FFd1 AND NOT iobs/TS_FSM_FFd2 AND fsb/ASrf AND nADoutLE1)
	OR (NOT iobs/TS_FSM_FFd1 AND iobs/TS_FSM_FFd2 AND IOWRREQ)
	OR (iobs/TS_FSM_FFd2 AND NOT iobs/IOACTr AND IOWRREQ)
	OR (NOT iobs/IORW1 AND NOT iobs/TS_FSM_FFd1 AND NOT iobs/TS_FSM_FFd2 AND 
	NOT nADoutLE1)
	OR (A_FSB(23) AND NOT iobs/Sent AND NOT nWE_FSB AND NOT nAS_FSB AND 
	NOT iobs/TS_FSM_FFd1 AND NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (A_FSB(23) AND NOT iobs/Sent AND NOT nWE_FSB AND 
	NOT iobs/TS_FSM_FFd1 AND NOT iobs/TS_FSM_FFd2 AND fsb/ASrf AND nADoutLE1));

FDCPE_QoSReady: FDCPE port map (QoSReady,QoSReady_D,FCLK,'0','0');
QoSReady_D <= ((A_FSB(22) AND NOT A_FSB(17) AND 
	NOT $OpTx$$OpTx$FX_DC$354_INV$541)
	OR (A_FSB(22) AND NOT A_FSB(16) AND 
	NOT $OpTx$$OpTx$FX_DC$354_INV$541)
	OR (A_FSB(22) AND NOT A_FSB(13) AND 
	NOT $OpTx$$OpTx$FX_DC$354_INV$541)
	OR (A_FSB(22) AND NOT A_FSB(14) AND 
	NOT $OpTx$$OpTx$FX_DC$354_INV$541)
	OR (A_FSB(22) AND NOT A_FSB(10) AND 
	NOT $OpTx$$OpTx$FX_DC$354_INV$541)
	OR (nRESout.EXP)
	OR (A_FSB(22) AND A_FSB(21) AND 
	NOT $OpTx$$OpTx$FX_DC$354_INV$541)
	OR (A_FSB(22) AND A_FSB(19) AND 
	NOT $OpTx$$OpTx$FX_DC$354_INV$541)
	OR (A_FSB(22) AND A_FSB(18) AND 
	NOT $OpTx$$OpTx$FX_DC$354_INV$541)
	OR (A_FSB(22) AND A_FSB(15) AND 
	NOT $OpTx$$OpTx$FX_DC$354_INV$541)
	OR (A_FSB(22) AND A_FSB(12) AND 
	NOT $OpTx$$OpTx$FX_DC$354_INV$541)
	OR (A_FSB(23) AND NOT $OpTx$$OpTx$FX_DC$354_INV$541)
	OR (NOT cnt/LTimer(0) AND NOT cnt/LTimer(1))
	OR (NOT nWE_FSB AND NOT $OpTx$$OpTx$FX_DC$354_INV$541)
	OR (QoSReady AND NOT $OpTx$$OpTx$FX_DC$354_INV$541)
	OR (A_FSB(22) AND A_FSB(20) AND 
	NOT $OpTx$$OpTx$FX_DC$354_INV$541));


RA(0) <= ((ram/RASEL AND A_FSB(1))
	OR (NOT ram/RASEL AND A_FSB(9)));


RA(1) <= ((A_FSB(10) AND NOT ram/RASEL)
	OR (ram/RASEL AND A_FSB(2)));


RA(2) <= ((A_FSB(16) AND NOT ram/RASEL)
	OR (ram/RASEL AND A_FSB(7)));


RA(3) <= ((A_FSB(20) AND ram/RASEL)
	OR (A_FSB(19) AND NOT ram/RASEL));


RA(4) <= ((A_FSB(11) AND NOT ram/RASEL)
	OR (ram/RASEL AND A_FSB(3)));


RA(5) <= ((A_FSB(12) AND NOT ram/RASEL)
	OR (ram/RASEL AND A_FSB(4)));


RA(6) <= ((A_FSB(13) AND NOT ram/RASEL)
	OR (ram/RASEL AND A_FSB(5)));


RA(7) <= ((A_FSB(14) AND NOT ram/RASEL)
	OR (ram/RASEL AND A_FSB(6)));


RA(8) <= ((A_FSB(21) AND ram/RASEL)
	OR (A_FSB(18) AND NOT ram/RASEL));


RA(9) <= ((A_FSB(15) AND NOT ram/RASEL)
	OR (ram/RASEL AND A_FSB(8)));


RA(10) <= ((A_FSB(17) AND NOT ram/RASEL)
	OR (ram/RASEL AND A_FSB(7)));


RA(11) <= ((A_FSB(20) AND ram/RASEL)
	OR (A_FSB(19) AND NOT ram/RASEL));

FDCPE_RAMReady: FDCPE port map (RAMReady,RAMReady_D,FCLK,'0','0');
RAMReady_D <= ((NOT ram/RS_FSM_FFd8 AND NOT ram/RS_FSM_FFd4 AND NOT RAMReady)
	OR (nAS_FSB AND NOT ram/RS_FSM_FFd8 AND NOT ram/RS_FSM_FFd4 AND 
	NOT fsb/ASrf)
	OR (RefUrg AND NOT ram/RefDone AND nAS_FSB AND 
	NOT ram/RS_FSM_FFd4 AND NOT fsb/ASrf)
	OR (NOT ram/RefDone AND RefReq AND nAS_FSB AND 
	NOT ram/RS_FSM_FFd4 AND NOT fsb/ASrf));

FDCPE_RefReq: FDCPE port map (RefReq,RefReq_D,FCLK,'0','0',RefReq_CE);
RefReq_D <= (NOT cnt/Timer(0) AND cnt/Timer(1) AND NOT cnt/Timer(2) AND 
	cnt/Timer(3));
RefReq_CE <= (NOT cnt/Er(0) AND cnt/Er(1));

FDCPE_RefUrg: FDCPE port map (RefUrg,RefUrg_D,FCLK,'0','0',RefUrg_CE);
RefUrg_D <= (cnt/Timer(0) AND NOT cnt/Timer(1) AND NOT cnt/Timer(2) AND 
	cnt/Timer(3));
RefUrg_CE <= (NOT cnt/Er(0) AND cnt/Er(1));

FDCPE_cnt/Er0: FDCPE port map (cnt/Er(0),E,FCLK,'0','0');

FDCPE_cnt/Er1: FDCPE port map (cnt/Er(1),cnt/Er(0),FCLK,'0','0');

FTCPE_cnt/IS_FSM_FFd1: FTCPE port map (cnt/IS_FSM_FFd1,cnt/IS_FSM_FFd1_T,FCLK,'0','0');
cnt/IS_FSM_FFd1_T <= (RefUrg AND NOT cnt/IS_FSM_FFd1 AND cnt/IS_FSM_FFd2 AND 
	NOT cnt/Er(0) AND cnt/nIPL2r AND cnt/Er(1) AND cnt/LTimerTC);

FTCPE_cnt/IS_FSM_FFd2: FTCPE port map (cnt/IS_FSM_FFd2,cnt/IS_FSM_FFd2_T,FCLK,'0','0');
cnt/IS_FSM_FFd2_T <= ((RefUrg AND cnt/IS_FSM_FFd1 AND cnt/IS_FSM_FFd2 AND 
	NOT cnt/Er(0) AND cnt/Er(1) AND cnt/LTimerTC)
	OR (RefUrg AND NOT cnt/IS_FSM_FFd1 AND NOT cnt/IS_FSM_FFd2 AND 
	NOT cnt/Er(0) AND cnt/Er(1) AND cnt/LTimerTC));

FDCPE_cnt/LTimer0: FDCPE port map (cnt/LTimer(0),cnt/LTimer_D(0),FCLK,'0','0');
cnt/LTimer_D(0) <= ((nROMCS_OBUF.EXP)
	OR (NOT cnt/LTimer(0) AND cnt/LTimer(10) AND 
	cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2)
	OR (NOT cnt/LTimer(0) AND cnt/LTimer(8) AND 
	cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2)
	OR (NOT cnt/LTimer(0) AND cnt/LTimer(9) AND 
	cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2)
	OR (NOT cnt/LTimer(0) AND cnt/LTimer(11) AND 
	cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(15) AND 
	A_FSB(13) AND A_FSB(12) AND A_FSB(14) AND A_FSB(11) AND A_FSB(10) AND 
	NOT nWE_FSB AND NOT nAS_FSB AND cnt/IS_FSM_FFd1 AND NOT cnt/IS_FSM_FFd2 AND 
	A_FSB(8) AND cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2)
	OR (ALE0S.EXP)
	OR (NOT cnt/LTimer(0) AND cnt/LTimer(3) AND 
	cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2)
	OR (NOT cnt/LTimer(0) AND cnt/LTimer(4) AND 
	cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2)
	OR (NOT cnt/LTimer(0) AND cnt/LTimer(5) AND 
	cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2)
	OR (NOT cnt/LTimer(0) AND cnt/LTimer(6) AND 
	cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2)
	OR (NOT cnt/LTimer(0) AND cnt/LTimer(7) AND 
	cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2)
	OR (cnt/LTimer(0) AND 
	NOT cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2)
	OR (NOT cnt/LTimer(0) AND cnt/LTimer(1) AND 
	cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2)
	OR (NOT cnt/LTimer(0) AND cnt/LTimer(2) AND 
	cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2)
	OR (NOT cnt/LTimer(0) AND NOT cnt/IS_FSM_FFd1 AND 
	cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2)
	OR (NOT cnt/LTimer(0) AND cnt/IS_FSM_FFd2 AND 
	cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2));

FDCPE_cnt/LTimer1: FDCPE port map (cnt/LTimer(1),cnt/LTimer_D(1),FCLK,'0','0');
cnt/LTimer_D(1) <= ((NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(15) AND 
	A_FSB(13) AND A_FSB(12) AND A_FSB(14) AND A_FSB(11) AND A_FSB(10) AND 
	NOT nWE_FSB AND NOT nAS_FSB AND cnt/IS_FSM_FFd1 AND NOT cnt/IS_FSM_FFd2 AND 
	A_FSB(9) AND cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(15) AND 
	A_FSB(13) AND A_FSB(12) AND A_FSB(14) AND A_FSB(11) AND A_FSB(10) AND 
	NOT nWE_FSB AND cnt/IS_FSM_FFd1 AND NOT cnt/IS_FSM_FFd2 AND A_FSB(8) AND 
	fsb/ASrf AND cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(15) AND 
	A_FSB(13) AND NOT A_FSB(12) AND NOT A_FSB(14) AND NOT A_FSB(11) AND NOT A_FSB(10) AND 
	NOT nWE_FSB AND NOT nAS_FSB AND cnt/IS_FSM_FFd1 AND NOT cnt/IS_FSM_FFd2 AND 
	A_FSB(9) AND cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(15) AND 
	A_FSB(13) AND NOT A_FSB(12) AND NOT A_FSB(14) AND NOT A_FSB(11) AND NOT A_FSB(10) AND 
	NOT nWE_FSB AND cnt/IS_FSM_FFd1 AND NOT cnt/IS_FSM_FFd2 AND A_FSB(8) AND 
	fsb/ASrf AND cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(15) AND 
	A_FSB(13) AND A_FSB(12) AND A_FSB(14) AND A_FSB(11) AND A_FSB(10) AND 
	NOT nWE_FSB AND cnt/IS_FSM_FFd1 AND NOT cnt/IS_FSM_FFd2 AND A_FSB(9) AND 
	fsb/ASrf AND cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(15) AND 
	A_FSB(13) AND NOT A_FSB(12) AND NOT A_FSB(14) AND NOT A_FSB(11) AND NOT A_FSB(10) AND 
	NOT nWE_FSB AND cnt/IS_FSM_FFd1 AND NOT cnt/IS_FSM_FFd2 AND A_FSB(9) AND 
	fsb/ASrf AND cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2)
	OR (NOT cnt/LTimer(0) AND NOT cnt/LTimer(1))
	OR (NOT cnt/LTimer(1) AND 
	NOT cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2)
	OR (cnt/LTimer(0) AND cnt/LTimer(1) AND 
	cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(15) AND 
	A_FSB(13) AND A_FSB(12) AND A_FSB(14) AND A_FSB(11) AND A_FSB(10) AND 
	NOT nWE_FSB AND NOT nAS_FSB AND cnt/IS_FSM_FFd1 AND NOT cnt/IS_FSM_FFd2 AND 
	A_FSB(8) AND cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(15) AND 
	A_FSB(13) AND NOT A_FSB(12) AND NOT A_FSB(14) AND NOT A_FSB(11) AND NOT A_FSB(10) AND 
	NOT nWE_FSB AND NOT nAS_FSB AND cnt/IS_FSM_FFd1 AND NOT cnt/IS_FSM_FFd2 AND 
	A_FSB(8) AND cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2));

FTCPE_cnt/LTimer2: FTCPE port map (cnt/LTimer(2),cnt/LTimer_T(2),FCLK,'0','0');
cnt/LTimer_T(2) <= ((cnt/LTimer(2) AND cnt/IS_FSM_FFd1 AND 
	NOT cnt/IS_FSM_FFd2)
	OR (RefUrg AND cnt/LTimer(0) AND cnt/LTimer(1) AND 
	NOT cnt/IS_FSM_FFd1 AND NOT cnt/Er(0) AND cnt/Er(1))
	OR (RefUrg AND cnt/LTimer(0) AND cnt/LTimer(1) AND 
	cnt/IS_FSM_FFd2 AND NOT cnt/Er(0) AND cnt/Er(1)));

FTCPE_cnt/LTimer3: FTCPE port map (cnt/LTimer(3),cnt/LTimer_T(3),FCLK,'0','0');
cnt/LTimer_T(3) <= ((cnt/LTimer(3) AND cnt/IS_FSM_FFd1 AND 
	NOT cnt/IS_FSM_FFd2)
	OR (RefUrg AND cnt/LTimer(0) AND cnt/LTimer(1) AND 
	cnt/LTimer(2) AND NOT cnt/IS_FSM_FFd1 AND NOT cnt/Er(0) AND cnt/Er(1))
	OR (RefUrg AND cnt/LTimer(0) AND cnt/LTimer(1) AND 
	cnt/LTimer(2) AND cnt/IS_FSM_FFd2 AND NOT cnt/Er(0) AND cnt/Er(1)));

FTCPE_cnt/LTimer4: FTCPE port map (cnt/LTimer(4),cnt/LTimer_T(4),FCLK,'0','0');
cnt/LTimer_T(4) <= ((cnt/LTimer(4) AND cnt/IS_FSM_FFd1 AND 
	NOT cnt/IS_FSM_FFd2)
	OR (RefUrg AND cnt/LTimer(0) AND cnt/LTimer(1) AND 
	cnt/LTimer(2) AND cnt/LTimer(3) AND NOT cnt/IS_FSM_FFd1 AND NOT cnt/Er(0) AND 
	cnt/Er(1))
	OR (RefUrg AND cnt/LTimer(0) AND cnt/LTimer(1) AND 
	cnt/LTimer(2) AND cnt/LTimer(3) AND cnt/IS_FSM_FFd2 AND NOT cnt/Er(0) AND 
	cnt/Er(1)));

FTCPE_cnt/LTimer5: FTCPE port map (cnt/LTimer(5),cnt/LTimer_T(5),FCLK,'0','0');
cnt/LTimer_T(5) <= ((cnt/LTimer(5) AND cnt/IS_FSM_FFd1 AND 
	NOT cnt/IS_FSM_FFd2)
	OR (RefUrg AND cnt/LTimer(0) AND cnt/LTimer(1) AND 
	cnt/LTimer(2) AND cnt/LTimer(3) AND cnt/LTimer(4) AND NOT cnt/IS_FSM_FFd1 AND 
	NOT cnt/Er(0) AND cnt/Er(1))
	OR (RefUrg AND cnt/LTimer(0) AND cnt/LTimer(1) AND 
	cnt/LTimer(2) AND cnt/LTimer(3) AND cnt/LTimer(4) AND cnt/IS_FSM_FFd2 AND 
	NOT cnt/Er(0) AND cnt/Er(1)));

FTCPE_cnt/LTimer6: FTCPE port map (cnt/LTimer(6),cnt/LTimer_T(6),FCLK,'0','0');
cnt/LTimer_T(6) <= ((cnt/LTimer(6) AND cnt/IS_FSM_FFd1 AND 
	NOT cnt/IS_FSM_FFd2)
	OR (RefUrg AND cnt/LTimer(0) AND cnt/LTimer(1) AND 
	cnt/LTimer(2) AND cnt/LTimer(3) AND cnt/LTimer(4) AND cnt/LTimer(5) AND 
	NOT cnt/IS_FSM_FFd1 AND NOT cnt/Er(0) AND cnt/Er(1))
	OR (RefUrg AND cnt/LTimer(0) AND cnt/LTimer(1) AND 
	cnt/LTimer(2) AND cnt/LTimer(3) AND cnt/LTimer(4) AND cnt/LTimer(5) AND 
	cnt/IS_FSM_FFd2 AND NOT cnt/Er(0) AND cnt/Er(1)));

FTCPE_cnt/LTimer7: FTCPE port map (cnt/LTimer(7),cnt/LTimer_T(7),FCLK,'0','0');
cnt/LTimer_T(7) <= ((cnt/LTimer(7) AND cnt/IS_FSM_FFd1 AND 
	NOT cnt/IS_FSM_FFd2)
	OR (RefUrg AND cnt/LTimer(0) AND cnt/LTimer(1) AND 
	cnt/LTimer(2) AND cnt/LTimer(3) AND cnt/LTimer(4) AND cnt/LTimer(5) AND 
	cnt/LTimer(6) AND NOT cnt/IS_FSM_FFd1 AND NOT cnt/Er(0) AND cnt/Er(1))
	OR (RefUrg AND cnt/LTimer(0) AND cnt/LTimer(1) AND 
	cnt/LTimer(2) AND cnt/LTimer(3) AND cnt/LTimer(4) AND cnt/LTimer(5) AND 
	cnt/LTimer(6) AND cnt/IS_FSM_FFd2 AND NOT cnt/Er(0) AND cnt/Er(1)));

FTCPE_cnt/LTimer8: FTCPE port map (cnt/LTimer(8),cnt/LTimer_T(8),FCLK,'0','0');
cnt/LTimer_T(8) <= ((cnt/LTimer(8) AND cnt/IS_FSM_FFd1 AND 
	NOT cnt/IS_FSM_FFd2)
	OR (RefUrg AND cnt/LTimer(0) AND cnt/LTimer(1) AND 
	cnt/LTimer(2) AND cnt/LTimer(3) AND cnt/LTimer(4) AND cnt/LTimer(5) AND 
	cnt/LTimer(6) AND cnt/LTimer(7) AND NOT cnt/IS_FSM_FFd1 AND NOT cnt/Er(0) AND 
	cnt/Er(1))
	OR (RefUrg AND cnt/LTimer(0) AND cnt/LTimer(1) AND 
	cnt/LTimer(2) AND cnt/LTimer(3) AND cnt/LTimer(4) AND cnt/LTimer(5) AND 
	cnt/LTimer(6) AND cnt/LTimer(7) AND cnt/IS_FSM_FFd2 AND NOT cnt/Er(0) AND 
	cnt/Er(1)));

FTCPE_cnt/LTimer9: FTCPE port map (cnt/LTimer(9),cnt/LTimer_T(9),FCLK,'0','0');
cnt/LTimer_T(9) <= ((RefUrg AND cnt/LTimer(0) AND cnt/LTimer(1) AND 
	cnt/LTimer(2) AND cnt/LTimer(3) AND cnt/LTimer(4) AND cnt/LTimer(5) AND 
	cnt/LTimer(6) AND cnt/LTimer(7) AND cnt/LTimer(8) AND cnt/IS_FSM_FFd2 AND 
	NOT cnt/Er(0) AND cnt/Er(1))
	OR (cnt/LTimer(9) AND cnt/IS_FSM_FFd1 AND 
	NOT cnt/IS_FSM_FFd2)
	OR (RefUrg AND cnt/LTimer(0) AND cnt/LTimer(1) AND 
	cnt/LTimer(2) AND cnt/LTimer(3) AND cnt/LTimer(4) AND cnt/LTimer(5) AND 
	cnt/LTimer(6) AND cnt/LTimer(7) AND cnt/LTimer(8) AND NOT cnt/IS_FSM_FFd1 AND 
	NOT cnt/Er(0) AND cnt/Er(1)));

FTCPE_cnt/LTimer10: FTCPE port map (cnt/LTimer(10),cnt/LTimer_T(10),FCLK,'0','0');
cnt/LTimer_T(10) <= ((cnt/LTimer(10) AND cnt/IS_FSM_FFd1 AND 
	NOT cnt/IS_FSM_FFd2)
	OR (RefUrg AND cnt/LTimer(0) AND cnt/LTimer(1) AND 
	cnt/LTimer(2) AND cnt/LTimer(3) AND cnt/LTimer(4) AND cnt/LTimer(5) AND 
	cnt/LTimer(6) AND cnt/LTimer(7) AND cnt/LTimer(8) AND cnt/LTimer(9) AND 
	NOT cnt/IS_FSM_FFd1 AND NOT cnt/Er(0) AND cnt/Er(1))
	OR (RefUrg AND cnt/LTimer(0) AND cnt/LTimer(1) AND 
	cnt/LTimer(2) AND cnt/LTimer(3) AND cnt/LTimer(4) AND cnt/LTimer(5) AND 
	cnt/LTimer(6) AND cnt/LTimer(7) AND cnt/LTimer(8) AND cnt/LTimer(9) AND 
	cnt/IS_FSM_FFd2 AND NOT cnt/Er(0) AND cnt/Er(1)));

FTCPE_cnt/LTimer11: FTCPE port map (cnt/LTimer(11),cnt/LTimer_T(11),FCLK,'0','0');
cnt/LTimer_T(11) <= ((cnt/LTimer(11) AND cnt/IS_FSM_FFd1 AND 
	NOT cnt/IS_FSM_FFd2)
	OR (RefUrg AND cnt/LTimer(0) AND cnt/LTimer(1) AND 
	cnt/LTimer(10) AND cnt/LTimer(2) AND cnt/LTimer(3) AND cnt/LTimer(4) AND 
	cnt/LTimer(5) AND cnt/LTimer(6) AND cnt/LTimer(7) AND cnt/LTimer(8) AND 
	cnt/LTimer(9) AND NOT cnt/IS_FSM_FFd1 AND NOT cnt/Er(0) AND cnt/Er(1))
	OR (RefUrg AND cnt/LTimer(0) AND cnt/LTimer(1) AND 
	cnt/LTimer(10) AND cnt/LTimer(2) AND cnt/LTimer(3) AND cnt/LTimer(4) AND 
	cnt/LTimer(5) AND cnt/LTimer(6) AND cnt/LTimer(7) AND cnt/LTimer(8) AND 
	cnt/LTimer(9) AND cnt/IS_FSM_FFd2 AND NOT cnt/Er(0) AND cnt/Er(1)));

FDCPE_cnt/LTimerTC: FDCPE port map (cnt/LTimerTC,cnt/LTimerTC_D,FCLK,'0','0');
cnt/LTimerTC_D <= (NOT cnt/LTimer(0) AND cnt/LTimer(1) AND cnt/LTimer(10) AND 
	cnt/LTimer(2) AND cnt/LTimer(3) AND cnt/LTimer(4) AND cnt/LTimer(5) AND 
	cnt/LTimer(6) AND cnt/LTimer(7) AND cnt/LTimer(8) AND cnt/LTimer(9) AND 
	cnt/LTimer(11));


cnt/LTimer_1_not0001/cnt/LTimer_1_not0001_D2 <= ((NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(15) AND 
	A_FSB(13) AND A_FSB(12) AND A_FSB(14) AND A_FSB(11) AND A_FSB(10) AND 
	NOT nWE_FSB AND cnt/IS_FSM_FFd1 AND NOT cnt/IS_FSM_FFd2 AND A_FSB(9) AND 
	fsb/ASrf)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(15) AND 
	A_FSB(13) AND NOT A_FSB(12) AND NOT A_FSB(14) AND NOT A_FSB(11) AND NOT A_FSB(10) AND 
	NOT nWE_FSB AND cnt/IS_FSM_FFd1 AND NOT cnt/IS_FSM_FFd2 AND A_FSB(9) AND 
	fsb/ASrf)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(15) AND 
	A_FSB(13) AND NOT A_FSB(12) AND NOT A_FSB(14) AND NOT A_FSB(11) AND NOT A_FSB(10) AND 
	NOT nWE_FSB AND cnt/IS_FSM_FFd1 AND NOT cnt/IS_FSM_FFd2 AND A_FSB(8) AND 
	fsb/ASrf)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(15) AND 
	A_FSB(13) AND A_FSB(12) AND A_FSB(14) AND A_FSB(11) AND A_FSB(10) AND 
	NOT nWE_FSB AND cnt/IS_FSM_FFd1 AND NOT cnt/IS_FSM_FFd2 AND A_FSB(8) AND 
	fsb/ASrf)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(15) AND 
	A_FSB(13) AND NOT A_FSB(12) AND NOT A_FSB(14) AND NOT A_FSB(11) AND NOT A_FSB(10) AND 
	NOT nWE_FSB AND NOT nAS_FSB AND cnt/IS_FSM_FFd1 AND NOT cnt/IS_FSM_FFd2 AND 
	A_FSB(9))
	OR (RefUrg AND NOT cnt/Er(0) AND cnt/Er(1))
	OR (NOT cnt/LTimer(0) AND NOT cnt/LTimer(1) AND NOT cnt/LTimer(10) AND 
	NOT cnt/LTimer(2) AND NOT cnt/LTimer(3) AND NOT cnt/LTimer(4) AND NOT cnt/LTimer(5) AND 
	NOT cnt/LTimer(6) AND NOT cnt/LTimer(7) AND NOT cnt/LTimer(8) AND NOT cnt/LTimer(9) AND 
	NOT cnt/LTimer(11) AND cnt/IS_FSM_FFd1 AND NOT cnt/IS_FSM_FFd2)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(15) AND 
	A_FSB(13) AND A_FSB(12) AND A_FSB(14) AND A_FSB(11) AND A_FSB(10) AND 
	NOT nWE_FSB AND NOT nAS_FSB AND cnt/IS_FSM_FFd1 AND NOT cnt/IS_FSM_FFd2 AND 
	A_FSB(9))
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(15) AND 
	A_FSB(13) AND A_FSB(12) AND A_FSB(14) AND A_FSB(11) AND A_FSB(10) AND 
	NOT nWE_FSB AND NOT nAS_FSB AND cnt/IS_FSM_FFd1 AND NOT cnt/IS_FSM_FFd2 AND 
	A_FSB(8))
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(15) AND 
	A_FSB(13) AND NOT A_FSB(12) AND NOT A_FSB(14) AND NOT A_FSB(11) AND NOT A_FSB(10) AND 
	NOT nWE_FSB AND NOT nAS_FSB AND cnt/IS_FSM_FFd1 AND NOT cnt/IS_FSM_FFd2 AND 
	A_FSB(8)));

FTCPE_cnt/Timer0: FTCPE port map (cnt/Timer(0),cnt/Timer_T(0),FCLK,'0','0',cnt/Timer_CE(0));
cnt/Timer_T(0) <= (RefUrg AND NOT cnt/Timer(0) AND NOT cnt/Er(0) AND cnt/Er(1));
cnt/Timer_CE(0) <= (NOT cnt/Er(0) AND cnt/Er(1));

FDCPE_cnt/Timer1: FDCPE port map (cnt/Timer(1),cnt/Timer_D(1),FCLK,'0','0',cnt/Timer_CE(1));
cnt/Timer_D(1) <= ((cnt/Timer(0) AND cnt/Timer(1))
	OR (NOT cnt/Timer(0) AND NOT cnt/Timer(1))
	OR (RefUrg AND NOT cnt/Er(0) AND cnt/Er(1)));
cnt/Timer_CE(1) <= (NOT cnt/Er(0) AND cnt/Er(1));

FDCPE_cnt/Timer2: FDCPE port map (cnt/Timer(2),cnt/Timer_D(2),FCLK,'0','0',cnt/Timer_CE(2));
cnt/Timer_D(2) <= ((NOT cnt/Timer(0) AND NOT cnt/Timer(2))
	OR (NOT cnt/Timer(1) AND NOT cnt/Timer(2))
	OR (RefUrg AND NOT cnt/Er(0) AND cnt/Er(1))
	OR (cnt/Timer(0) AND cnt/Timer(1) AND cnt/Timer(2)));
cnt/Timer_CE(2) <= (NOT cnt/Er(0) AND cnt/Er(1));

FTCPE_cnt/Timer3: FTCPE port map (cnt/Timer(3),cnt/Timer_T(3),FCLK,'0','0',cnt/Timer_CE(3));
cnt/Timer_T(3) <= ((RefUrg AND cnt/Timer(3) AND NOT cnt/Er(0) AND cnt/Er(1))
	OR (NOT RefUrg AND cnt/Timer(0) AND cnt/Timer(1) AND 
	cnt/Timer(2))
	OR (cnt/Timer(0) AND cnt/Timer(1) AND cnt/Timer(2) AND 
	cnt/Er(0))
	OR (cnt/Timer(0) AND cnt/Timer(1) AND cnt/Timer(2) AND 
	NOT cnt/Er(1)));
cnt/Timer_CE(3) <= (NOT cnt/Er(0) AND cnt/Er(1));

FTCPE_cnt/WS0: FTCPE port map (cnt/WS(0),cnt/WS_T(0),FCLK,'0','0');
cnt/WS_T(0) <= (nAS_FSB AND NOT cnt/WS(0) AND NOT fsb/ASrf);

FDCPE_cnt/WS1: FDCPE port map (cnt/WS(1),cnt/WS_D(1),FCLK,'0','0');
cnt/WS_D(1) <= ((nAS_FSB AND NOT fsb/ASrf)
	OR (NOT cnt/WS(0) AND NOT cnt/WS(1))
	OR (cnt/WS(0) AND cnt/WS(1)));

FTCPE_cnt/WS2: FTCPE port map (cnt/WS(2),cnt/WS_T(2),FCLK,'0','0');
cnt/WS_T(2) <= ((nAS_FSB AND cnt/WS(2) AND NOT fsb/ASrf)
	OR (NOT nAS_FSB AND cnt/WS(0) AND cnt/WS(1))
	OR (cnt/WS(0) AND cnt/WS(1) AND fsb/ASrf));

FTCPE_cnt/WS3: FTCPE port map (cnt/WS(3),cnt/WS_T(3),FCLK,'0','0');
cnt/WS_T(3) <= ((nAS_FSB AND cnt/WS(3) AND NOT fsb/ASrf)
	OR (NOT nAS_FSB AND cnt/WS(0) AND cnt/WS(1) AND cnt/WS(2))
	OR (cnt/WS(0) AND cnt/WS(1) AND cnt/WS(2) AND fsb/ASrf));

FDCPE_cnt/nIPL2r: FDCPE port map (cnt/nIPL2r,nIPL2,FCLK,'0','0');

FDCPE_cs/ODCSr: FDCPE port map (cs/ODCSr,cs/ODCSr_D,FCLK,'0','0');
cs/ODCSr_D <= ((NOT A_FSB(23) AND A_FSB(22) AND NOT A_FSB(21) AND NOT A_FSB(20) AND 
	NOT nAS_FSB)
	OR (NOT A_FSB(23) AND A_FSB(22) AND NOT A_FSB(21) AND NOT A_FSB(20) AND 
	fsb/ASrf));

FTCPE_cs/nOverlay: FTCPE port map (cs/nOverlay,cs/nOverlay_T,FCLK,'0','0');
cs/nOverlay_T <= ((NOT nRES.PIN AND cs/nOverlay AND nAS_FSB AND NOT fsb/ASrf)
	OR (nRES.PIN AND NOT cs/nOverlay AND nAS_FSB AND cs/ODCSr AND 
	NOT fsb/ASrf));

FDCPE_fsb/ASrf: FDCPE port map (fsb/ASrf,NOT nAS_FSB,NOT FCLK,'0','0');

FDCPE_iobm/C8Mr: FDCPE port map (iobm/C8Mr,C8M,C16M,'0','0');

FTCPE_iobm/DoutOE: FTCPE port map (iobm/DoutOE,iobm/DoutOE_T,C16M,'0','0');
iobm/DoutOE_T <= ((iobm/IOS_FSM_FFd7 AND NOT iobm/C8Mr AND NOT iobm/DoutOE AND 
	iobm/IOWRREQr)
	OR (NOT iobm/IOS_FSM_FFd7 AND NOT iobm/IOS_FSM_FFd3 AND 
	NOT iobm/IOS_FSM_FFd4 AND NOT iobm/IOS_FSM_FFd5 AND NOT iobm/IOS_FSM_FFd6 AND 
	iobm/DoutOE)
	OR (NOT iobm/IOS_FSM_FFd3 AND iobm/C8Mr AND 
	NOT iobm/IOS_FSM_FFd4 AND NOT iobm/IOS_FSM_FFd5 AND NOT iobm/IOS_FSM_FFd6 AND 
	iobm/DoutOE)
	OR (NOT iobm/IOS_FSM_FFd3 AND NOT iobm/IOS_FSM_FFd4 AND 
	NOT iobm/IOS_FSM_FFd5 AND NOT iobm/IOS_FSM_FFd6 AND iobm/DoutOE AND NOT iobm/IOWRREQr));

FTCPE_iobm/ES0: FTCPE port map (iobm/ES(0),iobm/ES_T(0),NOT C8M,'0','0');
iobm/ES_T(0) <= ((iobm/ES(0) AND NOT E AND iobm/Er)
	OR (NOT iobm/ES(0) AND NOT iobm/ES(2) AND NOT iobm/ES(1) AND 
	NOT iobm/ES(3) AND E)
	OR (NOT iobm/ES(0) AND NOT iobm/ES(2) AND NOT iobm/ES(1) AND 
	NOT iobm/ES(3) AND NOT iobm/Er));

FDCPE_iobm/ES1: FDCPE port map (iobm/ES(1),iobm/ES_D(1),NOT C8M,'0','0');
iobm/ES_D(1) <= ((iobm/ES(0) AND iobm/ES(1))
	OR (NOT iobm/ES(0) AND NOT iobm/ES(1))
	OR (NOT E AND iobm/Er)
	OR (iobm/ES(0) AND NOT iobm/ES(2) AND iobm/ES(3)));

FTCPE_iobm/ES2: FTCPE port map (iobm/ES(2),iobm/ES_T(2),NOT C8M,'0','0');
iobm/ES_T(2) <= ((iobm/ES(0) AND iobm/ES(1) AND E)
	OR (iobm/ES(0) AND iobm/ES(1) AND NOT iobm/Er)
	OR (iobm/ES(2) AND NOT E AND iobm/Er));

FTCPE_iobm/ES3: FTCPE port map (iobm/ES(3),iobm/ES_T(3),NOT C8M,'0','0');
iobm/ES_T(3) <= ((iobm/ES(3) AND NOT E AND iobm/Er)
	OR (iobm/ES(0) AND iobm/ES(2) AND iobm/ES(1) AND E)
	OR (iobm/ES(0) AND iobm/ES(2) AND iobm/ES(1) AND NOT iobm/Er)
	OR (iobm/ES(0) AND NOT iobm/ES(2) AND NOT iobm/ES(1) AND 
	iobm/ES(3)));

FDCPE_iobm/Er: FDCPE port map (iobm/Er,E,NOT C8M,'0','0');

FDCPE_iobm/IORDREQr: FDCPE port map (iobm/IORDREQr,IORDREQ,C16M,'0','0');

FDCPE_iobm/IOS0: FDCPE port map (iobm/IOS0,iobm/IOS0_D,C16M,'0','0');
iobm/IOS0_D <= ((iobm/IOS_FSM_FFd1)
	OR (iobm/IOS_FSM_FFd7 AND iobm/C8Mr)
	OR (iobm/IOS_FSM_FFd7 AND nAoutOE)
	OR (iobm/IOS_FSM_FFd7 AND NOT iobm/IORDREQr AND 
	NOT iobm/IOWRREQr)
	OR (NOT iobm/IOS_FSM_FFd7 AND NOT iobm/IOS_FSM_FFd3 AND 
	NOT iobm/IOS_FSM_FFd4 AND NOT iobm/IOS_FSM_FFd5 AND NOT iobm/IOS_FSM_FFd6 AND 
	NOT iobm/IOS_FSM_FFd2 AND iobm/IOS0));

FDCPE_iobm/IOS_FSM_FFd1: FDCPE port map (iobm/IOS_FSM_FFd1,iobm/IOS_FSM_FFd2,C16M,'0','0');

FDCPE_iobm/IOS_FSM_FFd2: FDCPE port map (iobm/IOS_FSM_FFd2,iobm/IOS_FSM_FFd2_D,C16M,'0','0');
iobm/IOS_FSM_FFd2_D <= ((IOBERR AND iobm/IOS_FSM_FFd3 AND NOT iobm/C8Mr)
	OR (IODONE AND iobm/IOS_FSM_FFd3 AND NOT iobm/C8Mr));

FDCPE_iobm/IOS_FSM_FFd3: FDCPE port map (iobm/IOS_FSM_FFd3,iobm/IOS_FSM_FFd3_D,C16M,'0','0');
iobm/IOS_FSM_FFd3_D <= ((iobm/IOS_FSM_FFd4)
	OR (iobm/IOS_FSM_FFd3 AND iobm/C8Mr)
	OR (NOT IOBERR AND NOT IODONE AND iobm/IOS_FSM_FFd3));

FDCPE_iobm/IOS_FSM_FFd4: FDCPE port map (iobm/IOS_FSM_FFd4,iobm/IOS_FSM_FFd5,C16M,'0','0');

FDCPE_iobm/IOS_FSM_FFd5: FDCPE port map (iobm/IOS_FSM_FFd5,iobm/IOS_FSM_FFd6,C16M,'0','0');

FDCPE_iobm/IOS_FSM_FFd6: FDCPE port map (iobm/IOS_FSM_FFd6,iobm/IOS_FSM_FFd6_D,C16M,'0','0');
iobm/IOS_FSM_FFd6_D <= ((iobm/IOS_FSM_FFd7 AND NOT iobm/C8Mr AND iobm/IORDREQr AND 
	NOT nAoutOE)
	OR (iobm/IOS_FSM_FFd7 AND NOT iobm/C8Mr AND iobm/IOWRREQr AND 
	NOT nAoutOE));

FDCPE_iobm/IOS_FSM_FFd7: FDCPE port map (iobm/IOS_FSM_FFd7,iobm/IOS_FSM_FFd7_D,C16M,'0','0');
iobm/IOS_FSM_FFd7_D <= ((NOT iobm/IOS_FSM_FFd7 AND NOT iobm/IOS_FSM_FFd1)
	OR (NOT iobm/C8Mr AND NOT iobm/IOS_FSM_FFd1 AND iobm/IORDREQr AND 
	NOT nAoutOE)
	OR (NOT iobm/C8Mr AND NOT iobm/IOS_FSM_FFd1 AND iobm/IOWRREQr AND 
	NOT nAoutOE));

FDCPE_iobm/IOWRREQr: FDCPE port map (iobm/IOWRREQr,IOWRREQ,C16M,'0','0');

FDCPE_iobm/VPAr: FDCPE port map (iobm/VPAr,NOT nVPA_IOB,NOT C8M,'0','0');

FDCPE_iobs/Clear1: FDCPE port map (iobs/Clear1,iobs/Clear1_D,FCLK,'0','0');
iobs/Clear1_D <= (NOT iobs/TS_FSM_FFd1 AND iobs/TS_FSM_FFd2);

FDCPE_iobs/IOACTr: FDCPE port map (iobs/IOACTr,IOACT,FCLK,'0','0');

FDCPE_iobs/IODONEr: FDCPE port map (iobs/IODONEr,IODONE,FCLK,'0','0');

FDCPE_iobs/IOL1: FDCPE port map (iobs/IOL1,NOT nLDS_FSB,FCLK,'0','0',iobs/Load1);

FTCPE_iobs/IORW1: FTCPE port map (iobs/IORW1,iobs/IORW1_T,FCLK,'0','0');
iobs/IORW1_T <= ((NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(13) AND 
	NOT iobs/Sent AND NOT nWE_FSB AND iobs/IORW1 AND iobs/TS_FSM_FFd1 AND 
	fsb/ASrf AND nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(13) AND 
	NOT iobs/Sent AND NOT nWE_FSB AND iobs/IORW1 AND iobs/TS_FSM_FFd2 AND 
	fsb/ASrf AND nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(14) AND 
	NOT iobs/Sent AND NOT nWE_FSB AND iobs/IORW1 AND iobs/TS_FSM_FFd1 AND 
	fsb/ASrf AND nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(14) AND 
	NOT iobs/Sent AND NOT nWE_FSB AND iobs/IORW1 AND iobs/TS_FSM_FFd2 AND 
	fsb/ASrf AND nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(13) AND 
	NOT iobs/Sent AND NOT nWE_FSB AND iobs/IORW1 AND NOT nAS_FSB AND 
	iobs/TS_FSM_FFd1 AND nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(13) AND 
	NOT iobs/Sent AND NOT nWE_FSB AND iobs/IORW1 AND NOT nAS_FSB AND 
	iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(14) AND 
	NOT iobs/Sent AND NOT nWE_FSB AND iobs/IORW1 AND NOT nAS_FSB AND 
	iobs/TS_FSM_FFd1 AND nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(14) AND 
	NOT iobs/Sent AND NOT nWE_FSB AND iobs/IORW1 AND NOT nAS_FSB AND 
	iobs/TS_FSM_FFd2 AND nADoutLE1));

FDCPE_iobs/IOU1: FDCPE port map (iobs/IOU1,NOT nUDS_FSB,FCLK,'0','0',iobs/Load1);

FDCPE_iobs/Load1: FDCPE port map (iobs/Load1,iobs/Load1_D,FCLK,'0','0');
iobs/Load1_D <= ((NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(13) AND 
	NOT iobs/Sent AND NOT nWE_FSB AND iobs/TS_FSM_FFd1 AND fsb/ASrf AND 
	nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(13) AND 
	NOT iobs/Sent AND NOT nWE_FSB AND iobs/TS_FSM_FFd2 AND fsb/ASrf AND 
	nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(14) AND 
	NOT iobs/Sent AND NOT nWE_FSB AND iobs/TS_FSM_FFd1 AND fsb/ASrf AND 
	nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(13) AND 
	NOT iobs/Sent AND NOT nWE_FSB AND NOT nAS_FSB AND iobs/TS_FSM_FFd1 AND 
	nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(13) AND 
	NOT iobs/Sent AND NOT nWE_FSB AND NOT nAS_FSB AND iobs/TS_FSM_FFd2 AND 
	nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(14) AND 
	NOT iobs/Sent AND NOT nWE_FSB AND NOT nAS_FSB AND iobs/TS_FSM_FFd1 AND 
	nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(14) AND 
	NOT iobs/Sent AND NOT nWE_FSB AND NOT nAS_FSB AND iobs/TS_FSM_FFd2 AND 
	nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(14) AND 
	NOT iobs/Sent AND NOT nWE_FSB AND iobs/TS_FSM_FFd2 AND fsb/ASrf AND 
	nADoutLE1));

FTCPE_iobs/Sent: FTCPE port map (iobs/Sent,iobs/Sent_T,FCLK,'0','0');
iobs/Sent_T <= ((NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(13) AND 
	NOT iobs/Sent AND NOT nWE_FSB AND NOT nAS_FSB AND nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(13) AND 
	NOT iobs/Sent AND NOT nWE_FSB AND fsb/ASrf AND nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(14) AND 
	NOT iobs/Sent AND NOT nWE_FSB AND fsb/ASrf AND nADoutLE1)
	OR (A_FSB(22) AND A_FSB(21) AND NOT iobs/Sent AND 
	NOT iobs/TS_FSM_FFd1 AND NOT iobs/TS_FSM_FFd2 AND fsb/ASrf AND nADoutLE1)
	OR (A_FSB(22) AND A_FSB(20) AND NOT iobs/Sent AND 
	NOT iobs/TS_FSM_FFd1 AND NOT iobs/TS_FSM_FFd2 AND fsb/ASrf AND nADoutLE1)
	OR (A_FSB(22) AND NOT iobs/Sent AND NOT cs/nOverlay AND NOT nAS_FSB AND 
	NOT iobs/TS_FSM_FFd1 AND NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (A_FSB(22) AND NOT iobs/Sent AND NOT cs/nOverlay AND 
	NOT iobs/TS_FSM_FFd1 AND NOT iobs/TS_FSM_FFd2 AND fsb/ASrf AND nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND A_FSB(14) AND 
	NOT iobs/Sent AND NOT nWE_FSB AND NOT nAS_FSB AND nADoutLE1)
	OR (iobs/Sent AND nAS_FSB AND NOT fsb/ASrf)
	OR (A_FSB(23) AND NOT iobs/Sent AND NOT nAS_FSB AND 
	NOT iobs/TS_FSM_FFd1 AND NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (A_FSB(23) AND NOT iobs/Sent AND NOT iobs/TS_FSM_FFd1 AND 
	NOT iobs/TS_FSM_FFd2 AND fsb/ASrf AND nADoutLE1)
	OR (A_FSB(22) AND A_FSB(21) AND NOT iobs/Sent AND NOT nAS_FSB AND 
	NOT iobs/TS_FSM_FFd1 AND NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (A_FSB(22) AND A_FSB(20) AND NOT iobs/Sent AND NOT nAS_FSB AND 
	NOT iobs/TS_FSM_FFd1 AND NOT iobs/TS_FSM_FFd2 AND nADoutLE1));

FDCPE_iobs/TS_FSM_FFd1: FDCPE port map (iobs/TS_FSM_FFd1,iobs/TS_FSM_FFd1_D,FCLK,'0','0');
iobs/TS_FSM_FFd1_D <= ((iobs/TS_FSM_FFd2)
	OR (iobs/TS_FSM_FFd1 AND iobs/IOACTr));

FDCPE_iobs/TS_FSM_FFd2: FDCPE port map (iobs/TS_FSM_FFd2,iobs/TS_FSM_FFd2_D,FCLK,'0','0');
iobs/TS_FSM_FFd2_D <= ((nRAS_OBUF.EXP)
	OR (nAS_FSB AND NOT iobs/TS_FSM_FFd2 AND NOT fsb/ASrf AND 
	nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT A_FSB(21) AND 
	NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT A_FSB(20) AND 
	NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT A_FSB(16) AND 
	NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND nWE_FSB AND 
	NOT iobs/TS_FSM_FFd2 AND nADoutLE1)
	OR (iobs/TS_FSM_FFd1 AND NOT iobs/TS_FSM_FFd2)
	OR (iobs/TS_FSM_FFd1 AND iobs/IOACTr)
	OR (iobs/Sent AND NOT iobs/TS_FSM_FFd2 AND nADoutLE1));


nADoutLE0 <= (NOT ALE0M AND NOT ALE0S);

FDCPE_nADoutLE1: FDCPE port map (nADoutLE1,nADoutLE1_D,FCLK,'0','0');
nADoutLE1_D <= ((iobs/Load1)
	OR (NOT iobs/Clear1 AND NOT nADoutLE1));

FDCPE_nAS_IOB: FDCPE port map (nAS_IOB_I,nAS_IOB,NOT C16M,'0','0');
nAS_IOB <= ((NOT iobm/IOS_FSM_FFd7 AND NOT iobm/IOS_FSM_FFd3 AND 
	NOT iobm/IOS_FSM_FFd4 AND NOT iobm/IOS_FSM_FFd5 AND NOT iobm/IOS_FSM_FFd6)
	OR (NOT iobm/IOS_FSM_FFd3 AND iobm/C8Mr AND 
	NOT iobm/IOS_FSM_FFd4 AND NOT iobm/IOS_FSM_FFd5 AND NOT iobm/IOS_FSM_FFd6)
	OR (NOT iobm/IOS_FSM_FFd3 AND NOT iobm/IOS_FSM_FFd4 AND 
	NOT iobm/IOS_FSM_FFd5 AND NOT iobm/IOS_FSM_FFd6 AND NOT iobm/IORDREQr AND 
	NOT iobm/IOWRREQr));
nAS_IOB <= nAS_IOB_I when nAS_IOB_OE = '1' else 'Z';
nAS_IOB_OE <= NOT nAoutOE;

FDCPE_nAoutOE: FDCPE port map (nAoutOE,nAoutOE_D,FCLK,'0','0');
nAoutOE_D <= ((NOT nBR_IOB AND cnt/IS_FSM_FFd1 AND cnt/IS_FSM_FFd2)
	OR (cnt/IS_FSM_FFd1 AND NOT cnt/IS_FSM_FFd2 AND NOT nAoutOE));

FDCPE_nBERR_FSB: FDCPE port map (nBERR_FSB,nBERR_FSB_D,FCLK,'0','0');
nBERR_FSB_D <= ((NOT IOBERR AND nBERR_FSB)
	OR (NOT iobs/Sent AND nBERR_FSB)
	OR (nAS_FSB AND NOT fsb/ASrf));

FTCPE_nBR_IOB: FTCPE port map (nBR_IOB,nBR_IOB_T,FCLK,'0','0');
nBR_IOB_T <= ((nBR_IOB AND NOT cnt/IS_FSM_FFd1 AND NOT cnt/IS_FSM_FFd2)
	OR (NOT nBR_IOB AND NOT cnt/IS_FSM_FFd1 AND cnt/IS_FSM_FFd2 AND 
	NOT cnt/nIPL2r));

FDCPE_nCAS: FDCPE port map (nCAS,NOT ram/CAS,NOT FCLK,'0','0');

FDCPE_nDTACK_FSB: FDCPE port map (nDTACK_FSB,nDTACK_FSB_D,FCLK,'0','0');
nDTACK_FSB_D <= ((NOT QoSReady)
	OR (NOT A_FSB(22) AND NOT IONPReady AND NOT RAMReady)
	OR (A_FSB(23) AND A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16))
	OR (A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND A_FSB(18) AND 
	A_FSB(17) AND A_FSB(16) AND A_FSB(13) AND NOT nWE_FSB AND NOT IONPReady AND 
	NOT IOPWReady)
	OR (A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND A_FSB(18) AND 
	A_FSB(17) AND A_FSB(16) AND A_FSB(14) AND NOT nWE_FSB AND NOT IONPReady AND 
	NOT IOPWReady)
	OR (A_FSB(23) AND NOT IONPReady)
	OR (nAS_FSB AND NOT fsb/ASrf)
	OR (A_FSB(22) AND A_FSB(21) AND NOT IONPReady)
	OR (A_FSB(22) AND A_FSB(20) AND NOT IONPReady));

FDCPE_nDinLE: FDCPE port map (nDinLE,nDinLE_D,NOT C16M,'0','0');
nDinLE_D <= (NOT iobm/IOS_FSM_FFd3 AND NOT iobm/IOS_FSM_FFd4);


nDinOE <= NOT (((A_FSB(23) AND nWE_FSB AND NOT nAS_FSB)
	OR (A_FSB(22) AND A_FSB(21) AND nWE_FSB AND NOT nAS_FSB)
	OR (A_FSB(22) AND A_FSB(20) AND nWE_FSB AND NOT nAS_FSB)));


nDoutOE <= NOT (((iobm/DoutOE AND NOT nAoutOE)
	OR (NOT iobm/IORDREQr AND iobm/IOS0 AND NOT iobm/IOWRREQr AND 
	NOT nAoutOE)));

FDCPE_nLDS_IOB: FDCPE port map (nLDS_IOB_I,nLDS_IOB,NOT C16M,'0','0');
nLDS_IOB <= ((iobm/IOS_FSM_FFd7 AND NOT iobm/C8Mr AND IOL0 AND 
	iobm/IORDREQr)
	OR (iobm/IOS_FSM_FFd3 AND IOL0)
	OR (iobm/IOS_FSM_FFd4 AND IOL0)
	OR (iobm/IOS_FSM_FFd5 AND IOL0)
	OR (NOT nLDS_IOB AND iobm/IOS_FSM_FFd6 AND IOL0));
nLDS_IOB <= nLDS_IOB_I when nLDS_IOB_OE = '1' else 'Z';
nLDS_IOB_OE <= NOT nAoutOE;


nOE <= NOT ((nWE_FSB AND NOT nAS_FSB));


nRAMLWE <= NOT ((ram/RAMEN AND NOT nWE_FSB AND NOT nLDS_FSB AND NOT nAS_FSB));


nRAMUWE <= NOT ((ram/RAMEN AND NOT nWE_FSB AND NOT nUDS_FSB AND NOT nAS_FSB));


nRAS <= NOT (((ram/RASrf)
	OR (ram/RASrr)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND ram/RAMEN AND cs/nOverlay AND 
	NOT nAS_FSB)));


nRES_I <= '0';
nRES <= nRES_I when nRES_OE = '1' else 'Z';
nRES_OE <= NOT nRESout;

FDCPE_nRESout: FDCPE port map (nRESout,nRESout_D,FCLK,'0','0');
nRESout_D <= (cnt/IS_FSM_FFd1 AND NOT cnt/IS_FSM_FFd2);


nROMCS <= NOT (((NOT A_FSB(23) AND A_FSB(22) AND NOT A_FSB(21) AND NOT A_FSB(20))
	OR (NOT A_FSB(23) AND NOT A_FSB(21) AND NOT A_FSB(20) AND NOT cs/nOverlay)));


nROMWE <= NOT ((NOT nWE_FSB AND NOT nAS_FSB));

FDCPE_nUDS_IOB: FDCPE port map (nUDS_IOB_I,nUDS_IOB,NOT C16M,'0','0');
nUDS_IOB <= ((iobm/IOS_FSM_FFd7 AND NOT iobm/C8Mr AND IOU0 AND 
	iobm/IORDREQr)
	OR (iobm/IOS_FSM_FFd3 AND IOU0)
	OR (iobm/IOS_FSM_FFd4 AND IOU0)
	OR (iobm/IOS_FSM_FFd5 AND IOU0)
	OR (NOT nUDS_IOB AND iobm/IOS_FSM_FFd6 AND IOU0));
nUDS_IOB <= nUDS_IOB_I when nUDS_IOB_OE = '1' else 'Z';
nUDS_IOB_OE <= NOT nAoutOE;

FTCPE_nVMA_IOB: FTCPE port map (nVMA_IOB_I,nVMA_IOB_T,C8M,'0','0');
nVMA_IOB_T <= ((NOT nVMA_IOB AND NOT iobm/ES(0) AND NOT iobm/ES(2) AND NOT iobm/ES(1) AND 
	NOT iobm/ES(3))
	OR (nVMA_IOB AND iobm/ES(0) AND iobm/ES(2) AND NOT iobm/ES(1) AND 
	NOT iobm/ES(3) AND IOACT AND iobm/VPAr));
nVMA_IOB <= nVMA_IOB_I when nVMA_IOB_OE = '1' else 'Z';
nVMA_IOB_OE <= NOT nAoutOE;

FDCPE_nVPA_FSB: FDCPE port map (nVPA_FSB,nVPA_FSB_D,FCLK,'0',nAS_FSB);
nVPA_FSB_D <= ((A_FSB(23) AND A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND IONPReady AND 
	NOT nAS_FSB AND QoSReady)
	OR (A_FSB(23) AND A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND 
	A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND IONPReady AND 
	QoSReady AND fsb/ASrf));

FDCPE_ram/CAS: FDCPE port map (ram/CAS,ram/CAS_D,FCLK,'0','0');
ram/CAS_D <= ((ram/RS_FSM_FFd7)
	OR (ram/RS_FSM_FFd6)
	OR (RefUrg AND NOT ram/RefDone AND ram/RS_FSM_FFd5)
	OR (RefUrg AND NOT ram/RefDone AND nAS_FSB AND 
	ram/RS_FSM_FFd8 AND NOT fsb/ASrf)
	OR (NOT ram/RefDone AND RefReq AND nAS_FSB AND 
	ram/RS_FSM_FFd8 AND NOT fsb/ASrf)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND ram/RAMEN AND cs/nOverlay AND 
	NOT nAS_FSB AND ram/RS_FSM_FFd8)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND ram/RAMEN AND cs/nOverlay AND 
	ram/RS_FSM_FFd8 AND fsb/ASrf));

FTCPE_ram/Once: FTCPE port map (ram/Once,ram/Once_T,FCLK,'0','0');
ram/Once_T <= ((NOT A_FSB(23) AND NOT A_FSB(22) AND ram/RAMEN AND cs/nOverlay AND 
	NOT ram/Once AND NOT nAS_FSB AND ram/RS_FSM_FFd8)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND ram/RAMEN AND cs/nOverlay AND 
	NOT ram/Once AND ram/RS_FSM_FFd8 AND fsb/ASrf)
	OR (ram/Once AND nAS_FSB AND NOT fsb/ASrf));

FDCPE_ram/RAMEN: FDCPE port map (ram/RAMEN,ram/RAMEN_D,FCLK,'0','0');
ram/RAMEN_D <= ((ram/RS_FSM_FFd7)
	OR (RefUrg AND NOT ram/RefDone AND nAS_FSB AND 
	ram/RS_FSM_FFd8 AND NOT fsb/ASrf)
	OR (NOT ram/RAMEN AND ram/Once AND NOT nAS_FSB)
	OR (NOT ram/RAMEN AND ram/Once AND fsb/ASrf)
	OR (NOT ram/RAMEN AND NOT ram/RS_FSM_FFd8 AND NOT ram/RS_FSM_FFd4)
	OR (NOT ram/RefDone AND RefReq AND nAS_FSB AND 
	ram/RS_FSM_FFd8 AND NOT fsb/ASrf));

FDCPE_ram/RASEL: FDCPE port map (ram/RASEL,ram/RASEL_D,FCLK,'0','0');
ram/RASEL_D <= ((ram/RS_FSM_FFd7)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND ram/RAMEN AND cs/nOverlay AND 
	NOT nAS_FSB AND ram/RS_FSM_FFd8)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND ram/RAMEN AND cs/nOverlay AND 
	ram/RS_FSM_FFd8 AND fsb/ASrf));

FDCPE_ram/RASrf: FDCPE port map (ram/RASrf,ram/RS_FSM_FFd7,NOT FCLK,'0','0');

FDCPE_ram/RASrr: FDCPE port map (ram/RASrr,ram/RASrr_D,FCLK,'0','0');
ram/RASrr_D <= ((ram/RS_FSM_FFd3)
	OR (ram/RS_FSM_FFd6)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND ram/RAMEN AND cs/nOverlay AND 
	NOT nAS_FSB AND ram/RS_FSM_FFd8)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND ram/RAMEN AND cs/nOverlay AND 
	ram/RS_FSM_FFd8 AND fsb/ASrf));

FDCPE_ram/RS_FSM_FFd1: FDCPE port map (ram/RS_FSM_FFd1,ram/RS_FSM_FFd2,FCLK,'0','0');

FDCPE_ram/RS_FSM_FFd2: FDCPE port map (ram/RS_FSM_FFd2,ram/RS_FSM_FFd3,FCLK,'0','0');

FDCPE_ram/RS_FSM_FFd3: FDCPE port map (ram/RS_FSM_FFd3,ram/RS_FSM_FFd6,FCLK,'0','0');

FDCPE_ram/RS_FSM_FFd4: FDCPE port map (ram/RS_FSM_FFd4,ram/RS_FSM_FFd4_D,FCLK,'0','0');
ram/RS_FSM_FFd4_D <= ((NOT ram/RS_FSM_FFd5 AND NOT ram/RS_FSM_FFd1)
	OR (RefUrg AND NOT ram/RefDone AND NOT ram/RS_FSM_FFd1));

FDCPE_ram/RS_FSM_FFd5: FDCPE port map (ram/RS_FSM_FFd5,ram/RS_FSM_FFd7,FCLK,'0','0');

FDCPE_ram/RS_FSM_FFd6: FDCPE port map (ram/RS_FSM_FFd6,ram/RS_FSM_FFd6_D,FCLK,'0','0');
ram/RS_FSM_FFd6_D <= ((RefUrg AND NOT ram/RefDone AND ram/RS_FSM_FFd5)
	OR (RefUrg AND NOT ram/RefDone AND nAS_FSB AND 
	ram/RS_FSM_FFd8 AND NOT fsb/ASrf)
	OR (NOT ram/RefDone AND RefReq AND nAS_FSB AND 
	ram/RS_FSM_FFd8 AND NOT fsb/ASrf));

FDCPE_ram/RS_FSM_FFd7: FDCPE port map (ram/RS_FSM_FFd7,ram/RS_FSM_FFd7_D,FCLK,'0','0');
ram/RS_FSM_FFd7_D <= ((NOT A_FSB(23) AND NOT A_FSB(22) AND ram/RAMEN AND cs/nOverlay AND 
	NOT nAS_FSB AND ram/RS_FSM_FFd8)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND ram/RAMEN AND cs/nOverlay AND 
	ram/RS_FSM_FFd8 AND fsb/ASrf));

FDCPE_ram/RS_FSM_FFd8: FDCPE port map (ram/RS_FSM_FFd8,ram/RS_FSM_FFd8_D,FCLK,'0','0');
ram/RS_FSM_FFd8_D <= ((NOT A_FSB(23) AND NOT A_FSB(22) AND ram/RAMEN AND cs/nOverlay AND 
	NOT ram/RS_FSM_FFd4 AND fsb/ASrf)
	OR (NOT ram/RS_FSM_FFd8 AND NOT ram/RS_FSM_FFd4)
	OR (RefUrg AND NOT ram/RefDone AND nAS_FSB AND 
	NOT ram/RS_FSM_FFd4 AND NOT fsb/ASrf)
	OR (NOT ram/RefDone AND RefReq AND nAS_FSB AND 
	NOT ram/RS_FSM_FFd4 AND NOT fsb/ASrf)
	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND ram/RAMEN AND cs/nOverlay AND 
	NOT nAS_FSB AND NOT ram/RS_FSM_FFd4));

FDCPE_ram/RefDone: FDCPE port map (ram/RefDone,ram/RefDone_D,FCLK,'0','0');
ram/RefDone_D <= ((NOT RefUrg AND NOT RefReq)
	OR (NOT ram/RefDone AND NOT ram/RS_FSM_FFd3 AND NOT ram/RS_FSM_FFd2));

Register Legend:
 FDCPE (Q,D,C,CLR,PRE,CE); 
 FTCPE (Q,D,C,CLR,PRE,CE); 
 LDCP  (Q,D,G,CLR,PRE); 

******************************  Device Pin Out *****************************

Device : XC95144XL-10-TQ100


   --------------------------------------------------  
  /100 98  96  94  92  90  88  86  84  82  80  78  76  \
 |   99  97  95  93  91  89  87  85  83  81  79  77    |
 | 1                                               75  | 
 | 2                                               74  | 
 | 3                                               73  | 
 | 4                                               72  | 
 | 5                                               71  | 
 | 6                                               70  | 
 | 7                                               69  | 
 | 8                                               68  | 
 | 9                                               67  | 
 | 10                                              66  | 
 | 11                                              65  | 
 | 12                                              64  | 
 | 13              XC95144XL-10-TQ100              63  | 
 | 14                                              62  | 
 | 15                                              61  | 
 | 16                                              60  | 
 | 17                                              59  | 
 | 18                                              58  | 
 | 19                                              57  | 
 | 20                                              56  | 
 | 21                                              55  | 
 | 22                                              54  | 
 | 23                                              53  | 
 | 24                                              52  | 
 | 25                                              51  | 
 |   27  29  31  33  35  37  39  41  43  45  47  49    |
  \26  28  30  32  34  36  38  40  42  44  46  48  50  /
   --------------------------------------------------  


Pin Signal                         Pin Signal                        
No. Name                           No. Name                          
  1 KPR                              51 VCC                           
  2 A_FSB<5>                         52 RA<7>                         
  3 A_FSB<6>                         53 RA<0>                         
  4 A_FSB<7>                         54 RA<8>                         
  5 VCC                              55 RA<10>                        
  6 A_FSB<8>                         56 RA<9>                         
  7 A_FSB<9>                         57 VCC                           
  8 A_FSB<10>                        58 C25MEN                        
  9 A_FSB<11>                        59 KPR                           
 10 A_FSB<12>                        60 KPR                           
 11 A_FSB<13>                        61 KPR                           
 12 A_FSB<14>                        62 GND                           
 13 A_FSB<15>                        63 RA<11>                        
 14 A_FSB<16>                        64 nRAS                          
 15 A_FSB<17>                        65 nRAMLWE                       
 16 A_FSB<18>                        66 nRAMUWE                       
 17 A_FSB<19>                        67 KPR                           
 18 A_FSB<20>                        68 KPR                           
 19 A_FSB<21>                        69 GND                           
 20 A_FSB<22>                        70 nBERR_FSB                     
 21 GND                              71 KPR                           
 22 C16M                             72 nBR_IOB                       
 23 C8M                              73 KPR                           
 24 A_FSB<23>                        74 nVMA_IOB                      
 25 E                                75 GND                           
 26 VCC                              76 nBERR_IOB                     
 27 FCLK                             77 nVPA_IOB                      
 28 nDTACK_FSB                       78 nDTACK_IOB                    
 29 nWE_FSB                          79 nLDS_IOB                      
 30 nLDS_FSB                         80 nUDS_IOB                      
 31 GND                              81 nAS_IOB                       
 32 nAS_FSB                          82 nADoutLE1                     
 33 nUDS_FSB                         83 TDO                           
 34 nROMWE                           84 GND                           
 35 nROMCS                           85 nADoutLE0                     
 36 nCAS                             86 nDinLE                        
 37 nOE                              87 nAoutOE                       
 38 VCC                              88 VCC                           
 39 KPR                              89 nDoutOE                       
 40 RA<4>                            90 nDinOE                        
 41 RA<3>                            91 nRES                          
 42 RA<5>                            92 nIPL2                         
 43 RA<2>                            93 nVPA_FSB                      
 44 GND                              94 A_FSB<1>                      
 45 TDI                              95 A_FSB<2>                      
 46 RA<6>                            96 A_FSB<3>                      
 47 TMS                              97 A_FSB<4>                      
 48 TCK                              98 VCC                           
 49 KPR                              99 KPR                           
 50 RA<1>                           100 GND                           


Legend :  NC  = Not Connected, unbonded pin
         PGND = Unused I/O configured as additional Ground pin
         TIE  = Unused I/O floating -- must tie to VCC, GND or other signal
         KPR  = Unused I/O with weak keeper (leave unconnected)
         VCC  = Dedicated Power Pin
         GND  = Dedicated Ground Pin
         TDI  = Test Data In, JTAG pin
         TDO  = Test Data Out, JTAG pin
         TCK  = Test Clock, JTAG pin
         TMS  = Test Mode Select, JTAG pin
  PROHIBITED  = User reserved pin
****************************  Compiler Options  ****************************

Following is a list of all global compiler options used by the fitter run.

Device(s) Specified                         : xc95144xl-10-TQ100
Optimization Method                         : SPEED
Multi-Level Logic Optimization              : ON
Ignore Timing Specifications                : OFF
Default Register Power Up Value             : LOW
Keep User Location Constraints              : ON
What-You-See-Is-What-You-Get                : OFF
Exhaustive Fitting                          : OFF
Keep Unused Inputs                          : OFF
Slew Rate                                   : FAST
Power Mode                                  : STD
Ground on Unused IOs                        : OFF
Set I/O Pin Termination                     : KEEPER
Global Clock Optimization                   : ON
Global Set/Reset Optimization               : ON
Global Ouput Enable Optimization            : ON
Input Limit                                 : 54
Pterm Limit                                 : 25
