Signal Name | Total Product Terms | Product Terms | Location | Power Mode | Pin Number | PinType | Pin Use
--- | --- | --- | --- | --- | --- | --- | ---
ram/RegUrgSync | 1 | 1_1 | MC1 | STD |  | (b) | (b)
nAoutOE | 2 | 2_1 2_2 | MC2 | STD | 87 | I/O | O
ram/BACTr | 1 | 3_1 | MC3 | STD |  | (b) | (b)
nRESout | 1 | 4_1 | MC4 | STD |  | (b) | (b)
nDoutOE | 1 | 5_1 | MC5 | STD | 89 | I/O | O
nDinOE | 3 | 6_1 6_2 6_3 | MC6 | STD | 90 | I/O | O
fsb/ASrf | 1 | 7_1 | MC7 | STD |  | (b) | (b)
nRES | 1 | 8_1 | MC8 | STD | 91 | I/O | I/O
cnt/Er<1> | 1 | 9_1 | MC9 | STD | 92 | I/O | I
cnt/TimerTC | 2 | 10_1 10_2 | MC10 | STD |  | (b) | (b)
nVPA_FSB | 1 | 11_1 | MC11 | STD | 93 | I/O | O
cnt/LTimer<3> | 2 | 12_1 12_2 | MC12 | STD | 94 | I/O | I
cnt/LTimer<2> | 2 | 13_1 13_2 | MC13 | STD |  | (b) | (b)
cnt/LTimer<1> | 2 | 14_1 14_2 | MC14 | STD | 95 | I/O | I
RefReq | 2 | 15_1 15_2 | MC15 | STD | 96 | I/O | I
IOU0 | 3 | 16_1 16_2 16_3 | MC16 | STD |  | (b) | (b)
IOL0 | 3 | 17_1 17_2 17_3 | MC17 | STD | 97 | I/O | I
RefUrg | 5 | 18_1 18_2 18_3 18_4 18_5 | MC18 | STD |  | (b) | (b)

Signals Used By Logic in Function Block

1. A_FSB<20>
2. A_FSB<21>
3. A_FSB<22>
4. A_FSB<23>
5. RefUrg
6. cnt/Er<0>
7. cnt/Er<1>
8. cnt/INITS_FSM_FFd1
9. cnt/INITS_FSM_FFd2
10. cnt/LTimer<0>
11. cnt/LTimer<1>
12. cnt/LTimer<2>
13. cnt/Timer<0>
14. cnt/Timer<1>
15. cnt/Timer<2>
16. cnt/TimerTC
17. fsb/ASrf
18. fsb/VPA
19. iobm/DoutOE
20. iobs/IOL1
21. iobs/IOU1
22. iobs/PS_FSM_FFd1
23. iobs/PS_FSM_FFd2
24. nADoutLE1
25. nAS_FSB
26. nAoutOE
27. nBR_IOB
28. nLDS_FSB
29. nRESout
30. nUDS_FSB
31. nWE_FSB