(kicad_pcb (version 20221018) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" signal)
    (2 "In2.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "prepreg") (thickness 0.1) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "core") (thickness 1.24) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "prepreg") (thickness 0.1) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/")
    )
  )

  (net 0 "")
  (net 1 "+12V")
  (net 2 "GND")
  (net 3 "+5V")
  (net 4 "+3V3")
  (net 5 "-12V")
  (net 6 "-5V")
  (net 7 "/HSx")
  (net 8 "/VSx")
  (net 9 "/PWR_OK")
  (net 10 "+5VP")
  (net 11 "Net-(C17-Pad1)")
  (net 12 "/HSf")
  (net 13 "/Ci")
  (net 14 "/HSi")
  (net 15 "/VSi")
  (net 16 "/Ro")
  (net 17 "/Go")
  (net 18 "/Bo")
  (net 19 "/HSo")
  (net 20 "/VSo")
  (net 21 "Net-(R4-Pad1)")
  (net 22 "Net-(R5-Pad1)")
  (net 23 "Net-(R6-Pad1)")
  (net 24 "Net-(R8-Pad1)")
  (net 25 "Net-(R10-Pad1)")
  (net 26 "/Cx")
  (net 27 "unconnected-(J2-Pin_20-Pad20)")
  (net 28 "unconnected-(U2-Pad11)")
  (net 29 "unconnected-(U3-Pad11)")
  (net 30 "Net-(R12-Pad1)")
  (net 31 "/~{POR}")
  (net 32 "/~{PS_ON}")
  (net 33 "/AUDIO")
  (net 34 "/PBL")
  (net 35 "unconnected-(J5-Pad4)")
  (net 36 "unconnected-(J5-Pad9)")
  (net 37 "unconnected-(J5-Pad11)")
  (net 38 "unconnected-(J5-Pad12)")
  (net 39 "unconnected-(J5-Pad15)")

  (footprint "stdpads:C_0805" (layer "F.Cu")
    (tstamp 00734b2e-fd6e-4ed2-a472-d014a1807857)
    (at 106.26 175.8315)
    (tags "capacitor")
    (property "LCSC Part" "C15850")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/05d18bd8-8235-4337-a697-2d5e7f21af6d")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "C10" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 33cbb4fa-4056-422a-81eb-4e9f09a0fd78)
    )
    (fp_text value "10u" (at 0 0.35) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 6eadbbd6-1840-4e56-9a7e-cc2afdab9ba4)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 7ee57088-f4b8-4431-bcf0-723b6054a2a2)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 995906b9-6d44-4c9e-8d57-94ccd2822789))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 222bc584-b154-44ff-a1dd-579b4c34847a))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 148fb08c-5877-4989-809a-18d9c889952d))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ba42d27d-7a00-4bf8-8862-7153b5b1e290))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a7c4d35b-afeb-4c3c-a78f-f1ddda40d701))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5d7ed37f-f392-42a2-ba96-788533855115))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 7291b7c7-2f19-4d47-91bb-bf0e9f5bcf26))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp b47071a2-ede9-4975-b61a-60cd115f50bd))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 26847028-283e-4a8d-950b-f674b5969208))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp bc275705-b565-4594-9680-9a3c9625146b))
    (pad "1" smd roundrect (at -0.85 0) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3") (pintype "passive") (tstamp 7073b701-ba5f-434f-8de4-93c7d403d8c9))
    (pad "2" smd roundrect (at 0.85 0) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 1e4291fa-794d-4b6c-b50e-bce4f1529a9b))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:TO-220-3_Horizontal_TabDown" (layer "F.Cu")
    (tstamp 0b398785-9147-42e2-8e04-abeb16bf62a2)
    (at 91.567 136.271)
    (descr "TO-220-3, Horizontal, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Horizontal RM 2.54mm")
    (property "LCSC Part" "C9411")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Negative 1A 35V Linear Regulator, Fixed Output 5V, TO-220")
    (property "ki_keywords" "Voltage Regulator 1A Negative")
    (path "/852229de-faec-448d-b9d8-333457d2dc02")
    (attr through_hole)
    (fp_text reference "U1" (at 0 -20.58) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bcc42a10-254e-4b59-974b-9e53229b341c)
    )
    (fp_text value "LM7905_TO220" (at 0 2) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f11f4edc-4f7d-46c8-a3ce-5e98c6bf6c28)
    )
    (fp_line (start -5.12 -19.58) (end -5.12 -3.69)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a92fecd7-fcdd-4662-bf7e-0f0ead02fa68))
    (fp_line (start -5.12 -19.58) (end 5.12 -19.58)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 401133cc-c66b-4069-9017-0a031b9241ac))
    (fp_line (start -5.12 -3.69) (end 5.12 -3.69)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a5efe6fa-e299-4151-9d62-b817192a5276))
    (fp_line (start -2.54 -3.69) (end -2.54 -1.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8c8a9bc9-f732-45fb-8783-9676cc6e2956))
    (fp_line (start 0 -3.69) (end 0 -1.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 93dcbdb8-68ee-425e-9282-46cecfa3c5b8))
    (fp_line (start 2.54 -3.69) (end 2.54 -1.15)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e4d52c58-e10a-46b0-828e-06f6a974175f))
    (fp_line (start 5.12 -19.58) (end 5.12 -3.69)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b83c9e4b-d277-4b3e-a9c6-4338b43e8521))
    (fp_line (start -5.25 -19.71) (end -5.25 1.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8ba6c661-d652-4769-96ad-7d0b8e535c11))
    (fp_line (start -5.25 1.25) (end 5.25 1.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 33984d2c-1a16-4eb7-8116-21fd46d7f771))
    (fp_line (start 5.25 -19.71) (end -5.25 -19.71)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c811b0d7-77c6-4faa-b437-810fce65920e))
    (fp_line (start 5.25 1.25) (end 5.25 -19.71)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 007c9269-a186-4438-9be8-cd028e3955bf))
    (fp_line (start -5 -19.46) (end 5 -19.46)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 44f4d5f0-e86b-4fb2-acb2-d009560d6e6e))
    (fp_line (start -5 -13.06) (end -5 -19.46)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 865b8e57-628d-403a-b20f-ae88b050a883))
    (fp_line (start -5 -13.06) (end 5 -13.06)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f8aef3c6-d70d-44bd-a2b6-b3085d45e6b8))
    (fp_line (start -5 -3.81) (end -5 -13.06)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 92c77f0c-2710-4f04-beb9-081284a231f1))
    (fp_line (start -2.54 -3.81) (end -2.54 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 684746c4-1887-4b1d-9bbf-734e8ddab14d))
    (fp_line (start 0 -3.81) (end 0 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4dd70f95-498a-417d-b014-1312e4b640ff))
    (fp_line (start 2.54 -3.81) (end 2.54 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4fe9887d-5e1c-4a5f-ad0e-39bfa520fb24))
    (fp_line (start 5 -19.46) (end 5 -13.06)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ffc89eae-c529-47e2-a899-49dfcf0c6812))
    (fp_line (start 5 -13.06) (end -5 -13.06)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 87d36f32-7889-4541-b24f-598053c7ce5d))
    (fp_line (start 5 -13.06) (end 5 -3.81)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a9898807-7e58-4348-99a0-c86d6ec5e1ed))
    (fp_line (start 5 -3.81) (end -5 -3.81)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 710a902c-a359-4d20-89a3-7c2b1217c470))
    (fp_circle (center 0 -16.66) (end 1.85 -16.66)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 80cdcd5e-1cda-4960-bb5a-a62e491120fb))
    (pad "" np_thru_hole oval (at 0 -16.66) (size 3.5 3.5) (drill 3.5) (layers "*.Cu" "*.Mask") (tstamp d248b3be-f74c-4a33-aa84-a68f86b6dd17))
    (pad "1" thru_hole rect (at -2.54 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 5b5d3625-33b7-4269-a8b1-53a2a9a1668b))
    (pad "2" thru_hole oval (at 0 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 5 "-12V") (pinfunction "VI") (pintype "power_in") (tstamp ac3da8a0-4f52-4cbd-a15f-28d90320e537))
    (pad "3" thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 6 "-5V") (pinfunction "VO") (pintype "power_out") (tstamp 339a1de7-f596-4e8e-9cc6-131faa182c5b))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Horizontal_TabDown.wrl"
      (offset (xyz -2.54 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:PasteHole_1.152mm_NPTH" (layer "F.Cu")
    (tstamp 0c57982b-fd1f-4f23-8e8c-e3c6f453370d)
    (at 61.2775 100.838)
    (descr "Circular Fiducial, 1mm bare copper top; 2mm keepout (Level A)")
    (tags "marker")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.1)))
      (tstamp 8cc02a41-9129-4ad0-90cd-8136a5a7b840)
    )
    (fp_text value " " (at 0 2) (layer "F.Fab") hide
        (effects (font (size 0.508 0.508) (thickness 0.127)))
      (tstamp 55136e4c-e7d9-4126-a407-1fed2cd0e042)
    )
    (fp_circle (center 0 0) (end 1 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 4419a848-dbaf-48d3-912e-44945cd26393))
    (pad "" np_thru_hole circle (at 0 0) (size 1.152 1.152) (drill 1.152) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.148) (tstamp bbb04057-357e-4b62-8d2f-5dfa53ba4044))
  )

  (footprint "stdpads:R_0805" (layer "F.Cu")
    (tstamp 0f8f8e90-f5c3-4149-ac6b-718871da829f)
    (at 35.0545 128.5875 180)
    (tags "resistor")
    (property "LCSC Part" "C17513")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (path "/5b3ac888-948c-4467-a787-d7740ac5e9aa")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "R1" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 7080ec60-0a1a-429f-b035-5dcf56b7ed74)
    )
    (fp_text value "2k2" (at 0 0.35) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp f65a0d89-2969-4368-a5c6-5c49e30b4589)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp df37ada9-321d-4637-a0ae-419d8bdbb3ad)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 06ee7684-735d-43d0-b344-690134daae43))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 41001320-8a6d-4578-96e2-817f13fdfe38))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4dcdff34-090a-4fc7-bf0d-930ad601342b))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e6c64514-8a61-4916-98f4-619f65700db7))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 63b079fd-9e13-4fc0-afd0-505733805080))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3de1c701-13a9-4c1a-8902-ef1b93e42431))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ec67a38d-901d-4900-9d17-daa12569ef9c))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 00900357-7471-4b77-8b3a-f0f927579837))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b9bd48f8-a23d-4fb4-90c2-c7a4173e9a45))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cd540531-38c3-413e-a78e-ec10b3c1667e))
    (pad "1" smd roundrect (at -0.95 0 180) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/Cx") (pintype "passive") (tstamp 39b4eec4-59db-421a-8240-6eed76501bb8))
    (pad "2" smd roundrect (at 0.95 0 180) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3") (pintype "passive") (tstamp 2d01b4c4-61bf-4d38-ab95-b992552511e9))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:C_0805" (layer "F.Cu")
    (tstamp 1a9166cc-0fd4-4241-b24c-f4826b33c2a7)
    (at 74.75 177.35 90)
    (tags "capacitor")
    (property "LCSC Part" "C15850")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/7d905cf2-a5e4-4d21-8776-a2a32901fb7a")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "C23" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 78d64adc-1dc3-47c7-9e4a-863bd7a189ad)
    )
    (fp_text value "10u" (at 0 0.35 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp dd95d714-aa8d-4e6e-9e00-b8ea884908e4)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 0ec14569-927e-483b-a354-9c6aa7b0b223)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 242aa4ca-308b-45de-af59-5b82dbe72b78))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp cc1908ff-885c-4ed5-bc70-8bb5444de6bd))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d92d77bf-9bc7-4da7-81fe-60ba3dc85a22))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp afe8f1dd-46a6-4ed6-8ad8-a10bd0c55c29))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 16e9e57d-aa6b-49f1-85b4-cdf7424581c9))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0b7ba3a9-5cce-4b76-b693-fde453de2b68))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 5c7c407e-50ea-4015-86c4-3e7b19d096d5))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp ad8f8f0d-13e2-4cf3-94f7-d14720abeda2))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 44f01952-d9fb-42bd-af85-67fec633e102))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 650737f5-88f3-47a9-afea-f2e9b970826f))
    (pad "1" smd roundrect (at -0.85 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+5V") (pintype "passive") (tstamp 261134f1-4392-4acd-8311-42c448465319))
    (pad "2" smd roundrect (at 0.85 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 8a342f8d-2e2b-4a77-9f90-e4fdf90b4885))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:C_0805" (layer "F.Cu")
    (tstamp 1b1a3b96-52f3-4ef5-b358-35c05245ba00)
    (at 109.5 147.15 -90)
    (tags "capacitor")
    (property "LCSC Part" "C15850")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/ad51357a-b7c4-4245-92f1-6ec6d4fe9d0c")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "C2" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp d510446f-4aae-4d2f-ad65-d470dde75abe)
    )
    (fp_text value "10u" (at 0 0.35 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 5125c4c2-00db-498a-9337-1cb93990d4da)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 885a021f-a2c5-462d-ac7b-5e95109a74cc)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 32666bdf-07b1-4070-b56f-f4a1c0f2768b))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 19742d78-a7b4-40b5-b5b0-c0403a9957b1))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ed6b7d6c-a082-4dd8-a051-4650bfdbdd4c))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 30d0f2dc-1ed3-44e8-bb64-fe87d2ccb953))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0125ea0f-184a-4c79-b17d-4dd4b5eeb724))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7836ddce-b522-4886-87c3-963d5e0ff489))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp b299d289-92f2-4191-a211-d24eca537592))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp f2470842-0dc0-44c8-9bc1-0faabf333206))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp c53813f4-07cb-4f89-babf-ebea87555095))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp ba020962-7d03-4b02-9f97-3773acbc55de))
    (pad "1" smd roundrect (at -0.85 0 270) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive") (tstamp fffe2220-9a1d-4063-aa22-2b0bd670163d))
    (pad "2" smd roundrect (at 0.85 0 270) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 61189fc3-e790-4f63-b8c6-cb91c3d6338e))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:Molex_Mini-Fit_Jr_5569-14A1_2x07_P4.20mm_Horizontal" (layer "F.Cu")
    (tstamp 1e7b30cf-ac4c-4ef2-ba53-177b318c2c66)
    (at 65.85 171.9 90)
    (descr "Molex Mini-Fit Jr. Power Connectors, old mpn/engineering number: 5569-14A1, example for new mpn: 39-29-4149, 7 Pins per row, Mounting: PCB Mounting Flange (http://www.molex.com/pdm_docs/sd/039291047_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Mini-Fit_Jr top entryscrew_flange")
    (property "LCSC Part" "C52216")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x07, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (path "/650175db-b6fe-4c50-9884-1bed99244522")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -34.15 90) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 94935a6e-b599-47fc-b2f6-5bef6d5f1b00)
    )
    (fp_text value "Classic" (at 0 8.55 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 11a9b797-6dcf-447c-83b7-d2fefb43d869)
    )
    (fp_line (start -20.41 -7.41) (end -20.41 -0.99)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0e041bfd-761c-41ac-ae2a-3012f872f6aa))
    (fp_line (start -20.41 -0.99) (end -14.6 -0.99)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b192c96f-9704-4bb3-86b6-a2665efa78dd))
    (fp_line (start -15.41 -14.01) (end -15.41 -7.41)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 79a62eb8-39f8-442a-92a0-f924afac7f0b))
    (fp_line (start -15.41 -7.41) (end -20.41 -7.41)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f69a2bd3-1384-41f4-93e1-adde91a6ae83))
    (fp_line (start -15.2 -0.3) (end -14.6 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a9317beb-aff8-4606-b666-fe0eac0ebd3a))
    (fp_line (start -15.2 0.3) (end -15.2 -0.3)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5b6f094e-cfab-4fcd-854e-27d15363d9ef))
    (fp_line (start -14.6 0) (end -15.2 0.3)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 48a1f898-bb74-4667-9cd2-529cd8d59b7c))
    (fp_line (start -12.9 2.11) (end -12.9 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a15d580a-50f1-4073-a727-bd5ba39806c3))
    (fp_line (start -12.3 2.11) (end -12.3 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp aa52f37a-4870-40fe-ae46-3c5294078284))
    (fp_line (start -10.99 -1) (end -10.01 -1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 99e122c1-975b-449f-94a2-a6114cbecc4d))
    (fp_line (start -8.7 2.11) (end -8.7 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2ff8d1a6-e5b0-47a8-a98a-53f03792824c))
    (fp_line (start -8.1 2.11) (end -8.1 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c7af4996-ea35-4748-9b04-2f2d0760270c))
    (fp_line (start -6.79 -1) (end -5.81 -1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp de688a16-b6ea-433b-a235-50a178ace66a))
    (fp_line (start -4.5 2.11) (end -4.5 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 94e12243-00d0-48ff-bdbb-3f08058d0e5a))
    (fp_line (start -3.9 2.11) (end -3.9 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dddfa065-b9b5-48d3-bf3d-cb011bb7f7fb))
    (fp_line (start -2.59 -1) (end -1.61 -1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 60eacc19-7040-475e-80f0-0710dc381bc7))
    (fp_line (start -0.3 2.11) (end -0.3 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c66a7b74-d4a0-47d9-aaac-087b42540fb6))
    (fp_line (start 0 -14.01) (end -15.41 -14.01)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp da71fbb9-3fc0-4ced-a8b1-de94ad1138ce))
    (fp_line (start 0 -14.01) (end 15.41 -14.01)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b59dd283-f60c-4507-a7b8-6d9bb0773bd1))
    (fp_line (start 0.3 2.11) (end 0.3 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a30e8d15-207a-4bb3-87da-c88d461b6c5a))
    (fp_line (start 1.61 -1) (end 2.59 -1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5fbe6cd0-9148-4b8e-a427-d57edb680a91))
    (fp_line (start 3.9 2.11) (end 3.9 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6ff9adcf-ad06-4006-b89e-fc87ec5df8e5))
    (fp_line (start 4.5 2.11) (end 4.5 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d09f8e57-e247-4da9-bcf0-c417fdf8141f))
    (fp_line (start 5.81 -1) (end 6.79 -1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dc13b27c-a745-48b7-9fdb-6a5bf06b13d9))
    (fp_line (start 8.1 2.11) (end 8.1 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 05f7497d-50fd-48bc-80f2-dcd762be23c8))
    (fp_line (start 8.7 2.11) (end 8.7 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d86e662f-508a-4f72-a9ed-d852f40f3b72))
    (fp_line (start 10.01 -1) (end 10.99 -1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp de457ee6-6ab0-47f4-878a-2675f74f4bde))
    (fp_line (start 12.3 2.11) (end 12.3 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e570bf23-c2d9-4476-90c6-90b5b16518fe))
    (fp_line (start 12.9 2.11) (end 12.9 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9a308cee-cc9f-4038-abf5-30e57da2ad26))
    (fp_line (start 15.41 -14.01) (end 15.41 -7.41)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp eef3dfff-54b2-4240-b79b-82c8bd52a93d))
    (fp_line (start 15.41 -7.41) (end 20.41 -7.41)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8e1774ff-30fe-4c93-910e-6888226eed55))
    (fp_line (start 20.41 -7.41) (end 20.41 -0.99)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ddf6c5c6-9893-4e3d-bd1d-739522c8dd84))
    (fp_line (start 20.41 -0.99) (end 14.6 -0.99)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 56cc20b2-60ca-4f5c-b503-26d685add599))
    (fp_line (start -20.8 -7.8) (end -20.8 -0.6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp dc93e64d-f7aa-4a85-a1d9-500c20b854d8))
    (fp_line (start -20.8 -0.6) (end -14.45 -0.6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 366f751b-8642-4242-9d20-51019b0cb43b))
    (fp_line (start -15.8 -14.4) (end -15.8 -7.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0c285de4-0abd-45d0-9d82-98fd895bd613))
    (fp_line (start -15.8 -7.8) (end -20.8 -7.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 83a20b57-a858-4abf-be93-4a06a7a3c82d))
    (fp_line (start -14.45 -0.6) (end -14.45 7.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6b88206f-2e27-41cc-9d70-b2985e92d2a2))
    (fp_line (start -14.45 7.85) (end 0 7.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c1ac4da1-43d7-4d1a-9b9e-b804aba23573))
    (fp_line (start 0 -14.4) (end -15.8 -14.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 194af157-a375-458b-a7b4-5a85aa81ed4f))
    (fp_line (start 0 -14.4) (end 15.8 -14.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9a3fe9ea-4a13-4529-bcdf-a73c56175202))
    (fp_line (start 14.45 -0.6) (end 14.45 7.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ca1675a1-0c5b-4d35-80ea-45000d0bd21d))
    (fp_line (start 14.45 7.85) (end 0 7.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 48aa10f1-6840-4e93-ad4d-f93790155399))
    (fp_line (start 15.8 -14.4) (end 15.8 -7.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5102d991-b166-4647-8363-80f6717f7604))
    (fp_line (start 15.8 -7.8) (end 20.8 -7.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6de430bc-ca7d-4b17-aff2-112b38aac6b7))
    (fp_line (start 20.8 -7.8) (end 20.8 -0.6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c543fd85-3503-42d1-be76-9d452194093d))
    (fp_line (start 20.8 -0.6) (end 14.45 -0.6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 97c7b170-5e83-462a-96df-b0935382cbc2))
    (fp_line (start -20.3 -7.3) (end -20.3 -1.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp aa7f6789-5ec6-4fb5-8778-68fe8f54af1a))
    (fp_line (start -20.3 -1.1) (end -15.3 -1.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 71ad67ea-e9c7-439e-847b-925c8548f95c))
    (fp_line (start -15.3 -13.9) (end -15.3 -1.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 17742ba0-dc93-4d62-87c6-6a628506bb0b))
    (fp_line (start -15.3 -7.3) (end -20.3 -7.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 87ecf2da-5b03-4e7e-9ff3-8966bda2608a))
    (fp_line (start -15.3 -1.1) (end 15.3 -1.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4eb2d194-504f-477d-a526-d33e0be024de))
    (fp_line (start -13.6 -1.1) (end -12.6 -2.514214)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fc911703-db10-4c3f-a5ed-61ea7d9b2b3b))
    (fp_line (start -12.6 -2.514214) (end -11.6 -1.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 175bf45d-049b-429f-8fa5-cc7b3775ff6f))
    (fp_line (start 15.3 -13.9) (end -15.3 -13.9)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 913a6eb1-2717-4405-912f-897f331448e4))
    (fp_line (start 15.3 -7.3) (end 20.3 -7.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp caeee43b-187b-4d15-8ee8-c1f7ba2717f3))
    (fp_line (start 15.3 -1.1) (end 15.3 -13.9)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 77f54a2b-b621-4331-bd43-0877bc388dde))
    (fp_line (start 20.3 -7.3) (end 20.3 -1.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c55cc370-fd09-4fed-83c4-fbb3da322e21))
    (fp_line (start 20.3 -1.1) (end 15.3 -1.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a8164b6a-cb2e-4162-bd4c-3326645445b1))
    (pad "" np_thru_hole circle (at -17.1 -4.2 90) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask") (tstamp 8aef74f8-d07c-4799-92ab-881d18f17faa))
    (pad "" np_thru_hole circle (at 17.1 -4.2 90) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask") (tstamp b48889d4-eb7f-440a-ad83-e7132f8f6822))
    (pad "1" thru_hole roundrect (at -12.6 0 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.09259296296)
      (net 1 "+12V") (pinfunction "Pin_1") (pintype "passive") (tstamp 91891e81-9ba8-44fc-bbbc-4c0bfc4d8ba9))
    (pad "2" thru_hole oval (at -8.4 0 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 3 "+5V") (pinfunction "Pin_2") (pintype "passive") (tstamp 9602bed2-f6c4-4999-b40a-6342c7be7ea5))
    (pad "3" thru_hole oval (at -4.2 0 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 3 "+5V") (pinfunction "Pin_3") (pintype "passive") (tstamp 63029f04-5086-4f4c-bbab-b82cf6c1c4a8))
    (pad "4" thru_hole oval (at 0 0 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 15 "/VSi") (pinfunction "Pin_4") (pintype "passive") (tstamp 079e54f4-32d2-42ed-98b2-0a7f1be31605))
    (pad "5" thru_hole oval (at 4.2 0 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 14 "/HSi") (pinfunction "Pin_5") (pintype "passive") (tstamp 817252a9-9c63-4d91-b667-833c64ffa753))
    (pad "6" thru_hole oval (at 8.4 0 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 13 "/Ci") (pinfunction "Pin_6") (pintype "passive") (tstamp dd109137-f591-44e3-9a2b-5bd8d815cb3c))
    (pad "7" thru_hole oval (at 12.6 0 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 33 "/AUDIO") (pinfunction "Pin_7") (pintype "passive") (tstamp 2c9b9dd4-5fca-488a-9eab-46e2f218e648))
    (pad "8" thru_hole oval (at -12.6 5.5 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 5 "-12V") (pinfunction "Pin_8") (pintype "passive") (tstamp 7d6f946d-db0a-487e-aba3-86307a040f1a))
    (pad "9" thru_hole oval (at -8.4 5.5 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 34 "/PBL") (pinfunction "Pin_9") (pintype "passive") (tstamp 55529a0f-55db-4c95-b4c2-7c9e63ee82b8))
    (pad "10" thru_hole oval (at -4.2 5.5 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_10") (pintype "passive") (tstamp 5076a14c-f82c-4205-b628-c44bfedd569a))
    (pad "11" thru_hole oval (at 0 5.5 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_11") (pintype "passive") (tstamp d6652b3d-8f1b-431a-b6fb-3b72c7db10d3))
    (pad "12" thru_hole oval (at 4.2 5.5 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_12") (pintype "passive") (tstamp 3c649af3-2f14-4b29-823b-8d34e3cc14bd))
    (pad "13" thru_hole oval (at 8.4 5.5 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_13") (pintype "passive") (tstamp 9960e4b7-c78f-46cc-951b-58b666b64b09))
    (pad "14" thru_hole oval (at 12.6 5.5 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_14") (pintype "passive") (tstamp 61fe3fa1-a22d-4da0-945d-a318ac9d2ca4))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Mini-Fit_Jr_5569-14A1_2x07_P4.20mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:C_0805" (layer "F.Cu")
    (tstamp 22126d94-0ab2-4c92-886e-d244786466b7)
    (at 74.75 110.499999 -90)
    (tags "capacitor")
    (property "LCSC Part" "C15850")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/dd94a119-9712-4d95-b2a9-d18f454aea5b")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "C12" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp b8c8e55d-7408-4446-95f2-66586eb93112)
    )
    (fp_text value "10u" (at 0 0.35 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp d9349b00-7306-4b76-af7f-98befb32554c)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 477e17ea-75fb-46af-ad1b-9235a938ff0c)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 9efa82dd-ac9b-4abe-b664-cc882e0d1aad))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp f20a13b6-72b3-40fc-8a27-335343c11097))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f61922c1-3c28-4a09-9f39-0198f3540554))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0edd8d3f-3ba3-461b-9a74-7d00b23ddc69))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 67688ad4-37b8-4cbe-be3f-8c961c60141b))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ad1e47e4-0659-4022-a0e5-a857f711d20d))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 9569adf9-44b2-4268-84e7-62ed7d1b5996))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 0f7d26f9-a0d9-4190-9502-7c16f30470e8))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 95bb07e5-fc8c-42d1-9769-c48544f3509e))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 76bad799-9581-461c-bdd1-b08ad5d7e660))
    (pad "1" smd roundrect (at -0.85 0 270) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 4e7616f5-e36f-4d55-8572-0d40147bb8d8))
    (pad "2" smd roundrect (at 0.85 0 270) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "-12V") (pintype "passive") (tstamp 8a48f4cf-7f1a-4afe-9720-392645d51d97))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:R_0805" (layer "F.Cu")
    (tstamp 22801aa6-f14b-41ce-ab35-bd67c08316a3)
    (at 109.8525 164.2745 180)
    (tags "resistor")
    (property "LCSC Part" "C17437")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (path "/603933f2-4e23-44f3-8753-1f137e721592")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "R7" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 44fc6eca-cc65-462d-b3e5-13b5e8b8d9c4)
    )
    (fp_text value "130" (at 0 0.35) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 26fb24f6-0105-4f6f-844a-670056df9f06)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 63c72b08-9a1e-453f-8302-a94bebcc022b)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp a84571a9-8f96-49cf-89c6-aa8c950cad5a))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp b19d02bf-4916-43e8-9085-dda91616d043))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp cd710f0b-d345-4efb-b8fb-519ce0cafa63))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp cb3f7d9a-eb6b-4c0e-8eb2-9cc4753b2df3))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 41bd029c-4820-4c1d-b16c-ac17c0e1ec8c))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 10e7683a-426a-4a9a-957b-2ce5412a874d))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 56a24353-be25-48a3-bb08-3803a035d2a0))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8ec5f367-8dce-4b65-b416-23bd7b35d377))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1d7d9ba4-427a-4049-adbe-60d8655eb9e6))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9237341b-eb5c-435f-8f65-dcecaeb02e15))
    (pad "1" smd roundrect (at -0.95 0 180) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp e525ef36-94d8-4fca-8657-3960b3dd5abe))
    (pad "2" smd roundrect (at 0.95 0 180) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/Ro") (pintype "passive") (tstamp 3e7f4d12-b63c-4480-bf4d-7b553b2a67cf))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:C_0805" (layer "F.Cu")
    (tstamp 29b0d09c-9c40-4c31-b77d-61b20e001b64)
    (at 109.5 126.15 -90)
    (tags "capacitor")
    (property "LCSC Part" "C15850")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/5b4989d1-9dc0-4d5f-8329-786aba06cc9d")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "C7" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 4dd8f081-1cfe-4025-9119-a56f72c8b554)
    )
    (fp_text value "10u" (at 0 0.35 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 5e757346-7283-4d25-96e6-227c8d1c84a8)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp ab6d0e28-c51d-4f6e-83f4-e24d36e506bc)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 68540c72-fedd-4f29-8316-7204498bc63f))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 934c8a54-543f-4eff-bf96-c7b015382837))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 05e7779b-d36c-4073-a20a-132cf5ee9bf9))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 44f7253c-94c3-4bdb-814a-01cdbab33af3))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3b5c8839-951c-43a3-9d4c-113a2cf2e71c))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ad02089b-5f63-4d4b-a5cc-031e991e2a29))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 5b637573-30c0-4eaf-afba-b0ae5ffa7ff5))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp f83485a3-ad57-49a5-bf81-d273c5b62bcb))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 95190bb4-1507-461d-9d7b-d82eed8714fc))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp bb0da6b3-4b0c-4dcf-9b82-980fa3edf5f2))
    (pad "1" smd roundrect (at -0.85 0 270) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+5V") (pintype "passive") (tstamp 11332726-254d-4f0a-af25-a0de69c17ea2))
    (pad "2" smd roundrect (at 0.85 0 270) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 736a5723-d742-4fcb-949d-093f7d6150f5))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:C_0805" (layer "F.Cu")
    (tstamp 2c9e9571-2c9e-4ff8-9ef4-8f16c253e0b1)
    (at 106.26 189.611)
    (tags "capacitor")
    (property "LCSC Part" "C15850")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/3bb35c84-f4b5-4b16-87e8-7b7e7edd9e31")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "C16" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 8e10462c-628d-47cb-bb9b-b03b46695291)
    )
    (fp_text value "10u" (at 0 0.35) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp a5380759-2048-48cd-90dc-c41b428d1566)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 8046fec2-006a-4462-b3a1-f6ae33c4f1e5)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp a2169280-8620-42d0-bcd1-64e355afd95c))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 13837056-264c-41ca-83fe-164696cd83a5))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9e61826f-4b25-4bf8-9f7b-5262fbe1d604))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b04dcc21-4b40-4b24-b55f-df6b00ea248c))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9926e495-889a-46f4-b587-6e88cc3e8335))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 188f0730-b640-4cc6-b15e-60f57a73db2e))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 2fc3dfe0-2ec1-4b35-bcaa-a2d00629c234))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 7c5d60de-a146-4576-968b-33dbef3e715b))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 00d6c652-b49b-468b-b322-ee8ff2e9da6f))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 99f061ba-9163-4239-92b9-5ac5aa2a140e))
    (pad "1" smd roundrect (at -0.85 0) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3") (pintype "passive") (tstamp 4962ff6a-5894-4814-8923-3326a4b23169))
    (pad "2" smd roundrect (at 0.85 0) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 11e6d8be-513f-45dd-b173-0f035bd32abc))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Molex:Molex_Mini-Fit_Jr_5569-24A1_2x12_P4.20mm_Horizontal" (layer "F.Cu")
    (tstamp 40a3fc71-f519-4269-ae7d-e399451333e5)
    (at 118.4 106.4 -90)
    (descr "Molex Mini-Fit Jr. Power Connectors, old mpn/engineering number: 5569-24A1, example for new mpn: 39-29-4249, 12 Pins per row, Mounting: PCB Mounting Flange (http://www.molex.com/pdm_docs/sd/039291047_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Mini-Fit_Jr top entryscrew_flange")
    (property "LCSC Part" "C477841")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x12, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (path "/7aafd51f-54dc-4ae7-8428-e205cdd5dbe1")
    (attr through_hole)
    (fp_text reference "J2" (at 23.1 -15.1 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fc7b7bb1-393c-48e3-b88a-c11d81735272)
    )
    (fp_text value "ATX" (at 23.1 8.55 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0a1e6b06-11cf-42a3-b80d-3a27ff38929d)
    )
    (fp_text user "${REFERENCE}" (at 23.1 -13.2 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e908852e-db5e-4ccb-b000-e3911ed39608)
    )
    (fp_line (start -7.81 -7.41) (end -7.81 -0.99)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d8f2d713-5170-4fb9-8295-ac5cbaea1d59))
    (fp_line (start -7.81 -0.99) (end -2 -0.99)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fea62d54-aab4-4b7e-9621-cb0860d5efd7))
    (fp_line (start -2.81 -14.01) (end -2.81 -7.41)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5bb9dc0a-424f-4c6e-8359-fd821167205c))
    (fp_line (start -2.81 -7.41) (end -7.81 -7.41)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6b2e5d34-e0db-4779-9d6e-fe1640818697))
    (fp_line (start -2.6 -0.3) (end -2 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d5cd1926-e091-4b39-8a80-31ea3f84bac4))
    (fp_line (start -2.6 0.3) (end -2.6 -0.3)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 771fc506-8805-4414-831d-be99e4efec2e))
    (fp_line (start -2 0) (end -2.6 0.3)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5540d82a-0a5d-4938-8818-c50607c89023))
    (fp_line (start -0.3 2.11) (end -0.3 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e3243638-d196-4000-8d7a-a04557082b16))
    (fp_line (start 0.3 2.11) (end 0.3 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0bd87142-9b40-4e5f-a9b5-4c0054224e70))
    (fp_line (start 1.61 -1) (end 2.59 -1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3746eb92-39af-4d85-b149-39a8ca5f52a6))
    (fp_line (start 3.9 2.11) (end 3.9 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7584011b-a8cd-4fbd-8910-0c55189349f1))
    (fp_line (start 4.5 2.11) (end 4.5 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d7a66732-5ae6-4653-91ae-18b913b7da87))
    (fp_line (start 5.81 -1) (end 6.79 -1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c7b45fd2-5b0e-4745-8db1-d0f38be0fdc8))
    (fp_line (start 8.1 2.11) (end 8.1 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a6079afa-340f-4527-a698-51fa4cb9e21c))
    (fp_line (start 8.7 2.11) (end 8.7 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b695d951-bc92-432c-864f-6f074c146857))
    (fp_line (start 10.01 -1) (end 10.99 -1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3c8fac85-b9b8-487c-9b94-a9f48d133c78))
    (fp_line (start 12.3 2.11) (end 12.3 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4f8f97c1-44cc-41c6-a0ef-b325fa8970a3))
    (fp_line (start 12.9 2.11) (end 12.9 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a5eba0a7-453e-4006-9748-e9193f82de93))
    (fp_line (start 14.21 -1) (end 15.19 -1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 58324621-d3f9-4026-b7fd-b265bac60257))
    (fp_line (start 16.5 2.11) (end 16.5 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7288906c-fca4-4f51-b258-adc224150a89))
    (fp_line (start 17.1 2.11) (end 17.1 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bf7bb7b8-708e-4903-902f-6082b9cc2443))
    (fp_line (start 18.41 -1) (end 19.39 -1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f2bf5a61-98a8-4569-9ece-85a6ea34719a))
    (fp_line (start 20.7 2.11) (end 20.7 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 688c8b34-50f3-423c-a86d-f942e6304608))
    (fp_line (start 21.3 2.11) (end 21.3 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 50d82c4c-33bb-4aba-8b58-1496f3eb4fb0))
    (fp_line (start 22.61 -1) (end 23.59 -1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bb129c47-ed52-4e5b-bac1-6d0c3c6d3fd0))
    (fp_line (start 23.1 -14.01) (end -2.81 -14.01)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 56b8be4a-8e24-45f5-b4d0-56ca2d01d339))
    (fp_line (start 23.1 -14.01) (end 49.01 -14.01)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 60de45b9-31b5-4db3-817c-290be6d28374))
    (fp_line (start 24.9 2.11) (end 24.9 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3e8ca6fc-13d1-43c2-ae31-2d01df2774dd))
    (fp_line (start 25.5 2.11) (end 25.5 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3aa56bd2-a33a-4356-a636-327c134cb2e9))
    (fp_line (start 26.81 -1) (end 27.79 -1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 383c7350-a24b-4b39-a8b5-e607c01a82b5))
    (fp_line (start 29.1 2.11) (end 29.1 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5132a611-52df-4674-845c-3fe2b48b10d6))
    (fp_line (start 29.7 2.11) (end 29.7 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp aaab4043-70c3-4080-ae98-14401a6cfc5d))
    (fp_line (start 31.01 -1) (end 31.99 -1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 088ea644-7927-4236-b1bb-c933ccdd6ccb))
    (fp_line (start 33.3 2.11) (end 33.3 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0aaebe37-c6f7-49d2-b0a0-df5ab90eba63))
    (fp_line (start 33.9 2.11) (end 33.9 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e4cf8398-1ea8-4055-a660-0b4441db871a))
    (fp_line (start 35.21 -1) (end 36.19 -1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a108047c-9479-4fb0-988d-09e71ad37659))
    (fp_line (start 37.5 2.11) (end 37.5 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1f0c9786-0ac8-4bc8-8229-28461f1d669b))
    (fp_line (start 38.1 2.11) (end 38.1 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 81788bc0-ce42-46b5-bfea-90fa580219bd))
    (fp_line (start 39.41 -1) (end 40.39 -1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 36b3ccfb-bf63-4764-838c-383c0828675d))
    (fp_line (start 41.7 2.11) (end 41.7 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5521443c-832c-49ef-9ad0-321058dd625e))
    (fp_line (start 42.3 2.11) (end 42.3 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ec67dd11-76db-4ba7-969c-c5a5e7d2e18e))
    (fp_line (start 43.61 -1) (end 44.59 -1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f99bc044-9be9-4379-8c30-5698d07529cb))
    (fp_line (start 45.9 2.11) (end 45.9 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp da579cac-7d5e-474f-9046-32346906c94d))
    (fp_line (start 46.5 2.11) (end 46.5 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5507a9c8-3854-4766-bcc0-6b0a70f9b2c6))
    (fp_line (start 49.01 -14.01) (end 49.01 -7.41)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 45af0373-f2b8-4f84-a1c8-0df08f5128e1))
    (fp_line (start 49.01 -7.41) (end 54.01 -7.41)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fb1a75b0-5d1c-4484-804c-b0d1b32959af))
    (fp_line (start 54.01 -7.41) (end 54.01 -0.99)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b249dfad-efe5-414e-bb85-f3ae04b9184c))
    (fp_line (start 54.01 -0.99) (end 48.2 -0.99)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dd079fa2-80b8-4dd2-a11a-24d9846c4412))
    (fp_line (start -8.2 -7.8) (end -8.2 -0.6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 26bc75ec-7e15-4dfa-b2db-97b3618132e6))
    (fp_line (start -8.2 -0.6) (end -1.85 -0.6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e455eaaf-bf6d-4356-9b0d-71a8dbc0fbbe))
    (fp_line (start -3.2 -14.4) (end -3.2 -7.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 732dfaad-1e29-458a-ab03-ed04ac562e56))
    (fp_line (start -3.2 -7.8) (end -8.2 -7.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c845ae57-aa40-462a-b151-38f219f5598d))
    (fp_line (start -1.85 -0.6) (end -1.85 7.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 50acf66a-4f66-4d2e-9c0d-231a902b0f2b))
    (fp_line (start -1.85 7.85) (end 23.1 7.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fb7e4471-7d0a-4b54-9d7f-4a70282ec875))
    (fp_line (start 23.1 -14.4) (end -3.2 -14.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp dc751ae5-3dd9-4d84-8aa1-77de27f2772f))
    (fp_line (start 23.1 -14.4) (end 49.4 -14.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9abe151d-1d14-430e-b7b1-a1c7107e2026))
    (fp_line (start 48.05 -0.6) (end 48.05 7.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2642645c-fc2c-4842-91d0-b5725a47a6d0))
    (fp_line (start 48.05 7.85) (end 23.1 7.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a10e4b11-7f6a-4178-9720-446768dc2fe4))
    (fp_line (start 49.4 -14.4) (end 49.4 -7.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 263edeb8-f71c-4029-9c72-8accc72104cf))
    (fp_line (start 49.4 -7.8) (end 54.4 -7.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 81f92f94-905d-4d4a-b9b1-d3e4eb867366))
    (fp_line (start 54.4 -7.8) (end 54.4 -0.6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp faa3995f-eccc-41e1-93eb-64bcc8e6c693))
    (fp_line (start 54.4 -0.6) (end 48.05 -0.6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5f8aa200-4993-4cfe-bbbf-d5c2481f490a))
    (fp_line (start -7.7 -7.3) (end -7.7 -1.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ce97f0e4-af46-4237-a30a-cb930e8f8158))
    (fp_line (start -7.7 -1.1) (end -2.7 -1.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b98b0fb3-ba48-448e-9d6e-b39194e07c1a))
    (fp_line (start -2.7 -13.9) (end -2.7 -1.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 573259b5-5bc0-486b-bcc6-e6c186abc442))
    (fp_line (start -2.7 -7.3) (end -7.7 -7.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 588d9381-469d-40f1-97bd-a4d6d769ea5e))
    (fp_line (start -2.7 -1.1) (end 48.9 -1.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3d32c98e-fd4a-4137-8a9d-8f7d86f6ba5a))
    (fp_line (start -1 -1.1) (end 0 -2.514214)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fe1dfd25-b2ae-4222-a364-a0fc1a908a58))
    (fp_line (start 0 -2.514214) (end 1 -1.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 94ec5ab3-7890-4186-b26a-19d0a5a1d5bc))
    (fp_line (start 48.9 -13.9) (end -2.7 -13.9)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3602141b-372b-460c-9d11-84f02b92923d))
    (fp_line (start 48.9 -7.3) (end 53.9 -7.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp deda8967-2946-439d-aa3e-ad6489f8dd7e))
    (fp_line (start 48.9 -1.1) (end 48.9 -13.9)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d3e3fccc-c5ba-4146-9b7c-f27e5fd0955f))
    (fp_line (start 53.9 -7.3) (end 53.9 -1.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1a3191aa-3003-4f8d-9baa-4f5a8e5c1273))
    (fp_line (start 53.9 -1.1) (end 48.9 -1.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 263037b8-ab3b-46de-a473-59bfb686cc19))
    (pad "" np_thru_hole circle (at -4.5 -4.2 270) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask") (tstamp d3b5886f-058c-42ca-8e8f-c27ff8630752))
    (pad "" np_thru_hole circle (at 50.7 -4.2 270) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask") (tstamp e37dbc6a-5654-44e8-8296-e5d28d8eff77))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.09259296296)
      (net 4 "+3V3") (pinfunction "Pin_1") (pintype "passive") (tstamp f17e5962-9d7e-4e54-8810-61493c261604))
    (pad "2" thru_hole oval (at 4.2 0 270) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 4 "+3V3") (pinfunction "Pin_2") (pintype "passive") (tstamp 46afe530-4f81-46a0-9a94-54dbd76ef041))
    (pad "3" thru_hole oval (at 8.4 0 270) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive") (tstamp bd3453d0-a43d-4026-86e0-00fed84be3a7))
    (pad "4" thru_hole oval (at 12.6 0 270) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 3 "+5V") (pinfunction "Pin_4") (pintype "passive") (tstamp f4af3047-c0b4-467b-8ea2-c7a7169bfa9e))
    (pad "5" thru_hole oval (at 16.8 0 270) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_5") (pintype "passive") (tstamp e1607593-4e44-4103-8f7d-ff6b9a293ad7))
    (pad "6" thru_hole oval (at 21 0 270) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 3 "+5V") (pinfunction "Pin_6") (pintype "passive") (tstamp a351317a-57b6-46c1-9eb7-eb39882237df))
    (pad "7" thru_hole oval (at 25.2 0 270) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_7") (pintype "passive") (tstamp e53c9e2e-cd87-41b3-a134-7bfdc67c3bf7))
    (pad "8" thru_hole oval (at 29.4 0 270) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 9 "/PWR_OK") (pinfunction "Pin_8") (pintype "passive") (tstamp 0ec45a1d-2ffa-4690-bdcd-79d28464e7c7))
    (pad "9" thru_hole oval (at 33.6 0 270) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 10 "+5VP") (pinfunction "Pin_9") (pintype "passive") (tstamp 571968e8-1c5f-4a84-a743-86d84095f5b3))
    (pad "10" thru_hole oval (at 37.8 0 270) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pinfunction "Pin_10") (pintype "passive") (tstamp b99389ef-d901-4b3f-b191-059c2b519215))
    (pad "11" thru_hole oval (at 42 0 270) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pinfunction "Pin_11") (pintype "passive") (tstamp 45574cbc-1a1a-498c-b75e-5f70cc7a1e7a))
    (pad "12" thru_hole oval (at 46.2 0 270) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 4 "+3V3") (pinfunction "Pin_12") (pintype "passive") (tstamp 59bb8570-8415-4cca-be54-1ad83c49f032))
    (pad "13" thru_hole oval (at 0 5.5 270) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 4 "+3V3") (pinfunction "Pin_13") (pintype "passive") (tstamp 1afd3943-41e5-4258-8cfb-590717c0a9d0))
    (pad "14" thru_hole oval (at 4.2 5.5 270) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 5 "-12V") (pinfunction "Pin_14") (pintype "passive") (tstamp dc5a4886-108e-433c-a019-e4f0606b8f29))
    (pad "15" thru_hole oval (at 8.4 5.5 270) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_15") (pintype "passive") (tstamp d0965233-1a18-4a96-b94b-738fa3895c18))
    (pad "16" thru_hole oval (at 12.6 5.5 270) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 32 "/~{PS_ON}") (pinfunction "Pin_16") (pintype "passive") (tstamp 8485a108-b61a-45f7-a527-c03228a5b62e))
    (pad "17" thru_hole oval (at 16.8 5.5 270) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_17") (pintype "passive") (tstamp 7645eaa2-0c9b-4ccc-831e-fb5a0a89a5d3))
    (pad "18" thru_hole oval (at 21 5.5 270) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_18") (pintype "passive") (tstamp db0848d5-efc1-4296-8c89-45b0bbf53a54))
    (pad "19" thru_hole oval (at 25.2 5.5 270) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_19") (pintype "passive") (tstamp 1c9d8af6-ab4b-48c0-b107-036190e379bb))
    (pad "20" thru_hole oval (at 29.4 5.5 270) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 27 "unconnected-(J2-Pin_20-Pad20)") (pinfunction "Pin_20") (pintype "passive+no_connect") (tstamp 06d1c701-62bd-4550-b611-73310f1b3b50))
    (pad "21" thru_hole oval (at 33.6 5.5 270) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 3 "+5V") (pinfunction "Pin_21") (pintype "passive") (tstamp 1df53fe1-9ccd-4c50-bfca-490d1c0dcb05))
    (pad "22" thru_hole oval (at 37.8 5.5 270) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 3 "+5V") (pinfunction "Pin_22") (pintype "passive") (tstamp 412c698c-8289-41e8-834c-b23abfac710c))
    (pad "23" thru_hole oval (at 42 5.5 270) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 3 "+5V") (pinfunction "Pin_23") (pintype "passive") (tstamp 031fcf8b-038b-4e1a-967a-a32754e429c8))
    (pad "24" thru_hole oval (at 46.2 5.5 270) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_24") (pintype "passive") (tstamp 845b2dd5-4742-466b-8890-bb045df26624))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Mini-Fit_Jr_5569-24A1_2x12_P4.20mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:C_0805" (layer "F.Cu")
    (tstamp 4d979971-40a9-498b-89de-e054f5bf7f7b)
    (at 109.5 143.35 90)
    (tags "capacitor")
    (property "LCSC Part" "C15850")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/268e9011-391d-4f14-ae15-f9316e74c4e8")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "C4" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp fe16e8cf-4e49-4456-9311-5e928e0b25c4)
    )
    (fp_text value "10u" (at 0 0.35 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 689bc40b-789e-4a47-be89-05cbf89f20f4)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 2808ce35-666c-4741-a436-94ef6014b091)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 9c28d2f6-d440-4356-b406-cb29488acc19))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp a4dd5df7-07c9-4c02-b3cb-a9d29c8aac68))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ef958447-67ca-42ce-9739-d4793773b97c))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7280a51e-a1d5-48e5-bf7b-732339e64cf1))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 65b33894-8fa9-4171-ba32-ae911d1decbc))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1fe4408d-5cf4-4512-b82d-856c797edd14))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp dc87fd87-85b1-4c03-a6a4-6c442b0c80dc))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 562fee0e-b2b7-4c14-b19b-ddd06dc816dd))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp f7494509-8177-4474-a69c-18ea12d4175c))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp bdbf1c50-b7db-4243-9ad8-4acb162095ef))
    (pad "1" smd roundrect (at -0.85 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+5V") (pintype "passive") (tstamp f39480af-f84e-4b89-84ed-959434e0d938))
    (pad "2" smd roundrect (at 0.85 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 04a5e764-4605-4752-aceb-028a72a764df))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:C_0805" (layer "F.Cu")
    (tstamp 59b7577b-fed1-47f3-b56f-12ffcbaaee89)
    (at 74.75 181.55 90)
    (tags "capacitor")
    (property "LCSC Part" "C15850")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/4f9024bd-2ffa-4c71-9a14-08e83dfd6d9d")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "C22" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp e46ca58f-cf8a-4174-8181-1a99f0931c3a)
    )
    (fp_text value "10u" (at 0 0.35 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 1c2c37d5-b3be-4155-9520-0cd77add4db7)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp e80325d5-e2c3-4f3f-9bb3-edfabd93fbca)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp cc961a2e-1034-4100-83bc-68c28159068b))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 9581f386-b437-4bbf-b983-2b30c5417fc8))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 10afe7d5-d7c5-4f25-b96c-170fe028aa24))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3636eae5-44cb-4d56-aa67-677ad68c73e1))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c7ba0746-5bc9-4590-acf5-980b6237168d))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b7d48bfe-6ba0-4680-8bac-8ebc5e6e91d6))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 86b9d58a-da4c-4c07-af0c-c9fef3e44d38))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp d54797dd-9059-4ff4-bfb4-8bc50fcd1e8b))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp bb5461a3-a5e2-44ad-b5d8-4abb745d4138))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 9bcbbfc1-90d8-407f-a4af-0e876768889e))
    (pad "1" smd roundrect (at -0.85 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+5V") (pintype "passive") (tstamp 508bbc4f-d786-42c6-887b-387c259d3394))
    (pad "2" smd roundrect (at 0.85 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp a0f5bc6e-a00f-4f87-a857-1b76a6ae0467))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical" (layer "F.Cu")
    (tstamp 644314a9-2555-4496-ac31-19dd5f92920d)
    (at 39.16 128.3)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (property "LCSC Part" "C65114")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (path "/e0630b04-5ad6-421c-bde5-f6976c9bf503")
    (attr through_hole)
    (fp_text reference "J1" (at 1.27 -2.33) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e676d732-699a-4fae-b1b9-2e8107a180a0)
    )
    (fp_text value "XOR" (at 1.27 7.41) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 59cbdc14-d747-41ab-b18e-ade17f92852b)
    )
    (fp_text user "${REFERENCE}" (at 1.27 2.54 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 75950aa6-dc55-4f24-9eb4-9e0f91b24381)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0397daab-f18b-49d4-857b-965d2ada20ac))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bf933c37-e49c-4dd9-b31a-7502619cc1a6))
    (fp_line (start -1.33 1.27) (end -1.33 6.41)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 914e18e0-27bd-4f53-a44d-9f06750e9e2b))
    (fp_line (start -1.33 1.27) (end 1.27 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a0b1365c-491e-4c5c-9d81-29c29a02f5ca))
    (fp_line (start -1.33 6.41) (end 3.87 6.41)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3db514e1-6b38-4de6-ac56-8f810cdefe20))
    (fp_line (start 1.27 -1.33) (end 3.87 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 59358b2e-1d6d-4551-8286-56868c5c52da))
    (fp_line (start 1.27 1.27) (end 1.27 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3aa47a26-7599-48fe-a9c5-8bb00403417f))
    (fp_line (start 3.87 -1.33) (end 3.87 6.41)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a68c80ad-6203-4d77-80f9-10f8d3aba4e9))
    (fp_line (start -1.8 -1.8) (end -1.8 6.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 34b64430-5110-4acb-89c7-eaae02b2bfca))
    (fp_line (start -1.8 6.85) (end 4.35 6.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9074e87e-9603-4dce-b4ac-a80fe16fecad))
    (fp_line (start 4.35 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 954e52f0-bc5d-41c4-928e-2bc1a09f137e))
    (fp_line (start 4.35 6.85) (end 4.35 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a747d788-91b8-4e53-8771-31fdb3a34e66))
    (fp_line (start -1.27 0) (end 0 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f3d039c0-3afb-46ae-9f2a-35fd5de0dee8))
    (fp_line (start -1.27 6.35) (end -1.27 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5911aec6-be98-4c4a-b2c1-39b8f0bfc8d8))
    (fp_line (start 0 -1.27) (end 3.81 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9b66d103-f13f-40ff-aef5-e4aa9b471e40))
    (fp_line (start 3.81 -1.27) (end 3.81 6.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4f457b67-bb91-4a44-a6f5-68b8c2d09126))
    (fp_line (start 3.81 6.35) (end -1.27 6.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6815d227-f5c7-41c6-8572-39bf01265879))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "/VSx") (pinfunction "Pin_1") (pintype "passive") (tstamp 655d51b1-dd17-44ec-b97a-7fe0271b8883))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive") (tstamp ac745106-cd1f-4359-80b7-f3724c12ad27))
    (pad "3" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "/HSx") (pinfunction "Pin_3") (pintype "passive") (tstamp b41b012d-bc73-43f1-8a86-ed5d91fd86c6))
    (pad "4" thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_4") (pintype "passive") (tstamp b4d57a9a-2c34-4beb-86d9-95b8d2fdc600))
    (pad "5" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 26 "/Cx") (pinfunction "Pin_5") (pintype "passive") (tstamp d7cea250-dc60-4c73-863c-81001d8410ff))
    (pad "6" thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_6") (pintype "passive") (tstamp 849e7c79-72b0-4826-bed5-e471e783d3fd))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:PasteHole_1.152mm_NPTH" (layer "F.Cu")
    (tstamp 6e5000e1-20d2-4144-8dfb-4b82b7acfce6)
    (at 64.389 191.135)
    (descr "Circular Fiducial, 1mm bare copper top; 2mm keepout (Level A)")
    (tags "marker")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.1)))
      (tstamp 6a5ea8a0-c974-4d15-a94c-ba74d244984f)
    )
    (fp_text value " " (at 0 2) (layer "F.Fab") hide
        (effects (font (size 0.508 0.508) (thickness 0.127)))
      (tstamp 3a7199ea-6573-4e92-a2d5-4b44eb341db0)
    )
    (fp_circle (center 0 0) (end 1 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp c80121ce-3a24-43ba-a14b-5c1f0d3d2433))
    (pad "" np_thru_hole circle (at 0 0) (size 1.152 1.152) (drill 1.152) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.148) (tstamp 7a5bc1f8-72c9-449e-bdfa-9dac923a8a04))
  )

  (footprint "stdpads:R_0805" (layer "F.Cu")
    (tstamp 720d6621-8fab-4a01-94a0-3d4cbb8007c8)
    (at 35.0545 132.6515 180)
    (tags "resistor")
    (property "LCSC Part" "C17513")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (path "/8842ce2b-4498-44b0-8ecf-4172deec86bd")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "R2" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 868639c2-ac24-467f-bb1b-a76f8d39bd01)
    )
    (fp_text value "2k2" (at 0 0.35) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 551b3b58-bceb-49d6-a852-6af311147105)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp d8807f9f-d1f5-4ed8-8da9-bb6facf3474f)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 503d4ac7-e7f0-4ea4-af65-3bcb68aaf8aa))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp c118c90d-3f0d-4b20-b19b-b0bc29a0c513))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b26ca268-f8ec-43d5-942e-ac89337fcf9e))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b6cb0182-f8c8-43ed-9e40-6d7f6f4b9181))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0604e7fc-8bf4-4ee2-a0a8-00730df900a3))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ca9713a2-e0c1-4abc-bd8e-8cf53fc3ae37))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e5a6af57-1e18-4900-8ff9-eea7cd7d624b))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1dea25a6-f292-4cdc-9ae3-df29a5536ae7))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bb14de9b-c4d3-4b51-a9b8-49b1842abc30))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 448b63d2-6411-47d4-8909-6c5c0ebf76bc))
    (pad "1" smd roundrect (at -0.95 0 180) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/HSx") (pintype "passive") (tstamp 035d3963-8957-4495-a35e-27206b956dbf))
    (pad "2" smd roundrect (at 0.95 0 180) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3") (pintype "passive") (tstamp a79114bd-9175-4c6a-9ada-4376cf77648e))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:R_0805" (layer "F.Cu")
    (tstamp 73b7173b-c2aa-4017-a5ad-83cec039ff09)
    (at 106.36 164.2745)
    (tags "resistor")
    (property "LCSC Part" "C17471")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (path "/d29f7460-4e99-482d-8f17-135e1a88e6c9")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "R6" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp e0fdbb2e-ca6b-4971-88f7-4674cce7ecbf)
    )
    (fp_text value "150" (at 0 0.35) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp f2970d88-27d7-4fab-8896-e93c6c7b064b)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp c9ecd113-33f1-45b1-9e51-104c994cb07f)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 881487ca-9ed6-429a-add5-3a227cc36c52))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp b736b902-96b7-4bd6-be09-cadb281897b4))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 46407817-1360-4780-9601-d07bf1ffdc25))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a66eb396-0410-43f5-a37d-ef2abb980a3a))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp db040fd7-85c4-4e0f-a5ad-ce3599f47efa))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3a1c242e-c8b6-4cbf-ba6f-474b170eb075))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ad1344da-c854-436d-aeb7-0a72541a073f))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c8c3c5a6-481c-49d6-9d61-ccc20095a806))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0768ccc2-734b-4a02-9ab0-4e4bdb07d6bb))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 34ce5f70-42f6-44bf-87de-360708d28b83))
    (pad "1" smd roundrect (at -0.95 0) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(R6-Pad1)") (pintype "passive") (tstamp 723725ba-4c8f-4e59-bb95-edf37aab8126))
    (pad "2" smd roundrect (at 0.95 0) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/Ro") (pintype "passive") (tstamp 80919938-79ac-4a1d-958e-60fc50d682c5))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:R_0805" (layer "F.Cu")
    (tstamp 7a6a8cb5-5575-4105-9510-066555129b61)
    (at 113.3475 181.229)
    (tags "resistor")
    (property "LCSC Part" "C17714")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (path "/5d7a86a0-89d5-4751-acf3-e01c5e12b8e6")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "R5" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp d44c9e78-9716-4a66-bffa-39ac67b03711)
    )
    (fp_text value "47" (at 0 0.35) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp b3599bf0-dfeb-4ac6-abe9-d625558d1294)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 381dad02-0862-48ac-9715-4defdd4701ed)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp ce4ec2a9-b4b1-4ee8-9aa0-fb8615fe550b))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 7f836bcb-1cfb-44cc-9d14-b7a87a9ad62b))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5804f68f-738b-41bf-9268-c6b55035ee48))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1335e3c3-3724-4eca-b7e1-8e7135fe285c))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 914c836a-b0c1-41dd-9f25-e666f6e939aa))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f3ca632d-0f70-40dc-bffb-24825362c007))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b183805f-2ead-467a-aa9a-4a1cf2df154e))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 41519696-bf91-4b07-95ab-ad9cb45374ce))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8acedadc-2fa6-4fde-b3c9-4cd449605212))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3f15f7e1-6573-4abc-8253-117352fcf348))
    (pad "1" smd roundrect (at -0.95 0) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(R5-Pad1)") (pintype "passive") (tstamp e9983c43-62bd-4183-a131-97d57a4ecd74))
    (pad "2" smd roundrect (at 0.95 0) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/VSo") (pintype "passive") (tstamp cae9e9c8-bede-4aa9-830c-cb3b00617c19))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:C_0805" (layer "F.Cu")
    (tstamp 8107bb48-897a-46d9-87a0-bef50ca9163c)
    (at 100.247 177.927 180)
    (tags "capacitor")
    (property "LCSC Part" "C15850")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/2c2096d6-d370-45dd-89cc-03d88097cbcb")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "C17" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp ea620a82-9a65-46db-8df4-d8e3fa138b96)
    )
    (fp_text value "1n" (at 0 0.35) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 0f527e70-ee2e-41e7-9499-7d46fce22a10)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 3d9231ae-0e63-4f50-bd16-325a3d29312e)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp cf064cbb-4d73-477a-beff-05993129b252))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 042063e8-1829-48d5-95cb-22bce39f05db))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e1b47e47-f563-43b5-83a4-462aa1222b70))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 194fd2c4-2ff2-4f8f-8bb1-90f89f89c6ee))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 933752b0-ed73-4941-9965-210c0d123427))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b33af0ba-b372-465b-94ce-4e1042aa5837))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp d145a1f0-4b48-4c1a-87b2-e7093546fcad))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 8a946306-8cb9-4cbf-bbbd-48d8bfd49f8b))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp de5b807c-874a-47b0-a8ee-046afdadb52d))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp e9d8ff50-8808-4472-92d8-6d6a71f3c341))
    (pad "1" smd roundrect (at -0.85 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(C17-Pad1)") (pintype "passive") (tstamp 1a800aec-1b58-4b35-aea6-b8184b82c354))
    (pad "2" smd roundrect (at 0.85 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/HSf") (pintype "passive") (tstamp ec25e083-5e08-4e9f-843a-069aadcc6c06))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:C_0805" (layer "F.Cu")
    (tstamp 820ae180-8694-443a-9433-251e2db3f40c)
    (at 74.75 122.4 90)
    (tags "capacitor")
    (property "LCSC Part" "C15850")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/d4ea4e32-3f34-4afc-86b3-ceede9f70da2")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "C6" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 66518670-634d-4b34-9120-16a79f822b43)
    )
    (fp_text value "10u" (at 0 0.35 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp bc06630a-3ac1-46c4-a166-bf4cfe164f4d)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 24124c23-9199-426e-a22c-16507727d026)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 6e5d2c49-e036-4314-b4e9-23f4520b1a27))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 8f28b0d9-7335-41e0-a6c3-c6a5b31e1f01))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b8a4cd10-7b1d-4b28-96fd-cd5214b75d0e))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6ec78ea8-28c3-4d4b-a479-97c181b48eba))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4fd5c232-61cb-4248-81b9-22a59930bacd))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fb37c198-4ad2-4d36-88a9-c74374438110))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp cfb20c29-c92c-417d-9533-6e8bfb43e15c))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 58824d07-c120-435a-99d1-910b008d5dac))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 00fc3a3f-87ae-4013-ba3a-880ad665766b))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 2fdd7cae-3a2a-4cbd-8da1-8aa63f287861))
    (pad "1" smd roundrect (at -0.85 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+5V") (pintype "passive") (tstamp cb36f71b-f9f1-4fbe-a373-82e91ba7d747))
    (pad "2" smd roundrect (at 0.85 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp f794afca-4b3d-4464-bda9-a001701d9718))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:R_0805" (layer "F.Cu")
    (tstamp 989c0bfc-69b9-4f59-8f19-65df38c10964)
    (at 112.9665 168.3995 -90)
    (tags "resistor")
    (property "LCSC Part" "C17471")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (path "/8fad9e94-00d8-436f-816f-d6b0f6215742")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "R8" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp d3595252-2807-4006-9bf7-10751b93625f)
    )
    (fp_text value "150" (at 0 0.35 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 934bf5ca-9e3b-44e3-80ec-39b0bffe40ba)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 24345771-3156-4fd8-abbe-41d362385a2d)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 48ca9205-0369-4356-9ba5-50fd50929a6c))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 9fbfd5c3-39e5-4709-8028-9375fbc40f88))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp da2fa93c-337b-4a85-9947-8f2a5177ac85))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp acea8251-050f-424b-9f4f-a4a5a6d351f5))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e4f5e757-4a90-46ab-b913-941814f0a1d9))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9d2c86c5-2909-4f10-bb09-688646474c17))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4003972e-6810-48e8-8982-7782f36694fe))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 948e1b45-8bd2-4dff-9812-c962dc79de1c))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a9b27b68-831f-473a-bbb7-0c87c175d6b3))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0198e4ed-ffe4-4e19-b60c-970cc6da779d))
    (pad "1" smd roundrect (at -0.95 0 270) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(R8-Pad1)") (pintype "passive") (tstamp 42bd4309-121f-4d39-bb5c-a4f289939822))
    (pad "2" smd roundrect (at 0.95 0 270) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "/Go") (pintype "passive") (tstamp 99e3f50d-06a5-4a2e-9312-7487dd278f14))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:C_0805" (layer "F.Cu")
    (tstamp 9bbaef6f-46d1-455a-b41d-ebc3316d6a0f)
    (at 109.5 111.45 90)
    (tags "capacitor")
    (property "LCSC Part" "C15850")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/d2a337c2-ae15-4ed8-a3a5-86d959936007")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "C13" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp ed170d68-4cd9-4a33-a531-211185edad8a)
    )
    (fp_text value "10u" (at 0 0.35 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp c33c9adb-272b-48f0-acf5-ea6da38440b9)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 09b117f3-ed70-4f3a-babe-047608839f8c)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 5476c61d-d81c-4327-888c-8faf20c03a8e))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 002b0e2c-decc-4684-bea9-85795e90223d))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9cdb308b-3686-4eff-9704-a8835ceb6411))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e4edfff5-bb7b-4946-9760-0c3ea76343cf))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6d4dc768-2cad-41e1-b65c-ff82aca8085e))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7fa5f646-6f61-4929-820e-edda7a8799a9))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp c5145614-9fbd-498c-a14b-cee19fd2590c))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 5e4050ff-870c-4b3d-888d-01121325f5ad))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 11424060-ae34-44d4-b5ff-e5f1ce357b62))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 3ae03e67-66b9-4410-a4f7-7970e4eba60d))
    (pad "1" smd roundrect (at -0.85 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 970bbf08-33e9-4101-a4fb-48c09ce82804))
    (pad "2" smd roundrect (at 0.85 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "-12V") (pintype "passive") (tstamp 81ac6b46-c925-400b-9464-dafed45a84f6))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:PasteHole_1.152mm_NPTH" (layer "F.Cu")
    (tstamp 9cfa52d1-33fa-4097-959f-7f3370464024)
    (at 119.5705 99.7585)
    (descr "Circular Fiducial, 1mm bare copper top; 2mm keepout (Level A)")
    (tags "marker")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.1)))
      (tstamp 33589176-11d8-4216-bef4-779cb2e294a8)
    )
    (fp_text value " " (at 0 2) (layer "F.Fab") hide
        (effects (font (size 0.508 0.508) (thickness 0.127)))
      (tstamp e3968d77-4a0e-49a6-b1f9-2be25f597e09)
    )
    (fp_circle (center 0 0) (end 1 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp b052afb8-e525-431d-831c-c7f3c3845dce))
    (pad "" np_thru_hole circle (at 0 0) (size 1.152 1.152) (drill 1.152) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.148) (tstamp 3c2f44a0-ff78-4daf-8982-687d8d093ea3))
  )

  (footprint "stdpads:C_0805" (layer "F.Cu")
    (tstamp a00a08d0-cd15-4b95-8841-f0ae4f7e6f43)
    (at 90.717 138.684)
    (tags "capacitor")
    (property "LCSC Part" "C15850")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/ba479457-b3a9-407a-9ea3-4cbd424e7a98")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "C11" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp bf305326-cdf0-41c2-ad2e-6d3d6cfb03f0)
    )
    (fp_text value "10u" (at 0 0.35) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp e30cd634-f4d2-4240-ba82-7c8196230c19)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 292e266f-7c00-4b5e-86e3-3fc352dd23a0)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 0f018052-6a66-49ee-9db4-56830a681ec1))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 97c84dad-cc4c-482d-be6b-c67c3c6f30aa))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 873da199-d2ca-4165-820f-5e8780ac9ed8))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e0a107ae-511b-4f2f-bd0e-8fcbe2434e6a))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0917eb15-2a11-491e-ac3a-dda5a42b4a22))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 24be8dea-7ffc-43b6-ad7c-5c0e753ca220))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 64c9f4eb-cf21-499f-9159-45048ba0751a))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 92caef5c-b8f7-429f-821a-0a45b7f585ba))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp ee4ec7d2-dffe-4eb8-abc1-790504fc825e))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 3d955f27-eae8-4ddc-bbc6-568ef6908ff7))
    (pad "1" smd roundrect (at -0.85 0) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp ead47928-cfd4-4489-ba56-e055c78c147e))
    (pad "2" smd roundrect (at 0.85 0) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "-12V") (pintype "passive") (tstamp 6c6dbbcc-c28c-4c5b-9390-d8855fe6cb82))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:R_0805" (layer "F.Cu")
    (tstamp a7e1a6a7-aade-46d1-98ce-a8104aea613e)
    (at 92.3 161.85)
    (tags "resistor")
    (property "LCSC Part" "C17471")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (path "/d4821e4a-a66d-472c-a56e-eb701bba7a5f")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "R14" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 9b350825-470b-4c48-84b0-fbc9ee23724c)
    )
    (fp_text value "22k" (at 0 0.35) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 1e742f87-4a11-4138-8178-33d6e205ea00)
    )
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 6ce74e33-c91f-4355-8345-7f35478a4494)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp fcedabf1-d8d8-4dfb-86ba-9d7fae9ddb13))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 48a52824-f107-421e-9cae-8c8c5d8b429f))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6c763e7e-9d11-4ff8-859b-ac81d4eaa8b4))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 411f9196-11b8-4bc2-bc3d-8d660636250d))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bcb390b9-0476-403e-b117-afd1262baedd))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp db38bb1f-b1f3-4529-970b-4754bc77136e))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 922bfa1c-8ad6-49ca-b385-7286cd078445))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9d408352-8b18-45a4-8b63-4276c13d38d2))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c4dde333-f49e-4bdf-9595-8d8469388eb7))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 79c43e21-415e-4f6b-8fbb-d2779644b470))
    (pad "1" smd roundrect (at -0.95 0) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "+5VP") (pintype "passive") (tstamp ff964e57-d985-4621-b2bc-08b4236e1061))
    (pad "2" smd roundrect (at 0.95 0) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/~{POR}") (pintype "passive") (tstamp 362fef1e-7534-481f-a76d-f632636f4a93))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:R_0805" (layer "F.Cu")
    (tstamp ab1e3c4c-abb6-410e-a1d0-bae6e7b5c818)
    (at 115.1255 172.2145 -90)
    (tags "resistor")
    (property "LCSC Part" "C17437")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (path "/98215e3a-a587-4653-a3c3-aa038f19473c")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "R11" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp e336bb2d-d5bc-401a-bc46-2ca9ecf1e675)
    )
    (fp_text value "130" (at 0 0.35 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp f855e03a-7286-4acc-830d-1610726dfbd6)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 31a68887-e6f8-44ed-866f-95c85ecf5d3f)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 994b1f92-58ed-4877-8a27-4aa6c0d4307e))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 6cb1d0a8-885a-4e83-8764-a3281f9b4216))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 918ed0b2-810c-4d23-a9bc-ff95f56cbc77))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 901354ae-e553-4027-97d3-c146557b67da))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 60b3337f-c4a2-4983-9337-57d055823319))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c1ed01bc-4e3c-48d7-b71f-eb74869a03b8))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9e433a3a-d9c2-4705-ac9c-1c4244343b22))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 28a5e718-11e0-4e8e-aefb-4dfa8f36a5ee))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f5f50692-1d46-4b3a-9a5b-640a682ede36))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2ba9dc16-de37-4194-b97b-5f70941cc8ce))
    (pad "1" smd roundrect (at -0.95 0 270) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp fa003acd-1f91-4e55-95ee-97c681a6334f))
    (pad "2" smd roundrect (at 0.95 0 270) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/Bo") (pintype "passive") (tstamp 466d0aaa-da60-4667-8912-9eb3a2103065))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:SOIC-14_3.9mm" (layer "F.Cu")
    (tstamp aba0f6d7-6ba6-4936-86a7-d6f180704daa)
    (at 107.8865 183.769 90)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "LCSC Part" "C548853")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Quad 2-input XOR")
    (property "ki_keywords" "TTL XOR2")
    (path "/fee582da-d8ee-4ffd-9b39-10f6951de264")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "U2" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
      (tstamp 144789b2-ade3-4a15-8599-24c021a7a492)
    )
    (fp_text value "74LVC86AD" (at 0 1.016 90) (layer "F.Fab")
        (effects (font (size 0.508 0.508) (thickness 0.127)))
      (tstamp 6313dc37-b7d7-451d-b86f-4428c2d4b1d3)
    )
    (fp_line (start -4.425 0) (end -4.425 -1.95)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 299b4669-13f7-4dbd-940a-6ada43bf0fe4))
    (fp_line (start -4.425 0) (end -4.425 3.45)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fa7eec8f-6016-4695-8591-b952ebef19d3))
    (fp_line (start 4.425 0) (end 4.425 -1.95)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0b0fc818-681a-4109-92bb-fcb67bd1d107))
    (fp_line (start 4.425 0) (end 4.425 1.95)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f65ee9bb-cd2d-4dc7-9a10-d28d2a86fda4))
    (fp_line (start -4.565 -3.7) (end -4.565 3.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp de947b5d-5e72-43e1-9261-ee248984aae9))
    (fp_line (start -4.565 3.7) (end 4.565 3.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9fc764a0-1bdf-41df-9fb0-7bd0e6eba8f0))
    (fp_line (start 4.565 -3.7) (end -4.565 -3.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1682532c-8c3d-4c3e-b6a9-4e7cf639369a))
    (fp_line (start 4.565 3.7) (end 4.565 -3.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ad76347e-a2e0-4309-ab66-445173ebc69e))
    (fp_line (start -4.315 -1.95) (end 4.315 -1.95)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fc805d9f-6a6e-4fc5-a146-a02c719739d9))
    (fp_line (start -4.315 0.975) (end -4.315 -1.95)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b518ffdd-758f-4179-8e16-bec8066336e1))
    (fp_line (start -3.34 1.95) (end -4.315 0.975)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 66e2e7fe-e667-4aae-8d51-38a0e3e0f52a))
    (fp_line (start 4.315 -1.95) (end 4.315 1.95)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5845514e-878a-4453-a2c0-a81c27c6bd15))
    (fp_line (start 4.315 1.95) (end -3.34 1.95)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a5b11cc3-b615-4c50-be38-887679247c68))
    (pad "1" smd roundrect (at -3.81 2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/HSf") (pintype "input") (tstamp a908c23d-93f7-488b-8e24-0f3a2db8d2d4))
    (pad "2" smd roundrect (at -2.54 2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "input") (tstamp dbd05a4a-6f63-4c94-9f90-a818caef0c17))
    (pad "3" smd roundrect (at -1.27 2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(R4-Pad1)") (pintype "output") (tstamp e4697557-e145-4187-90cf-39f9c131e595))
    (pad "4" smd roundrect (at 0 2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/VSi") (pintype "input") (tstamp 851229ae-e1c2-4cac-8b4b-7f8f43cee7bd))
    (pad "5" smd roundrect (at 1.27 2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/VSx") (pintype "input") (tstamp f4432edc-d467-45b6-87b6-5122f0e7c7d5))
    (pad "6" smd roundrect (at 2.54 2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(R5-Pad1)") (pintype "output") (tstamp 26012b6d-3b10-4e4b-b7d3-5c03fc62bd24))
    (pad "7" smd roundrect (at 3.81 2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp ad0472a8-d847-4467-a4d7-504cd3d387f0))
    (pad "8" smd roundrect (at 3.81 -2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(R12-Pad1)") (pintype "output") (tstamp 7f37cec1-f019-45af-8ca6-8923ea387684))
    (pad "9" smd roundrect (at 2.54 -2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/HSi") (pintype "input") (tstamp c456002f-aeb9-4803-bfe7-c4672a8e9c0b))
    (pad "10" smd roundrect (at 1.27 -2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/HSx") (pintype "input") (tstamp d2cffed5-1222-429f-a5fe-9cf581f752fe))
    (pad "11" smd roundrect (at 0 -2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "unconnected-(U2-Pad11)") (pintype "output+no_connect") (tstamp 5572436f-d8e5-454a-b4fb-b7ab18085293))
    (pad "12" smd roundrect (at -1.27 -2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "input") (tstamp 4ed4a10c-e2ab-4fdd-8034-b1e5fca5333e))
    (pad "13" smd roundrect (at -2.54 -2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "input") (tstamp 000c584e-c3d7-4b55-b597-cf7725c2a6f6))
    (pad "14" smd roundrect (at -3.81 -2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3") (pinfunction "VCC") (pintype "power_in") (tstamp 6820f0bf-4c85-4753-92cb-498dbb4634f4))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (footprint "Connector_Dsub:DSUB-15-HD_Female_Horizontal_P2.29x1.98mm_EdgePinOffset3.03mm_Housed_MountingHolesOffset4.94mm" (layer "F.Cu")
    (tstamp b503854d-2ac8-4eb3-82a6-9ddd4419c4b4)
    (at 118.299669 172.45 90)
    (descr "15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x1.98mm, pin-PCB-offset 3.0300000000000002mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 4.9399999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x1.98mm pin-PCB-offset 3.0300000000000002mm mounting-holes-distance 25mm mounting-hole-offset 25mm")
    (property "LCSC Part" "C75754")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "15-pin female D-SUB connector, High density (3 columns), Triple Row, Generic, VGA-connector, Mounting Hole")
    (property "ki_keywords" "connector db15 female D-SUB VGA")
    (path "/a20e4bbe-5294-4407-84e6-cd57ae0c7071")
    (attr through_hole)
    (fp_text reference "J5" (at -4.315 -2.61 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 679af1c4-1afb-4ab8-aa52-39e36bcb375d)
    )
    (fp_text value "VGA" (at -4.315 14.89 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b9db7fea-f028-4481-89eb-f76870ef3c5e)
    )
    (fp_text user "${REFERENCE}" (at -4.315 10.39 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 78b75e7e-ffef-4a02-a370-f1a36667538f)
    )
    (fp_line (start -19.8 -1.67) (end 11.17 -1.67)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 81e598af-6285-4c7f-9834-76cfaa1acb5d))
    (fp_line (start -19.8 6.93) (end -19.8 -1.67)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 46b9a33b-9265-476d-be96-0e2d293a5d24))
    (fp_line (start -0.25 -2.564338) (end 0.25 -2.564338)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b7add21b-380e-468f-9a73-a310c8915c64))
    (fp_line (start 0 -2.131325) (end -0.25 -2.564338)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2f6bec7f-3838-4f7f-b63f-10924c481109))
    (fp_line (start 0.25 -2.564338) (end 0 -2.131325)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b1099408-2b9c-4c42-a9b6-2755e39f10e6))
    (fp_line (start 11.17 -1.67) (end 11.17 6.93)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6d075784-2754-439a-a81e-3c52aa74e9af))
    (fp_line (start -20.25 -2.15) (end -20.25 13.9)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f486647f-1026-4341-819c-f1c16d5daed1))
    (fp_line (start -20.25 13.9) (end 11.65 13.9)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 09fce947-24b8-4d01-b49e-f0fc8f909110))
    (fp_line (start 11.65 -2.15) (end -20.25 -2.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 75da35f0-b7db-47ee-bef6-4f7ba02e3be7))
    (fp_line (start 11.65 13.9) (end 11.65 -2.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d41cef33-2816-4f07-9fb0-af0f8f1dbb1b))
    (fp_line (start -19.74 -1.61) (end -19.74 6.99)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 721913b2-69e9-4209-98c5-c9112523aa2f))
    (fp_line (start -19.74 6.99) (end -19.74 7.39)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d9f66e33-2abe-4958-a447-b1312acb558e))
    (fp_line (start -19.74 6.99) (end 11.11 6.99)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 099a0c4e-e430-4c76-9368-a2efac12a501))
    (fp_line (start -19.74 7.39) (end 11.11 7.39)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 56a6569d-8daa-40d7-b5f7-755534cbaed7))
    (fp_line (start -19.315 7.39) (end -19.315 12.39)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7361fc4d-c948-40da-af0c-0c2e4915d2a2))
    (fp_line (start -19.315 12.39) (end -14.315 12.39)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9f2af288-6235-44fb-ad6b-0aa497620894))
    (fp_line (start -18.415 6.99) (end -18.415 2.05)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d9978ad0-814c-40ac-8299-21e89542859b))
    (fp_line (start -15.215 6.99) (end -15.215 2.05)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c8bd3937-2b36-4129-8d38-91ae7f0c1f40))
    (fp_line (start -14.315 7.39) (end -19.315 7.39)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 590cde78-1675-42c5-97f1-8eb83e6027fa))
    (fp_line (start -14.315 12.39) (end -14.315 7.39)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ba262ac9-e890-4a18-a0d2-1ebffb783f6e))
    (fp_line (start -12.465 7.39) (end -12.465 13.39)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5dc4e0a1-877c-49ec-b19f-2a36e04e8056))
    (fp_line (start -12.465 13.39) (end 3.835 13.39)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0d3e40b2-a82c-42b3-9bdd-3183247b5c36))
    (fp_line (start 3.835 7.39) (end -12.465 7.39)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp edae7adb-f2ee-4611-bd23-80a6170d17af))
    (fp_line (start 3.835 13.39) (end 3.835 7.39)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d2ecd78c-6410-4bef-b0ba-ceaa25349f3d))
    (fp_line (start 5.685 7.39) (end 5.685 12.39)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a2574197-112b-42e9-ad69-34ce591327a8))
    (fp_line (start 5.685 12.39) (end 10.685 12.39)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8409a6e7-edd9-482c-bc78-f0a2bb9070a5))
    (fp_line (start 6.585 6.99) (end 6.585 2.05)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a1edd090-078b-4c0c-8892-1d558356bef2))
    (fp_line (start 9.785 6.99) (end 9.785 2.05)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 09461a54-09c4-465f-bdb9-896fb57c83d6))
    (fp_line (start 10.685 7.39) (end 5.685 7.39)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ae8fc194-a59c-439d-a056-b1daf2889358))
    (fp_line (start 10.685 12.39) (end 10.685 7.39)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 25bf1edc-fa50-4055-93b9-c401f032392c))
    (fp_line (start 11.11 -1.61) (end -19.74 -1.61)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 408ebb3b-919e-4fd0-933c-b35c7b50954f))
    (fp_line (start 11.11 6.99) (end -19.74 6.99)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b1ecd913-2c74-4942-8cc3-e4fcb64bfded))
    (fp_line (start 11.11 6.99) (end 11.11 -1.61)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e5d847a0-2000-43b1-98af-9586d4aac0c2))
    (fp_line (start 11.11 7.39) (end 11.11 6.99)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a759fbab-35dc-440a-b66d-527878368c7a))
    (fp_arc (start -18.415 2.05) (mid -16.815 0.45) (end -15.215 2.05)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 38528e83-54cb-46d0-8651-42dab22586e5))
    (fp_arc (start 6.585 2.05) (mid 8.185 0.45) (end 9.785 2.05)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 53128422-a057-4f84-af75-6786b44bc56a))
    (pad "0" thru_hole circle (at -16.815 2.05 90) (size 4 4) (drill 3.2) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive") (tstamp 8a7f8cc6-e300-4ad3-9674-e56773b2a07e))
    (pad "0" thru_hole circle (at 8.185 2.05 90) (size 4 4) (drill 3.2) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive") (tstamp 56d02688-93dc-4a2c-b651-dc12ea7be942))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "/Ro") (pintype "passive") (tstamp 9951b8ec-e378-4512-b7ae-4648df71fb7d))
    (pad "2" thru_hole circle (at -2.29 0 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "/Go") (pintype "passive") (tstamp c1358503-47f1-4f7b-ba40-fffdec9c3967))
    (pad "3" thru_hole circle (at -4.58 0 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "/Bo") (pintype "passive") (tstamp 0d4dfe90-67a2-4477-ac8e-2c68a1f8ec38))
    (pad "4" thru_hole circle (at -6.87 0 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 35 "unconnected-(J5-Pad4)") (pintype "passive+no_connect") (tstamp d4844ab1-1666-4844-8e85-f9b7d470572d))
    (pad "5" thru_hole circle (at -9.16 0 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive") (tstamp 92ffafa2-4d61-46e9-91fa-2aaa061e733b))
    (pad "6" thru_hole circle (at 1.145 1.98 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive") (tstamp 1ca25b74-189e-4c27-9c7b-2223c08ded0e))
    (pad "7" thru_hole circle (at -1.145 1.98 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive") (tstamp d08c1ae4-21da-43a2-9e00-fb651b3eda7c))
    (pad "8" thru_hole circle (at -3.435 1.98 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive") (tstamp 6f25ec48-e532-4c77-b079-bda18ceb666a))
    (pad "9" thru_hole circle (at -5.725 1.98 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 36 "unconnected-(J5-Pad9)") (pintype "passive+no_connect") (tstamp 6c669d01-8f1c-49b2-97ec-5cb46ee6d57d))
    (pad "10" thru_hole circle (at -8.015 1.98 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive") (tstamp 8ac62436-c733-404a-b7e4-3045b1f815cb))
    (pad "11" thru_hole circle (at 0 3.96 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 37 "unconnected-(J5-Pad11)") (pintype "passive+no_connect") (tstamp 2082894f-0df0-48e7-973c-238ae4516271))
    (pad "12" thru_hole circle (at -2.29 3.96 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 38 "unconnected-(J5-Pad12)") (pintype "passive+no_connect") (tstamp 24e43e3f-56e8-4818-a975-ca16b0a25f87))
    (pad "13" thru_hole circle (at -4.58 3.96 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "/HSo") (pintype "passive") (tstamp 3523a980-2216-4008-a88a-93a25f9529a6))
    (pad "14" thru_hole circle (at -6.87 3.96 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 20 "/VSo") (pintype "passive") (tstamp a2dd951d-9b74-4a7e-be71-0772b02ebe82))
    (pad "15" thru_hole circle (at -9.16 3.96 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 39 "unconnected-(J5-Pad15)") (pintype "passive+no_connect") (tstamp 017b80be-9526-4e03-ab9f-c93a7550bfc0))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-15-HD_Female_Horizontal_P2.29x1.98mm_EdgePinOffset3.03mm_Housed_MountingHolesOffset4.94mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:R_0805" (layer "F.Cu")
    (tstamp b63b643e-9d65-415c-9ff3-2db4a9177acd)
    (at 115.1255 168.4045 -90)
    (tags "resistor")
    (property "LCSC Part" "C17437")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (path "/a35b65d7-b900-4e65-9382-0d16cab06f17")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "R9" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp d483e808-b373-49ff-9b29-3da2b5c9bbfb)
    )
    (fp_text value "130" (at 0 0.35 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp aa545787-2a5e-43dc-8f4b-9eb5f8ff879a)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 31820a50-538e-48d4-89fe-20ae21bce125)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 539d7e5b-245c-43b1-94a7-6209ca24ad34))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp f772675a-575a-4d22-9d75-8479a9a40ddb))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f9e3a42c-195e-4259-8b4d-b2de5a18bfa1))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6597d3ee-f115-4baa-b3ba-599a4f3316ff))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1cb4ec5e-8d3e-4d8b-b585-f1efc74bd5a9))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2f75e88f-f478-419b-a128-834c14b19ee9))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0925390d-78a9-4395-88cd-66416452b904))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 85ae8e75-ed8a-46d7-bd70-bada9bd8d6e7))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d16cc0e6-6522-412a-bac0-f775d8a3680b))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c20cb9ea-4ad3-4d34-82e7-42df5c8543c3))
    (pad "1" smd roundrect (at -0.95 0 270) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 7a89a9aa-1aac-454e-bc2a-c9583f606c97))
    (pad "2" smd roundrect (at 0.95 0 270) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "/Go") (pintype "passive") (tstamp 01d99a99-fdef-4e87-9f8d-f755800aefd8))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:R_0805" (layer "F.Cu")
    (tstamp c4805b26-ba77-4f21-a2b8-eed0f3ad67eb)
    (at 112.9665 172.2095 -90)
    (tags "resistor")
    (property "LCSC Part" "C17471")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (path "/6c475a95-2a5e-43b2-9952-83c86eec8ca8")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "R10" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 169ffd0e-c198-4eb4-99b9-96582774f950)
    )
    (fp_text value "150" (at 0 0.35 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp a79aaf49-e365-4e75-a48d-987c4a04c76f)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 1eca7ea0-3234-4640-9d3b-b065e306c553)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 96e8cdea-922a-4def-94b5-093fa5450321))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp fa7d4208-cd77-4786-83de-9dfa38e52cb2))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e198b764-4be5-405e-a3f6-b42eee047364))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0b50f678-1c05-4da3-bf81-d24eddd1029b))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8ef8fd7a-547b-4246-b459-9ea8b63566b9))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c1e947f4-b688-4a9d-8e02-c1a96aeed2c0))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9a27ad3c-34b1-44cb-8986-a25ef935a61d))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 495b946e-4b24-456a-a10e-5ee4ec98f460))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp eeafb1af-5957-4ad6-8bb6-0f490a9bf3c2))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8eb03226-a88b-47d7-9d46-3805ef28d44e))
    (pad "1" smd roundrect (at -0.95 0 270) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(R10-Pad1)") (pintype "passive") (tstamp 4ac8301d-9b72-457c-8bcc-6a9076bfab49))
    (pad "2" smd roundrect (at 0.95 0 270) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/Bo") (pintype "passive") (tstamp d01b7c55-1413-4a43-9da4-c38de5b15156))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:PasteHole_1.152mm_NPTH" (layer "F.Cu")
    (tstamp ca35c226-dab8-4d0d-a6ca-a80dbb770597)
    (at 123.952 189.2935)
    (descr "Circular Fiducial, 1mm bare copper top; 2mm keepout (Level A)")
    (tags "marker")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.1)))
      (tstamp 89f4663a-43ca-467c-ae59-dbc0fd31b663)
    )
    (fp_text value " " (at 0 2) (layer "F.Fab") hide
        (effects (font (size 0.508 0.508) (thickness 0.127)))
      (tstamp 9d9a0f4b-3683-439d-b31e-4136ceac06f2)
    )
    (fp_circle (center 0 0) (end 1 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 1a8a8aef-1df2-4d0f-8ed7-16ea4141e995))
    (pad "" np_thru_hole circle (at 0 0) (size 1.152 1.152) (drill 1.152) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.148) (tstamp 6c657ba5-7687-4dbf-8c3f-2f514157bab6))
  )

  (footprint "stdpads:R_0805" (layer "F.Cu")
    (tstamp cc31250b-12f8-4e94-b895-4a2986709c12)
    (at 113.3475 185.039)
    (tags "resistor")
    (property "LCSC Part" "C17714")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (path "/b4e51fec-e576-42e3-ba2e-3bbb1ce12540")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "R4" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 4987e207-eb23-4401-b56e-0d4a505f4d22)
    )
    (fp_text value "47" (at 0 0.35) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 4f648e6c-f880-4264-9775-24fb8e5563a5)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 50496bdd-9710-4bae-a9f7-12dbff4ffc4a)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 78256525-ead6-4588-aae9-3d11976ebe2e))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp ef6c19d3-d0ab-42a0-8c23-3edb684da7d9))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 86c7010d-b7c0-4950-93e5-1399e20b2191))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4092980e-48f4-4e9d-ad7a-7e4ee9dd91a1))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 000fd790-d30d-4573-97cc-ac3c375cc24e))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 258c24b0-4326-4f71-b75e-95b5feedf2c9))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7089617d-8d3f-4f47-8b6f-cc7f9c0fdff0))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ecac0f55-b3e5-470c-b1c7-038f397c4f56))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 39004bf3-c958-4421-a3ba-f3efe19d804d))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1f6b5158-998b-4f94-85ac-8b09f6ac2fca))
    (pad "1" smd roundrect (at -0.95 0) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(R4-Pad1)") (pintype "passive") (tstamp e08966af-a1eb-41cb-a3a5-16a199be95fd))
    (pad "2" smd roundrect (at 0.95 0) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/HSo") (pintype "passive") (tstamp f8e92cd9-9dee-4d0d-8c2e-d35e6152acec))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:R_0805" (layer "F.Cu")
    (tstamp d53c0d9d-88c1-41a2-973a-a171475cf196)
    (at 35.052 130.6215 180)
    (tags "resistor")
    (property "LCSC Part" "C17513")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (path "/f9e9f6b3-dfe2-4d2f-8e85-10c3d17264f6")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "R3" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 16ef5e89-7567-4368-811c-aa86f11db76c)
    )
    (fp_text value "2k2" (at 0 0.35) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 6f0722ef-b025-48ac-9ef5-45771298eab7)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp fcfafcb1-c993-43a3-9c45-10eb3b524eef)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 36616d88-360f-4b40-b227-8555a3341415))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 6a7ed161-a23a-4005-b78b-da7399b8bcb1))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 51a33961-456f-4a66-899f-863adb64a595))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4914ccac-67df-43b9-969a-c9b57fe42a9d))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c1810c71-a5ff-4c08-9734-039df69c88bf))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 295e690e-9f82-45b0-aa73-6baa9d73e0d4))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1df38255-6cc6-41a0-97dd-e9e045bd977f))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ed8bfb37-5ff0-49ea-9e51-8b88c1b0ac63))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 06557254-4960-4974-abea-65a32f6e4e33))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c9d39dff-3ec0-475b-850f-1d89043fc645))
    (pad "1" smd roundrect (at -0.95 0 180) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/VSx") (pintype "passive") (tstamp 2f84518f-401d-4b06-835c-bf87b2996833))
    (pad "2" smd roundrect (at 0.95 0 180) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3") (pintype "passive") (tstamp 835157af-2baa-4508-9d9e-d8d88299ae76))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:C_0805" (layer "F.Cu")
    (tstamp db2ce92b-6e03-4216-ae6d-900577411ed8)
    (at 74.75 188.75 90)
    (tags "capacitor")
    (property "LCSC Part" "C15850")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/72cddd6a-223f-4f29-9d5c-86a63005f0ad")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "C19" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 34c381e9-b1bc-47e9-b94b-a387ed5ed7a1)
    )
    (fp_text value "10u" (at 0 0.35 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp f6cbfd74-27b7-4194-88d6-aee58921f0eb)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 2715a193-87c4-445e-9443-98934765d3bc)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 5cbdc724-0381-4f09-a66a-2869ba13d3cb))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp ab3ffea7-ae86-4b50-b0c5-d02ba8774b27))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ae5191b9-ba8f-4279-a96f-b8da5ccdd55a))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 85bfb9ed-8931-4cfc-a6e1-0d5db13e995b))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fee3be5f-b868-45ba-96b8-9046a69750ad))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5db5c334-e15f-40ac-a6c1-6f94af4af444))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 0aec9a39-b69b-4585-a001-d3e7ffa1f36b))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 073dc275-22d1-4fe7-a79a-2ad4cc202e80))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp fde2c14a-44ef-4179-b376-d076476f95f2))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp e40242ac-ad58-491a-8350-1c1491325e8f))
    (pad "1" smd roundrect (at -0.85 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive") (tstamp 3e54de54-596a-4a72-9dfa-2f9d98d37aa8))
    (pad "2" smd roundrect (at 0.85 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 665a8fbf-0152-46ce-ae4a-5bfb25ce8b28))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:C_0805" (layer "F.Cu")
    (tstamp dfb8a9c0-da22-4821-9cac-fc8099bacd9b)
    (at 94.957 138.684 180)
    (tags "capacitor")
    (property "LCSC Part" "C15850")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/a506b918-297e-4edb-adb1-144c3d1a4a2d")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "C14" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp f469df8c-c0ee-4201-a2ca-61b7351e09d4)
    )
    (fp_text value "10u" (at 0 0.35) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 74a3d6ba-86f1-4a43-8988-4842a85d4003)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 5e5382cb-7b6a-4f70-a426-bb759177a720)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 1cbe20fb-0882-461c-beaf-ad21a14eb5fc))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 974d9e6f-31de-4ef1-b493-36aef86cbcc8))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1ce546fe-bee6-45ad-a92d-90c4d69bacb3))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 21633bf8-8d78-43fb-aec4-5ae4ff92274a))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9c24a9e7-1fa3-49e9-9666-29eb39a7e307))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8257c082-c9cd-4b28-97ef-2bc0573940b1))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp b837cc22-68f2-407a-b7d5-40631044da8b))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 571b5d91-9fbe-4b0e-a5e7-15ce05a370c1))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 7dfa3416-f87c-46c0-8edc-daa8a3e39f29))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 0e49a8ef-77a7-4bad-b7aa-e222560d7a4b))
    (pad "1" smd roundrect (at -0.85 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 47daf2ed-89df-4d5f-b9fc-cc31d6317914))
    (pad "2" smd roundrect (at 0.85 0 180) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "-5V") (pintype "passive") (tstamp e8777644-8713-4512-9df0-112c88030fc5))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:R_0805" (layer "F.Cu")
    (tstamp e1eded56-36c2-4e99-8e5b-e0935e0f93cc)
    (at 102.047 179.959 180)
    (tags "resistor")
    (property "LCSC Part" "C17471")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (path "/fe34098e-4adf-4a98-8798-f0846dd56b3e")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "R12" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 02969038-73c3-492c-8c0c-6e6fabb3f0d4)
    )
    (fp_text value "47" (at 0 0.35) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 5c27f529-374f-4193-ab9e-0b8c95ee8402)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp c8511581-d6a2-4134-bb9f-652ed0fdfdcb)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 8f4ee979-cc2d-4c52-a369-9b7216b36728))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp b745377d-1cbf-441f-92c4-89de36f78c1f))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c364f917-aaf1-48c7-a2d2-926004e09671))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e009b668-758d-4383-973d-c264e8df7dd8))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f8ee62a8-abcf-45f7-8164-5a58db1fe32a))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 98f7b071-70a6-44dd-aab0-b2b3792047c8))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dc91ad38-ef71-49dd-b641-f24bb3b9efd2))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a0a483c7-d5cc-49db-9597-0ef0e9e65d24))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5da0b745-7ff5-4b96-b924-2b9f16b98510))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dc47d0a5-922e-4069-8689-ec0afafcf9ce))
    (pad "1" smd roundrect (at -0.95 0 180) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(R12-Pad1)") (pintype "passive") (tstamp 377f0a76-ea3d-4dbb-a82c-f5784c36d6f5))
    (pad "2" smd roundrect (at 0.95 0 180) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(C17-Pad1)") (pintype "passive") (tstamp f822d780-8f77-476f-b895-6548ba318f95))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:C_0805" (layer "F.Cu")
    (tstamp e559ea6e-99d0-402c-a240-a1421cf30239)
    (at 109.5 107.25 -90)
    (tags "capacitor")
    (property "LCSC Part" "C15850")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/6b2ef891-e1ef-4746-aba8-d72b4e3b995e")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "C9" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 40194fab-f8e3-4940-8406-3f90e98f0851)
    )
    (fp_text value "10u" (at 0 0.35 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp e4471b4d-d9b4-4ac6-b494-5b6bd4402f6c)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp b7eeb0e2-1788-48f7-a38a-a9634a31b530)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 65afbc6d-ea0a-4516-8034-3f8a06f87745))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 3a755100-8478-44e4-b3ac-ec9a7a311164))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 49a56e64-2744-49b4-8bef-be365c126831))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 727bfff0-d306-46a3-9e93-d08f9009a6a6))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8129a13c-5236-4d11-a180-dba021f015b0))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 913e7efd-65ee-4d43-8fc1-f483d90b0934))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp de22ce35-fa4a-49b9-9050-876d036d6a64))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 65447fd4-6904-4414-9314-0a1a0b337b94))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 7cc7c0ff-0d4c-4049-88ed-fe45c7067502))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp fc20396d-6e8c-48ee-bbfa-08a42a87ceba))
    (pad "1" smd roundrect (at -0.85 0 270) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3") (pintype "passive") (tstamp b016c0ce-3944-41ac-a8b6-cb4b47ca4a77))
    (pad "2" smd roundrect (at 0.85 0 270) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 4c639f33-65bd-4e5a-ae3c-c233180ad96a))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:R_0805" (layer "F.Cu")
    (tstamp e81a9959-b7df-4b6b-a89b-1c4d0a7d9d59)
    (at 111.313 189.611 180)
    (tags "resistor")
    (property "LCSC Part" "C17714")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (path "/6bac1f40-9d87-4836-87c9-9ae8d71d55c7")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "R13" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 9b40d95a-0a4e-4207-8d90-2f40372cda42)
    )
    (fp_text value "2k2" (at 0 0.35) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 9d14c964-d9f4-40a0-8148-1e3ba4d95ca0)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 9076b7e8-0786-4646-b21c-56bc99446185)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 43ea844f-1bab-4e68-9044-8a14306a32f6))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp c7cb87c6-d588-44d7-af01-05b6dab6243a))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a962abb1-7d79-452c-b1dc-c2fdaeaf8ca3))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5c9f5d46-0400-4a00-8677-15a549799aa7))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3bc74079-5210-4984-b089-7be3938d84a7))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a918f812-6fdb-4935-9c27-2307c617e63c))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5fab8e95-1b9d-40eb-b3f9-2f56f44fab12))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 757e7c3a-5b66-420e-bfd4-55e82758364f))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cf32088b-7a70-4208-a210-c54a8eaf298b))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 60cd95f8-5b6d-4dcb-840a-b63ea08af037))
    (pad "1" smd roundrect (at -0.95 0 180) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+5V") (pintype "passive") (tstamp 95b57f24-0679-4939-bfbd-cef177253caa))
    (pad "2" smd roundrect (at 0.95 0 180) (size 0.85 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/HSf") (pintype "passive") (tstamp 63148b3a-566c-464e-8773-165865d06b24))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:C_0805" (layer "F.Cu")
    (tstamp eb382152-0734-4a3a-8ba6-fde867ca6ccc)
    (at 109.5 121.95 -90)
    (tags "capacitor")
    (property "LCSC Part" "C15850")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/5f34064e-c529-4a9a-bd57-89ea3da37081")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "C5" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp fb22eec0-e154-48fb-bee5-bb98abcbda7c)
    )
    (fp_text value "10u" (at 0 0.35 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 6e6ecc7b-fe0f-4b14-8c94-9b3f8b6c956f)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp a0c30738-dd9a-4d5e-b5d8-786a96d53ca1)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 5060bfaf-61f0-4c70-b9ec-3a34ab3dd113))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 68c2d67d-0367-4be1-a6c0-bc4d0362b0ae))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1787d277-f2e7-4732-9ad9-482b2e186752))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 12bfbc45-9795-46d8-a621-898efe122cf0))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3f35c14f-4e64-4548-98b1-8f904d0e5a7d))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 816d6e3e-9de5-4d91-861f-4297ed4b3bdd))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 55a4f4b6-aa06-4de0-b3ad-5fe5e0441532))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 74893215-2f32-4dbc-a6d0-9e488b44e367))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 612c0a4b-c4a8-4f1a-9227-e4bcd1b6c6e5))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp cc0d4dfb-802a-4503-b015-d158c909e8db))
    (pad "1" smd roundrect (at -0.85 0 270) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+5V") (pintype "passive") (tstamp d69bc45c-825b-4299-938b-7219f7ad366f))
    (pad "2" smd roundrect (at 0.85 0 270) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp c715d4ee-cafe-4c18-a1ef-b50f06c05303))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:C_0805" (layer "F.Cu")
    (tstamp ec4403fd-099f-45b2-81f2-f33741584dab)
    (at 92.32039 163.978098)
    (tags "capacitor")
    (property "LCSC Part" "C15850")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/75689b41-0a89-4e58-96ef-71c20af98787")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "C18" (at 0 0 180) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 3a739513-e28e-4467-8266-2fc1e3219bba)
    )
    (fp_text value "10u" (at 0 0.35) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp e117f8ac-262f-4cbf-8df6-859d6092c4b8)
    )
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp c2833577-aea4-4825-8d39-18b755f17070)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 94f10b4e-c391-4848-b603-c3b397874061))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 1ac19b98-ae2e-42b3-8e5f-e5ba8fbc7443))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 16251938-01d0-49f3-9f3a-548d6e2ec2ab))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4d4bec39-f9b7-468e-bea7-54fff719688c))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 86d5b335-0ba2-4dd0-83a9-0b411834b96c))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a6b4c5c5-9edf-45e8-8521-9c1b854ff7a8))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp b1efcb3b-dd1a-4d9d-b171-d63c0cdca493))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp a051e08c-aec6-4665-9029-404a69abda62))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 121293b6-9a1e-48cf-96bb-eaca3878485c))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 6b119579-a99c-4d2c-9877-15c42189e9ef))
    (pad "1" smd roundrect (at -0.85 0) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/~{POR}") (pintype "passive") (tstamp 7341137d-bfee-4105-a123-daff85764402))
    (pad "2" smd roundrect (at 0.85 0) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp c5743be1-df91-45a7-bea8-b844b352f642))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:C_0805" (layer "F.Cu")
    (tstamp ec93e869-04b6-443c-81d0-99afa2301336)
    (at 74.75 117.8 90)
    (tags "capacitor")
    (property "LCSC Part" "C15850")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/f668ce4b-3782-409e-9e8e-2585d07c4c3a")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "C15" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 0157ab85-e571-40d8-a0e2-72634748a3cb)
    )
    (fp_text value "10u" (at 0 0.35 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp f932118c-5bbf-4d06-ad47-e122dd884bc8)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp cfdea76a-b340-4f75-bfce-75f6462e325c)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 812c1889-e2d9-4adf-8354-1792b7d9f9eb))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 94c02e16-0118-4a9d-8619-8aeada3a4894))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 21b35a09-0cb6-4b64-b43c-953daa140656))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 28fa3c24-ec47-4486-a0c4-fc102791e079))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 00c71068-2818-4482-a3ea-b2d2f9dacd4e))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 42eeda05-2693-4c8f-b3df-e50c8928b497))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 605cac70-08d7-4892-8d8f-bc9e37a76905))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 7ee00012-c20a-49e8-86ad-7c80eb39c319))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 9c369f4a-669f-4d99-8a7c-b0181d163927))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 592f0257-d5fc-4477-bee6-9efa1a54202c))
    (pad "1" smd roundrect (at -0.85 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp ac9b8dca-7588-43ef-8e14-e1017b1898ee))
    (pad "2" smd roundrect (at 0.85 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "-5V") (pintype "passive") (tstamp b743221f-c0eb-40a4-b3ef-4d84a208d24d))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:C_0805" (layer "F.Cu")
    (tstamp ee639651-210d-42d1-a8d6-ce7142e7bdca)
    (at 109.5 139.15 90)
    (tags "capacitor")
    (property "LCSC Part" "C15850")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/46579f81-d62d-4a0d-af13-659e763d7118")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "C3" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp cc15be33-a8a1-4f80-8035-e6d231cb3011)
    )
    (fp_text value "10u" (at 0 0.35 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 22f25854-acb3-401f-a6b0-218fab67ea05)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp a2860c71-cbac-4804-9543-fbb959fe3a26)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp b121b379-3660-4945-a964-c9de59d50e9b))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 3c159530-a0e4-4b79-a516-117db7f1ac9d))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp be4eb575-e9ae-4347-a90e-ee8cda7c8745))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7af1a378-b147-4ca4-ba8f-89e405711732))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5d143c8b-0922-4380-929a-0c28199aaa62))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9fc96108-bcce-47c1-abb6-ca48098c4a01))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 1181fae9-7bd6-4e92-adbb-d45818f37cde))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp c9ab3ea3-4381-4340-9c8b-677747e03f7e))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 11416fa1-339a-4adf-a409-b8b356bf7484))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 057d0a8b-4168-4f65-b24c-d966e3b14f01))
    (pad "1" smd roundrect (at -0.85 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+5V") (pintype "passive") (tstamp 76397ba4-43a8-426b-a391-ce6bd47cbd6b))
    (pad "2" smd roundrect (at 0.85 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp ae01cee8-b9c1-4060-9f50-815806c32381))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:Molex_Mini-Fit_Jr_5569-14A1_2x07_P4.20mm_Horizontal" (layer "F.Cu")
    (tstamp ef56989b-7907-4cc0-8a02-01adbbe80cd1)
    (at 65.85 127.45 90)
    (descr "Molex Mini-Fit Jr. Power Connectors, old mpn/engineering number: 5569-14A1, example for new mpn: 39-29-4149, 7 Pins per row, Mounting: PCB Mounting Flange (http://www.molex.com/pdm_docs/sd/039291047_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Mini-Fit_Jr top entryscrew_flange")
    (property "LCSC Part" "C52216")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x07, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (path "/9b506ac6-697b-43f7-808d-1e59d762580b")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -34.15 90) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d4a11a93-939f-4a45-bf82-64dff76e7fc9)
    )
    (fp_text value "SE" (at 0 8.55 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 20fb7039-750d-4be5-9f1a-3a25c2f0b090)
    )
    (fp_line (start -20.41 -7.41) (end -20.41 -0.99)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 083f74e0-b0be-46e0-be65-9897ab807fa9))
    (fp_line (start -20.41 -0.99) (end -14.6 -0.99)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3833ccf8-5992-4986-9fc6-b69069b3661f))
    (fp_line (start -15.41 -14.01) (end -15.41 -7.41)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1d6dd2c7-6cea-4b99-867c-ca2de4288732))
    (fp_line (start -15.41 -7.41) (end -20.41 -7.41)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f9df4b78-b9c2-4874-a93d-c0d06300f6ee))
    (fp_line (start -15.2 -0.3) (end -14.6 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4e4d791f-2c65-4e4b-ac6a-1bb609e40bfb))
    (fp_line (start -15.2 0.3) (end -15.2 -0.3)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 30e0fbed-f9ff-41b3-b362-a7d47ee907ad))
    (fp_line (start -14.6 0) (end -15.2 0.3)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ab8e99b0-0799-436a-9a29-6b339b528a92))
    (fp_line (start -12.9 2.11) (end -12.9 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4fedacf9-7c12-48d3-a673-880604758cf8))
    (fp_line (start -12.3 2.11) (end -12.3 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8dbac2e9-74be-4b88-a534-b0fcbef02ae1))
    (fp_line (start -10.99 -1) (end -10.01 -1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a944601e-0e6c-4639-b62c-aaca892e1f7a))
    (fp_line (start -8.7 2.11) (end -8.7 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a2cfe9d5-15d4-4720-9128-185ff0209c8f))
    (fp_line (start -8.1 2.11) (end -8.1 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cbe399cd-d899-45d7-9921-cece8dcfb6c6))
    (fp_line (start -6.79 -1) (end -5.81 -1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f534d7d0-1506-40e4-b26d-2392b7081a91))
    (fp_line (start -4.5 2.11) (end -4.5 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 04de248b-e1e1-4a40-b61f-9a515577fe06))
    (fp_line (start -3.9 2.11) (end -3.9 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 32dc5767-d734-490a-9a00-9ce991158b39))
    (fp_line (start -2.59 -1) (end -1.61 -1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dead628a-3fc9-4299-8854-8a89077f33e4))
    (fp_line (start -0.3 2.11) (end -0.3 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 54fa29dd-3d1e-4071-b2d1-3928090b3c40))
    (fp_line (start 0 -14.01) (end -15.41 -14.01)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c8d7d5c5-adfa-42f9-9a7a-0c415742f103))
    (fp_line (start 0 -14.01) (end 15.41 -14.01)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 277aea0a-ba4a-4932-b3d6-f53b6eee2bb7))
    (fp_line (start 0.3 2.11) (end 0.3 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp da0eb4ba-79c4-452f-89cf-e120bce58bb0))
    (fp_line (start 1.61 -1) (end 2.59 -1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e7134c81-cd10-4f0b-b423-30bc64e81df8))
    (fp_line (start 3.9 2.11) (end 3.9 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6557a29a-ffbd-43ae-8230-d4791714d2a2))
    (fp_line (start 4.5 2.11) (end 4.5 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 10e3990e-76dc-44c1-b090-2ab9cecfbf1e))
    (fp_line (start 5.81 -1) (end 6.79 -1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9851ea0e-1e51-4eb4-ad90-05aad47e7614))
    (fp_line (start 8.1 2.11) (end 8.1 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 70a56985-ed98-446b-9e41-e51d12fbba25))
    (fp_line (start 8.7 2.11) (end 8.7 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 92b72929-7727-43d8-b4f1-36a8b2a788d0))
    (fp_line (start 10.01 -1) (end 10.99 -1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 93b77e40-21d5-4a2c-b82c-d117d89690d0))
    (fp_line (start 12.3 2.11) (end 12.3 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7afdfef3-2e9a-4a5b-ad8c-aa0c64278100))
    (fp_line (start 12.9 2.11) (end 12.9 3.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3a6c8ec1-eddd-4bb3-8938-2dc84034382d))
    (fp_line (start 15.41 -14.01) (end 15.41 -7.41)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 498c9284-2f20-484c-96b6-5035d8cf655d))
    (fp_line (start 15.41 -7.41) (end 20.41 -7.41)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e6404192-8e38-44b1-9d5e-537e9cf65548))
    (fp_line (start 20.41 -7.41) (end 20.41 -0.99)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 478c3678-4cf4-4dd6-9d55-f63921b516c8))
    (fp_line (start 20.41 -0.99) (end 14.6 -0.99)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f5169190-61b7-4509-9883-16c93788e902))
    (fp_line (start -20.8 -7.8) (end -20.8 -0.6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f48c73ea-e34a-46c2-879d-a9d1df3cbd2a))
    (fp_line (start -20.8 -0.6) (end -14.45 -0.6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 428f4579-a321-4b21-a670-b5c18a5fdcd2))
    (fp_line (start -15.8 -14.4) (end -15.8 -7.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 198ab0a1-eb60-42fe-b85b-a9a62a5d9b26))
    (fp_line (start -15.8 -7.8) (end -20.8 -7.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ac3355e2-5b29-4ec9-ba9d-cf39951b3264))
    (fp_line (start -14.45 -0.6) (end -14.45 7.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 19d7e73b-c476-46ec-9902-79311a7596c6))
    (fp_line (start -14.45 7.85) (end 0 7.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3a3c14f0-0fbd-4b6f-9075-eee0c23204e0))
    (fp_line (start 0 -14.4) (end -15.8 -14.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b9f07aa1-c26c-45e5-8d12-d57b990809e4))
    (fp_line (start 0 -14.4) (end 15.8 -14.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 30a7f3fd-1f25-4b5e-ae7a-71a79baa5d9e))
    (fp_line (start 14.45 -0.6) (end 14.45 7.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9e6f2a9d-5969-468b-9791-561c3f4b51bd))
    (fp_line (start 14.45 7.85) (end 0 7.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4969e864-62ed-4899-8651-d1299b6eae2a))
    (fp_line (start 15.8 -14.4) (end 15.8 -7.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b08875d5-28be-41b5-a80c-53e217b5d7af))
    (fp_line (start 15.8 -7.8) (end 20.8 -7.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8a006dfa-9e1e-4a09-b94a-0cfdcb5ba3de))
    (fp_line (start 20.8 -7.8) (end 20.8 -0.6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 702c704b-8373-462c-a24e-7b94bba04ff8))
    (fp_line (start 20.8 -0.6) (end 14.45 -0.6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3672195f-82c5-41a7-9414-48852192184c))
    (fp_line (start -20.3 -7.3) (end -20.3 -1.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b9e3800d-33a7-4b26-aed3-387ef2557afc))
    (fp_line (start -20.3 -1.1) (end -15.3 -1.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 74467775-c66d-43c6-87d2-9abe7dc685c7))
    (fp_line (start -15.3 -13.9) (end -15.3 -1.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 97896a14-57d9-4176-87d4-faaaeab553a2))
    (fp_line (start -15.3 -7.3) (end -20.3 -7.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ba15805c-cc9c-49a2-9be3-31239acb7a93))
    (fp_line (start -15.3 -1.1) (end 15.3 -1.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 68c1bb3f-50df-4ac4-8590-1dcc9114187d))
    (fp_line (start -13.6 -1.1) (end -12.6 -2.514214)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 43d5abd5-4225-445e-bbf8-4c12bb98ed63))
    (fp_line (start -12.6 -2.514214) (end -11.6 -1.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 743b19c7-ff78-433e-817e-9a0e97fc1247))
    (fp_line (start 15.3 -13.9) (end -15.3 -13.9)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 16ad92c2-9320-44c3-828f-d6f1f3e2d917))
    (fp_line (start 15.3 -7.3) (end 20.3 -7.3)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a181b998-683c-4bb9-90a9-fa2f7f8f9489))
    (fp_line (start 15.3 -1.1) (end 15.3 -13.9)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ceeb3ae7-443a-4832-81e6-b6e1c280f6d5))
    (fp_line (start 20.3 -7.3) (end 20.3 -1.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fd2fe580-df27-4cc3-b1e5-36a5bc1a7622))
    (fp_line (start 20.3 -1.1) (end 15.3 -1.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bf4ff365-1c24-468e-8a44-9203dfbc13da))
    (pad "" np_thru_hole circle (at -17.1 -4.2 90) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask") (tstamp cc1cdf5a-eec3-4254-9b3e-8822cda9a27c))
    (pad "" np_thru_hole circle (at 17.1 -4.2 90) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask") (tstamp b6d75ef9-3159-4a1a-9b7a-5888d509c3f8))
    (pad "1" thru_hole roundrect (at -12.6 0 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.09259296296)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive") (tstamp 67bdb03e-dd63-4551-bf0c-03bc1b67d420))
    (pad "2" thru_hole oval (at -8.4 0 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive") (tstamp b67507a1-2bbd-4fbb-b17d-bb4e00ea8300))
    (pad "3" thru_hole oval (at -4.2 0 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive") (tstamp 49e05fa5-0a2c-48de-869c-a6342b3a16d4))
    (pad "4" thru_hole oval (at 0 0 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_4") (pintype "passive") (tstamp 1b43716a-fa6b-46ec-bfa5-b2ab6b7f4a6c))
    (pad "5" thru_hole oval (at 4.2 0 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_5") (pintype "passive") (tstamp b9c0a51f-216e-4444-bca8-7867f1be6622))
    (pad "6" thru_hole oval (at 8.4 0 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 6 "-5V") (pinfunction "Pin_6") (pintype "passive") (tstamp b6de2409-2e57-4499-99ff-a6e2e91f9ea8))
    (pad "7" thru_hole oval (at 12.6 0 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 5 "-12V") (pinfunction "Pin_7") (pintype "passive") (tstamp ed40f9a3-18ba-4572-92a2-490f82a80b08))
    (pad "8" thru_hole oval (at -12.6 5.5 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_8") (pintype "passive") (tstamp 3e86d3c2-542e-4a6f-9052-c3a7fa3240ac))
    (pad "9" thru_hole oval (at -8.4 5.5 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 13 "/Ci") (pinfunction "Pin_9") (pintype "passive") (tstamp ddd760e0-8218-4d8b-a6c5-6742a33231c3))
    (pad "10" thru_hole oval (at -4.2 5.5 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 14 "/HSi") (pinfunction "Pin_10") (pintype "passive") (tstamp 4fc86ad8-44b8-4488-97c5-a6bf7f9a84f3))
    (pad "11" thru_hole oval (at 0 5.5 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 15 "/VSi") (pinfunction "Pin_11") (pintype "passive") (tstamp 1838298d-5077-4788-83aa-9030934d4f4d))
    (pad "12" thru_hole oval (at 4.2 5.5 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 3 "+5V") (pinfunction "Pin_12") (pintype "passive") (tstamp 6e8a7465-a052-4f5d-8422-748eafe4be3c))
    (pad "13" thru_hole oval (at 8.4 5.5 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 3 "+5V") (pinfunction "Pin_13") (pintype "passive") (tstamp 971b962c-48d3-4cdd-b109-19c387672b1a))
    (pad "14" thru_hole oval (at 12.6 5.5 90) (size 2.7 3.7) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pinfunction "Pin_14") (pintype "passive") (tstamp 6b9f9844-21d1-40a5-8da3-33c2b36ece31))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Mini-Fit_Jr_5569-14A1_2x07_P4.20mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:C_0805" (layer "F.Cu")
    (tstamp ef882efd-70b5-4e7e-ab8a-1dd9520a834b)
    (at 109.5 151.35 -90)
    (tags "capacitor")
    (property "LCSC Part" "C15850")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/3f2a435f-f316-4a88-9632-9a86627c7880")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "C8" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 923585f7-8a4f-4340-8a63-5f12112ccf88)
    )
    (fp_text value "10u" (at 0 0.35 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp f1397650-8085-4ba4-bc43-57a147c6eda6)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 59679295-c7c9-44de-aa2d-9401ec109674)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 68bdf941-13ba-4c4b-8848-0c289c1cc31d))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 10b68f7d-6754-409a-917b-4cba4acd3e3e))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 32dda7bc-d1ee-4e14-8120-f4e2d6816d6e))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c2b75d59-764f-424f-918b-dcf3a6bd50ac))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp dfaf7faa-d5de-4284-af23-0e741dd50938))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3ddc1e5f-867d-4bd7-abd9-8645dbc918f4))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 3e9eb6f8-929e-4f27-ae68-487ef4c80a8f))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp fc96282b-c91c-4853-815f-69adf8a63e79))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 3cf95f69-d0e6-4d51-8732-881bfebe7cd0))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 7ab24205-ca7a-4f4b-b84c-98f5446b36bb))
    (pad "1" smd roundrect (at -0.85 0 270) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3") (pintype "passive") (tstamp 0b690693-b21f-47cb-a7ca-a910d17482d0))
    (pad "2" smd roundrect (at 0.85 0 270) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp c1d0a574-600d-4a2d-9c29-d5cdcc033a74))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:C_0805" (layer "F.Cu")
    (tstamp f30a70d1-cccb-457a-a501-4fb42cd197d8)
    (at 74.75 114 90)
    (tags "capacitor")
    (property "LCSC Part" "C15850")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/acd8be35-1b05-4c86-9d7b-0e65e350cd4b")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "C1" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp f36ec51d-c5b6-4ebf-a197-2e1bbe337d34)
    )
    (fp_text value "10u" (at 0 0.35 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp bf03b4b1-3151-4222-b380-0157735f6032)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp f3a60e9a-197a-48f0-af3f-ae9e52b2cc29)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp b16e576c-ebba-452d-9df3-993fc9de59d8))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 94401cc1-fd0e-4237-aae1-6756973e811d))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2c2c7063-a29a-49ce-aefe-8742a709ca3f))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 65d7d53e-5b16-4c28-9dd7-57af2e6a30bd))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f5eb32e7-d8ca-4aa5-a299-eb9eaa7f65af))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c262a9d6-3cb9-4cde-ac39-b3fa153d8c96))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp db8a22df-96e4-45d9-84a0-639aa6684a05))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp ce08fbed-714b-4b7b-aba4-4b6a466b8035))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 8fe85989-0008-423f-a64d-d3a6a652818b))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp fb9ff7d9-d648-4194-82dd-614e64248bb1))
    (pad "1" smd roundrect (at -0.85 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive") (tstamp 3e0260dd-73cf-4d92-b647-311ae445af8f))
    (pad "2" smd roundrect (at 0.85 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 1143417f-1e1c-424e-9fad-f853f1f7ccdd))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "stdpads:SOIC-14_3.9mm" (layer "F.Cu")
    (tstamp f3e3b3a1-3f2b-4ce2-89a7-ccfad320abce)
    (at 107.8865 169.9895 90)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "LCSC Part" "C548853")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Quad 2-input XOR")
    (property "ki_keywords" "TTL XOR2")
    (path "/8dfddad0-ffd6-4222-92d9-eca80437562d")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "U3" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
      (tstamp 3f745956-54e1-4a85-ae6a-058819dc91dd)
    )
    (fp_text value "74LVC86AD" (at 0 1.016 90) (layer "F.Fab")
        (effects (font (size 0.508 0.508) (thickness 0.127)))
      (tstamp 1ccb073c-eb42-4cc3-9f83-42aef16ff00a)
    )
    (fp_line (start -4.425 0) (end -4.425 -1.95)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 17fc0965-3aa2-4037-aa72-8abf6ae021b4))
    (fp_line (start -4.425 0) (end -4.425 3.45)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d97abe33-6ef4-4c3b-9aeb-f5bcba50c584))
    (fp_line (start 4.425 0) (end 4.425 -1.95)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5e7ed5e5-43c8-4f3a-a8a4-bfe6641bfbd8))
    (fp_line (start 4.425 0) (end 4.425 1.95)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d66ffac5-58aa-4e07-bba9-1880c62b018b))
    (fp_line (start -4.565 -3.7) (end -4.565 3.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0892920a-3d1d-4bb0-b709-58aceeddd378))
    (fp_line (start -4.565 3.7) (end 4.565 3.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4ab0d0bf-0925-47cd-8cb1-f48e73bc254a))
    (fp_line (start 4.565 -3.7) (end -4.565 -3.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c78c4580-a1c3-4060-896c-8cfacdd066fd))
    (fp_line (start 4.565 3.7) (end 4.565 -3.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b814bb4b-55d3-40a5-8f8c-bfe3e0d02582))
    (fp_line (start -4.315 -1.95) (end 4.315 -1.95)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0d15c65d-32b1-47f9-b101-4b84df83a871))
    (fp_line (start -4.315 0.975) (end -4.315 -1.95)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0c41c9b8-f0de-4a47-b4c9-44af803f4443))
    (fp_line (start -3.34 1.95) (end -4.315 0.975)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d851665b-e8d4-4cc8-ae8f-ee782bf00fe3))
    (fp_line (start 4.315 -1.95) (end 4.315 1.95)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a6b8757b-64eb-4edd-b109-3903a656dccf))
    (fp_line (start 4.315 1.95) (end -3.34 1.95)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f8cea0e6-8e73-42fb-a72e-86da4b90e2b5))
    (pad "1" smd roundrect (at -3.81 2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/Ci") (pintype "input") (tstamp 94175106-6364-4237-9d2b-69575d2a4efc))
    (pad "2" smd roundrect (at -2.54 2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/Cx") (pintype "input") (tstamp 7a36671b-dec3-4160-b86b-df240c4f0f7d))
    (pad "3" smd roundrect (at -1.27 2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(R10-Pad1)") (pintype "output") (tstamp 70ce11f5-5b8c-4b99-8e71-ab2372eff8f6))
    (pad "4" smd roundrect (at 0 2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/Ci") (pintype "input") (tstamp ef655c68-7bd2-4623-a7b8-4ad002639a91))
    (pad "5" smd roundrect (at 1.27 2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/Cx") (pintype "input") (tstamp 39986961-ed99-4ae4-9f05-289b92e3754a))
    (pad "6" smd roundrect (at 2.54 2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(R8-Pad1)") (pintype "output") (tstamp bba17d87-6fb1-4536-8409-682a2e4d1e09))
    (pad "7" smd roundrect (at 3.81 2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp b176f322-e11c-4ede-8341-12842d0a442d))
    (pad "8" smd roundrect (at 3.81 -2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(R6-Pad1)") (pintype "output") (tstamp f265ab49-b584-4ba8-b54d-7e840ae4eb05))
    (pad "9" smd roundrect (at 2.54 -2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/Ci") (pintype "input") (tstamp 0fb1a407-6806-4a9c-821f-c9f69200ad7e))
    (pad "10" smd roundrect (at 1.27 -2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/Cx") (pintype "input") (tstamp f716571d-c2c5-4441-844d-28c80a0fab61))
    (pad "11" smd roundrect (at 0 -2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "unconnected-(U3-Pad11)") (pintype "output+no_connect") (tstamp eba33e18-54e5-4bca-88c9-75a0cbdc438b))
    (pad "12" smd roundrect (at -1.27 -2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "input") (tstamp e8030b20-e36e-4069-8b63-207b42da8a46))
    (pad "13" smd roundrect (at -2.54 -2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "input") (tstamp afa69195-a474-447a-9332-140fc10a0bb0))
    (pad "14" smd roundrect (at -3.81 -2.475 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3") (pinfunction "VCC") (pintype "power_in") (tstamp a5b4918e-5bbb-472c-a6c7-2d0e64be07a3))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (footprint "stdpads:C_0805" (layer "F.Cu")
    (tstamp f85fd1b6-b80c-4d54-aa1e-e098f3f30cc4)
    (at 74.75 185.35 90)
    (tags "capacitor")
    (property "LCSC Part" "C15850")
    (property "Sheetfile" "SEPowerAdapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/18fee885-0cb9-490b-ae79-32e7c6933f44")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference "C20" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 212b41aa-ed6e-4116-841f-4bd97f86967b)
    )
    (fp_text value "10u" (at 0 0.35 90) (layer "F.Fab")
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp 361c7ca5-d67b-41d1-bfb8-b08f881513df)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.SilkS") hide
        (effects (font (size 0.254 0.254) (thickness 0.0635)))
      (tstamp e096998a-b286-48be-b1cd-d6ea43d27b6a)
    )
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 42061360-038f-4c56-b0a6-632b4c978c39))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8)
      (stroke (width 0.1524) (type solid)) (layer "F.SilkS") (tstamp 0f0df98b-8bfb-4071-ab3b-87f4a393489f))
    (fp_line (start -1.7 -1) (end 1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0e2f13aa-058c-4b96-a213-115df9fbf1a0))
    (fp_line (start -1.7 1) (end -1.7 -1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9eae9558-cf8e-4993-8924-396fd052b280))
    (fp_line (start 1.7 -1) (end 1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3ec8333a-97ce-4dbf-bb26-ceaeaad5f7d8))
    (fp_line (start 1.7 1) (end -1.7 1)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3d4c4f48-faeb-45c4-a7ab-c7e8d354227a))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 49aa96f1-3505-4cc7-aca5-23d0cf43feb3))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp b617b87c-d79b-437c-ad21-1a70f65c52b2))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp df5df30f-4280-4a29-a1e9-cc9acbbb2445))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp ab6e677e-3237-4a9b-8de0-e41e2b87abf5))
    (pad "1" smd roundrect (at -0.85 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 15d20106-16d4-46a1-8a60-edb0d22d4f38))
    (pad "2" smd roundrect (at 0.85 0 90) (size 1.05 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "-12V") (pintype "passive") (tstamp 1326bda1-a099-48e9-8fab-be367c3f2289))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_rect (start 85.2805 115.5065) (end 97.8535 132.588)
    (stroke (width 0.15) (type solid)) (fill solid) (layer "F.Mask") (tstamp 4e0272fc-784e-40ab-a620-74c725f9455e))
  (gr_arc (start 125.6665 191.8335) (mid 125.406118 192.462118) (end 124.7775 192.7225)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp 4a31981e-5ffe-4202-b226-badd921c9422))
  (gr_arc (start 124.7775 98.1075) (mid 125.406118 98.367882) (end 125.6665 98.9965)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp 650f1a1f-4682-4fa7-b393-f0cb8ba59e04))
  (gr_line (start 59.4995 98.1075) (end 124.7775 98.1075)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp 81c827c4-17b4-49b6-b436-0f87fc7668c5))
  (gr_arc (start 59.4995 192.7225) (mid 58.870882 192.462118) (end 58.6105 191.8335)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp 821938b4-0e32-4c24-9113-2198dc70fd0a))
  (gr_line (start 59.4995 192.7225) (end 124.7775 192.7225)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp bae797df-d8ab-47b8-8df0-cc6dbb496fb8))
  (gr_line (start 125.6665 191.8335) (end 125.6665 98.9965)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp f25eba3f-d163-4889-9fd1-063c6aa0ea32))
  (gr_arc (start 58.6105 98.9965) (mid 58.870882 98.367882) (end 59.4995 98.1075)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp fe7146f2-3a67-48a2-8d33-d84f6eb359a5))
  (gr_line (start 58.6105 191.8335) (end 58.6105 98.9965)
    (stroke (width 0.1) (type solid)) (layer "Edge.Cuts") (tstamp feb788d7-3d43-4390-bd62-df987828a2f4))
  (gr_text "SE" (at 76.3 167.9 90) (layer "F.SilkS") (tstamp 3d8e4f8e-bcfe-4554-b367-137277be9cdd)
    (effects (font (size 1.5 1.5) (thickness 0.3) bold) (justify left bottom))
  )
  (gr_text "Classic" (at 76.75 138.3 90) (layer "F.SilkS") (tstamp 5bf92686-b9c8-4c60-80d2-30d84b1b54ad)
    (effects (font (size 1.5 1.5) (thickness 0.3) bold) (justify left bottom))
  )

  (segment (start 117.15 146.3) (end 118.4 146.3) (width 1) (layer "F.Cu") (net 1) (tstamp 010de6fa-b4d3-4eb2-b53c-89b8aff9d336))
  (segment (start 109.5 146.3) (end 116.3 146.3) (width 1) (layer "F.Cu") (net 1) (tstamp 18035404-c5d2-47c0-b4d6-b19eb490b616))
  (segment (start 116.3 146.3) (end 118.4 148.4) (width 1) (layer "F.Cu") (net 1) (tstamp 471680f6-3d9c-49cd-8197-1aaeafd57ae4))
  (segment (start 117.15 146.3) (end 117.9 147.05) (width 1) (layer "F.Cu") (net 1) (tstamp 629d976c-3e0a-4fb5-ac13-b12ec199cf02))
  (segment (start 116.3 146.3) (end 118.4 144.2) (width 1) (layer "F.Cu") (net 1) (tstamp 7cf82df6-0511-459c-8408-f5e0919f5ccb))
  (segment (start 76.0945 114.85) (end 74.75 114.85) (width 1) (layer "F.Cu") (net 1) (tstamp 994cffd2-e8d9-4212-a066-6c117ee09da5))
  (segment (start 116.3 146.3) (end 117.15 146.3) (width 1) (layer "F.Cu") (net 1) (tstamp bb0e3497-7588-419f-afb0-05d9a29a02ef))
  (segment (start 118.4 144.2) (end 118.4 146.3) (width 1) (layer "F.Cu") (net 1) (tstamp c37a6558-91a3-46c1-ba3b-0d8ef45aeca8))
  (segment (start 65.85 184.5) (end 65.85 186.45) (width 1) (layer "F.Cu") (net 1) (tstamp c3a9f039-72a4-463d-9c7b-8773c8033d12))
  (segment (start 109.5 146.3) (end 108.1445 146.3) (width 1) (layer "F.Cu") (net 1) (tstamp c6278bb9-412c-4a36-8b13-1b39138d074e))
  (segment (start 74.75 114.85) (end 71.35 114.85) (width 1) (layer "F.Cu") (net 1) (tstamp d7f74d63-a5d3-4f5c-a278-ef00021b456c))
  (segment (start 65.85 186.45) (end 69 189.6) (width 1) (layer "F.Cu") (net 1) (tstamp de5ec44d-fe5e-4945-87c9-0300950b7800))
  (segment (start 69 189.6) (end 74.75 189.6) (width 1) (layer "F.Cu") (net 1) (tstamp e69ee139-f747-46fd-be3e-ebfc428153a9))
  (segment (start 118.4 146.3) (end 118.4 148.4) (width 1) (layer "F.Cu") (net 1) (tstamp e95433b7-2d14-4c84-9c17-1290f6b59b7e))
  (segment (start 117.15 146.3) (end 117.9 145.55) (width 1) (layer "F.Cu") (net 1) (tstamp ff49a450-a3f3-476a-8813-ea4dbb026f72))
  (segment (start 110.8025 164.2745) (end 111.6965 164.2745) (width 0.6) (layer "F.Cu") (net 2) (tstamp 00b0a1c0-421a-40ab-a9f7-70ddcead75c0))
  (segment (start 95.807 139.7145) (end 95.5675 139.954) (width 0.8) (layer "F.Cu") (net 2) (tstamp 022d8394-0e10-48da-bd07-d669b1298121))
  (segment (start 74.75 113.15) (end 76.05 113.15) (width 0.8) (layer "F.Cu") (net 2) (tstamp 02f15610-9b0e-422c-b9a1-7271d092eee8))
  (segment (start 105.4115 171.2595) (end 106.8705 171.2595) (width 0.6) (layer "F.Cu") (net 2) (tstamp 033f2478-875f-40f5-9c12-ab8ee303cf41))
  (segment (start 109.5 142.5) (end 108.2 142.5) (width 0.8) (layer "F.Cu") (net 2) (tstamp 05dc297c-c604-4b11-9b6d-3da9664b6a44))
  (segment (start 109.5 138.3) (end 108.2 138.3) (width 0.8) (layer "F.Cu") (net 2) (tstamp 0e28e526-5759-4378-ad9f-a74f42f42c34))
  (segment (start 74.75 118.65) (end 76.05 118.65) (width 0.8) (layer "F.Cu") (net 2) (tstamp 0e77bd86-170a-4f8f-b9fd-9466d5664429))
  (segment (start 107.11 176.862) (end 106.934 177.038) (width 0.6) (layer "F.Cu") (net 2) (tstamp 1b68786d-8904-49f6-8680-bca144029f07))
  (segment (start 74.75 176.5) (end 74.75 175.4) (width 0.8) (layer "F.Cu") (net 2) (tstamp 1d14aed0-c4cc-4cea-97ec-67596b5e5b33))
  (segment (start 107.11 189.611) (end 107.11 190.6415) (width 0.6) (layer "F.Cu") (net 2) (tstamp 21f206b3-deaa-4dbb-8bf4-85ff32578a7d))
  (segment (start 109.5 108.1) (end 110.8 108.1) (width 0.8) (layer "F.Cu") (net 2) (tstamp 23e1a672-0517-4a1c-b4fa-c1c47756d433))
  (segment (start 74.75 186.2) (end 73.45 186.2) (width 0.8) (layer "F.Cu") (net 2) (tstamp 2422c99e-cd2e-4011-b7aa-ee8e526d8053))
  (segment (start 110.3615 179.959) (end 111.8235 179.959) (width 0.6) (layer "F.Cu") (net 2) (tstamp 26547c2d-bae0-4066-bcf0-56300f3c99be))
  (segment (start 109.5 112.3) (end 110.8 112.3) (width 0.8) (layer "F.Cu") (net 2) (tstamp 28a92509-d046-44c6-b221-1b9c6de46631))
  (segment (start 110.3615 179.135) (end 110.363 179.1335) (width 0.6) (layer "F.Cu") (net 2) (tstamp 2b2e709b-cf45-40bf-b633-c0ffcf2d59cb))
  (segment (start 109.5 127) (end 108.2 127) (width 0.8) (layer "F.Cu") (net 2) (tstamp 2c62ec9f-209b-44de-a13b-41b2f77bfb12))
  (segment (start 110.3615 179.959) (end 110.3615 179.135) (width 0.6) (layer "F.Cu") (net 2) (tstamp 2d9ca7b0-22fd-4649-86b1-ffd7667b4250))
  (segment (start 89.867 138.684) (end 89.867 139.7145) (width 0.8) (layer "F.Cu") (net 2) (tstamp 32af6ebe-2dd8-4979-b22d-7a541930d2ea))
  (segment (start 65.85 131.65) (end 65.85 127.45) (width 0.8) (layer "F.Cu") (net 2) (tstamp 38b5726c-535b-4779-b23a-008d79e4104c))
  (segment (start 110.3615 166.1795) (end 110.3615 165.543) (width 0.6) (layer "F.Cu") (net 2) (tstamp 3eee7d62-cdce-4d22-b327-1867d22246ca))
  (segment (start 65.85 135.85) (end 65.85 131.65) (width 0.8) (layer "F.Cu") (net 2) (tstamp 4063c2fb-79b0-4459-be21-dadfd4b3bc38))
  (segment (start 109.5 142.5) (end 110.8 142.5) (width 0.8) (layer "F.Cu") (net 2) (tstamp 45e4a5f1-a20a-4ccf-ba7c-0a8404792ed3))
  (segment (start 74.75 180.7) (end 74.75 179.6) (width 0.8) (layer "F.Cu") (net 2) (tstamp 4852ae74-78f5-46b5-aa3b-de67bb6d5e7c))
  (segment (start 112.5 152.2) (end 112.9 152.6) (width 0.8) (layer "F.Cu") (net 2) (tstamp 4da09c0f-d6c2-495f-aa56-d6d37185909a))
  (segment (start 71.35 140.05) (end 65.85 140.05) (width 0.8) (layer "F.Cu") (net 2) (tstamp 4f2a8d28-1991-4379-bea7-da38ed59c8f8))
  (segment (start 108.4485 152.2) (end 108.204 151.9555) (width 0.8) (layer "F.Cu") (net 2) (tstamp 53c491f0-3287-4fd4-af0c-157c6634a204))
  (segment (start 112.5 127) (end 112.9 127.4) (width 0.8) (layer "F.Cu") (net 2) (tstamp 5873edd2-9a55-4201-b915-eeb154ff9e1a))
  (segment (start 105.4115 172.5295) (end 103.9495 172.5295) (width 0.6) (layer "F.Cu") (net 2) (tstamp 5b7e2faf-5835-45aa-b148-21eb477b7c2a))
  (segment (start 65.85 140.05) (end 65.85 135.85) (width 0.8) (layer "F.Cu") (net 2) (tstamp 5ed27e61-3730-4711-9594-5317140a57c0))
  (segment (start 74.75 187.9) (end 76.05 187.9) (width 0.8) (layer "F.Cu") (net 2) (tstamp 6a02bee7-0edf-4658-8478-3e3158e90df6))
  (segment (start 115.1255 167.4545) (end 115.1255 166.5605) (width 0.6) (layer "F.Cu") (net 2) (tstamp 780f2f4b-cb12-4fcc-90bc-66e9e51dda05))
  (segment (start 89.867 139.7145) (end 90.1065 139.954) (width 0.8) (layer "F.Cu") (net 2) (tstamp 7ce52c2b-6b54-4b65-b4c3-6fbf7498bfbf))
  (segment (start 109.5 127) (end 112.5 127) (width 0.8) (layer "F.Cu") (net 2) (tstamp 80e69090-1c3f-48e9-9158-af9b340d3857))
  (segment (start 118.4 131.6) (end 112.9 131.6) (width 0.8) (layer "F.Cu") (net 2) (tstamp 858c767d-6cbc-480f-825d-520e2c505c4e))
  (segment (start 109.5 122.8) (end 108.2 122.8) (width 0.8) (layer "F.Cu") (net 2) (tstamp 866ab5df-5af1-4bb6-b82b-b3fa5896d6c5))
  (segment (start 74.75 109.649999) (end 76.05 109.65) (width 0.8) (layer "F.Cu") (net 2) (tstamp 8af71bee-1a6b-4a28-92a6-804767062490))
  (segment (start 109.5 152.2) (end 112.5 152.2) (width 0.8) (layer "F.Cu") (net 2) (tstamp 8fe0f400-10bc-414a-8348-bc2d2c8bf2eb))
  (segment (start 65.85 123.25) (end 65.85 127.45) (width 0.8) (layer "F.Cu") (net 2) (tstamp 91eebf4d-32e9-46f8-a1fc-63a97fd52fc8))
  (segment (start 107.11 174.801) (end 106.934 174.625) (width 0.6) (layer "F.Cu") (net 2) (tstamp 91f08315-4b09-4382-9b61-17e35e8a2fb1))
  (segment (start 74.75 180.7) (end 76.05 180.7) (width 0.8) (layer "F.Cu") (net 2) (tstamp 975d20da-625e-43c9-808f-2d71e51ec32c))
  (segment (start 74.75 109.649999) (end 73.45 109.65) (width 0.8) (layer "F.Cu") (net 2) (tstamp aa3d1848-22ae-4e7c-9241-c4a5307621df))
  (segment (start 110.3615 166.1795) (end 111.8235 166.1795) (width 0.6) (layer "F.Cu") (net 2) (tstamp aa69fc80-8aee-4ef7-b383-3a8cb2f0b476))
  (segment (start 112.5 122.8) (end 112.9 123.2) (width 0.8) (layer "F.Cu") (net 2) (tstamp aca881a6-e96b-4176-a750-f1d6e7f65034))
  (segment (start 74.75 176.5) (end 76.05 176.5) (width 0.8) (layer "F.Cu") (net 2) (tstamp af07bef6-daea-4051-a9ba-a817d6d1db6a))
  (segment (start 109.5 112.3) (end 108.2 112.3) (width 0.8) (layer "F.Cu") (net 2) (tstamp b217edbf-1d32-4e2e-95c8-fc928dbe535b))
  (segment (start 110.3615 165.543) (end 110.1725 165.354) (width 0.6) (layer "F.Cu") (net 2) (tstamp b692b54c-a109-4fe6-a7bb-102954e77627))
  (segment (start 107.11 189.611) (end 108.1405 189.611) (width 0.6) (layer "F.Cu") (net 2) (tstamp ba61f916-3c8b-44d1-8f11-195b3b87e6d2))
  (segment (start 110.3615 179.959) (end 108.9025 179.959) (width 0.6) (layer "F.Cu") (net 2) (tstamp ba7e8b62-d7a9-48ce-b391-75f4c090a45d))
  (segment (start 74.75 187.9) (end 73.45 187.9) (width 0.8) (layer "F.Cu") (net 2) (tstamp c16cf990-8b4f-402e-808e-b753145a51f3))
  (segment (start 109.5 138.3) (end 110.8 138.3) (width 0.8) (layer "F.Cu") (net 2) (tstamp c211d249-e8d1-4d18-bc75-310ae826ce73))
  (segment (start 107.11 175.8315) (end 108.1405 175.8315) (width 0.6) (layer "F.Cu") (net 2) (tstamp c4f3c493-cc7a-41ff-9459-2aac0d890388))
  (segment (start 109.5 152.2) (end 108.4485 152.2) (width 0.8) (layer "F.Cu") (net 2) (tstamp c52f7a75-98e4-4916-be66-a36d79444896))
  (segment (start 107.11 175.8315) (end 107.11 176.862) (width 0.6) (layer "F.Cu") (net 2) (tstamp c7165dc0-5344-43b3-8cea-6f467330ab9c))
  (segment (start 95.807 138.684) (end 95.807 139.7145) (width 0.8) (layer "F.Cu") (net 2) (tstamp c8e2fc68-85b7-48bf-8d94-3da3965b82db))
  (segment (start 107.11 189.611) (end 107.11 188.5805) (width 0.6) (layer "F.Cu") (net 2) (tstamp cc9a2514-cad4-4c22-9a08-cb1f98a5a695))
  (segment (start 105.4115 172.5295) (end 106.8705 172.5295) (width 0.6) (layer "F.Cu") (net 2) (tstamp ce095dc4-c8ad-4474-b3e5-62f737bb72b5))
  (segment (start 109.5 122.8) (end 112.5 122.8) (width 0.8) (layer "F.Cu") (net 2) (tstamp d0256ab0-0620-4619-9dc4-b4a0c735ef6c))
  (segment (start 107.11 190.6415) (end 106.934 190.8175) (width 0.6) (layer "F.Cu") (net 2) (tstamp d1a652b4-bea0-4850-8f82-e960476a18c6))
  (segment (start 109.5 148) (end 108.2 148) (width 0.8) (layer "F.Cu") (net 2) (tstamp d2abdcfe-666f-4f9b-972b-bd7bfc0bb5ba))
  (segment (start 74.75 186.2) (end 76.05 186.2) (width 0.8) (layer "F.Cu") (net 2) (tstamp d349989d-8bf3-4b35-bfb2-5a82b85bdb93))
  (segment (start 74.75 121.55) (end 76.05 121.55) (width 0.8) (layer "F.Cu") (net 2) (tstamp d8c8ae18-5cf8-4811-89ee-27b6869db564))
  (segment (start 74.75 121.55) (end 73.45 121.55) (width 0.8) (layer "F.Cu") (net 2) (tstamp db1ac470-b3f5-4185-85ba-5588615b68f2))
  (segment (start 107.11 175.8315) (end 107.11 174.801) (width 0.6) (layer "F.Cu") (net 2) (tstamp e6df7764-205f-48cd-b872-5ff7ecabd2b7))
  (segment (start 109.5 108.1) (end 108.2 108.1) (width 0.8) (layer "F.Cu") (net 2) (tstamp e99e1396-beb1-4032-87cc-e256c27f86d0))
  (segment (start 110.3615 166.1795) (end 108.9025 166.1795) (width 0.6) (layer "F.Cu") (net 2) (tstamp ed46ec9a-c769-41f8-ad47-9e9ea991a7d5))
  (segment (start 74.75 113.15) (end 73.45 113.15) (width 0.8) (layer "F.Cu") (net 2) (tstamp f0b233a9-9282-4e7b-941f-3ef27190cc2f))
  (segment (start 115.1255 171.2645) (end 115.1255 170.3705) (width 0.6) (layer "F.Cu") (net 2) (tstamp f8d72cc1-1c92-46e3-9090-ff6067439388))
  (segment (start 107.11 188.5805) (end 106.934 188.4045) (width 0.6) (layer "F.Cu") (net 2) (tstamp fed27c62-3df1-496c-a4ef-fce62dce905d))
  (via (at 108.1405 189.611) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 2) (tstamp 0417cba2-fa72-4475-9f01-816d7846794f))
  (via (at 76.05 187.9) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 04d59221-a9ce-4b28-8066-741a813b76e7))
  (via (at 110.1725 165.354) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 2) (tstamp 0b80931b-54c8-4828-a322-0444dca7265e))
  (via (at 59.4995 191.8335) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 0bca0887-fe11-4ff9-990e-5ebeff056e0f))
  (via (at 122.047 129.159) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 0f72fc4a-71be-4989-8a05-485d691b7255))
  (via (at 110.8 142.5) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 11cb428f-fa8b-47b3-a290-1e35663dfc99))
  (via (at 108.2 122.8) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 1f4251cd-b0d0-4843-bf33-3a53460d31d7))
  (via (at 111.8235 179.959) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 2) (tstamp 20760024-5b8c-4d65-9fa3-3979e5fc0d8f))
  (via (at 108.204 151.9555) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 2c906b9a-fe39-49cc-8f48-0aa779ce91e4))
  (via (at 106.8705 172.5295) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 2) (tstamp 31d82b1f-b99f-48b3-ac21-e97c2a33ea5f))
  (via (at 110.363 179.1335) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 2) (tstamp 3604133a-8bc5-43a5-8522-caf6bc095edd))
  (via (at 108.9025 179.959) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 2) (tstamp 3641c902-040f-4b0c-be98-72b2764dd94e))
  (via (at 101.6635 150.9395) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 36937d0c-3411-40e8-a657-aec26c23670c))
  (via (at 110.0455 154.1145) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 36dd8a8a-7b21-458b-bd4d-e13a68007996))
  (via (at 73.45 186.2) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 3e7523fc-510f-45c6-9f78-68bb90472ef8))
  (via (at 106.934 174.625) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 2) (tstamp 3e9727b3-583a-4c80-ab0a-be10431cb30e))
  (via (at 124.7775 98.9965) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 42170a0d-44ef-4959-9eca-022e923f6e2b))
  (via (at 99.314 145.923) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 2) (tstamp 45c6205d-6257-4374-b237-d70ca0206d5a))
  (via (at 108.2 127) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 5396a94c-92c6-4834-ad68-6b8c97818c9d))
  (via (at 106.934 177.038) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 2) (tstamp 5408da48-19cd-4021-8f2c-db04d7a41828))
  (via (at 106.934 190.8175) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 2) (tstamp 5471c3be-5081-459d-aa0b-f51f6ae7cb19))
  (via (at 76.05 186.2) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 59060d85-a72e-47e6-8f67-16cbb50c4ea1))
  (via (at 108.2 142.5) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 60554e35-5200-481c-a432-adfddab63c15))
  (via (at 109.9185 191.8335) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 646fefee-4223-4c35-b696-fc44e2f4f6fa))
  (via (at 92.329 145.8595) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 2) (tstamp 65b4dc8d-e2e8-47d6-933e-038d0f58374f))
  (via (at 106.8705 171.2595) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 2) (tstamp 6cfc2870-062b-4ead-94f5-26a4002327f0))
  (via (at 74.75 179.6) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 6e50ada1-ee7e-43ed-b03a-c13ca6e41c85))
  (via (at 108.2 148) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 6f347530-78e5-43a7-9b70-71ca93011b89))
  (via (at 73.45 187.9) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 70dbf29e-e49c-4707-a9d6-86d452d7fbba))
  (via (at 106.4895 158.877) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 71d17597-2d42-4985-a476-a3420504c4e7))
  (via (at 106.426 140.0175) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 7d90204f-f702-4049-96b5-2f3b4abca14c))
  (via (at 108.2 112.3) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 7f9fc83d-d6a9-493f-8682-c5feb27bae76))
  (via (at 76.05 109.65) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 8173ff03-4c53-4cf0-a2a3-161d31536cea))
  (via (at 108.2 108.1) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 8765d9c0-1acd-45de-a686-ce9dd1081d93))
  (via (at 73.45 121.55) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 89f6cf6c-2a2e-455f-ba0a-03f258ec3865))
  (via (at 95.5675 139.954) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 8e8e0409-1673-4c7e-8489-524443c77ae4))
  (via (at 122.1105 184.277) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 8e8f302f-b845-469d-baa8-69f2469ab842))
  (via (at 115.1255 166.5605) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 2) (tstamp 9616790b-d896-4b4b-8bc9-7205c563c429))
  (via (at 76.05 113.15) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 99653f25-67ab-4227-b409-dd542d8f0dc7))
  (via (at 108.2 138.3) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp 9979203d-bc9b-4ab7-807f-c4baee3f18ee))
  (via (at 106.934 188.4045) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 2) (tstamp a0000dbe-88b9-4bc4-a608-f786604b0c7f))
  (via (at 106.934 145.288) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp a44e83d7-dc07-4114-ac15-5dd1b02ef139))
  (via (at 123.2535 154.3685) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp a72a6e8b-c479-4675-b179-f1c13924b770))
  (via (at 111.8235 166.1795) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 2) (tstamp aa0b4775-0071-4282-b23b-971ea5542e01))
  (via (at 106.3625 125.2855) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp adcc0c66-8984-468e-9872-e0e69a389eeb))
  (via (at 108.9025 166.1795) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 2) (tstamp ae5f7a4e-8b8e-4134-b55b-c0e7214b932e))
  (via (at 76.05 176.5) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp b00c59d6-9f87-4c63-b133-3a2092479336))
  (via (at 59.4995 98.9965) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp b2420938-7d71-4dcd-ab50-813a469df8c7))
  (via (at 114.173 174.3075) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp b59a0bf1-d7f4-42c0-8b51-c84053e107fe))
  (via (at 90.1065 139.954) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp b63f0454-0e66-414f-9747-4e573ad689b0))
  (via (at 111.6965 164.2745) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 2) (tstamp ba588ef9-688c-4cf9-9455-1ae98f3fd245))
  (via (at 76.05 121.55) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp c9a89409-86fb-44d8-add5-ec6e8d8cff95))
  (via (at 108.1405 175.8315) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 2) (tstamp cb59ef2e-0ede-4390-bff1-b6820b4d72b1))
  (via (at 103.8225 153.67) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 2) (tstamp cdb58be5-721d-4739-a789-c62133bbe7d4))
  (via (at 110.8 108.1) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp d07ff6ce-f11e-4cbd-92c7-60b0a807594b))
  (via (at 76.05 180.7) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp d52739e9-c76a-40da-b9f8-67d39aabaa65))
  (via (at 124.7775 191.8335) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp d6fc1b01-5bd0-4c84-9ad7-e23f5579d011))
  (via (at 110.8 138.3) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp d9458612-730f-4a04-a833-a8a6ad4d2843))
  (via (at 110.8 112.3) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp df6b3339-e647-4794-9a98-31d506d04fcd))
  (via (at 74.75 175.4) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp e02661ee-0f17-4ffe-b5e0-8a08281167ea))
  (via (at 103.9495 172.5295) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 2) (tstamp e15a777a-be20-4404-b266-b6b3b8a03b52))
  (via (at 76.05 118.65) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp e2134fd0-c297-4187-a7f0-584643c95202))
  (via (at 113.3475 183.134) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp e64ac58a-26d2-4596-bba8-ed76388cbed8))
  (via (at 76.454 116.3955) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp e680e477-d9a0-4879-88e1-91bdbf371cc3))
  (via (at 98.933 150.876) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp e73b1955-dd89-4526-a9a8-049a63585f27))
  (via (at 73.45 113.15) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp e742a517-bc87-45d2-a6d9-a27a34112cd9))
  (via (at 104.4575 156.9085) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp e8a3c6d3-c10b-4d11-9797-63ab082e1b9b))
  (via (at 107.569 168.0845) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 2) (tstamp eceb85dc-6464-427d-8342-3def0b64f4b6))
  (via (at 115.1255 170.3705) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 2) (tstamp ef3d10b9-79c8-4164-a262-98c823aa4fcb))
  (via (at 73.45 109.65) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 2) (tstamp f36229f7-cf3d-41a8-9a00-6f9646343adb))
  (segment (start 119.761 155.575) (end 103.3145 155.575) (width 1) (layer "F.Cu") (net 3) (tstamp 03ed57b5-925c-49b7-8370-dca35ac9247a))
  (segment (start 71.35 123.25) (end 71.35 119.05) (width 1) (layer "F.Cu") (net 3) (tstamp 0b1167c0-d8a0-4b52-bafd-f122a3a5827d))
  (segment (start 112.263 189.611) (end 113.284 189.611) (width 0.8) (layer "F.Cu") (net 3) (tstamp 10b48c89-b62d-433a-b04c-affb819c959c))
  (segment (start 74.75 178.2) (end 65.85 178.2) (width 1) (layer "F.Cu") (net 3) (tstamp 16b20014-0111-4e61-8294-2d568ce97175))
  (segment (start 121.539 153.797) (end 119.761 155.575) (width 1) (layer "F.Cu") (net 3) (tstamp 19f6b439-cf08-4d10-ad28-9564346e5594))
  (segment (start 109.5 121.1) (end 116.3 121.1) (width 1) (layer "F.Cu") (net 3) (tstamp 1fc4fc70-c626-4c19-a869-ce3af218c3ee))
  (segment (start 74.75 123.25) (end 71.35 123.25) (width 1) (layer "F.Cu") (net 3) (tstamp 20d2bbab-5ee1-4549-ab18-d2fae3b66136))
  (segment (start 76.0765 123.25) (end 74.75 123.25) (width 1) (layer "F.Cu") (net 3) (tstamp 27760f4f-eb21-4bd1-addb-95fc7bd71ba9))
  (segment (start 69.05 182.4) (end 66.95 180.3) (width 1) (layer "F.Cu") (net 3) (tstamp 2b050dc3-04e3-4db5-93af-745401e29a13))
  (segment (start 65.85 178.2) (end 65.85 176.1) (width 1) (layer "F.Cu") (net 3) (tstamp 31a61119-f098-4163-8636-8b810fa9f40b))
  (segment (start 65.85 180.3) (end 65.85 178.2) (width 1) (layer "F.Cu") (net 3) (tstamp 35745aea-2f21-4411-a8fa-9f7d3900ada0))
  (segment (start 107.061 140.9985) (end 108.0595 140) (width 1) (layer "F.Cu") (net 3) (tstamp 35cb33f9-64e7-49a2-976e-363e2b0d2e38))
  (segment (start 109.5 140) (end 108.0595 140) (width 1) (layer "F.Cu") (net 3) (tstamp 411fdf01-3a16-413a-8b18-4a6840f6f733))
  (segment (start 121.539 130.539) (end 121.539 153.797) (width 1) (layer "F.Cu") (net 3) (tstamp 50357729-0663-4083-b81e-df9c1b0b50dc))
  (segment (start 77.216 118.1735) (end 77.216 122.1105) (width 1) (layer "F.Cu") (net 3) (tstamp 64774612-902d-4025-b12a-52a2ccfcf40c))
  (segment (start 116.3 125.3) (end 118.4 127.4) (width 1) (layer "F.Cu") (net 3) (tstamp 80d83da8-cc10-424c-805b-18a049e60525))
  (segment (start 118.4 127.4) (end 121.539 130.539) (width 1) (layer "F.Cu") (net 3) (tstamp 858f6351-d11f-4f61-8ebc-dea63bfc8cfd))
  (segment (start 77.216 122.1105) (end 76.0765 123.25) (width 1) (layer "F.Cu") (net 3) (tstamp 8c7db81e-4e0d-42b2-a7cd-c680edce2e54))
  (segment (start 107.061 139.0015) (end 107.061 126.189) (width 1) (layer "F.Cu") (net 3) (tstamp 8d6beeba-9ff2-468b-9682-12e333d08f5a))
  (segment (start 107.061 121.9835) (end 107.9445 121.1) (width 1) (layer "F.Cu") (net 3) (tstamp 9267a679-2769-4617-aee9-f1f3b1935f0a))
  (segment (start 109.5 144.2) (end 108.132 144.2) (width 1) (layer "F.Cu") (net 3) (tstamp a0942fce-d871-4bab-900b-b801d22176e1))
  (segment (start 107.9445 121.1) (end 109.5 121.1) (width 1) (layer "F.Cu") (net 3) (tstamp a6960a73-88a6-4b73-a885-385e52ecf6be))
  (segment (start 66.95 180.3) (end 65.85 180.3) (width 1) (layer "F.Cu") (net 3) (tstamp ab0e2c23-eac5-4455-b9a1-cec54777cc21))
  (segment (start 107.061 143.129) (end 107.061 140.9985) (width 1) (layer "F.Cu") (net 3) (tstamp c11e9ea9-b024-4d45-b7af-dde124c70bdf))
  (segment (start 74.75 182.4) (end 69.05 182.4) (width 1) (layer "F.Cu") (net 3) (tstamp c1ce6c39-fe7e-4e8a-a994-ee89eaf09aef))
  (segment (start 109.5 140) (end 112.9 140) (width 1) (layer "F.Cu") (net 3) (tstamp c2deed55-85b4-43d5-ab9b-0edc6247d894))
  (segment (start 112.9 144.2) (end 109.5 144.2) (width 1) (layer "F.Cu") (net 3) (tstamp c65a54c1-5c15-4523-a58c-1790df76c684))
  (segment (start 107.061 126.189) (end 107.95 125.3) (width 1) (layer "F.Cu") (net 3) (tstamp cba500df-5450-4aa2-ab30-18b31e7a55f4))
  (segment (start 109.5 125.3) (end 107.95 125.3) (width 1) (layer "F.Cu") (net 3) (tstamp d025caee-a935-40eb-a940-93fbc77bad41))
  (segment (start 116.3 121.1) (end 118.4 119) (width 1) (layer "F.Cu") (net 3) (tstamp d3f7673e-381c-4c89-8645-9653fe734c12))
  (segment (start 108.0595 140) (end 107.061 139.0015) (width 1) (layer "F.Cu") (net 3) (tstamp daaf83d7-1e79-46f4-b695-d169f72e8ab0))
  (segment (start 107.061 124.411) (end 107.061 121.9835) (width 1) (layer "F.Cu") (net 3) (tstamp ddde7efc-77af-4f89-854f-65b26c9d35fd))
  (segment (start 107.95 125.3) (end 107.061 124.411) (width 1) (layer "F.Cu") (net 3) (tstamp e52793a9-859a-4f61-af68-d61ee5f23863))
  (segment (start 108.132 144.2) (end 107.061 143.129) (width 1) (layer "F.Cu") (net 3) (tstamp f02b2f33-f940-4077-8729-87320f99d4f1))
  (segment (start 109.5 125.3) (end 116.3 125.3) (width 1) (layer "F.Cu") (net 3) (tstamp ff06d6ab-4329-4985-b761-57d32a52b1b2))
  (via (at 113.284 189.611) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 3) (tstamp 558e8521-5539-4386-95c5-fe604166a5e5))
  (segment (start 109.5 150.5) (end 116.3 150.5) (width 1) (layer "F.Cu") (net 4) (tstamp 17308743-2055-40fb-a020-b8daca287453))
  (segment (start 105.41 175.8315) (end 105.41 176.8475) (width 0.6) (layer "F.Cu") (net 4) (tstamp 173219c5-5e64-41c6-9827-33d453a3f78e))
  (segment (start 105.41 189.611) (end 105.41 188.4045) (width 0.6) (layer "F.Cu") (net 4) (tstamp 25a238c7-9662-4576-a2f3-889c03a9c4c1))
  (segment (start 105.4115 175.703) (end 105.41 175.7045) (width 0.6) (layer "F.Cu") (net 4) (tstamp 25b049a4-a3fa-4686-aa9e-d2b76c556045))
  (segment (start 105.4115 187.579) (end 105.4115 188.403) (width 0.6) (layer "F.Cu") (net 4) (tstamp 389faa22-e87c-43e6-b237-8eecc45286e5))
  (segment (start 105.4115 187.579) (end 103.9495 187.579) (width 0.6) (layer "F.Cu") (net 4) (tstamp 396c8b65-213d-48aa-b5e8-bcb1806190b1))
  (segment (start 105.4115 173.7995) (end 103.9495 173.7995) (width 0.6) (layer "F.Cu") (net 4) (tstamp 3b57a144-a819-4d27-bf67-3269d688f9ca))
  (segment (start 123.317 112.0775) (end 121.8395 110.6) (width 1) (layer "F.Cu") (net 4) (tstamp 46ed28d8-0305-40dd-b2c1-8624b6817517))
  (segment (start 105.41 175.8315) (end 105.41 174.625) (width 0.6) (layer "F.Cu") (net 4) (tstamp 5ebabc20-8d40-4d85-aeab-d14f82447eb0))
  (segment (start 105.41 190.627) (end 105.6005 190.8175) (width 0.6) (layer "F.Cu") (net 4) (tstamp 711a8523-6531-4ce7-8acb-2bf938b4dd64))
  (segment (start 105.41 176.8475) (end 105.6005 177.038) (width 0.6) (layer "F.Cu") (net 4) (tstamp 71ffaa2b-d637-4633-8879-f466ee728267))
  (segment (start 118.4 106.4) (end 112.9 106.4) (width 1) (layer "F.Cu") (net 4) (tstamp 8e302466-a804-49d4-ac2c-97a4b447f530))
  (segment (start 105.4115 174.6235) (end 105.41 174.625) (width 0.6) (layer "F.Cu") (net 4) (tstamp a3a6bee1-9630-471d-a2ef-8c02b2354a46))
  (segment (start 109.5 106.4) (end 112.9 106.4) (width 1) (layer "F.Cu") (net 4) (tstamp bd6d132e-6b3d-42d7-8a4c-d0c39bbbe035))
  (segment (start 105.41 189.611) (end 105.41 190.627) (width 0.6) (layer "F.Cu") (net 4) (tstamp c23dd5e0-6808-4680-b7d9-2f8c77bf73ee))
  (segment (start 121.8395 110.6) (end 118.4 110.6) (width 1) (layer "F.Cu") (net 4) (tstamp c53705f8-35ed-4cf0-896e-90e2f57df045))
  (segment (start 118.4 110.6) (end 118.4 106.4) (width 1) (layer "F.Cu") (net 4) (tstamp c9a655b0-9bfb-4536-94cb-c6c6a2d0a05f))
  (segment (start 105.4115 173.7995) (end 105.4115 174.6235) (width 0.6) (layer "F.Cu") (net 4) (tstamp ce198b82-99e2-43d0-a4a5-84d2cb4d48a6))
  (segment (start 105.4115 188.403) (end 105.41 188.4045) (width 0.6) (layer "F.Cu") (net 4) (tstamp de7d2180-f645-497c-afea-41add73dc9a2))
  (segment (start 123.317 152.6) (end 123.317 112.0775) (width 1) (layer "F.Cu") (net 4) (tstamp df82bfed-c2cc-4297-b1f4-16af86a081b6))
  (segment (start 116.3 150.5) (end 118.4 152.6) (width 1) (layer "F.Cu") (net 4) (tstamp e1720c08-5ec5-44ab-8c35-b45acb2a6cd8))
  (via (at 123.317 152.6) (size 1) (drill 0.5) (layers "F.Cu" "B.Cu") (net 4) (tstamp 281fa849-6fc2-4c6d-b05b-29e86c39f369))
  (via (at 103.9495 173.7995) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 4) (tstamp 7a323e74-d822-459e-9039-fa4ba783ea64))
  (via (at 105.6005 177.038) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 4) (tstamp 9de2eeaf-fbec-4d98-9819-d37f330028a9))
  (via (at 105.6005 190.8175) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 4) (tstamp b0452bf5-b77a-4afb-900f-31be1f5972de))
  (via (at 105.41 188.4045) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 4) (tstamp bae9bc90-d766-49a8-9605-bf8e50336f0b))
  (via (at 105.41 174.625) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 4) (tstamp e25ddb02-534c-4354-a56e-9957e5295b37))
  (via (at 103.9495 187.579) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 4) (tstamp e711f930-9c35-45dc-919e-e2d484571a3d))
  (segment (start 123.317 152.6) (end 118.4 152.6) (width 1) (layer "B.Cu") (net 4) (tstamp 43ff33ed-edbc-4c24-8d40-117ba9907d18))
  (segment (start 91.567 123.5075) (end 104.4745 110.6) (width 1) (layer "F.Cu") (net 5) (tstamp 21ee7ae5-f03b-470a-aae0-8c702673625e))
  (segment (start 95.5675 132.207) (end 100.3935 137.033) (width 1) (layer "F.Cu") (net 5) (tstamp 25c8979a-182c-40ac-b534-535d0f9c2785))
  (segment (start 79.409499 111.349999) (end 74.75 111.349999) (width 1) (layer "F.Cu") (net 5) (tstamp 2bad4178-c87f-47ff-9982-abd9773448c1))
  (segment (start 112.9 110.6) (end 109.5 110.6) (width 1) (layer "F.Cu") (net 5) (tstamp 527846d2-b789-4076-a0e1-21b524be32d7))
  (segment (start 69.350001 111.349999) (end 65.85 114.85) (width 1) (layer "F.Cu") (net 5) (tstamp 6ceced5b-b9e3-4275-8ed5-7878bffe1186))
  (segment (start 100.3935 137.033) (end 100.3935 151.384) (width 1) (layer "F.Cu") (net 5) (tstamp 8585c021-5193-4d8a-b5d7-7a586fc2d18e))
  (segment (start 74.75 111.349999) (end 69.350001 111.349999) (width 1) (layer "F.Cu") (net 5) (tstamp 94ca27f5-c9ae-421f-b5c6-040fb43f45a4))
  (segment (start 91.567 132.207) (end 95.5675 132.207) (width 1) (layer "F.Cu") (net 5) (tstamp 9ee640e9-c76a-46cd-80f7-8e60516e7355))
  (segment (start 91.567 136.271) (end 91.567 132.207) (width 1) (layer "F.Cu") (net 5) (tstamp a2c45dbe-23e8-426a-a402-b6f1d7dfa431))
  (segment (start 104.4745 110.6) (end 109.5 110.6) (width 1) (layer "F.Cu") (net 5) (tstamp b52f7206-30d6-46f1-864e-325b957e5613))
  (segment (start 91.567 123.5075) (end 79.409499 111.349999) (width 1) (layer "F.Cu") (net 5) (tstamp c6c97958-c0d8-4bdf-9794-b3e5f9d86892))
  (segment (start 91.567 132.207) (end 91.567 123.5075) (width 1) (layer "F.Cu") (net 5) (tstamp c99c8ee6-9297-408e-9511-2d8f8ca44854))
  (segment (start 91.567 136.271) (end 91.567 138.684) (width 1) (layer "F.Cu") (net 5) (tstamp e4f7214e-e4f3-447d-9f4b-2eece078d1ec))
  (segment (start 74.75 184.5) (end 71.35 184.5) (width 1) (layer "F.Cu") (net 5) (tstamp f362c7b6-94c5-4f7b-9044-7da13a8a7204))
  (segment (start 67.95 116.95) (end 65.85 119.05) (width 1) (layer "F.Cu") (net 6) (tstamp 0717ff19-fa5d-4d18-853f-763773e943f2))
  (segment (start 74.75 116.95) (end 67.95 116.95) (width 1) (layer "F.Cu") (net 6) (tstamp 26938f3f-2db2-48bb-a3b2-d31baa2eba3b))
  (segment (start 94.107 136.271) (end 94.107 138.684) (width 1) (layer "F.Cu") (net 6) (tstamp 5ffd4f59-03ad-48c5-86b9-0d2d4a8c3875))
  (segment (start 94.107 138.684) (end 94.107 145.743) (width 1) (layer "F.Cu") (net 6) (tstamp a3dd7f80-0c52-4120-b0e6-f6084b37264b))
  (segment (start 107.823 179.959) (end 107.823 179.578) (width 0.2) (layer "F.Cu") (net 7) (tstamp 2e1cd33c-f2b9-40ae-bf8f-10656c528697))
  (segment (start 107.823 181.9275) (end 107.823 179.959) (width 0.2) (layer "F.Cu") (net 7) (tstamp 47926a49-bf33-4812-9e18-a9c0c5de11ee))
  (segment (start 107.823 179.578) (end 109.2835 178.1175) (width 0.2) (layer "F.Cu") (net 7) (tstamp 4aa0010d-4418-4427-b3f9-4e8f3207c348))
  (segment (start 107.569 182.1815) (end 107.823 181.9275) (width 0.2) (layer "F.Cu") (net 7) (tstamp 5a712cab-d13b-4138-ae13-6733221fc263))
  (segment (start 105.4115 182.499) (end 107.2515 182.499) (width 0.2) (layer "F.Cu") (net 7) (tstamp 8bc22957-edeb-4d97-b9cd-e11ff2cda9e2))
  (segment (start 107.2515 182.499) (end 107.569 182.1815) (width 0.2) (layer "F.Cu") (net 7) (tstamp 9b7b2623-dee1-4f6a-b5f2-0d4d56b3dc3c))
  (segment (start 108.2675 179.705) (end 109.855 178.1175) (width 0.2) (layer "F.Cu") (net 8) (tstamp 0027e69b-80d5-43a1-bfbd-8608ed718b39))
  (segment (start 108.2675 179.7685) (end 108.2675 179.705) (width 0.2) (layer "F.Cu") (net 8) (tstamp 103e5dae-a57a-407d-b703-0bb819852327))
  (segment (start 108.585 182.245) (end 108.2675 181.9275) (width 0.2) (layer "F.Cu") (net 8) (tstamp 1e1a4bfd-5c33-4ef5-892a-f8514a7d506e))
  (segment (start 108.839 182.499) (end 108.585 182.245) (width 0.2) (layer "F.Cu") (net 8) (tstamp 94c154b9-993e-4760-ac5e-d83fe140add4))
  (segment (start 108.2675 181.9275) (end 108.2675 179.7685) (width 0.2) (layer "F.Cu") (net 8) (tstamp acca18a3-aa4f-41d0-b549-ceffc62e90b4))
  (segment (start 110.3615 182.499) (end 108.839 182.499) (width 0.2) (layer "F.Cu") (net 8) (tstamp f1e3d17a-860f-441f-9d3c-39d63cfe6dda))
  (segment (start 101.097 179.959) (end 101.097 177.927) (width 0.25) (layer "F.Cu") (net 11) (tstamp 8eff3675-4d8c-47c2-abaa-d11eb21e6b7b))
  (segment (start 110.363 187.5805) (end 110.3615 187.579) (width 0.25) (layer "F.Cu") (net 12) (tstamp 2df73c5a-adbb-4bc7-b47d-8d0bd56609c1))
  (segment (start 99.397 179.119) (end 99.3825 179.1335) (width 0.25) (layer "F.Cu") (net 12) (tstamp c38bd870-1398-4123-bb66-f03bdec98865))
  (segment (start 99.397 177.927) (end 99.397 179.119) (width 0.25) (layer "F.Cu") (net 12) (tstamp c4bb1d76-7553-484c-ba6c-5112de2e2370))
  (segment (start 110.363 189.611) (end 110.363 187.5805) (width 0.25) (layer "F.Cu") (net 12) (tstamp e206a0d6-ec21-46f8-a7d2-a2d3c33c528d))
  (segment (start 110.3615 187.579) (end 111.8235 187.579) (width 0.25) (layer "F.Cu") (net 12) (tstamp e83a8d79-3219-4a09-aae0-942cadc2246c))
  (via (at 111.8235 187.579) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 12) (tstamp a13ed7a2-c423-4fc6-992a-f59ed5a0273c))
  (via (at 99.3825 179.1335) (size 0.6) (drill 0.3) (layers "F.Cu" "B.Cu") (net 12) (tstamp c86025cf-1d8d-4775-befe-6e7049de98a4))
  (segment (start 99.3825 179.1335) (end 103.378 179.1335) (width 0.25) (layer "B.Cu") (net 12) (tstamp a072dd78-0fb3-4f60-bab8-99746e286d6c))
  (segment (start 103.378 179.1335) (end 111.8235 187.579) (width 0.25) (layer "B.Cu") (net 12) (tstamp ca87affc-4fbe-45bb-b391-ec0b16ed3e86))
  (segment (start 67.95 161.4) (end 65.85 163.5) (width 0.25) (layer "F.Cu") (net 13) (tstamp 03fcb067-9f18-4625-9566-0350764ca111))
  (segment (start 111.8235 169.799) (end 111.5695 170.053) (width 0.25) (layer "F.Cu") (net 13) (tstamp 05c68e03-868a-43df-80dc-48abedd30df6))
  (segment (start 65.85 163.5) (end 67.95 165.6) (width 0.25) (layer "F.Cu") (net 13) (tstamp 0991e9f5-f4fc-45c7-930a-ddea33e6b91e))
  (segment (start 107.8865 167.4495) (end 108.5215 168.0845) (width 0.25) (layer "F.Cu") (net 13) (tstamp 140dfb94-d2ab-4514-8bf6-2a53246b1969))
  (segment (start 105.4115 167.4495) (end 107.8865 167.4495) (width 0.25) (layer "F.Cu") (net 13) (tstamp 22dc8f97-a35f-4526-b0c0-233094657a87))
  (segment (start 111.4425 171.8945) (end 111.76 172.212) (width 0.25) (layer "F.Cu") (net 13) (tstamp 30b7e206-6784-4adf-8a18-95a4f4950006))
  (segment (start 109.0295 169.9895) (end 108.712 170.307) (width 0.25) (layer "F.Cu") (net 13) (tstamp 4f009557-09d5-4a13-912d-2013013f91a8))
  (segment (start 111.5695 168.0845) (end 111.8235 168.3385) (width 0.25) (layer "F.Cu") (net 13) (tstamp 5cb03f87-add7-463a-ab28-1fe93983bfb2))
  (segment (start 111.506 173.7995) (end 110.3615 173.7995) (width 0.25) (layer "F.Cu") (net 13) (tstamp 6289387f-1124-4d12-ac03-d637e6f7f592))
  (segment (start 109.2835 171.8945) (end 111.4425 171.8945) (width 0.25) (layer "F.Cu") (net 13) (tstamp 67928fc3-2084-49a9-81fa-27b2b55dcbe5))
  (segment (start 67.95 165.6) (end 74.3505 165.6) (width 0.25) (layer "F.Cu") (net 13) (tstamp 72520ffe-1605-4242-a469-70cf476d6090))
  (segment (start 110.3615 169.9895) (end 109.0295 169.9895) (width 0.25) (layer "F.Cu") (net 13) (tstamp 733e0df2-548b-45e0-946c-239222774a0d))
  (segment (start 111.76 173.5455) (end 111.506 173.7995) (width 0.25) (layer "F.Cu") (net 13) (tstamp 737ab562-094b-4898-be96-9ecc55ff2e37))
  (segment (start 111.76 172.212) (end 111.76 173.5455) (width 0.25) (layer "F.Cu") (net 13) (tstamp 766fd440-6629-48d6-96a3-bbde9b817735))
  (segment (start 108.712 171.323) (end 109.2835 171.8945) (width 0.25) (layer "F.Cu") (net 13) (tstamp 84a1aaa6-96f3-48aa-b0ae-396162bbd40b))
  (segment (start 111.8235 168.3385) (end 111.8235 169.799) (width 0.25) (layer "F.Cu") (net 13) (tstamp 911b5735-7f00-42df-9b05-11801efd8471))
  (segment (start 108.712 170.307) (end 108.712 171.323) (width 0.25) (layer "F.Cu") (net 13) (tstamp 98f45bb3-f808-403b-95cb-cd871f6e0eef))
  (segment (start 71.35 135.85) (end 76.15 140.65) (width 0.25) (layer "F.Cu") (net 13) (tstamp 9a54611d-392c-462f-bd17-0a29babfccef))
  (segment (start 102.9335 176.403) (end 104.648 178.1175) (width 0.25) (layer "F.Cu") (net 13) (tstamp 9dad4f50-021e-42ff-bfc2-bfb2011cfbb9))
  (segment (start 104.648 178.1175) (end 107.2515 178.1175) (width 0.25) (layer "F.Cu") (net 13) (tstamp b0d57df3-cb76-4df1-8664-721153541ddd))
  (segment (start 76.15 140.65) (end 76.15 158.725) (width 0.25) (layer "F.Cu") (net 13) (tstamp b6556a83-548a-495b-88c4-3aea72bd8200))
  (segment (start 85.1535 176.403) (end 102.9335 176.403) (width 0.25) (layer "F.Cu") (net 13) (tstamp bac4f19b-8ed3-4f01-bcf1-cba228abfc2b))
  (segment (start 108.5215 168.0845) (end 111.5695 168.0845) (width 0.25) (layer "F.Cu") (net 13) (tstamp ce9c0d66-528d-4c5e-be3a-644305987097))
  (segment (start 110.425 170.053) (end 110.3615 169.9895) (width 0.25) (layer "F.Cu") (net 13) (tstamp de87f370-66de-4fda-a193-101e33b6c920))
  (segment (start 107.2515 178.1175) (end 110.3615 175.0075) (width 0.25) (layer "F.Cu") (net 13) (tstamp e8f8776e-863f-49bd-b34e-554c61121a19))
  (segment (start 111.5695 170.053) (end 110.425 170.053) (width 0.25) (layer "F.Cu") (net 13) (tstamp eec6afef-5ed6-4fe5-8c49-82f386af3ae8))
  (segment (start 73.475 161.4) (end 67.95 161.4) (width 0.25) (layer "F.Cu") (net 13) (tstamp f05208be-fc3c-4a6b-a3ca-d001e05ad958))
  (segment (start 76.15 158.725) (end 73.475 161.4) (width 0.25) (layer "F.Cu") (net 13) (tstamp f86054b7-4946-41c2-a422-5e2a18468c83))
  (segment (start 110.3615 175.0075) (end 110.3615 173.7995) (width 0.25) (layer "F.Cu") (net 13) (tstamp f8d772d5-d536-442f-aa50-9cd1d4747f7e))
  (segment (start 74.3505 165.6) (end 85.1535 176.403) (width 0.25) (layer "F.Cu") (net 13) (tstamp f9da3ed6-5965-4b7d-a662-afdb1cda8d4b))
  (segment (start 103.886 181.229) (end 105.4115 181.229) (width 0.25) (layer "F.Cu") (net 14) (tstamp 0996f39b-a408-4058-ac5f-4a21729c2615))
  (segment (start 67.95 169.8) (end 74.296 169.8) (width 0.25) (layer "F.Cu") (net 14) (tstamp 0fa44d89-826e-4b2c-bf8e-4a18100d63cc))
  (segment (start 62.5 158.75) (end 65.25 156) (width 0.25) (layer "F.Cu") (net 14) (tstamp 3685fdf0-f2d1-4771-98ba-15fc044aba44))
  (segment (start 77.65 137.95) (end 77.65 141.5) (width 0.25) (layer "F.Cu") (net 14) (tstamp 3728a4d9-668f-44fa-87f6-22ed3741d5e5))
  (segment (start 85.979 181.483) (end 103.632 181.483) (width 0.25) (layer "F.Cu") (net 14) (tstamp 3fe1d36b-2339-49d4-b309-62766d1ebfda))
  (segment (start 75.2 146.9) (end 75.2 143.8) (width 0.25) (layer "F.Cu") (net 14) (tstamp 4229b8e0-3f2d-45b1-a1d1-696b1f0d5b0e))
  (segment (start 74.6 147.5) (end 75.2 146.9) (width 0.25) (layer "F.Cu") (net 14) (tstamp 4ce8f3b3-e23b-4f52-8e27-15041e376467))
  (segment (start 74.296 169.8) (end 85.979 181.483) (width 0.25) (layer "F.Cu") (net 14) (tstamp 60cd3826-8d06-4488-b6d4-029e18eedc7f))
  (segment (start 71.35 131.65) (end 77.65 137.95) (width 0.25) (layer "F.Cu") (net 14) (tstamp 7248f799-4455-446a-85ac-1a7ea722681e))
  (segment (start 65.85 167.7) (end 62.5 164.35) (width 0.25) (layer "F.Cu") (net 14) (tstamp 8ec1d6da-9908-48b4-a2b8-677192658bf2))
  (segment (start 65.25 156) (end 73.75 147.5) (width 0.25) (layer "F.Cu") (net 14) (tstamp 8f342787-a2dd-4b58-95bd-174eda7c2fc8))
  (segment (start 103.632 181.483) (end 103.886 181.229) (width 0.25) (layer "F.Cu") (net 14) (tstamp 99c8de4b-9492-493b-8bca-5b1807bf5a69))
  (segment (start 73.75 147.5) (end 74.6 147.5) (width 0.25) (layer "F.Cu") (net 14) (tstamp 9ec1ba90-47b8-46e8-b412-e17f6352d27c))
  (segment (start 62.5 164.35) (end 62.5 158.75) (width 0.25) (layer "F.Cu") (net 14) (tstamp a6ca0fbf-72b1-4357-8078-14a434037f8c))
  (segment (start 65.85 167.7) (end 67.95 169.8) (width 0.25) (layer "F.Cu") (net 14) (tstamp f0a337e2-70c9-4645-8262-e455e68f6c1b))
  (via (at 75.2 143.8) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 14) (tstamp 4687a93e-8203-4d10-8062-153206e9d6a8))
  (via (at 77.65 141.5) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 14) (tstamp 65cbf64e-daad-41fe-8073-1bf9f93590b5))
  (segment (start 75.2 143.8) (end 77.5 141.5) (width 0.25) (layer "B.Cu") (net 14) (tstamp 0e69e81e-3908-4703-9aa2-2688c43168d3))
  (segment (start 77.5 141.5) (end 77.65 141.5) (width 0.25) (layer "B.Cu") (net 14) (tstamp 967a1e03-4650-474e-93d2-aa7eca127ee8))
  (segment (start 78.9 145.65) (end 78.9 135) (width 0.25) (layer "F.Cu") (net 15) (tstamp 080b189c-5eff-47e8-9b0c-6d46979659ab))
  (segment (start 62 168.05) (end 62 158.6) (width 0.25) (layer "F.Cu") (net 15) (tstamp 2427c765-c1ae-43f2-add8-1dd452f339fa))
  (segment (start 74.25 146.35) (end 74.25 146.3) (width 0.25) (layer "F.Cu") (net 15) (tstamp 2b3c6466-a0f2-4884-bb50-6b94f292d51e))
  (segment (start 62 158.6) (end 65.1 155.5) (width 0.25) (layer "F.Cu") (net 15) (tstamp 3e93d472-9c57-4b5f-b65e-51e5c1014b44))
  (segment (start 74.686 174) (end 85.086 184.4) (width 0.25) (layer "F.Cu") (net 15) (tstamp 4d9569e2-62b9-4048-a46f-10061fd28ea2))
  (segment (start 65.85 171.9) (end 67.95 174) (width 0.25) (layer "F.Cu") (net 15) (tstamp 4e46affe-87ae-4ce3-bf05-6bbdde84b879))
  (segment (start 65.1 155.5) (end 74.25 146.35) (width 0.25) (layer "F.Cu") (net 15) (tstamp 6d38f7db-5648-4285-88ba-dda6dbb1de69))
  (segment (start 67.95 174) (end 74.686 174) (width 0.25) (layer "F.Cu") (net 15) (tstamp 9106567c-1994-4d1b-a28d-9dab4601ddbe))
  (segment (start 106.6 184.4) (end 107.231 183.769) (width 0.25) (layer "F.Cu") (net 15) (tstamp 923303d4-5aa7-458b-8672-58e14750cc81))
  (segment (start 78.9 135) (end 71.35 127.45) (width 0.25) (layer "F.Cu") (net 15) (tstamp 9e13560b-01f8-405e-a6ac-d315c1e9b918))
  (segment (start 65.85 171.9) (end 62 168.05) (width 0.25) (layer "F.Cu") (net 15) (tstamp a7a0b997-e381-4d77-a207-478720a28619))
  (segment (start 85.086 184.4) (end 106.6 184.4) (width 0.25) (layer "F.Cu") (net 15) (tstamp cb32142c-9dd7-4d11-a4c2-64fd3993d769))
  (segment (start 107.231 183.769) (end 110.3615 183.769) (width 0.25) (layer "F.Cu") (net 15) (tstamp da311762-d564-43a3-8711-6aad70bc7c8d))
  (via (at 74.25 146.3) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 15) (tstamp 54499cdf-988b-4f70-a520-9dc04c01194c))
  (via (at 78.9 145.65) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 15) (tstamp 8659a48a-eb54-44fd-9cc5-753a7070cd2d))
  (segment (start 74.9 145.65) (end 78.9 145.65) (width 0.25) (layer "B.Cu") (net 15) (tstamp d798bab7-2ad2-413f-9a92-c7dd415fd5ae))
  (segment (start 74.25 146.3) (end 74.9 145.65) (width 0.25) (layer "B.Cu") (net 15) (tstamp ef7284f3-1543-4680-a21e-0c43c9d22ce5))
  (segment (start 111.887 161.9885) (end 109.6645 161.9885) (width 0.3) (layer "F.Cu") (net 16) (tstamp 4007b745-fb27-491c-8b23-10edb65dcb37))
  (segment (start 108.9025 162.7505) (end 108.9025 164.2745) (width 0.3) (layer "F.Cu") (net 16) (tstamp 5ad2f6b5-d983-4f8c-ac9b-2c5270e64045))
  (segment (start 118.299669 168.401169) (end 111.887 161.9885) (width 0.3) (layer "F.Cu") (net 16) (tstamp 94ef772c-6d41-4b34-9d9e-9caa8c571099))
  (segment (start 108.9025 164.2745) (end 107.31 164.2745) (width 0.25) (layer "F.Cu") (net 16) (tstamp 9fb98c3a-6d6e-440d-a7cd-2f1e0d7f64b3))
  (segment (start 109.6645 161.9885) (end 108.9025 162.7505) (width 0.3) (layer "F.Cu") (net 16) (tstamp ce2cdd76-d52c-476d-8ecf-a1e40d3505b9))
  (segment (start 118.299669 172.45) (end 118.299669 168.401169) (width 0.3) (layer "F.Cu") (net 16) (tstamp e3491a5b-f902-4c52-a5a2-9d79e122f4b9))
  (segment (start 116.6495 169.7355) (end 116.6495 173.609) (width 0.25) (layer "F.Cu") (net 17) (tstamp 099d202c-1350-4862-90a6-8fec271ca08e))
  (segment (start 117.7805 174.74) (end 118.299669 174.74) (width 0.25) (layer "F.Cu") (net 17) (tstamp 231d1800-9d4e-4ff9-a23e-f5f4ab7f3324))
  (segment (start 115.1255 169.3545) (end 116.2685 169.3545) (width 0.25) (layer "F.Cu") (net 17) (tstamp 2c4e9791-07ee-4c64-8861-52505f930100))
  (segment (start 115.1205 169.3495) (end 115.1255 169.3545) (width 0.25) (layer "F.Cu") (net 17) (tstamp 5271f5b6-7a3c-4581-aca4-b435cedbb00e))
  (segment (start 112.9665 169.3495) (end 115.1205 169.3495) (width 0.25) (layer "F.Cu") (net 17) (tstamp a7b9756f-b0c3-43dd-a845-127788e6189e))
  (segment (start 116.6495 173.609) (end 117.7805 174.74) (width 0.25) (layer "F.Cu") (net 17) (tstamp a94b79f2-852a-417b-b0e7-817b5aa0666c))
  (segment (start 116.2685 169.3545) (end 116.6495 169.7355) (width 0.25) (layer "F.Cu") (net 17) (tstamp b20e52f9-04db-4444-a671-c4dad77c7e0d))
  (segment (start 115.1255 173.1645) (end 112.9715 173.1645) (width 0.25) (layer "F.Cu") (net 18) (tstamp 07cb63b5-fa4a-4bb7-b491-2a92c645c4e9))
  (segment (start 115.1255 174.244) (end 117.9115 177.03) (width 0.25) (layer "F.Cu") (net 18) (tstamp 16c6d298-9da6-4ded-97cb-328a06993e34))
  (segment (start 115.1255 173.1645) (end 115.1255 174.244) (width 0.25) (layer "F.Cu") (net 18) (tstamp 5b52365c-bac4-46d9-a1d6-be0e0ae869cb))
  (segment (start 112.9715 173.1645) (end 112.9665 173.1595) (width 0.25) (layer "F.Cu") (net 18) (tstamp 98ad5d0c-fe3d-4a73-8a5a-45a398f4117e))
  (segment (start 117.9115 177.03) (end 118.299669 177.03) (width 0.25) (layer "F.Cu") (net 18) (tstamp b7b3ff71-e0aa-494e-94f8-e8da085ed952))
  (segment (start 124.3965 179.166831) (end 124.3965 183.2535) (width 0.2) (layer "F.Cu") (net 19) (tstamp 1a4733eb-f9ab-41e9-8208-ebf824caa056))
  (segment (start 122.611 185.039) (end 114.2975 185.039) (width 0.2) (layer "F.Cu") (net 19) (tstamp 3fb750a1-6bbb-4226-b2a7-b57435193ec4))
  (segment (start 122.259669 177.03) (end 124.3965 179.166831) (width 0.2) (layer "F.Cu") (net 19) (tstamp b178e307-3ec8-42bc-8689-c2b11de110fe))
  (segment (start 124.3965 183.2535) (end 122.611 185.039) (width 0.2) (layer "F.Cu") (net 19) (tstamp d1540cb7-8849-4701-84fe-a1dd5750ce93))
  (segment (start 123.185 183.515) (end 117.6655 183.515) (width 0.2) (layer "F.Cu") (net 20) (tstamp 0df397e5-9564-458f-88e7-634eacdf34f0))
  (segment (start 122.259669 179.32) (end 123.952 181.012331) (width 0.2) (layer "F.Cu") (net 20) (tstamp 24df232f-8195-4a0c-af20-5f575402d2aa))
  (segment (start 123.952 182.748) (end 123.185 183.515) (width 0.2) (layer "F.Cu") (net 20) (tstamp 43ca42a5-a235-473c-95e1-6a960850e35a))
  (segment (start 123.952 181.012331) (end 123.952 182.748) (width 0.2) (layer "F.Cu") (net 20) (tstamp 7f08227f-c177-4b94-a6bf-755cf37eef7a))
  (segment (start 115.3795 181.229) (end 114.2975 181.229) (width 0.2) (layer "F.Cu") (net 20) (tstamp 9dba7653-30f3-404a-bcd7-01e03528a028))
  (segment (start 117.6655 183.515) (end 115.3795 181.229) (width 0.2) (layer "F.Cu") (net 20) (tstamp d611d2cf-4579-4753-8c6e-bef9e9ce6d79))
  (segment (start 112.3975 185.039) (end 110.3615 185.039) (width 0.2) (layer "F.Cu") (net 21) (tstamp 7f517a4f-cd05-463a-b471-7dcbe4684e32))
  (segment (start 110.3615 181.229) (end 112.3975 181.229) (width 0.2) (layer "F.Cu") (net 22) (tstamp bb993de7-415d-43e1-88d0-87020f6149cb))
  (segment (start 105.4115 166.1795) (end 105.4115 164.276) (width 0.25) (layer "F.Cu") (net 23) (tstamp 38ea26a6-d21a-488d-95d4-3d2782c8127a))
  (segment (start 105.4115 164.276) (end 105.41 164.2745) (width 0.25) (layer "F.Cu") (net 23) (tstamp 97884470-ad08-4cee-8980-6965d3b07794))
  (segment (start 110.3615 167.4495) (end 112.9665 167.4495) (width 0.25) (layer "F.Cu") (net 24) (tstamp 577b03a1-7cd9-41cc-b783-3cf7cd5d59c7))
  (segment (start 110.3615 171.2595) (end 112.9665 171.2595) (width 0.25) (layer "F.Cu") (net 25) (tstamp a1cd021e-e8e0-4b46-bee2-4380f39f512f))
  (segment (start 105.4115 168.7195) (end 108.204 168.7195) (width 0.2) (layer "F.Cu") (net 26) (tstamp 6325eff7-a6eb-4f23-a258-ee4661d12c84))
  (segment (start 108.6485 169.164) (end 108.204 169.6085) (width 0.2) (layer "F.Cu") (net 26) (tstamp 635820c1-230b-4e92-8ef2-e19c06bad385))
  (segment (start 108.204 169.6085) (end 108.204 171.6405) (width 0.2) (layer "F.Cu") (net 26) (tstamp 694feb26-7f72-4200-97dd-104c8c44b94d))
  (segment (start 109.093 172.5295) (end 110.3615 172.5295) (width 0.2) (layer "F.Cu") (net 26) (tstamp aec9bb20-6b54-47e3-92d7-f727d603cfd6))
  (segment (start 109.093 168.7195) (end 108.6485 169.164) (width 0.2) (layer "F.Cu") (net 26) (tstamp b2e77844-6aac-4d9a-bdba-66051cd4e0d2))
  (segment (start 110.3615 168.7195) (end 109.093 168.7195) (width 0.2) (layer "F.Cu") (net 26) (tstamp d346cbd1-3b78-439b-a8ce-39f202c00287))
  (segment (start 108.204 168.7195) (end 108.6485 169.164) (width 0.2) (layer "F.Cu") (net 26) (tstamp e52cfd30-a714-44fe-abc5-945e265de9bd))
  (segment (start 108.204 171.6405) (end 109.093 172.5295) (width 0.2) (layer "F.Cu") (net 26) (tstamp f431a380-9acb-45a5-b297-5078bc9c9de6))
  (segment (start 102.997 179.959) (end 105.4115 179.959) (width 0.25) (layer "F.Cu") (net 30) (tstamp 8ac1c240-9fcf-46d8-aba3-ff3980247518))

  (zone (net 5) (net_name "-12V") (layer "F.Cu") (tstamp 7d885566-4f62-4106-9158-e5d06d7ee064) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill (thermal_gap 0.2) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 105.791 145.288)
        (xy 79.1845 145.288)
        (xy 79.1845 99.6315)
        (xy 105.791 99.6315)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layers "F.Cu" "In1.Cu" "B.Cu") (tstamp ae37886e-fbd1-40cb-9bdf-bc963cfc63bc) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill (thermal_gap 0.2) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 72.8 96.45)
        (xy 134.3 96.75)
        (xy 135.6 194.55)
        (xy 57.404 193.9)
        (xy 53.0225 95.95)
      )
    )
  )
  (zone (net 4) (net_name "+3V3") (layer "In2.Cu") (tstamp 947a59aa-9bf9-45d8-9a31-4c0e74cc3295) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill (thermal_gap 0.2) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 72.8 96.45)
        (xy 134.3 96.75)
        (xy 135.6 194.55)
        (xy 57.404 193.9)
        (xy 53.0225 95.95)
      )
    )
  )
)
