    cpldfit:  version P.20131013                        Xilinx Inc.
                                      Fitter Report
    Design Name: WarpSE                              Date:  3-26-2023,  4:30AM
    Device Used: XC95144XL-10-TQ100
    Fitting Status: Successful

    *************************  Mapped Resource Summary  **************************

    Macrocells     Product Terms    Function Block   Registers      Pins
    Used/Tot       Used/Tot         Inps Used/Tot    Used/Tot       Used/Tot
    118/144 ( 82%) 384 /720  ( 53%) 224/432 ( 52%)   93 /144 ( 65%) 71 /81  ( 88%)

    ** Function Block Resources **

    Function    Mcells      FB Inps     Pterms      IO
    Block       Used/Tot    Used/Tot    Used/Tot    Used/Tot
    FB1          18/18*      21/54       25/90      11/11*
    FB2           6/18        4/54        6/90       8/10
    FB3           9/18       34/54       82/90      10/10*
    FB4          18/18*      31/54       34/90      10/10*
    FB5          14/18       34/54       69/90       8/10
    FB6          18/18*      34/54       63/90      10/10*
    FB7          18/18*      31/54       34/90       8/10
    FB8          17/18       35/54       71/90       6/10
                 -----       -----       -----      -----
                118/144     224/432     384/720     71/81

    * - Resource is exhausted

    ** Global Control Resources **

    Signal 'C16M' mapped onto global clock net GCK1.
    Signal 'C8M' mapped onto global clock net GCK2.
    Signal 'FCLK' mapped onto global clock net GCK3.
    Global output enable net(s) unused.
    Global set/reset net(s) unused.

    ** Pin Resources **

    Signal Type    Required     Mapped  |  Pin Type            Used    Total
    ------------------------------------|------------------------------------
    Input         :   32          32    |  I/O              :    65      73
    Output        :   35          35    |  GCK/IO           :     3       3
    Bidirectional :    1           1    |  GTS/IO           :     3       4
    GCK           :    3           3    |  GSR/IO           :     0       1
    GTS           :    0           0    |
    GSR           :    0           0    |
                     ----        ----
            Total     71          71

    ** Power Data **

    There are 118 macrocells in high performance mode (MCHP).
    There are 0 macrocells in low power mode (MCLP).
    End of Mapped Resource Summary
    **************************  Errors and Warnings  ***************************

    WARNING:Cpld - Unable to retrieve the path to the iSE Project Repository. Will
       use the default filename of 'WarpSE.ise'.
    INFO:Cpld - Inferring BUFG constraint for signal 'C16M' based upon the LOC
       constraint 'P22'. It is recommended that you declare this BUFG explicitedly
       in your design. Note that for certain device families the output of a BUFG
       constraint can not drive a gated clock, and the BUFG constraint will be
       ignored.
    INFO:Cpld - Inferring BUFG constraint for signal 'C8M' based upon the LOC
       constraint 'P23'. It is recommended that you declare this BUFG explicitedly
       in your design. Note that for certain device families the output of a BUFG
       constraint can not drive a gated clock, and the BUFG constraint will be
       ignored.
    INFO:Cpld - Inferring BUFG constraint for signal 'FCLK' based upon the LOC
       constraint 'P27'. It is recommended that you declare this BUFG explicitedly
       in your design. Note that for certain device families the output of a BUFG
       constraint can not drive a gated clock, and the BUFG constraint will be
       ignored.
    WARNING:Cpld:1007 - Removing unused input(s) 'SW<1>'.  The input(s) are unused
       after optimization. Please verify functionality via simulation.
    WARNING:Cpld:1007 - Removing unused input(s) 'SW<2>'.  The input(s) are unused
       after optimization. Please verify functionality via simulation.
    WARNING:Cpld:1007 - Removing unused input(s) 'SW<3>'.  The input(s) are unused
       after optimization. Please verify functionality via simulation.
    WARNING:Cpld:1007 - Removing unused input(s) 'nBG_IOB'.  The input(s) are unused
       after optimization. Please verify functionality via simulation.
    *************************  Summary of Mapped Logic  ************************

    ** 36 Outputs **

    Signal              Total Total Loc     Pin  Pin     Pin     Pwr  Slew Reg Init
    Name                Pts   Inps          No.  Type    Use     Mode Rate State
    nDTACK_FSB          9     26    FB3_9   28   I/O     O       STD  FAST RESET
    nROMWE              1     2     FB3_17  34   I/O     O       STD  FAST
    nAoutOE             2     4     FB4_2   87   I/O     O       STD  FAST SET
    nDoutOE             1     2     FB4_5   89   I/O     O       STD  FAST
    nDinOE              3     6     FB4_6   90   I/O     O       STD  FAST
    nRES                1     1     FB4_8   91   I/O     I/O     STD  FAST
    nVPA_FSB            1     2     FB4_11  93   I/O     O       STD  FAST
    nROMCS              2     5     FB5_2   35   I/O     O       STD  FAST
    nCAS                1     1     FB5_5   36   I/O     O       STD  FAST RESET
    nOE                 1     2     FB5_6   37   I/O     O       STD  FAST
    RA<4>               2     3     FB5_9   40   I/O     O       STD  FAST
    RA<3>               2     3     FB5_11  41   I/O     O       STD  FAST
    RA<5>               2     3     FB5_12  42   I/O     O       STD  FAST
    RA<2>               2     3     FB5_14  43   I/O     O       STD  FAST
    RA<6>               2     3     FB5_15  46   I/O     O       STD  FAST
    nVMA_IOB            3     10    FB6_2   74   I/O     O       STD  FAST RESET
    nLDS_IOB            4     6     FB6_9   79   I/O     O       STD  FAST RESET
    nUDS_IOB            4     6     FB6_11  80   I/O     O       STD  FAST RESET
    nAS_IOB             3     4     FB6_12  81   I/O     O       STD  FAST RESET
    nADoutLE1           2     3     FB6_14  82   I/O     O       STD  FAST SET
    nADoutLE0           1     2     FB6_15  85   I/O     O       STD  FAST
    nDinLE              1     2     FB6_17  86   I/O     O       STD  FAST RESET
    RA<1>               2     3     FB7_2   50   I/O     O       STD  FAST
    RA<7>               2     3     FB7_5   52   I/O     O       STD  FAST
    RA<0>               2     3     FB7_6   53   I/O     O       STD  FAST
    RA<8>               5     6     FB7_8   54   I/O     O       STD  FAST
    RA<10>              1     1     FB7_9   55   I/O     O       STD  FAST
    RA<9>               2     3     FB7_11  56   I/O     O       STD  FAST
    C25MEN              0     0     FB7_12  58   I/O     O       STD  FAST
    C20MEN              0     0     FB7_14  59   I/O     O       STD  FAST
    RA<11>              1     1     FB8_2   63   I/O     O       STD  FAST
    nRAS                0     0     FB8_5   64   I/O     O       STD  FAST
    nRAMLWE             1     4     FB8_6   65   I/O     O       STD  FAST
    nRAMUWE             1     4     FB8_8   66   I/O     O       STD  FAST
    nBERR_FSB           4     8     FB8_12  70   I/O     O       STD  FAST RESET
    nBR_IOB             2     4     FB8_15  72   I/O     O       STD  FAST RESET

    ** 82 Buried Nodes **

    Signal              Total Total Loc     Pwr  Reg Init
    Name                Pts   Inps          Mode State
    ram/RefUrg          1     2     FB1_1   STD  RESET
    ram/RefReqSync      1     1     FB1_2   STD  RESET
    ram/RefReq          1     2     FB1_3   STD  RESET
    iobs/IOACTr         1     1     FB1_4   STD  RESET
    iobm/Er             1     1     FB1_5   STD  RESET
    iobm/DTACKrr        1     1     FB1_6   STD  RESET
    iobm/DTACKrf        1     1     FB1_7   STD  RESET
    iobm/BERRrr         1     1     FB1_8   STD  RESET
    iobm/BERRrf         1     1     FB1_9   STD  RESET
    cnt/nIPL2r          1     1     FB1_10  STD  RESET
    cnt/Er<0>           1     1     FB1_11  STD  RESET
    ALE0S               1     2     FB1_12  STD  RESET
    ram/RS_FSM_FFd1     2     3     FB1_13  STD  RESET
    iobs/IOU1           2     2     FB1_14  STD  RESET
    iobs/IOL1           2     2     FB1_15  STD  RESET
    iobm/IOS_FSM_FFd1   2     3     FB1_16  STD  RESET
    ALE0M               2     4     FB1_17  STD  RESET
    ram/RefDone         3     5     FB1_18  STD  RESET
    iobm/VPArr          1     1     FB2_13  STD  RESET
    iobm/VPArf          1     1     FB2_14  STD  RESET
    iobm/RESrr          1     1     FB2_15  STD  RESET
    iobm/RESrf          1     1     FB2_16  STD  RESET
    iobm/IOREQr         1     1     FB2_17  STD  RESET
    iobm/Er2            1     1     FB2_18  STD  RESET
    IORW0               17    20    FB3_1   STD  RESET
    fsb/VPA             16    26    FB3_6   STD  RESET
    iobs/IORW1          16    19    FB3_11  STD  RESET
    fsb/Ready1r         6     17    FB3_13  STD  RESET
    cs/nOverlay         3     8     FB3_14  STD  RESET
    IOREQ               13    19    FB3_16  STD  RESET
    iobs/Clear1         1     3     FB3_18  STD  RESET
    ram/RegUrgSync      1     1     FB4_1   STD  RESET
    ram/BACTr           1     2     FB4_3   STD  RESET
    nRESout             1     2     FB4_4   STD  RESET
    fsb/ASrf            1     1     FB4_7   STD  RESET
    cnt/Er<1>           1     1     FB4_9   STD  RESET
    cnt/TimerTC         2     6     FB4_10  STD  RESET
    cnt/LTimer<3>       2     6     FB4_12  STD  RESET
    cnt/LTimer<2>       2     5     FB4_13  STD  RESET
    cnt/LTimer<1>       2     4     FB4_14  STD  RESET

    Signal              Total Total Loc     Pwr  Reg Init
    Name                Pts   Inps          Mode State
    RefReq              2     5     FB4_15  STD  RESET
    IOU0                3     5     FB4_16  STD  RESET
    IOL0                3     5     FB4_17  STD  RESET
    RefUrg              5     7     FB4_18  STD  RESET
    iobs/Load1          14    18    FB5_3   STD  RESET
    iobs/PS_FSM_FFd2    12    19    FB5_7   STD  RESET
    ram/RS_FSM_FFd2     8     10    FB5_8   STD  RESET
    iobs/PS_FSM_FFd1    2     3     FB5_10  STD  RESET
    iobs/IOReady        4     8     FB5_16  STD  RESET
    iobs/Once           15    18    FB5_17  STD  RESET
    iobm/ETACK          1     6     FB6_1   STD  RESET
    iobm/IOS_FSM_FFd3   3     6     FB6_3   STD  RESET
    iobm/ES<3>          3     6     FB6_4   STD  RESET
    iobm/ES<1>          3     4     FB6_5   STD  RESET
    iobm/ES<0>          3     7     FB6_6   STD  RESET
    iobm/DoutOE         3     6     FB6_7   STD  RESET
    iobm/ES<4>          4     7     FB6_8   STD  RESET
    iobm/IOS_FSM_FFd2   5     11    FB6_10  STD  RESET
    iobm/ES<2>          5     7     FB6_13  STD  RESET
    IOACT               6     12    FB6_16  STD  RESET
    IOBERR              9     13    FB6_18  STD  RESET
    cnt/LTimerTC        2     16    FB7_1   STD  RESET
    cnt/LTimer<9>       2     12    FB7_3   STD  RESET
    cnt/LTimer<8>       2     11    FB7_4   STD  RESET
    cnt/LTimer<7>       2     10    FB7_7   STD  RESET
    cnt/LTimer<6>       2     9     FB7_10  STD  RESET
    cnt/LTimer<5>       2     8     FB7_13  STD  RESET
    cnt/LTimer<4>       2     7     FB7_15  STD  RESET
    cnt/LTimer<12>      2     15    FB7_16  STD  RESET
    cnt/LTimer<11>      2     14    FB7_17  STD  RESET
    cnt/LTimer<10>      2     13    FB7_18  STD  RESET
    ram/RASEL           14    12    FB8_1   STD  RESET
    cnt/Timer<2>        5     6     FB8_3   STD  RESET
    cnt/Timer<0>        2     4     FB8_4   STD  RESET
    cnt/INITS_FSM_FFd2  2     6     FB8_7   STD  RESET
    fsb/Ready0r         2     7     FB8_9   STD  RESET
    cnt/Timer<1>        4     5     FB8_10  STD  RESET
    ram/RAMReady        9     12    FB8_11  STD  RESET
    ram/RAMEN           9     12    FB8_14  STD  RESET
    ram/RS_FSM_FFd3     13    12    FB8_16  STD  RESET

    Signal              Total Total Loc     Pwr  Reg Init
    Name                Pts   Inps          Mode State
    cnt/INITS_FSM_FFd1  1     7     FB8_17  STD  RESET
    cnt/LTimer<0>       1     3     FB8_18  STD  RESET

    ** 35 Inputs **

    Signal              Loc     Pin  Pin     Pin
    Name                        No.  Type    Use
    A_FSB<13>           FB1_2   11   I/O     I
    A_FSB<14>           FB1_3   12   I/O     I
    A_FSB<15>           FB1_5   13   I/O     I
    A_FSB<16>           FB1_6   14   I/O     I
    A_FSB<17>           FB1_8   15   I/O     I
    A_FSB<18>           FB1_9   16   I/O     I
    A_FSB<19>           FB1_11  17   I/O     I
    A_FSB<20>           FB1_12  18   I/O     I
    A_FSB<21>           FB1_14  19   I/O     I
    A_FSB<22>           FB1_15  20   I/O     I
    C16M                FB1_17  22   GCK/I/O GCK
    A_FSB<5>            FB2_6   2    GTS/I/O I
    A_FSB<6>            FB2_8   3    GTS/I/O I
    A_FSB<7>            FB2_9   4    GTS/I/O I
    A_FSB<8>            FB2_11  6    I/O     I
    A_FSB<9>            FB2_12  7    I/O     I
    A_FSB<10>           FB2_14  8    I/O     I
    A_FSB<11>           FB2_15  9    I/O     I
    A_FSB<12>           FB2_17  10   I/O     I
    C8M                 FB3_2   23   GCK/I/O GCK/I
    A_FSB<23>           FB3_5   24   I/O     I
    E                   FB3_6   25   I/O     I
    FCLK                FB3_8   27   GCK/I/O GCK
    nWE_FSB             FB3_11  29   I/O     I
    nLDS_FSB            FB3_12  30   I/O     I
    nAS_FSB             FB3_14  32   I/O     I
    nUDS_FSB            FB3_15  33   I/O     I
    nIPL2               FB4_9   92   I/O     I
    A_FSB<1>            FB4_12  94   I/O     I
    A_FSB<2>            FB4_14  95   I/O     I
    A_FSB<3>            FB4_15  96   I/O     I
    A_FSB<4>            FB4_17  97   I/O     I
    nBERR_IOB           FB6_5   76   I/O     I
    nVPA_IOB            FB6_6   77   I/O     I
    nDTACK_IOB          FB6_8   78   I/O     I

    Legend:
    Pin No. - ~ - User Assigned
    **************************  Function Block Details  ************************
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Imp Pt       - Product terms imported from other macrocells
    Exp Pt       - Product terms exported to other macrocells
                   in direction shown
    Unused Pt    - Unused local product terms remaining in macrocell
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global Clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    X            - Signal used as input to the macrocell logic.
    Pin No.      - ~  - User Assigned
    *********************************** FB1  ***********************************
    Number of function block inputs used/remaining:               21/33
    Number of signals used by logic mapping into function block:  21
    Signal              Total   Imp   Exp Unused  Loc     Pin   Pin     Pin
    Name                Pt      Pt    Pt  Pt               #    Type    Use
    ram/RefUrg            1       0     0   4     FB1_1         (b)     (b)
    ram/RefReqSync        1       0     0   4     FB1_2   11    I/O     I
    ram/RefReq            1       0     0   4     FB1_3   12    I/O     I
    iobs/IOACTr           1       0     0   4     FB1_4         (b)     (b)
    iobm/Er               1       0     0   4     FB1_5   13    I/O     I
    iobm/DTACKrr          1       0     0   4     FB1_6   14    I/O     I
    iobm/DTACKrf          1       0     0   4     FB1_7         (b)     (b)
    iobm/BERRrr           1       0     0   4     FB1_8   15    I/O     I
    iobm/BERRrf           1       0     0   4     FB1_9   16    I/O     I
    cnt/nIPL2r            1       0     0   4     FB1_10        (b)     (b)
    cnt/Er<0>             1       0     0   4     FB1_11  17    I/O     I
    ALE0S                 1       0     0   4     FB1_12  18    I/O     I
    ram/RS_FSM_FFd1       2       0     0   3     FB1_13        (b)     (b)
    iobs/IOU1             2       0     0   3     FB1_14  19    I/O     I
    iobs/IOL1             2       0     0   3     FB1_15  20    I/O     I
    iobm/IOS_FSM_FFd1     2       0     0   3     FB1_16        (b)     (b)
    ALE0M                 2       0     0   3     FB1_17  22    GCK/I/O GCK
    ram/RefDone           3       0     0   2     FB1_18        (b)     (b)

    Signals Used by Logic in Function Block
      1: E                   8: iobs/Load1        15: nUDS_FSB
      2: IOACT               9: iobs/PS_FSM_FFd1  16: ram/RS_FSM_FFd1
      3: RefReq             10: iobs/PS_FSM_FFd2  17: ram/RS_FSM_FFd2
      4: iobm/IOREQr        11: nBERR_IOB         18: ram/RS_FSM_FFd3
      5: iobm/IOS_FSM_FFd1  12: nDTACK_IOB        19: ram/RefDone
      6: iobm/IOS_FSM_FFd2  13: nIPL2             20: ram/RefReqSync
      7: iobm/IOS_FSM_FFd3  14: nLDS_FSB          21: ram/RegUrgSync

    Signal                        1         2         3         4 FB
    Name                0----+----0----+----0----+----0----+----0 Inputs
    ram/RefUrg           ..................X.X................... 2
    ram/RefReqSync       ..X..................................... 1
    ram/RefReq           ..................XX.................... 2
    iobs/IOACTr          .X...................................... 1
    iobm/Er              X....................................... 1
    iobm/DTACKrr         ...........X............................ 1
    iobm/DTACKrf         ...........X............................ 1
    iobm/BERRrr          ..........X............................. 1
    iobm/BERRrf          ..........X............................. 1
    cnt/nIPL2r           ............X........................... 1
    cnt/Er<0>            X....................................... 1
    ALE0S                ........XX.............................. 2
    ram/RS_FSM_FFd1      ...............XXX...................... 3
    iobs/IOU1            .......X......X......................... 2
    iobs/IOL1            .......X.....X.......................... 2
    iobm/IOS_FSM_FFd1    ....XXX................................. 3
    ALE0M                ...XXXX................................. 4
    ram/RefDone          ...............XXXXX.................... 5
                        0----+----1----+----2----+----3----+----4
                                  0         0         0         0
    *********************************** FB2  ***********************************
    Number of function block inputs used/remaining:               4/50
    Number of signals used by logic mapping into function block:  4
    Signal              Total   Imp   Exp Unused  Loc     Pin   Pin     Pin
    Name                Pt      Pt    Pt  Pt               #    Type    Use
    (unused)              0       0     0   5     FB2_1         (b)
    (unused)              0       0     0   5     FB2_2   99    GSR/I/O
    (unused)              0       0     0   5     FB2_3         (b)
    (unused)              0       0     0   5     FB2_4         (b)
    (unused)              0       0     0   5     FB2_5   1     GTS/I/O
    (unused)              0       0     0   5     FB2_6   2     GTS/I/O I
    (unused)              0       0     0   5     FB2_7         (b)
    (unused)              0       0     0   5     FB2_8   3     GTS/I/O I
    (unused)              0       0     0   5     FB2_9   4     GTS/I/O I
    (unused)              0       0     0   5     FB2_10        (b)
    (unused)              0       0     0   5     FB2_11  6     I/O     I
    (unused)              0       0     0   5     FB2_12  7     I/O     I
    iobm/VPArr            1       0     0   4     FB2_13        (b)     (b)
    iobm/VPArf            1       0     0   4     FB2_14  8     I/O     I
    iobm/RESrr            1       0     0   4     FB2_15  9     I/O     I
    iobm/RESrf            1       0     0   4     FB2_16        (b)     (b)
    iobm/IOREQr           1       0     0   4     FB2_17  10    I/O     I
    iobm/Er2              1       0     0   4     FB2_18        (b)     (b)

    Signals Used by Logic in Function Block
      1: IOREQ              3: iobm/Er            4: nVPA_IOB
      2: nRES.PIN

    Signal                        1         2         3         4 FB
    Name                0----+----0----+----0----+----0----+----0 Inputs
    iobm/VPArr           ...X.................................... 1
    iobm/VPArf           ...X.................................... 1
    iobm/RESrr           .X...................................... 1
    iobm/RESrf           .X...................................... 1
    iobm/IOREQr          X....................................... 1
    iobm/Er2             ..X..................................... 1
                        0----+----1----+----2----+----3----+----4
                                  0         0         0         0
    *********************************** FB3  ***********************************
    Number of function block inputs used/remaining:               34/20
    Number of signals used by logic mapping into function block:  34
    Signal              Total   Imp   Exp Unused  Loc     Pin   Pin     Pin
    Name                Pt      Pt    Pt  Pt               #    Type    Use
    IORW0                17      12<-   0   0     FB3_1         (b)     (b)
    (unused)              0       0   /\5   0     FB3_2   23    GCK/I/O GCK/I
    (unused)              0       0   /\3   2     FB3_3         (b)     (b)
    (unused)              0       0   \/1   4     FB3_4         (b)     (b)
    (unused)              0       0   \/5   0     FB3_5   24    I/O     I
    fsb/VPA              16      11<-   0   0     FB3_6   25    I/O     I
    (unused)              0       0   /\5   0     FB3_7         (b)     (b)
    (unused)              0       0   \/5   0     FB3_8   27    GCK/I/O GCK
    nDTACK_FSB            9       5<- \/1   0     FB3_9   28    I/O     O
    (unused)              0       0   \/5   0     FB3_10        (b)     (b)
    iobs/IORW1           16      11<-   0   0     FB3_11  29    I/O     I
    (unused)              0       0   /\5   0     FB3_12  30    I/O     I
    fsb/Ready1r           6       1<-   0   0     FB3_13        (b)     (b)
    cs/nOverlay           3       0   /\1   1     FB3_14  32    I/O     I
    (unused)              0       0   \/5   0     FB3_15  33    I/O     I
    IOREQ                13       8<-   0   0     FB3_16        (b)     (b)
    nROMWE                1       0   /\3   1     FB3_17  34    I/O     O
    iobs/Clear1           1       0   \/4   0     FB3_18        (b)     (b)

    Signals Used by Logic in Function Block
      1: A_FSB<10>         13: A_FSB<22>         24: iobs/IOACTr
      2: A_FSB<11>         14: A_FSB<23>         25: iobs/IORW1
      3: A_FSB<12>         15: A_FSB<8>          26: iobs/IOReady
      4: A_FSB<13>         16: A_FSB<9>          27: iobs/Once
      5: A_FSB<14>         17: IORW0             28: iobs/PS_FSM_FFd1
      6: A_FSB<15>         18: nRES.PIN          29: iobs/PS_FSM_FFd2
      7: A_FSB<16>         19: cs/nOverlay       30: nADoutLE1
      8: A_FSB<17>         20: fsb/ASrf          31: nAS_FSB
      9: A_FSB<18>         21: fsb/Ready0r       32: nDTACK_FSB
     10: A_FSB<19>         22: fsb/Ready1r       33: nWE_FSB
     11: A_FSB<20>         23: fsb/VPA           34: ram/RAMReady
     12: A_FSB<21>

    Signal                        1         2         3         4 FB
    Name                0----+----0----+----0----+----0----+----0 Inputs
    IORW0                ...XX.XXXXXXXX..X.XX....X.XXXXX.X....... 20
    fsb/VPA              XXXXXXXXXXXXXXXX..XXXXX..X...XX.XX...... 26
    nDTACK_FSB           XXXXXXXXXXXXXXXX..XXXX...X...XXXXX...... 26
    iobs/IORW1           ...XX.XXXXXXXX....XX....X.XXXXX.X....... 19
    fsb/Ready1r          ...XX.XXXXXXXX....XX.X...X...XX.X....... 17
    cs/nOverlay          ..........XXXX...XXX..........X......... 8
    IOREQ                ...XX.XXXXXXXX....XX...X..XXXXX.X....... 19
    nROMWE               ..............................X.X....... 2
    iobs/Clear1          ...........................XXX.......... 3
                        0----+----1----+----2----+----3----+----4
                                  0         0         0         0
    *********************************** FB4  ***********************************
    Number of function block inputs used/remaining:               31/23
    Number of signals used by logic mapping into function block:  31
    Signal              Total   Imp   Exp Unused  Loc     Pin   Pin     Pin
    Name                Pt      Pt    Pt  Pt               #    Type    Use
    ram/RegUrgSync        1       0     0   4     FB4_1         (b)     (b)
    nAoutOE               2       0     0   3     FB4_2   87    I/O     O
    ram/BACTr             1       0     0   4     FB4_3         (b)     (b)
    nRESout               1       0     0   4     FB4_4         (b)     (b)
    nDoutOE               1       0     0   4     FB4_5   89    I/O     O
    nDinOE                3       0     0   2     FB4_6   90    I/O     O
    fsb/ASrf              1       0     0   4     FB4_7         (b)     (b)
    nRES                  1       0     0   4     FB4_8   91    I/O     I/O
    cnt/Er<1>             1       0     0   4     FB4_9   92    I/O     I
    cnt/TimerTC           2       0     0   3     FB4_10        (b)     (b)
    nVPA_FSB              1       0     0   4     FB4_11  93    I/O     O
    cnt/LTimer<3>         2       0     0   3     FB4_12  94    I/O     I
    cnt/LTimer<2>         2       0     0   3     FB4_13        (b)     (b)
    cnt/LTimer<1>         2       0     0   3     FB4_14  95    I/O     I
    RefReq                2       0     0   3     FB4_15  96    I/O     I
    IOU0                  3       0     0   2     FB4_16        (b)     (b)
    IOL0                  3       0     0   2     FB4_17  97    I/O     I
    RefUrg                5       0     0   0     FB4_18        (b)     (b)

    Signals Used by Logic in Function Block
      1: A_FSB<20>           12: cnt/LTimer<2>     22: iobs/PS_FSM_FFd1
      2: A_FSB<21>           13: cnt/Timer<0>      23: iobs/PS_FSM_FFd2
      3: A_FSB<22>           14: cnt/Timer<1>      24: nADoutLE1
      4: A_FSB<23>           15: cnt/Timer<2>      25: nAS_FSB
      5: RefUrg              16: cnt/TimerTC       26: nAoutOE
      6: cnt/Er<0>           17: fsb/ASrf          27: nBR_IOB
      7: cnt/Er<1>           18: fsb/VPA           28: nLDS_FSB
      8: cnt/INITS_FSM_FFd1  19: iobm/DoutOE       29: nRESout
      9: cnt/INITS_FSM_FFd2  20: iobs/IOL1         30: nUDS_FSB
     10: cnt/LTimer<0>       21: iobs/IOU1         31: nWE_FSB
     11: cnt/LTimer<1>

    Signal                        1         2         3         4 FB
    Name                0----+----0----+----0----+----0----+----0 Inputs
    ram/RegUrgSync       ....X................................... 1
    nAoutOE              .......XX................XX............. 4
    ram/BACTr            ................X.......X............... 2
    nRESout              .......XX............................... 2
    nDoutOE              ..................X......X.............. 2
    nDinOE               XXXX....................X.....X......... 6
    fsb/ASrf             ........................X............... 1
    nRES                 ............................X........... 1
    cnt/Er<1>            .....X.................................. 1
    cnt/TimerTC          ....XXX.....XXX......................... 6
    nVPA_FSB             .................X......X............... 2
    cnt/LTimer<3>        .....XX..XXX...X........................ 6
    cnt/LTimer<2>        .....XX..XX....X........................ 5
    cnt/LTimer<1>        .....XX..X.....X........................ 4
    RefReq               ....XXX......XX......................... 5
    IOU0                 ....................XXXX.....X.......... 5
    IOL0                 ...................X.XXX...X............ 5
    RefUrg               ....XXX.....XXXX........................ 7
                        0----+----1----+----2----+----3----+----4
                                  0         0         0         0
    *********************************** FB5  ***********************************
    Number of function block inputs used/remaining:               34/20
    Number of signals used by logic mapping into function block:  34
    Signal              Total   Imp   Exp Unused  Loc     Pin   Pin     Pin
    Name                Pt      Pt    Pt  Pt               #    Type    Use
    (unused)              0       0   \/1   4     FB5_1         (b)     (b)
    nROMCS                2       1<- \/4   0     FB5_2   35    I/O     O
    iobs/Load1           14       9<-   0   0     FB5_3         (b)     (b)
    (unused)              0       0   /\5   0     FB5_4         (b)     (b)
    nCAS                  1       0   \/1   3     FB5_5   36    I/O     O
    nOE                   1       1<- \/5   0     FB5_6   37    I/O     O
    iobs/PS_FSM_FFd2     12       7<-   0   0     FB5_7         (b)     (b)
    ram/RS_FSM_FFd2       8       5<- /\2   0     FB5_8   39    I/O     (b)
    RA<4>                 2       2<- /\5   0     FB5_9   40    I/O     O
    iobs/PS_FSM_FFd1      2       0   /\2   1     FB5_10        (b)     (b)
    RA<3>                 2       0     0   3     FB5_11  41    I/O     O
    RA<5>                 2       0     0   3     FB5_12  42    I/O     O
    (unused)              0       0     0   5     FB5_13        (b)
    RA<2>                 2       0   \/1   2     FB5_14  43    I/O     O
    RA<6>                 2       1<- \/4   0     FB5_15  46    I/O     O
    iobs/IOReady          4       4<- \/5   0     FB5_16        (b)     (b)
    iobs/Once            15      10<-   0   0     FB5_17  49    I/O     (b)
    (unused)              0       0   /\5   0     FB5_18        (b)     (b)

    Signals Used by Logic in Function Block
      1: A_FSB<12>         13: A_FSB<3>          24: iobs/PS_FSM_FFd1
      2: A_FSB<13>         14: A_FSB<4>          25: iobs/PS_FSM_FFd2
      3: A_FSB<14>         15: A_FSB<5>          26: nADoutLE1
      4: A_FSB<15>         16: A_FSB<6>          27: nAS_FSB
      5: A_FSB<16>         17: A_FSB<7>          28: nWE_FSB
      6: A_FSB<17>         18: IOBERR            29: ram/RAMEN
      7: A_FSB<18>         19: cs/nOverlay       30: ram/RASEL
      8: A_FSB<19>         20: fsb/ASrf          31: ram/RS_FSM_FFd1
      9: A_FSB<20>         21: iobs/IOACTr       32: ram/RS_FSM_FFd2
     10: A_FSB<21>         22: iobs/IOReady      33: ram/RS_FSM_FFd3
     11: A_FSB<22>         23: iobs/Once         34: ram/RefUrg
     12: A_FSB<23>

    Signal                        1         2         3         4 FB
    Name                0----+----0----+----0----+----0----+----0 Inputs
    nROMCS               ........XXXX......X..................... 5
    iobs/Load1           .XX.XXXXXXXX......XX..XXXXXX............ 18
    nCAS                 .............................X.......... 1
    nOE                  ..........................XX............ 2
    iobs/PS_FSM_FFd2     .XX.XXXXXXXX......XXX.XXXXXX............ 19
    ram/RS_FSM_FFd2      ..........XX......XX......X.X.XXXX...... 10
    RA<4>                ..X...........X..............X.......... 3
    iobs/PS_FSM_FFd1     ....................X..XX............... 3
    RA<3>                .X...........X...............X.......... 3
    RA<5>                ...X...........X.............X.......... 3
    RA<2>                X...........X................X.......... 3
    RA<6>                ....X...........X............X.......... 3
    iobs/IOReady         .................X.XXXX.XXX............. 8
    iobs/Once            .XX.XXXXXXXX......XX..XXXXXX............ 18
                        0----+----1----+----2----+----3----+----4
                                  0         0         0         0
    *********************************** FB6  ***********************************
    Number of function block inputs used/remaining:               34/20
    Number of signals used by logic mapping into function block:  34
    Signal              Total   Imp   Exp Unused  Loc     Pin   Pin     Pin
    Name                Pt      Pt    Pt  Pt               #    Type    Use
    iobm/ETACK            1       0     0   4     FB6_1         (b)     (b)
    nVMA_IOB              3       0     0   2     FB6_2   74    I/O     O
    iobm/IOS_FSM_FFd3     3       0     0   2     FB6_3         (b)     (b)
    iobm/ES<3>            3       0     0   2     FB6_4         (b)     (b)
    iobm/ES<1>            3       0     0   2     FB6_5   76    I/O     I
    iobm/ES<0>            3       0     0   2     FB6_6   77    I/O     I
    iobm/DoutOE           3       0     0   2     FB6_7         (b)     (b)
    iobm/ES<4>            4       0     0   1     FB6_8   78    I/O     I
    nLDS_IOB              4       0     0   1     FB6_9   79    I/O     O
    iobm/IOS_FSM_FFd2     5       0     0   0     FB6_10        (b)     (b)
    nUDS_IOB              4       0     0   1     FB6_11  80    I/O     O
    nAS_IOB               3       0     0   2     FB6_12  81    I/O     O
    iobm/ES<2>            5       0     0   0     FB6_13        (b)     (b)
    nADoutLE1             2       0     0   3     FB6_14  82    I/O     O
    nADoutLE0             1       0   \/1   3     FB6_15  85    I/O     O
    IOACT                 6       1<-   0   0     FB6_16        (b)     (b)
    nDinLE                1       0   \/4   0     FB6_17  86    I/O     O
    IOBERR                9       4<-   0   0     FB6_18        (b)     (b)

    Signals Used by Logic in Function Block
      1: ALE0M             13: iobm/ES<0>         24: iobm/IOS_FSM_FFd3
      2: ALE0S             14: iobm/ES<1>         25: iobm/RESrf
      3: C8M               15: iobm/ES<2>         26: iobm/RESrr
      4: IOACT             16: iobm/ES<3>         27: iobm/VPArf
      5: IOBERR            17: iobm/ES<4>         28: iobm/VPArr
      6: IOL0              18: iobm/ETACK         29: iobs/Clear1
      7: IORW0             19: iobm/Er            30: iobs/Load1
      8: IOU0              20: iobm/Er2           31: nADoutLE1
      9: iobm/BERRrf       21: iobm/IOREQr        32: nAoutOE
     10: iobm/BERRrr       22: iobm/IOS_FSM_FFd1  33: nBERR_IOB
     11: iobm/DTACKrf      23: iobm/IOS_FSM_FFd2  34: nVMA_IOB
     12: iobm/DTACKrr

    Signal                        1         2         3         4 FB
    Name                0----+----0----+----0----+----0----+----0 Inputs
    iobm/ETACK           ............XXXXX................X...... 6
    nVMA_IOB             ...X........XXXXX.........XX...X.X...... 10
    iobm/IOS_FSM_FFd3    ..X.................XXXX.......X........ 6
    iobm/ES<3>           ............XXXX..XX.................... 6
    iobm/ES<1>           ............XX....XX.................... 4
    iobm/ES<0>           ............XXXXX.XX.................... 7
    iobm/DoutOE          ......X.............XXXX.......X........ 6
    iobm/ES<4>           ............XXXXX.XX.................... 7
    nLDS_IOB             .....XX..............XXX.......X........ 6
    iobm/IOS_FSM_FFd2    ..X.....XXXX.....X...XXXXX.............. 11
    nUDS_IOB             ......XX.............XXX.......X........ 6
    nAS_IOB              .....................XXX.......X........ 4
    iobm/ES<2>           ............XXXXX.XX.................... 7
    nADoutLE1            ............................XXX......... 3
    nADoutLE0            XX...................................... 2
    IOACT                ..X.....XXXX.....X..XXXXXX.............. 12
    nDinLE               .....................XX................. 2
    IOBERR               ..X.X...XXXX.....X...XXXXX......X....... 13
                        0----+----1----+----2----+----3----+----4
                                  0         0         0         0
    *********************************** FB7  ***********************************
    Number of function block inputs used/remaining:               31/23
    Number of signals used by logic mapping into function block:  31
    Signal              Total   Imp   Exp Unused  Loc     Pin   Pin     Pin
    Name                Pt      Pt    Pt  Pt               #    Type    Use
    cnt/LTimerTC          2       0     0   3     FB7_1         (b)     (b)
    RA<1>                 2       0     0   3     FB7_2   50    I/O     O
    cnt/LTimer<9>         2       0     0   3     FB7_3         (b)     (b)
    cnt/LTimer<8>         2       0     0   3     FB7_4         (b)     (b)
    RA<7>                 2       0     0   3     FB7_5   52    I/O     O
    RA<0>                 2       0     0   3     FB7_6   53    I/O     O
    cnt/LTimer<7>         2       0     0   3     FB7_7         (b)     (b)
    RA<8>                 5       0     0   0     FB7_8   54    I/O     O
    RA<10>                1       0     0   4     FB7_9   55    I/O     O
    cnt/LTimer<6>         2       0     0   3     FB7_10        (b)     (b)
    RA<9>                 2       0     0   3     FB7_11  56    I/O     O
    C25MEN                0       0     0   5     FB7_12  58    I/O     O
    cnt/LTimer<5>         2       0     0   3     FB7_13        (b)     (b)
    C20MEN                0       0     0   5     FB7_14  59    I/O     O
    cnt/LTimer<4>         2       0     0   3     FB7_15  60    I/O     (b)
    cnt/LTimer<12>        2       0     0   3     FB7_16        (b)     (b)
    cnt/LTimer<11>        2       0     0   3     FB7_17  61    I/O     (b)
    cnt/LTimer<10>        2       0     0   3     FB7_18        (b)     (b)

    Signals Used by Logic in Function Block
      1: A_FSB<10>         12: A_FSB<8>          22: cnt/LTimer<3>
      2: A_FSB<11>         13: A_FSB<9>          23: cnt/LTimer<4>
      3: A_FSB<17>         14: cnt/Er<0>         24: cnt/LTimer<5>
      4: A_FSB<18>         15: cnt/Er<1>         25: cnt/LTimer<6>
      5: A_FSB<19>         16: cnt/LTimer<0>     26: cnt/LTimer<7>
      6: A_FSB<1>          17: cnt/LTimer<10>    27: cnt/LTimer<8>
      7: A_FSB<20>         18: cnt/LTimer<11>    28: cnt/LTimer<9>
      8: A_FSB<21>         19: cnt/LTimer<12>    29: cnt/TimerTC
      9: A_FSB<22>         20: cnt/LTimer<1>     30: cs/nOverlay
     10: A_FSB<23>         21: cnt/LTimer<2>     31: ram/RASEL
     11: A_FSB<2>

    Signal                        1         2         3         4 FB
    Name                0----+----0----+----0----+----0----+----0 Inputs
    cnt/LTimerTC         .............XXXXXXXXXXXXXXXX........... 16
    RA<1>                .X........X...................X......... 3
    cnt/LTimer<9>        .............XXX...XXXXXXXX.X........... 12
    cnt/LTimer<8>        .............XXX...XXXXXXX..X........... 11
    RA<7>                ..X........X..................X......... 3
    RA<0>                X....X........................X......... 3
    cnt/LTimer<7>        .............XXX...XXXXXX...X........... 10
    RA<8>                ...X....XX..X................XX......... 6
    RA<10>               .......X................................ 1
    cnt/LTimer<6>        .............XXX...XXXXX....X........... 9
    RA<9>                ....X.X.......................X......... 3
    C25MEN               ........................................ 0
    cnt/LTimer<5>        .............XXX...XXXX.....X........... 8
    C20MEN               ........................................ 0
    cnt/LTimer<4>        .............XXX...XXX......X........... 7
    cnt/LTimer<12>       .............XXXXX.XXXXXXXXXX........... 15
    cnt/LTimer<11>       .............XXXX..XXXXXXXXXX........... 14
    cnt/LTimer<10>       .............XXX...XXXXXXXXXX........... 13
                        0----+----1----+----2----+----3----+----4
                                  0         0         0         0
    *********************************** FB8  ***********************************
    Number of function block inputs used/remaining:               35/19
    Number of signals used by logic mapping into function block:  35
    Signal              Total   Imp   Exp Unused  Loc     Pin   Pin     Pin
    Name                Pt      Pt    Pt  Pt               #    Type    Use
    ram/RASEL            14       9<-   0   0     FB8_1         (b)     (b)
    RA<11>                1       1<- /\5   0     FB8_2   63    I/O     O
    cnt/Timer<2>          5       1<- /\1   0     FB8_3         (b)     (b)
    cnt/Timer<0>          2       0   /\1   2     FB8_4         (b)     (b)
    nRAS                  0       0     0   5     FB8_5   64    I/O     O
    nRAMLWE               1       0     0   4     FB8_6   65    I/O     O
    cnt/INITS_FSM_FFd2    2       0     0   3     FB8_7         (b)     (b)
    nRAMUWE               1       0     0   4     FB8_8   66    I/O     O
    fsb/Ready0r           2       0   \/2   1     FB8_9   67    I/O     (b)
    cnt/Timer<1>          4       2<- \/3   0     FB8_10        (b)     (b)
    ram/RAMReady          9       4<-   0   0     FB8_11  68    I/O     (b)
    nBERR_FSB             4       0   /\1   0     FB8_12  70    I/O     O
    (unused)              0       0   \/5   0     FB8_13        (b)     (b)
    ram/RAMEN             9       5<- \/1   0     FB8_14  71    I/O     (b)
    nBR_IOB               2       1<- \/4   0     FB8_15  72    I/O     O
    ram/RS_FSM_FFd3      13       8<-   0   0     FB8_16        (b)     (b)
    cnt/INITS_FSM_FFd1    1       0   /\4   0     FB8_17  73    I/O     (b)
    cnt/LTimer<0>         1       0   \/4   0     FB8_18        (b)     (b)

    Signals Used by Logic in Function Block
      1: A_FSB<19>           13: cnt/TimerTC       25: nLDS_FSB
      2: A_FSB<22>           14: cnt/nIPL2r        26: nUDS_FSB
      3: A_FSB<23>           15: cs/nOverlay       27: nWE_FSB
      4: IOBERR              16: fsb/ASrf          28: ram/BACTr
      5: cnt/Er<0>           17: fsb/Ready0r       29: ram/RAMEN
      6: cnt/Er<1>           18: iobs/IOACTr       30: ram/RAMReady
      7: cnt/INITS_FSM_FFd1  19: iobs/Once         31: ram/RS_FSM_FFd1
      8: cnt/INITS_FSM_FFd2  20: iobs/PS_FSM_FFd2  32: ram/RS_FSM_FFd2
      9: cnt/LTimerTC        21: nADoutLE1         33: ram/RS_FSM_FFd3
     10: cnt/Timer<0>        22: nAS_FSB           34: ram/RefReq
     11: cnt/Timer<1>        23: nBERR_FSB         35: ram/RefUrg
     12: cnt/Timer<2>        24: nBR_IOB

    Signal                        1         2         3         4 FB
    Name                0----+----0----+----0----+----0----+----0 Inputs
    ram/RASEL            .XX...........XX.....X.....XX.XXXXX..... 12
    RA<11>               X....................................... 1
    cnt/Timer<2>         ....XX...XXXX........................... 6
    cnt/Timer<0>         ....XX...X..X........................... 4
    nRAS                 ........................................ 0
    nRAMLWE              .....................X..X.X.X........... 4
    cnt/INITS_FSM_FFd2   ....XXXXX...X........................... 6
    nRAMUWE              .....................X...XX.X........... 4
    fsb/Ready0r          .XX...........XXX....X.......X.......... 7
    cnt/Timer<1>         ....XX...XX.X........................... 5
    ram/RAMReady         .XX...........XX.....X.....XX.XXXXX..... 12
    nBERR_FSB            ...X...........X.XXXXXX................. 8
    ram/RAMEN            .XX...........XX.....X.....XX.XXXXX..... 12
    nBR_IOB              ......XX.....X.........X................ 4
    ram/RS_FSM_FFd3      .XX...........XX.....X.....XX.XXXXX..... 12
    cnt/INITS_FSM_FFd1   ....XXXXX...XX.......................... 7
    cnt/LTimer<0>        ....XX......X........................... 3
                        0----+----1----+----2----+----3----+----4
                                  0         0         0         0
    *******************************  Equations  ********************************

    ********** Mapped Logic **********

    FDCPE_ALE0M: FDCPE port map (ALE0M,ALE0M_D,C16M,'0','0');
    ALE0M_D <= ((iobm/IOS_FSM_FFd1 AND NOT iobm/IOS_FSM_FFd2)
    	OR (NOT iobm/IOS_FSM_FFd3 AND NOT iobm/IOS_FSM_FFd2 AND
    	NOT iobm/IOREQr));

    FDCPE_ALE0S: FDCPE port map (ALE0S,ALE0S_D,FCLK,'0','0');
    ALE0S_D <= (iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1);

    C20MEN <= '1';

    C25MEN <= '1';

    FDCPE_IOACT: FDCPE port map (IOACT,IOACT_D,C16M,'0','0');
    IOACT_D <= ((C8M AND iobm/IOS_FSM_FFd3 AND iobm/IOS_FSM_FFd1 AND
    	iobm/RESrf AND iobm/RESrr)
    	OR (iobm/IOS_FSM_FFd1 AND NOT iobm/IOS_FSM_FFd2)
    	OR (NOT iobm/IOS_FSM_FFd3 AND NOT iobm/IOS_FSM_FFd2 AND
    	NOT iobm/IOREQr)
    	OR (C8M AND iobm/IOS_FSM_FFd3 AND iobm/IOS_FSM_FFd1 AND
    	iobm/ETACK)
    	OR (C8M AND iobm/IOS_FSM_FFd3 AND iobm/IOS_FSM_FFd1 AND
    	iobm/DTACKrf AND iobm/DTACKrr)
    	OR (C8M AND iobm/IOS_FSM_FFd3 AND iobm/IOS_FSM_FFd1 AND
    	iobm/BERRrf AND iobm/BERRrr));

    FTCPE_IOBERR: FTCPE port map (IOBERR,IOBERR_T,C16M,'0','0');
    IOBERR_T <= ((C8M AND nBERR_IOB AND iobm/IOS_FSM_FFd3 AND
    	iobm/IOS_FSM_FFd1 AND iobm/IOS_FSM_FFd2 AND IOBERR AND iobm/RESrf AND
    	iobm/RESrr)
    	OR (C8M AND NOT nBERR_IOB AND iobm/IOS_FSM_FFd3 AND
    	iobm/IOS_FSM_FFd1 AND iobm/IOS_FSM_FFd2 AND NOT IOBERR AND iobm/DTACKrf AND
    	iobm/DTACKrr)
    	OR (C8M AND NOT nBERR_IOB AND iobm/IOS_FSM_FFd3 AND
    	iobm/IOS_FSM_FFd1 AND iobm/IOS_FSM_FFd2 AND NOT IOBERR AND iobm/BERRrf AND
    	iobm/BERRrr)
    	OR (C8M AND NOT nBERR_IOB AND iobm/IOS_FSM_FFd3 AND
    	iobm/IOS_FSM_FFd1 AND iobm/IOS_FSM_FFd2 AND NOT IOBERR AND iobm/RESrf AND
    	iobm/RESrr)
    	OR (iobm/IOS_FSM_FFd3 AND NOT iobm/IOS_FSM_FFd1 AND
    	NOT iobm/IOS_FSM_FFd2 AND IOBERR)
    	OR (C8M AND nBERR_IOB AND iobm/IOS_FSM_FFd3 AND
    	iobm/IOS_FSM_FFd1 AND iobm/IOS_FSM_FFd2 AND IOBERR AND iobm/ETACK)
    	OR (C8M AND NOT nBERR_IOB AND iobm/IOS_FSM_FFd3 AND
    	iobm/IOS_FSM_FFd1 AND iobm/IOS_FSM_FFd2 AND NOT IOBERR AND iobm/ETACK)
    	OR (C8M AND nBERR_IOB AND iobm/IOS_FSM_FFd3 AND
    	iobm/IOS_FSM_FFd1 AND iobm/IOS_FSM_FFd2 AND IOBERR AND iobm/DTACKrf AND
    	iobm/DTACKrr)
    	OR (C8M AND nBERR_IOB AND iobm/IOS_FSM_FFd3 AND
    	iobm/IOS_FSM_FFd1 AND iobm/IOS_FSM_FFd2 AND IOBERR AND iobm/BERRrf AND
    	iobm/BERRrr));

    FDCPE_IOL0: FDCPE port map (IOL0,IOL0_D,FCLK,'0','0',IOL0_CE);
    IOL0_D <= ((NOT nLDS_FSB AND nADoutLE1)
    	OR (iobs/IOL1 AND NOT nADoutLE1));
    IOL0_CE <= (iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1);

    FDCPE_IOREQ: FDCPE port map (IOREQ,IOREQ_D,FCLK,'0','0');
    IOREQ_D <= ((A_FSB(22) AND A_FSB(21) AND NOT iobs/Once AND NOT nAS_FSB AND
    	NOT iobs/PS_FSM_FFd1)
    	OR (A_FSB(22) AND A_FSB(21) AND NOT iobs/Once AND
    	NOT iobs/PS_FSM_FFd1 AND fsb/ASrf)
    	OR (A_FSB(22) AND A_FSB(20) AND NOT iobs/Once AND NOT nAS_FSB AND
    	NOT iobs/PS_FSM_FFd1)
    	OR (A_FSB(22) AND A_FSB(20) AND NOT iobs/Once AND
    	NOT iobs/PS_FSM_FFd1 AND fsb/ASrf)
    	OR (A_FSB(14) AND A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND
    	A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND NOT iobs/Once AND cs/nOverlay AND
    	NOT nWE_FSB AND NOT nAS_FSB AND NOT iobs/PS_FSM_FFd1)
    	OR (A_FSB(14) AND A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND
    	A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND NOT iobs/Once AND cs/nOverlay AND
    	NOT nWE_FSB AND NOT iobs/PS_FSM_FFd1 AND fsb/ASrf)
    	OR (A_FSB(13) AND A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND
    	A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND NOT iobs/Once AND cs/nOverlay AND
    	NOT nWE_FSB AND NOT nAS_FSB AND NOT iobs/PS_FSM_FFd1)
    	OR (A_FSB(13) AND A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND
    	A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND NOT iobs/Once AND cs/nOverlay AND
    	NOT nWE_FSB AND NOT iobs/PS_FSM_FFd1 AND fsb/ASrf)
    	OR (iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1)
    	OR (iobs/PS_FSM_FFd2 AND NOT iobs/IOACTr)
    	OR (NOT iobs/PS_FSM_FFd1 AND NOT nADoutLE1)
    	OR (A_FSB(23) AND NOT iobs/Once AND NOT nAS_FSB AND
    	NOT iobs/PS_FSM_FFd1)
    	OR (A_FSB(23) AND NOT iobs/Once AND NOT iobs/PS_FSM_FFd1 AND
    	fsb/ASrf));

    FDCPE_IORW0: FDCPE port map (IORW0,IORW0_D,FCLK,'0','0');
    IORW0_D <= ((EXP11_.EXP)
    	OR (A_FSB(22) AND A_FSB(21) AND NOT iobs/Once AND NOT nWE_FSB AND
    	NOT nAS_FSB AND NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1 AND nADoutLE1)
    	OR (A_FSB(22) AND A_FSB(21) AND NOT iobs/Once AND NOT nWE_FSB AND
    	NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1 AND fsb/ASrf AND nADoutLE1)
    	OR (A_FSB(22) AND A_FSB(20) AND NOT iobs/Once AND NOT nWE_FSB AND
    	NOT nAS_FSB AND NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1 AND nADoutLE1)
    	OR (A_FSB(22) AND A_FSB(20) AND NOT iobs/Once AND NOT nWE_FSB AND
    	NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1 AND fsb/ASrf AND nADoutLE1)
    	OR (A_FSB(14) AND A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND
    	A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND NOT iobs/Once AND cs/nOverlay AND
    	NOT nWE_FSB AND NOT nAS_FSB AND NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1 AND
    	nADoutLE1)
    	OR (NOT iobs/IORW1 AND NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1 AND
    	NOT nADoutLE1)
    	OR (NOT A_FSB(23) AND NOT A_FSB(21) AND NOT A_FSB(20) AND NOT IORW0 AND
    	nADoutLE1)
    	OR (A_FSB(23) AND NOT iobs/Once AND NOT nWE_FSB AND NOT nAS_FSB AND
    	NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1 AND nADoutLE1)
    	OR (A_FSB(23) AND NOT iobs/Once AND NOT nWE_FSB AND
    	NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1 AND fsb/ASrf AND nADoutLE1)
    	OR (NOT IORW0 AND iobs/PS_FSM_FFd2)
    	OR (NOT IORW0 AND iobs/PS_FSM_FFd1)
    	OR (iobs/Once AND NOT IORW0 AND nADoutLE1)
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT IORW0 AND nADoutLE1)
    	OR (NOT IORW0 AND nAS_FSB AND NOT fsb/ASrf AND nADoutLE1));

    FDCPE_IOU0: FDCPE port map (IOU0,IOU0_D,FCLK,'0','0',IOU0_CE);
    IOU0_D <= ((NOT nUDS_FSB AND nADoutLE1)
    	OR (iobs/IOU1 AND NOT nADoutLE1));
    IOU0_CE <= (iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1);

    RA(0) <= ((A_FSB(10) AND NOT ram/RASEL)
    	OR (ram/RASEL AND A_FSB(1)));

    RA(1) <= ((A_FSB(11) AND NOT ram/RASEL)
    	OR (ram/RASEL AND A_FSB(2)));

    RA(2) <= ((A_FSB(12) AND NOT ram/RASEL)
    	OR (ram/RASEL AND A_FSB(3)));

    RA(3) <= ((A_FSB(13) AND NOT ram/RASEL)
    	OR (ram/RASEL AND A_FSB(4)));

    RA(4) <= ((A_FSB(14) AND NOT ram/RASEL)
    	OR (ram/RASEL AND A_FSB(5)));

    RA(5) <= ((A_FSB(15) AND NOT ram/RASEL)
    	OR (ram/RASEL AND A_FSB(6)));

    RA(6) <= ((ram/RASEL AND A_FSB(7))
    	OR (A_FSB(16) AND NOT ram/RASEL));

    RA(7) <= ((A_FSB(8) AND ram/RASEL)
    	OR (A_FSB(17) AND NOT ram/RASEL));

    RA(8) <= ((A_FSB(23) AND A_FSB(18))
    	OR (A_FSB(22) AND A_FSB(18))
    	OR (A_FSB(18) AND NOT cs/nOverlay)
    	OR (A_FSB(18) AND NOT ram/RASEL)
    	OR (A_FSB(9) AND NOT A_FSB(23) AND NOT A_FSB(22) AND cs/nOverlay AND
    	ram/RASEL));

    RA(9) <= ((A_FSB(20) AND ram/RASEL)
    	OR (A_FSB(19) AND NOT ram/RASEL));

    RA(10) <= A_FSB(21);

    RA(11) <= A_FSB(19);

    FDCPE_RefReq: FDCPE port map (RefReq,RefReq_D,FCLK,'0','0',RefReq_CE);
    RefReq_D <= (NOT RefUrg AND NOT cnt/Timer(1) AND NOT cnt/Timer(2));
    RefReq_CE <= (NOT cnt/Er(0) AND cnt/Er(1));

    FTCPE_RefUrg: FTCPE port map (RefUrg,RefUrg_T,FCLK,'0','0',RefUrg_CE);
    RefUrg_T <= ((RefUrg AND cnt/TimerTC AND NOT cnt/Er(0) AND cnt/Er(1))
    	OR (cnt/Timer(0) AND cnt/Timer(1) AND cnt/Timer(2) AND
    	NOT cnt/TimerTC)
    	OR (cnt/Timer(0) AND cnt/Timer(1) AND cnt/Timer(2) AND
    	cnt/Er(0))
    	OR (cnt/Timer(0) AND cnt/Timer(1) AND cnt/Timer(2) AND
    	NOT cnt/Er(1)));
    RefUrg_CE <= (NOT cnt/Er(0) AND cnt/Er(1));

    FDCPE_cnt/Er0: FDCPE port map (cnt/Er(0),E,FCLK,'0','0');

    FDCPE_cnt/Er1: FDCPE port map (cnt/Er(1),cnt/Er(0),FCLK,'0','0');

    FTCPE_cnt/INITS_FSM_FFd1: FTCPE port map (cnt/INITS_FSM_FFd1,cnt/INITS_FSM_FFd1_T,FCLK,'0','0');
    cnt/INITS_FSM_FFd1_T <= (cnt/TimerTC AND cnt/LTimerTC AND NOT cnt/INITS_FSM_FFd1 AND
    	cnt/INITS_FSM_FFd2 AND NOT cnt/Er(0) AND cnt/nIPL2r AND cnt/Er(1));

    FTCPE_cnt/INITS_FSM_FFd2: FTCPE port map (cnt/INITS_FSM_FFd2,cnt/INITS_FSM_FFd2_T,FCLK,'0','0');
    cnt/INITS_FSM_FFd2_T <= ((cnt/TimerTC AND cnt/LTimerTC AND cnt/INITS_FSM_FFd1 AND
    	cnt/INITS_FSM_FFd2 AND NOT cnt/Er(0) AND cnt/Er(1))
    	OR (cnt/TimerTC AND cnt/LTimerTC AND NOT cnt/INITS_FSM_FFd1 AND
    	NOT cnt/INITS_FSM_FFd2 AND NOT cnt/Er(0) AND cnt/Er(1)));

    FTCPE_cnt/LTimer0: FTCPE port map (cnt/LTimer(0),'1',FCLK,'0','0',cnt/LTimer_CE(0));
    cnt/LTimer_CE(0) <= (cnt/TimerTC AND NOT cnt/Er(0) AND cnt/Er(1));

    FTCPE_cnt/LTimer1: FTCPE port map (cnt/LTimer(1),cnt/LTimer(0),FCLK,'0','0',cnt/LTimer_CE(1));
    cnt/LTimer_CE(1) <= (cnt/TimerTC AND NOT cnt/Er(0) AND cnt/Er(1));

    FTCPE_cnt/LTimer2: FTCPE port map (cnt/LTimer(2),cnt/LTimer_T(2),FCLK,'0','0',cnt/LTimer_CE(2));
    cnt/LTimer_T(2) <= (cnt/LTimer(0) AND cnt/LTimer(1));
    cnt/LTimer_CE(2) <= (cnt/TimerTC AND NOT cnt/Er(0) AND cnt/Er(1));

    FTCPE_cnt/LTimer3: FTCPE port map (cnt/LTimer(3),cnt/LTimer_T(3),FCLK,'0','0',cnt/LTimer_CE(3));
    cnt/LTimer_T(3) <= (cnt/LTimer(0) AND cnt/LTimer(1) AND cnt/LTimer(2));
    cnt/LTimer_CE(3) <= (cnt/TimerTC AND NOT cnt/Er(0) AND cnt/Er(1));

    FTCPE_cnt/LTimer4: FTCPE port map (cnt/LTimer(4),cnt/LTimer_T(4),FCLK,'0','0',cnt/LTimer_CE(4));
    cnt/LTimer_T(4) <= (cnt/LTimer(0) AND cnt/LTimer(1) AND cnt/LTimer(2) AND
    	cnt/LTimer(3));
    cnt/LTimer_CE(4) <= (cnt/TimerTC AND NOT cnt/Er(0) AND cnt/Er(1));

    FTCPE_cnt/LTimer5: FTCPE port map (cnt/LTimer(5),cnt/LTimer_T(5),FCLK,'0','0',cnt/LTimer_CE(5));
    cnt/LTimer_T(5) <= (cnt/LTimer(0) AND cnt/LTimer(1) AND cnt/LTimer(2) AND
    	cnt/LTimer(3) AND cnt/LTimer(4));
    cnt/LTimer_CE(5) <= (cnt/TimerTC AND NOT cnt/Er(0) AND cnt/Er(1));

    FTCPE_cnt/LTimer6: FTCPE port map (cnt/LTimer(6),cnt/LTimer_T(6),FCLK,'0','0',cnt/LTimer_CE(6));
    cnt/LTimer_T(6) <= (cnt/LTimer(0) AND cnt/LTimer(1) AND cnt/LTimer(2) AND
    	cnt/LTimer(3) AND cnt/LTimer(4) AND cnt/LTimer(5));
    cnt/LTimer_CE(6) <= (cnt/TimerTC AND NOT cnt/Er(0) AND cnt/Er(1));

    FTCPE_cnt/LTimer7: FTCPE port map (cnt/LTimer(7),cnt/LTimer_T(7),FCLK,'0','0',cnt/LTimer_CE(7));
    cnt/LTimer_T(7) <= (cnt/LTimer(0) AND cnt/LTimer(1) AND cnt/LTimer(2) AND
    	cnt/LTimer(3) AND cnt/LTimer(4) AND cnt/LTimer(5) AND cnt/LTimer(6));
    cnt/LTimer_CE(7) <= (cnt/TimerTC AND NOT cnt/Er(0) AND cnt/Er(1));

    FTCPE_cnt/LTimer8: FTCPE port map (cnt/LTimer(8),cnt/LTimer_T(8),FCLK,'0','0',cnt/LTimer_CE(8));
    cnt/LTimer_T(8) <= (cnt/LTimer(0) AND cnt/LTimer(1) AND cnt/LTimer(2) AND
    	cnt/LTimer(3) AND cnt/LTimer(4) AND cnt/LTimer(5) AND cnt/LTimer(6) AND
    	cnt/LTimer(7));
    cnt/LTimer_CE(8) <= (cnt/TimerTC AND NOT cnt/Er(0) AND cnt/Er(1));

    FTCPE_cnt/LTimer9: FTCPE port map (cnt/LTimer(9),cnt/LTimer_T(9),FCLK,'0','0',cnt/LTimer_CE(9));
    cnt/LTimer_T(9) <= (cnt/LTimer(0) AND cnt/LTimer(1) AND cnt/LTimer(2) AND
    	cnt/LTimer(3) AND cnt/LTimer(4) AND cnt/LTimer(5) AND cnt/LTimer(6) AND
    	cnt/LTimer(7) AND cnt/LTimer(8));
    cnt/LTimer_CE(9) <= (cnt/TimerTC AND NOT cnt/Er(0) AND cnt/Er(1));

    FTCPE_cnt/LTimer10: FTCPE port map (cnt/LTimer(10),cnt/LTimer_T(10),FCLK,'0','0',cnt/LTimer_CE(10));
    cnt/LTimer_T(10) <= (cnt/LTimer(0) AND cnt/LTimer(1) AND cnt/LTimer(2) AND
    	cnt/LTimer(3) AND cnt/LTimer(4) AND cnt/LTimer(5) AND cnt/LTimer(6) AND
    	cnt/LTimer(7) AND cnt/LTimer(8) AND cnt/LTimer(9));
    cnt/LTimer_CE(10) <= (cnt/TimerTC AND NOT cnt/Er(0) AND cnt/Er(1));

    FTCPE_cnt/LTimer11: FTCPE port map (cnt/LTimer(11),cnt/LTimer_T(11),FCLK,'0','0',cnt/LTimer_CE(11));
    cnt/LTimer_T(11) <= (cnt/LTimer(0) AND cnt/LTimer(10) AND cnt/LTimer(1) AND
    	cnt/LTimer(2) AND cnt/LTimer(3) AND cnt/LTimer(4) AND cnt/LTimer(5) AND
    	cnt/LTimer(6) AND cnt/LTimer(7) AND cnt/LTimer(8) AND cnt/LTimer(9));
    cnt/LTimer_CE(11) <= (cnt/TimerTC AND NOT cnt/Er(0) AND cnt/Er(1));

    FTCPE_cnt/LTimer12: FTCPE port map (cnt/LTimer(12),cnt/LTimer_T(12),FCLK,'0','0',cnt/LTimer_CE(12));
    cnt/LTimer_T(12) <= (cnt/LTimer(0) AND cnt/LTimer(10) AND cnt/LTimer(11) AND
    	cnt/LTimer(1) AND cnt/LTimer(2) AND cnt/LTimer(3) AND cnt/LTimer(4) AND
    	cnt/LTimer(5) AND cnt/LTimer(6) AND cnt/LTimer(7) AND cnt/LTimer(8) AND
    	cnt/LTimer(9));
    cnt/LTimer_CE(12) <= (cnt/TimerTC AND NOT cnt/Er(0) AND cnt/Er(1));

    FDCPE_cnt/LTimerTC: FDCPE port map (cnt/LTimerTC,cnt/LTimerTC_D,FCLK,'0','0',cnt/LTimerTC_CE);
    cnt/LTimerTC_D <= (NOT cnt/LTimer(0) AND cnt/LTimer(10) AND cnt/LTimer(11) AND
    	cnt/LTimer(1) AND cnt/LTimer(2) AND cnt/LTimer(3) AND cnt/LTimer(4) AND
    	cnt/LTimer(5) AND cnt/LTimer(6) AND cnt/LTimer(7) AND cnt/LTimer(8) AND
    	cnt/LTimer(9) AND cnt/LTimer(12));
    cnt/LTimerTC_CE <= (cnt/TimerTC AND NOT cnt/Er(0) AND cnt/Er(1));

    FTCPE_cnt/Timer0: FTCPE port map (cnt/Timer(0),cnt/Timer_T(0),FCLK,'0','0',cnt/Timer_CE(0));
    cnt/Timer_T(0) <= (NOT cnt/Timer(0) AND cnt/TimerTC AND NOT cnt/Er(0) AND
    	cnt/Er(1));
    cnt/Timer_CE(0) <= (NOT cnt/Er(0) AND cnt/Er(1));

    FDCPE_cnt/Timer1: FDCPE port map (cnt/Timer(1),cnt/Timer_D(1),FCLK,'0','0',cnt/Timer_CE(1));
    cnt/Timer_D(1) <= ((NOT cnt/Timer(0) AND NOT cnt/Timer(1))
    	OR (cnt/TimerTC AND NOT cnt/Er(0) AND cnt/Er(1))
    	OR (cnt/Timer(0) AND cnt/Timer(1)));
    cnt/Timer_CE(1) <= (NOT cnt/Er(0) AND cnt/Er(1));

    FDCPE_cnt/Timer2: FDCPE port map (cnt/Timer(2),cnt/Timer_D(2),FCLK,'0','0',cnt/Timer_CE(2));
    cnt/Timer_D(2) <= ((cnt/Timer(0) AND cnt/Timer(1) AND cnt/Timer(2))
    	OR (NOT cnt/Timer(0) AND NOT cnt/Timer(2))
    	OR (NOT cnt/Timer(1) AND NOT cnt/Timer(2))
    	OR (cnt/TimerTC AND NOT cnt/Er(0) AND cnt/Er(1)));
    cnt/Timer_CE(2) <= (NOT cnt/Er(0) AND cnt/Er(1));

    FDCPE_cnt/TimerTC: FDCPE port map (cnt/TimerTC,cnt/TimerTC_D,FCLK,'0','0',cnt/TimerTC_CE);
    cnt/TimerTC_D <= (RefUrg AND cnt/Timer(0) AND NOT cnt/Timer(1) AND
    	NOT cnt/Timer(2));
    cnt/TimerTC_CE <= (NOT cnt/Er(0) AND cnt/Er(1));

    FDCPE_cnt/nIPL2r: FDCPE port map (cnt/nIPL2r,nIPL2,FCLK,'0','0');

    FTCPE_cs/nOverlay: FTCPE port map (cs/nOverlay,cs/nOverlay_T,FCLK,NOT nRES.PIN,'0');
    cs/nOverlay_T <= ((NOT A_FSB(23) AND A_FSB(22) AND NOT A_FSB(21) AND NOT A_FSB(20) AND
    	NOT cs/nOverlay AND NOT nAS_FSB)
    	OR (NOT A_FSB(23) AND A_FSB(22) AND NOT A_FSB(21) AND NOT A_FSB(20) AND
    	NOT cs/nOverlay AND fsb/ASrf));

    FDCPE_fsb/ASrf: FDCPE port map (fsb/ASrf,NOT nAS_FSB,NOT FCLK,'0','0');

    FDCPE_fsb/Ready0r: FDCPE port map (fsb/Ready0r,fsb/Ready0r_D,FCLK,'0','0');
    fsb/Ready0r_D <= ((nAS_FSB AND NOT fsb/ASrf)
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND cs/nOverlay AND
    	NOT fsb/Ready0r AND NOT ram/RAMReady));

    FDCPE_fsb/Ready1r: FDCPE port map (fsb/Ready1r,fsb/Ready1r_D,FCLK,'0','0');
    fsb/Ready1r_D <= ((A_FSB(13) AND A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND
    	A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND cs/nOverlay AND
    	NOT fsb/Ready1r AND NOT nWE_FSB AND NOT iobs/IOReady AND NOT nADoutLE1)
    	OR (nAS_FSB AND NOT fsb/ASrf)
    	OR (A_FSB(23) AND NOT fsb/Ready1r AND NOT iobs/IOReady)
    	OR (A_FSB(22) AND A_FSB(21) AND NOT fsb/Ready1r AND
    	NOT iobs/IOReady)
    	OR (A_FSB(22) AND A_FSB(20) AND NOT fsb/Ready1r AND
    	NOT iobs/IOReady)
    	OR (A_FSB(14) AND A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND
    	A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND cs/nOverlay AND
    	NOT fsb/Ready1r AND NOT nWE_FSB AND NOT iobs/IOReady AND NOT nADoutLE1));

    FDCPE_fsb/VPA: FDCPE port map (fsb/VPA,fsb/VPA_D,FCLK,'0','0');
    fsb/VPA_D <= ((EXP12_.EXP)
    	OR (A_FSB(22) AND A_FSB(20) AND NOT fsb/Ready1r AND fsb/VPA AND
    	NOT iobs/IOReady AND fsb/ASrf)
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND cs/nOverlay AND
    	NOT fsb/Ready0r AND fsb/VPA AND NOT nAS_FSB AND NOT ram/RAMReady)
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND cs/nOverlay AND
    	NOT fsb/Ready0r AND fsb/VPA AND fsb/ASrf AND NOT ram/RAMReady)
    	OR (A_FSB(14) AND A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND
    	A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND cs/nOverlay AND
    	NOT fsb/Ready1r AND fsb/VPA AND NOT nWE_FSB AND NOT iobs/IOReady AND NOT nAS_FSB AND
    	NOT nADoutLE1)
    	OR (A_FSB(13) AND A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND
    	A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND cs/nOverlay AND
    	NOT fsb/Ready1r AND fsb/VPA AND NOT nWE_FSB AND NOT iobs/IOReady AND NOT nAS_FSB AND
    	NOT nADoutLE1)
    	OR (A_FSB(14) AND A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND
    	A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND cs/nOverlay AND
    	NOT fsb/Ready1r AND fsb/VPA AND NOT nWE_FSB AND NOT iobs/IOReady AND fsb/ASrf AND
    	NOT nADoutLE1)
    	OR (A_FSB(13) AND A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND
    	A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND cs/nOverlay AND
    	NOT fsb/Ready1r AND fsb/VPA AND NOT nWE_FSB AND NOT iobs/IOReady AND fsb/ASrf AND
    	NOT nADoutLE1)
    	OR (A_FSB(9) AND A_FSB(8) AND A_FSB(15) AND A_FSB(14) AND
    	A_FSB(13) AND A_FSB(12) AND A_FSB(11) AND A_FSB(10) AND A_FSB(23) AND
    	A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND A_FSB(18) AND
    	A_FSB(17) AND A_FSB(16) AND fsb/Ready1r AND NOT nAS_FSB)
    	OR (A_FSB(9) AND A_FSB(8) AND A_FSB(15) AND A_FSB(14) AND
    	A_FSB(13) AND A_FSB(12) AND A_FSB(11) AND A_FSB(10) AND A_FSB(23) AND
    	A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND A_FSB(18) AND
    	A_FSB(17) AND A_FSB(16) AND iobs/IOReady AND NOT nAS_FSB)
    	OR (A_FSB(9) AND A_FSB(8) AND A_FSB(15) AND A_FSB(14) AND
    	A_FSB(13) AND A_FSB(12) AND A_FSB(11) AND A_FSB(10) AND A_FSB(23) AND
    	A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND A_FSB(18) AND
    	A_FSB(17) AND A_FSB(16) AND iobs/IOReady AND fsb/ASrf)
    	OR (A_FSB(23) AND NOT fsb/Ready1r AND fsb/VPA AND
    	NOT iobs/IOReady AND NOT nAS_FSB)
    	OR (A_FSB(23) AND NOT fsb/Ready1r AND fsb/VPA AND
    	NOT iobs/IOReady AND fsb/ASrf)
    	OR (A_FSB(22) AND A_FSB(21) AND NOT fsb/Ready1r AND fsb/VPA AND
    	NOT iobs/IOReady AND NOT nAS_FSB)
    	OR (A_FSB(22) AND A_FSB(21) AND NOT fsb/Ready1r AND fsb/VPA AND
    	NOT iobs/IOReady AND fsb/ASrf)
    	OR (A_FSB(22) AND A_FSB(20) AND NOT fsb/Ready1r AND fsb/VPA AND
    	NOT iobs/IOReady AND NOT nAS_FSB));

    FDCPE_iobm/BERRrf: FDCPE port map (iobm/BERRrf,NOT nBERR_IOB,NOT C16M,'0','0');

    FDCPE_iobm/BERRrr: FDCPE port map (iobm/BERRrr,NOT nBERR_IOB,C16M,'0','0');

    FDCPE_iobm/DTACKrf: FDCPE port map (iobm/DTACKrf,NOT nDTACK_IOB,NOT C16M,'0','0');

    FDCPE_iobm/DTACKrr: FDCPE port map (iobm/DTACKrr,NOT nDTACK_IOB,C16M,'0','0');

    FDCPE_iobm/DoutOE: FDCPE port map (iobm/DoutOE,iobm/DoutOE_D,C16M,'0','0');
    iobm/DoutOE_D <= ((NOT IORW0 AND iobm/IOS_FSM_FFd3)
    	OR (NOT IORW0 AND iobm/IOS_FSM_FFd2)
    	OR (NOT iobm/IOS_FSM_FFd3 AND NOT iobm/IOS_FSM_FFd1 AND
    	NOT iobm/IOS_FSM_FFd2 AND NOT iobm/IOREQr AND NOT nAoutOE));

    FTCPE_iobm/ES0: FTCPE port map (iobm/ES(0),iobm/ES_T(0),C16M,'0','0');
    iobm/ES_T(0) <= ((iobm/ES(0) AND NOT iobm/Er AND iobm/Er2)
    	OR (NOT iobm/ES(0) AND NOT iobm/ES(1) AND NOT iobm/ES(2) AND
    	NOT iobm/ES(3) AND NOT iobm/ES(4) AND iobm/Er)
    	OR (NOT iobm/ES(0) AND NOT iobm/ES(1) AND NOT iobm/ES(2) AND
    	NOT iobm/ES(3) AND NOT iobm/ES(4) AND NOT iobm/Er2));

    FDCPE_iobm/ES1: FDCPE port map (iobm/ES(1),iobm/ES_D(1),C16M,'0','0');
    iobm/ES_D(1) <= ((iobm/ES(0) AND iobm/ES(1))
    	OR (NOT iobm/ES(0) AND NOT iobm/ES(1))
    	OR (NOT iobm/Er AND iobm/Er2));

    FDCPE_iobm/ES2: FDCPE port map (iobm/ES(2),iobm/ES_D(2),C16M,'0','0');
    iobm/ES_D(2) <= ((NOT iobm/ES(0) AND NOT iobm/ES(2))
    	OR (NOT iobm/ES(1) AND NOT iobm/ES(2))
    	OR (NOT iobm/Er AND iobm/Er2)
    	OR (iobm/ES(0) AND iobm/ES(1) AND iobm/ES(2))
    	OR (NOT iobm/ES(2) AND NOT iobm/ES(3) AND iobm/ES(4)));

    FTCPE_iobm/ES3: FTCPE port map (iobm/ES(3),iobm/ES_T(3),C16M,'0','0');
    iobm/ES_T(3) <= ((iobm/ES(3) AND NOT iobm/Er AND iobm/Er2)
    	OR (iobm/ES(0) AND iobm/ES(1) AND iobm/ES(2) AND iobm/Er)
    	OR (iobm/ES(0) AND iobm/ES(1) AND iobm/ES(2) AND NOT iobm/Er2));

    FTCPE_iobm/ES4: FTCPE port map (iobm/ES(4),iobm/ES_T(4),C16M,'0','0');
    iobm/ES_T(4) <= ((iobm/ES(4) AND NOT iobm/Er AND iobm/Er2)
    	OR (iobm/ES(0) AND iobm/ES(1) AND iobm/ES(2) AND
    	iobm/ES(3) AND iobm/Er)
    	OR (iobm/ES(0) AND iobm/ES(1) AND iobm/ES(2) AND
    	iobm/ES(3) AND NOT iobm/Er2)
    	OR (iobm/ES(0) AND iobm/ES(1) AND NOT iobm/ES(2) AND
    	NOT iobm/ES(3) AND iobm/ES(4)));

    FDCPE_iobm/ETACK: FDCPE port map (iobm/ETACK,iobm/ETACK_D,C16M,'0','0');
    iobm/ETACK_D <= (NOT nVMA_IOB AND NOT iobm/ES(0) AND NOT iobm/ES(1) AND NOT iobm/ES(2) AND
    	NOT iobm/ES(3) AND iobm/ES(4));

    FDCPE_iobm/Er: FDCPE port map (iobm/Er,E,NOT C8M,'0','0');

    FDCPE_iobm/Er2: FDCPE port map (iobm/Er2,iobm/Er,C16M,'0','0');

    FDCPE_iobm/IOREQr: FDCPE port map (iobm/IOREQr,IOREQ,NOT C16M,'0','0');

    FDCPE_iobm/IOS_FSM_FFd1: FDCPE port map (iobm/IOS_FSM_FFd1,iobm/IOS_FSM_FFd1_D,C16M,'0','0');
    iobm/IOS_FSM_FFd1_D <= ((iobm/IOS_FSM_FFd3 AND iobm/IOS_FSM_FFd1)
    	OR (NOT iobm/IOS_FSM_FFd3 AND iobm/IOS_FSM_FFd2));

    FTCPE_iobm/IOS_FSM_FFd2: FTCPE port map (iobm/IOS_FSM_FFd2,iobm/IOS_FSM_FFd2_T,C16M,'0','0');
    iobm/IOS_FSM_FFd2_T <= ((iobm/IOS_FSM_FFd3 AND NOT iobm/IOS_FSM_FFd1 AND
    	NOT iobm/IOS_FSM_FFd2)
    	OR (C8M AND iobm/IOS_FSM_FFd3 AND iobm/IOS_FSM_FFd1 AND
    	iobm/IOS_FSM_FFd2 AND iobm/ETACK)
    	OR (C8M AND iobm/IOS_FSM_FFd3 AND iobm/IOS_FSM_FFd1 AND
    	iobm/IOS_FSM_FFd2 AND iobm/DTACKrf AND iobm/DTACKrr)
    	OR (C8M AND iobm/IOS_FSM_FFd3 AND iobm/IOS_FSM_FFd1 AND
    	iobm/IOS_FSM_FFd2 AND iobm/BERRrf AND iobm/BERRrr)
    	OR (C8M AND iobm/IOS_FSM_FFd3 AND iobm/IOS_FSM_FFd1 AND
    	iobm/IOS_FSM_FFd2 AND iobm/RESrf AND iobm/RESrr));

    FDCPE_iobm/IOS_FSM_FFd3: FDCPE port map (iobm/IOS_FSM_FFd3,iobm/IOS_FSM_FFd3_D,C16M,'0','0');
    iobm/IOS_FSM_FFd3_D <= ((iobm/IOS_FSM_FFd1 AND iobm/IOS_FSM_FFd2)
    	OR (iobm/IOS_FSM_FFd3 AND NOT iobm/IOS_FSM_FFd1 AND
    	NOT iobm/IOS_FSM_FFd2)
    	OR (NOT C8M AND NOT iobm/IOS_FSM_FFd1 AND NOT iobm/IOS_FSM_FFd2 AND
    	iobm/IOREQr AND NOT nAoutOE));

    FDCPE_iobm/RESrf: FDCPE port map (iobm/RESrf,NOT nRES.PIN,NOT C16M,'0','0');

    FDCPE_iobm/RESrr: FDCPE port map (iobm/RESrr,NOT nRES.PIN,C16M,'0','0');

    FDCPE_iobm/VPArf: FDCPE port map (iobm/VPArf,NOT nVPA_IOB,NOT C16M,'0','0');

    FDCPE_iobm/VPArr: FDCPE port map (iobm/VPArr,NOT nVPA_IOB,C16M,'0','0');

    FDCPE_iobs/Clear1: FDCPE port map (iobs/Clear1,iobs/Clear1_D,FCLK,'0','0');
    iobs/Clear1_D <= (iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1 AND NOT nADoutLE1);

    FDCPE_iobs/IOACTr: FDCPE port map (iobs/IOACTr,IOACT,FCLK,'0','0');

    FDCPE_iobs/IOL1: FDCPE port map (iobs/IOL1,NOT nLDS_FSB,FCLK,'0','0',iobs/Load1);

    FTCPE_iobs/IORW1: FTCPE port map (iobs/IORW1,iobs/IORW1_T,FCLK,'0','0');
    iobs/IORW1_T <= ((iobs/Once)
    	OR (NOT nADoutLE1)
    	OR (nDTACK_FSB_OBUF.EXP)
    	OR (nAS_FSB AND NOT fsb/ASrf)
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT A_FSB(21))
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT A_FSB(19))
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT cs/nOverlay)
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND nWE_FSB)
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT A_FSB(20))
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT A_FSB(18))
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT A_FSB(17))
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT A_FSB(16))
    	OR (NOT A_FSB(23) AND NOT A_FSB(21) AND NOT A_FSB(20))
    	OR (nWE_FSB AND iobs/IORW1)
    	OR (NOT nWE_FSB AND NOT iobs/IORW1)
    	OR (NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1));

    FTCPE_iobs/IOReady: FTCPE port map (iobs/IOReady,iobs/IOReady_T,FCLK,'0','0');
    iobs/IOReady_T <= ((iobs/IOReady AND nAS_FSB AND NOT fsb/ASrf)
    	OR (iobs/Once AND iobs/IOReady AND NOT iobs/PS_FSM_FFd2 AND
    	NOT iobs/IOACTr AND IOBERR AND nADoutLE1)
    	OR (iobs/Once AND NOT iobs/IOReady AND NOT nAS_FSB AND
    	NOT iobs/PS_FSM_FFd2 AND NOT iobs/IOACTr AND NOT IOBERR AND nADoutLE1)
    	OR (iobs/Once AND NOT iobs/IOReady AND NOT iobs/PS_FSM_FFd2 AND
    	NOT iobs/IOACTr AND NOT IOBERR AND fsb/ASrf AND nADoutLE1));

    FDCPE_iobs/IOU1: FDCPE port map (iobs/IOU1,NOT nUDS_FSB,FCLK,'0','0',iobs/Load1);

    FDCPE_iobs/Load1: FDCPE port map (iobs/Load1,iobs/Load1_D,FCLK,'0','0');
    iobs/Load1_D <= ((iobs/Once)
    	OR (NOT nADoutLE1)
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT A_FSB(21))
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT A_FSB(19))
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT A_FSB(16))
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND nWE_FSB)
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT A_FSB(20))
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT A_FSB(18))
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT A_FSB(17))
    	OR (NOT A_FSB(23) AND NOT A_FSB(21) AND NOT A_FSB(20))
    	OR (NOT A_FSB(14) AND NOT A_FSB(13) AND NOT A_FSB(23) AND NOT A_FSB(22))
    	OR (nAS_FSB AND NOT fsb/ASrf)
    	OR (NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1)
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND NOT cs/nOverlay));

    FTCPE_iobs/Once: FTCPE port map (iobs/Once,iobs/Once_T,FCLK,'0','0');
    iobs/Once_T <= ((A_FSB(22) AND A_FSB(21) AND NOT iobs/Once AND
    	NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1 AND fsb/ASrf)
    	OR (A_FSB(22) AND A_FSB(20) AND NOT iobs/Once AND
    	NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1 AND fsb/ASrf)
    	OR (A_FSB(14) AND A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND
    	A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND NOT iobs/Once AND cs/nOverlay AND
    	NOT nWE_FSB AND NOT nAS_FSB AND NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1)
    	OR (A_FSB(14) AND A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND
    	A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND NOT iobs/Once AND cs/nOverlay AND
    	NOT nWE_FSB AND NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1 AND fsb/ASrf)
    	OR (A_FSB(13) AND A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND
    	A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND NOT iobs/Once AND cs/nOverlay AND
    	NOT nWE_FSB AND NOT nAS_FSB AND NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1)
    	OR (A_FSB(13) AND A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND
    	A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND NOT iobs/Once AND cs/nOverlay AND
    	NOT nWE_FSB AND NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1 AND fsb/ASrf)
    	OR (A_FSB(14) AND NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND
    	A_FSB(20) AND A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND
    	NOT iobs/Once AND cs/nOverlay AND NOT nWE_FSB AND NOT nAS_FSB AND nADoutLE1)
    	OR (A_FSB(14) AND NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND
    	A_FSB(20) AND A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND
    	NOT iobs/Once AND cs/nOverlay AND NOT nWE_FSB AND fsb/ASrf AND nADoutLE1)
    	OR (A_FSB(13) AND NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND
    	A_FSB(20) AND A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND
    	NOT iobs/Once AND cs/nOverlay AND NOT nWE_FSB AND NOT nAS_FSB AND nADoutLE1)
    	OR (A_FSB(13) AND NOT A_FSB(23) AND NOT A_FSB(22) AND A_FSB(21) AND
    	A_FSB(20) AND A_FSB(19) AND A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND
    	NOT iobs/Once AND cs/nOverlay AND NOT nWE_FSB AND fsb/ASrf AND nADoutLE1)
    	OR (iobs/Once AND nAS_FSB AND NOT fsb/ASrf)
    	OR (A_FSB(23) AND NOT iobs/Once AND NOT nAS_FSB AND
    	NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1)
    	OR (A_FSB(23) AND NOT iobs/Once AND NOT iobs/PS_FSM_FFd2 AND
    	NOT iobs/PS_FSM_FFd1 AND fsb/ASrf)
    	OR (A_FSB(22) AND A_FSB(21) AND NOT iobs/Once AND NOT nAS_FSB AND
    	NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1)
    	OR (A_FSB(22) AND A_FSB(20) AND NOT iobs/Once AND NOT nAS_FSB AND
    	NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1));

    FDCPE_iobs/PS_FSM_FFd1: FDCPE port map (iobs/PS_FSM_FFd1,iobs/PS_FSM_FFd1_D,FCLK,'0','0');
    iobs/PS_FSM_FFd1_D <= ((iobs/PS_FSM_FFd2)
    	OR (iobs/PS_FSM_FFd1 AND iobs/IOACTr));

    FTCPE_iobs/PS_FSM_FFd2: FTCPE port map (iobs/PS_FSM_FFd2,iobs/PS_FSM_FFd2_T,FCLK,'0','0');
    iobs/PS_FSM_FFd2_T <= ((A_FSB(22) AND A_FSB(21) AND NOT iobs/Once AND
    	NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1 AND fsb/ASrf)
    	OR (A_FSB(22) AND A_FSB(20) AND NOT iobs/Once AND NOT nAS_FSB AND
    	NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1)
    	OR (A_FSB(22) AND A_FSB(20) AND NOT iobs/Once AND
    	NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1 AND fsb/ASrf)
    	OR (A_FSB(14) AND A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND
    	A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND NOT iobs/Once AND cs/nOverlay AND
    	NOT nWE_FSB AND NOT nAS_FSB AND NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1)
    	OR (A_FSB(13) AND A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND
    	A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND NOT iobs/Once AND cs/nOverlay AND
    	NOT nWE_FSB AND NOT nAS_FSB AND NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1)
    	OR (A_FSB(14) AND A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND
    	A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND NOT iobs/Once AND cs/nOverlay AND
    	NOT nWE_FSB AND NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1 AND fsb/ASrf)
    	OR (A_FSB(13) AND A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND
    	A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND NOT iobs/Once AND cs/nOverlay AND
    	NOT nWE_FSB AND NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1 AND fsb/ASrf)
    	OR (iobs/PS_FSM_FFd1 AND iobs/IOACTr)
    	OR (NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1 AND NOT nADoutLE1)
    	OR (A_FSB(23) AND NOT iobs/Once AND NOT nAS_FSB AND
    	NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1)
    	OR (A_FSB(23) AND NOT iobs/Once AND NOT iobs/PS_FSM_FFd2 AND
    	NOT iobs/PS_FSM_FFd1 AND fsb/ASrf)
    	OR (A_FSB(22) AND A_FSB(21) AND NOT iobs/Once AND NOT nAS_FSB AND
    	NOT iobs/PS_FSM_FFd2 AND NOT iobs/PS_FSM_FFd1));

    nADoutLE0 <= (NOT ALE0M AND NOT ALE0S);

    FDCPE_nADoutLE1: FDCPE port map (nADoutLE1,nADoutLE1_D,FCLK,'0','0');
    nADoutLE1_D <= ((iobs/Load1)
    	OR (NOT iobs/Clear1 AND NOT nADoutLE1));

    FDCPE_nAS_IOB: FDCPE port map (nAS_IOB_I,nAS_IOB,NOT C16M,'0','0');
    nAS_IOB <= ((NOT iobm/IOS_FSM_FFd3 AND NOT iobm/IOS_FSM_FFd2)
    	OR (iobm/IOS_FSM_FFd1 AND NOT iobm/IOS_FSM_FFd2));
    nAS_IOB <= nAS_IOB_I when nAS_IOB_OE = '1' else 'Z';
    nAS_IOB_OE <= NOT nAoutOE;

    FDCPE_nAoutOE: FDCPE port map (nAoutOE,nAoutOE_D,FCLK,'0','0');
    nAoutOE_D <= ((NOT nBR_IOB AND cnt/INITS_FSM_FFd1 AND
    	cnt/INITS_FSM_FFd2)
    	OR (cnt/INITS_FSM_FFd1 AND NOT cnt/INITS_FSM_FFd2 AND
    	NOT nAoutOE));

    FTCPE_nBERR_FSB: FTCPE port map (nBERR_FSB,nBERR_FSB_T,FCLK,'0','0');
    nBERR_FSB_T <= ((NOT nBERR_FSB AND nAS_FSB AND NOT fsb/ASrf)
    	OR (iobs/Once AND NOT nBERR_FSB AND NOT iobs/PS_FSM_FFd2 AND
    	NOT iobs/IOACTr AND NOT IOBERR AND nADoutLE1)
    	OR (iobs/Once AND nBERR_FSB AND NOT nAS_FSB AND
    	NOT iobs/PS_FSM_FFd2 AND NOT iobs/IOACTr AND IOBERR AND nADoutLE1)
    	OR (iobs/Once AND nBERR_FSB AND NOT iobs/PS_FSM_FFd2 AND
    	NOT iobs/IOACTr AND IOBERR AND fsb/ASrf AND nADoutLE1));

    FTCPE_nBR_IOB: FTCPE port map (nBR_IOB,nBR_IOB_T,FCLK,'0','0');
    nBR_IOB_T <= ((NOT nBR_IOB AND NOT cnt/INITS_FSM_FFd1 AND
    	cnt/INITS_FSM_FFd2 AND NOT cnt/nIPL2r)
    	OR (nBR_IOB AND NOT cnt/INITS_FSM_FFd1 AND
    	NOT cnt/INITS_FSM_FFd2));

    FDCPE_nCAS: FDCPE port map (nCAS,NOT ram/RASEL,NOT FCLK,'0','0');

    FDCPE_nDTACK_FSB: FDCPE port map (nDTACK_FSB,nDTACK_FSB_D,FCLK,'0','0');
    nDTACK_FSB_D <= ((nAS_FSB AND NOT fsb/ASrf)
    	OR (A_FSB(23) AND NOT fsb/Ready1r AND NOT iobs/IOReady AND
    	nDTACK_FSB)
    	OR (A_FSB(22) AND A_FSB(20) AND NOT fsb/Ready1r AND
    	NOT iobs/IOReady AND nDTACK_FSB)
    	OR (A_FSB(9) AND A_FSB(8) AND A_FSB(15) AND A_FSB(14) AND
    	A_FSB(13) AND A_FSB(12) AND A_FSB(11) AND A_FSB(10) AND A_FSB(23) AND
    	A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND A_FSB(18) AND
    	A_FSB(17) AND A_FSB(16) AND fsb/Ready1r)
    	OR (A_FSB(9) AND A_FSB(8) AND A_FSB(15) AND A_FSB(14) AND
    	A_FSB(13) AND A_FSB(12) AND A_FSB(11) AND A_FSB(10) AND A_FSB(23) AND
    	A_FSB(22) AND A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND A_FSB(18) AND
    	A_FSB(17) AND A_FSB(16) AND iobs/IOReady)
    	OR (A_FSB(22) AND A_FSB(21) AND NOT fsb/Ready1r AND
    	NOT iobs/IOReady AND nDTACK_FSB)
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND cs/nOverlay AND
    	NOT fsb/Ready0r AND nDTACK_FSB AND NOT ram/RAMReady)
    	OR (A_FSB(14) AND A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND
    	A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND cs/nOverlay AND
    	NOT fsb/Ready1r AND NOT nWE_FSB AND NOT iobs/IOReady AND nDTACK_FSB AND NOT nADoutLE1)
    	OR (A_FSB(13) AND A_FSB(21) AND A_FSB(20) AND A_FSB(19) AND
    	A_FSB(18) AND A_FSB(17) AND A_FSB(16) AND cs/nOverlay AND
    	NOT fsb/Ready1r AND NOT nWE_FSB AND NOT iobs/IOReady AND nDTACK_FSB AND NOT nADoutLE1));

    FDCPE_nDinLE: FDCPE port map (nDinLE,nDinLE_D,NOT C16M,'0','0');
    nDinLE_D <= (iobm/IOS_FSM_FFd1 AND iobm/IOS_FSM_FFd2);

    nDinOE <= ((A_FSB(23) AND nWE_FSB AND NOT nAS_FSB)
    	OR (A_FSB(22) AND A_FSB(21) AND nWE_FSB AND NOT nAS_FSB)
    	OR (A_FSB(22) AND A_FSB(20) AND nWE_FSB AND NOT nAS_FSB));

    nDoutOE <= NOT ((iobm/DoutOE AND NOT nAoutOE));

    FDCPE_nLDS_IOB: FDCPE port map (nLDS_IOB_I,nLDS_IOB,NOT C16M,'0','0');
    nLDS_IOB <= ((IOL0 AND NOT iobm/IOS_FSM_FFd3 AND iobm/IOS_FSM_FFd2)
    	OR (IOL0 AND iobm/IOS_FSM_FFd1 AND iobm/IOS_FSM_FFd2)
    	OR (IORW0 AND IOL0 AND iobm/IOS_FSM_FFd3 AND
    	NOT iobm/IOS_FSM_FFd1));
    nLDS_IOB <= nLDS_IOB_I when nLDS_IOB_OE = '1' else 'Z';
    nLDS_IOB_OE <= NOT nAoutOE;

    nOE <= NOT ((nWE_FSB AND NOT nAS_FSB));

    nRAMLWE <= NOT ((NOT nLDS_FSB AND NOT nWE_FSB AND NOT nAS_FSB AND ram/RAMEN));

    nRAMUWE <= NOT ((NOT nWE_FSB AND NOT nUDS_FSB AND NOT nAS_FSB AND ram/RAMEN));

    nRAS <= '1';

    nRES_I <= '0';
    nRES <= nRES_I when nRES_OE = '1' else 'Z';
    nRES_OE <= NOT nRESout;

    FDCPE_nRESout: FDCPE port map (nRESout,nRESout_D,FCLK,'0','0');
    nRESout_D <= (cnt/INITS_FSM_FFd1 AND NOT cnt/INITS_FSM_FFd2);

    nROMCS <= NOT (((NOT A_FSB(23) AND NOT A_FSB(21) AND NOT A_FSB(20) AND NOT cs/nOverlay)
    	OR (NOT A_FSB(23) AND A_FSB(22) AND NOT A_FSB(21) AND NOT A_FSB(20))));

    nROMWE <= NOT ((NOT nWE_FSB AND NOT nAS_FSB));

    FDCPE_nUDS_IOB: FDCPE port map (nUDS_IOB_I,nUDS_IOB,NOT C16M,'0','0');
    nUDS_IOB <= ((IOU0 AND NOT iobm/IOS_FSM_FFd3 AND iobm/IOS_FSM_FFd2)
    	OR (IOU0 AND iobm/IOS_FSM_FFd1 AND iobm/IOS_FSM_FFd2)
    	OR (IORW0 AND IOU0 AND iobm/IOS_FSM_FFd3 AND
    	NOT iobm/IOS_FSM_FFd1));
    nUDS_IOB <= nUDS_IOB_I when nUDS_IOB_OE = '1' else 'Z';
    nUDS_IOB_OE <= NOT nAoutOE;

    FTCPE_nVMA_IOB: FTCPE port map (nVMA_IOB_I,nVMA_IOB_T,C16M,'0','0');
    nVMA_IOB_T <= ((NOT nVMA_IOB AND NOT iobm/ES(0) AND NOT iobm/ES(1) AND NOT iobm/ES(2) AND
    	NOT iobm/ES(3) AND NOT iobm/ES(4))
    	OR (nVMA_IOB AND iobm/ES(0) AND iobm/ES(1) AND iobm/ES(2) AND
    	NOT iobm/ES(3) AND NOT iobm/ES(4) AND IOACT AND iobm/VPArf AND iobm/VPArr));
    nVMA_IOB <= nVMA_IOB_I when nVMA_IOB_OE = '1' else 'Z';
    nVMA_IOB_OE <= NOT nAoutOE;

    nVPA_FSB <= NOT ((fsb/VPA AND NOT nAS_FSB));

    FDCPE_ram/BACTr: FDCPE port map (ram/BACTr,ram/BACTr_D,FCLK,'0','0');
    ram/BACTr_D <= (nAS_FSB AND NOT fsb/ASrf);

    FDCPE_ram/RAMEN: FDCPE port map (ram/RAMEN,ram/RAMEN_D,FCLK,'0','0');
    ram/RAMEN_D <= ((ram/RS_FSM_FFd3 AND ram/RAMEN)
    	OR (ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2 AND ram/RAMEN)
    	OR (NOT ram/RS_FSM_FFd1 AND ram/RS_FSM_FFd2 AND ram/RAMEN)
    	OR (nAS_FSB AND ram/RS_FSM_FFd1 AND ram/RS_FSM_FFd2 AND
    	NOT ram/RS_FSM_FFd3 AND NOT ram/RefUrg AND NOT fsb/ASrf)
    	OR (nAS_FSB AND NOT ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2 AND
    	NOT ram/RS_FSM_FFd3 AND NOT ram/RefUrg AND NOT fsb/ASrf)
    	OR (NOT ram/RS_FSM_FFd1 AND NOT ram/RefUrg AND ram/RAMEN AND
    	ram/BACTr)
    	OR (NOT ram/RS_FSM_FFd1 AND NOT ram/RefUrg AND ram/RAMEN AND
    	NOT ram/RefReq)
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND cs/nOverlay AND NOT nAS_FSB AND
    	NOT ram/RS_FSM_FFd1 AND ram/RAMEN)
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND cs/nOverlay AND
    	NOT ram/RS_FSM_FFd1 AND ram/RAMEN AND fsb/ASrf));

    FDCPE_ram/RAMReady: FDCPE port map (ram/RAMReady,ram/RAMReady_D,FCLK,'0','0');
    ram/RAMReady_D <= ((A_FSB(23) AND NOT ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2 AND
    	NOT ram/RS_FSM_FFd3 AND NOT ram/RefUrg AND NOT ram/RefReq)
    	OR (A_FSB(22) AND NOT ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2 AND
    	NOT ram/RS_FSM_FFd3 AND NOT ram/RefUrg AND ram/BACTr)
    	OR (A_FSB(22) AND NOT ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2 AND
    	NOT ram/RS_FSM_FFd3 AND NOT ram/RefUrg AND NOT ram/RefReq)
    	OR (A_FSB(23) AND NOT ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2 AND
    	NOT ram/RS_FSM_FFd3 AND NOT ram/RefUrg AND ram/BACTr)
    	OR (ram/RS_FSM_FFd1 AND ram/RS_FSM_FFd2 AND
    	NOT ram/RS_FSM_FFd3 AND NOT ram/RefUrg)
    	OR (NOT cs/nOverlay AND NOT ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2 AND
    	NOT ram/RS_FSM_FFd3 AND NOT ram/RefUrg AND ram/BACTr)
    	OR (NOT cs/nOverlay AND NOT ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2 AND
    	NOT ram/RS_FSM_FFd3 AND NOT ram/RefUrg AND NOT ram/RefReq)
    	OR (nAS_FSB AND NOT ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2 AND
    	NOT ram/RS_FSM_FFd3 AND NOT ram/RefUrg AND NOT fsb/ASrf)
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND cs/nOverlay AND
    	NOT ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2 AND NOT ram/RS_FSM_FFd3 AND NOT ram/RefUrg AND
    	NOT ram/RAMEN));

    FDCPE_ram/RASEL: FDCPE port map (ram/RASEL,ram/RASEL_D,FCLK,'0','0');
    ram/RASEL_D <= ((A_FSB(23) AND NOT ram/RS_FSM_FFd2 AND NOT ram/RS_FSM_FFd3 AND
    	NOT ram/RefUrg AND NOT ram/RefReq)
    	OR (A_FSB(22) AND NOT ram/RS_FSM_FFd2 AND NOT ram/RS_FSM_FFd3 AND
    	NOT ram/RefUrg AND NOT ram/RefReq)
    	OR (nAS_FSB AND NOT ram/RS_FSM_FFd2 AND NOT ram/RS_FSM_FFd3 AND
    	NOT ram/RefUrg AND NOT fsb/ASrf)
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND cs/nOverlay AND NOT nAS_FSB AND
    	NOT ram/RS_FSM_FFd2 AND NOT ram/RS_FSM_FFd3 AND NOT ram/RAMEN)
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND cs/nOverlay AND
    	NOT ram/RS_FSM_FFd2 AND NOT ram/RS_FSM_FFd3 AND NOT ram/RAMEN AND fsb/ASrf)
    	OR (A_FSB(23) AND NOT ram/RS_FSM_FFd2 AND NOT ram/RS_FSM_FFd3 AND
    	NOT ram/RefUrg AND ram/BACTr)
    	OR (A_FSB(22) AND NOT ram/RS_FSM_FFd2 AND NOT ram/RS_FSM_FFd3 AND
    	NOT ram/RefUrg AND ram/BACTr)
    	OR (NOT cs/nOverlay AND NOT ram/RS_FSM_FFd2 AND NOT ram/RS_FSM_FFd3 AND
    	NOT ram/RefUrg AND ram/BACTr)
    	OR (NOT cs/nOverlay AND NOT ram/RS_FSM_FFd2 AND NOT ram/RS_FSM_FFd3 AND
    	NOT ram/RefUrg AND NOT ram/RefReq)
    	OR (NOT nAS_FSB AND ram/RS_FSM_FFd1)
    	OR (ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2)
    	OR (ram/RS_FSM_FFd1 AND ram/RS_FSM_FFd3)
    	OR (ram/RS_FSM_FFd1 AND NOT ram/RefUrg)
    	OR (ram/RS_FSM_FFd1 AND fsb/ASrf));

    FDCPE_ram/RS_FSM_FFd1: FDCPE port map (ram/RS_FSM_FFd1,ram/RS_FSM_FFd1_D,FCLK,'0','0');
    ram/RS_FSM_FFd1_D <= ((ram/RS_FSM_FFd3)
    	OR (ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2));

    FDCPE_ram/RS_FSM_FFd2: FDCPE port map (ram/RS_FSM_FFd2,ram/RS_FSM_FFd2_D,FCLK,'0','0');
    ram/RS_FSM_FFd2_D <= ((ram/RS_FSM_FFd1 AND ram/RS_FSM_FFd2 AND ram/RefUrg AND
    	fsb/ASrf)
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND cs/nOverlay AND NOT nAS_FSB AND
    	NOT ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2 AND NOT ram/RS_FSM_FFd3 AND ram/RefUrg)
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND cs/nOverlay AND NOT nAS_FSB AND
    	NOT ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2 AND NOT ram/RS_FSM_FFd3 AND ram/RAMEN)
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND cs/nOverlay AND
    	NOT ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2 AND NOT ram/RS_FSM_FFd3 AND ram/RefUrg AND
    	fsb/ASrf)
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND cs/nOverlay AND
    	NOT ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2 AND NOT ram/RS_FSM_FFd3 AND ram/RAMEN AND
    	fsb/ASrf)
    	OR (ram/RS_FSM_FFd1 AND ram/RS_FSM_FFd3)
    	OR (ram/RS_FSM_FFd2 AND ram/RS_FSM_FFd3)
    	OR (NOT nAS_FSB AND ram/RS_FSM_FFd1 AND ram/RS_FSM_FFd2 AND
    	ram/RefUrg));

    FTCPE_ram/RS_FSM_FFd3: FTCPE port map (ram/RS_FSM_FFd3,ram/RS_FSM_FFd3_T,FCLK,'0','0');
    ram/RS_FSM_FFd3_T <= ((A_FSB(23) AND NOT ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2 AND
    	NOT ram/RS_FSM_FFd3 AND NOT ram/RefUrg AND ram/BACTr)
    	OR (A_FSB(22) AND NOT ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2 AND
    	NOT ram/RS_FSM_FFd3 AND NOT ram/RefUrg AND ram/BACTr)
    	OR (A_FSB(22) AND NOT ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2 AND
    	NOT ram/RS_FSM_FFd3 AND NOT ram/RefUrg AND NOT ram/RefReq)
    	OR (NOT cs/nOverlay AND NOT ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2 AND
    	NOT ram/RS_FSM_FFd3 AND NOT ram/RefUrg AND NOT ram/RefReq)
    	OR (A_FSB(23) AND NOT ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2 AND
    	NOT ram/RS_FSM_FFd3 AND NOT ram/RefUrg AND NOT ram/RefReq)
    	OR (nAS_FSB AND NOT ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2 AND
    	NOT ram/RS_FSM_FFd3 AND NOT ram/RefUrg AND NOT fsb/ASrf)
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND cs/nOverlay AND NOT nAS_FSB AND
    	NOT ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2 AND NOT ram/RS_FSM_FFd3 AND NOT ram/RAMEN)
    	OR (NOT A_FSB(23) AND NOT A_FSB(22) AND cs/nOverlay AND
    	NOT ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2 AND NOT ram/RS_FSM_FFd3 AND NOT ram/RAMEN AND
    	fsb/ASrf)
    	OR (NOT ram/RS_FSM_FFd1 AND ram/RS_FSM_FFd2 AND
    	ram/RS_FSM_FFd3)
    	OR (NOT nAS_FSB AND ram/RS_FSM_FFd1 AND ram/RS_FSM_FFd2 AND
    	NOT ram/RS_FSM_FFd3)
    	OR (ram/RS_FSM_FFd1 AND ram/RS_FSM_FFd2 AND
    	NOT ram/RS_FSM_FFd3 AND NOT ram/RefUrg)
    	OR (ram/RS_FSM_FFd1 AND ram/RS_FSM_FFd2 AND
    	NOT ram/RS_FSM_FFd3 AND fsb/ASrf)
    	OR (NOT cs/nOverlay AND NOT ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2 AND
    	NOT ram/RS_FSM_FFd3 AND NOT ram/RefUrg AND ram/BACTr));

    FDCPE_ram/RefDone: FDCPE port map (ram/RefDone,ram/RefDone_D,FCLK,'0','0');
    ram/RefDone_D <= ((ram/RefDone AND ram/RefReqSync)
    	OR (ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2 AND
    	NOT ram/RS_FSM_FFd3 AND ram/RefReqSync)
    	OR (NOT ram/RS_FSM_FFd1 AND NOT ram/RS_FSM_FFd2 AND
    	ram/RS_FSM_FFd3 AND ram/RefReqSync));

    FDCPE_ram/RefReq: FDCPE port map (ram/RefReq,ram/RefReq_D,FCLK,'0','0');
    ram/RefReq_D <= (NOT ram/RefDone AND ram/RefReqSync);

    FDCPE_ram/RefReqSync: FDCPE port map (ram/RefReqSync,RefReq,FCLK,'0','0');

    FDCPE_ram/RefUrg: FDCPE port map (ram/RefUrg,ram/RefUrg_D,FCLK,'0','0');
    ram/RefUrg_D <= (NOT ram/RefDone AND ram/RegUrgSync);

    FDCPE_ram/RegUrgSync: FDCPE port map (ram/RegUrgSync,RefUrg,FCLK,'0','0');

    Register Legend:
     FDCPE (Q,D,C,CLR,PRE,CE);
     FTCPE (Q,D,C,CLR,PRE,CE);
     LDCP  (Q,D,G,CLR,PRE);

    ******************************  Device Pin Out *****************************

    Device : XC95144XL-10-TQ100

       --------------------------------------------------
      /100 98  96  94  92  90  88  86  84  82  80  78  76  \
     |   99  97  95  93  91  89  87  85  83  81  79  77    |
     | 1                                               75  |
     | 2                                               74  |
     | 3                                               73  |
     | 4                                               72  |
     | 5                                               71  |
     | 6                                               70  |
     | 7                                               69  |
     | 8                                               68  |
     | 9                                               67  |
     | 10                                              66  |
     | 11                                              65  |
     | 12                                              64  |
     | 13              XC95144XL-10-TQ100              63  |
     | 14                                              62  |
     | 15                                              61  |
     | 16                                              60  |
     | 17                                              59  |
     | 18                                              58  |
     | 19                                              57  |
     | 20                                              56  |
     | 21                                              55  |
     | 22                                              54  |
     | 23                                              53  |
     | 24                                              52  |
     | 25                                              51  |
     |   27  29  31  33  35  37  39  41  43  45  47  49    |
      \26  28  30  32  34  36  38  40  42  44  46  48  50  /
       --------------------------------------------------

    Pin Signal                         Pin Signal
    No. Name                           No. Name
      1 KPR                              51 VCC
      2 A_FSB<5>                         52 RA<7>
      3 A_FSB<6>                         53 RA<0>
      4 A_FSB<7>                         54 RA<8>
      5 VCC                              55 RA<10>
      6 A_FSB<8>                         56 RA<9>
      7 A_FSB<9>                         57 VCC
      8 A_FSB<10>                        58 C25MEN
      9 A_FSB<11>                        59 C20MEN
     10 A_FSB<12>                        60 KPR
     11 A_FSB<13>                        61 KPR
     12 A_FSB<14>                        62 GND
     13 A_FSB<15>                        63 RA<11>
     14 A_FSB<16>                        64 nRAS
     15 A_FSB<17>                        65 nRAMLWE
     16 A_FSB<18>                        66 nRAMUWE
     17 A_FSB<19>                        67 KPR
     18 A_FSB<20>                        68 KPR
     19 A_FSB<21>                        69 GND
     20 A_FSB<22>                        70 nBERR_FSB
     21 GND                              71 KPR
     22 C16M                             72 nBR_IOB
     23 C8M                              73 KPR
     24 A_FSB<23>                        74 nVMA_IOB
     25 E                                75 GND
     26 VCC                              76 nBERR_IOB
     27 FCLK                             77 nVPA_IOB
     28 nDTACK_FSB                       78 nDTACK_IOB
     29 nWE_FSB                          79 nLDS_IOB
     30 nLDS_FSB                         80 nUDS_IOB
     31 GND                              81 nAS_IOB
     32 nAS_FSB                          82 nADoutLE1
     33 nUDS_FSB                         83 TDO
     34 nROMWE                           84 GND
     35 nROMCS                           85 nADoutLE0
     36 nCAS                             86 nDinLE
     37 nOE                              87 nAoutOE
     38 VCC                              88 VCC
     39 KPR                              89 nDoutOE
     40 RA<4>                            90 nDinOE
     41 RA<3>                            91 nRES
     42 RA<5>                            92 nIPL2
     43 RA<2>                            93 nVPA_FSB
     44 GND                              94 A_FSB<1>
     45 TDI                              95 A_FSB<2>
     46 RA<6>                            96 A_FSB<3>
     47 TMS                              97 A_FSB<4>
     48 TCK                              98 VCC
     49 KPR                              99 KPR
     50 RA<1>                           100 GND

    Legend :  NC  = Not Connected, unbonded pin
             PGND = Unused I/O configured as additional Ground pin
             TIE  = Unused I/O floating -- must tie to VCC, GND or other signal
             KPR  = Unused I/O with weak keeper (leave unconnected)
             VCC  = Dedicated Power Pin
             GND  = Dedicated Ground Pin
             TDI  = Test Data In, JTAG pin
             TDO  = Test Data Out, JTAG pin
             TCK  = Test Clock, JTAG pin
             TMS  = Test Mode Select, JTAG pin
      PROHIBITED  = User reserved pin
    ****************************  Compiler Options  ****************************

    Following is a list of all global compiler options used by the fitter run.

    Device(s) Specified                         : xc95144xl-10-TQ100
    Optimization Method                         : SPEED
    Multi-Level Logic Optimization              : ON
    Ignore Timing Specifications                : OFF
    Default Register Power Up Value             : LOW
    Keep User Location Constraints              : ON
    What-You-See-Is-What-You-Get                : OFF
    Exhaustive Fitting                          : OFF
    Keep Unused Inputs                          : OFF
    Slew Rate                                   : FAST
    Power Mode                                  : STD
    Ground on Unused IOs                        : OFF
    Set I/O Pin Termination                     : KEEPER
    Global Clock Optimization                   : ON
    Global Set/Reset Optimization               : ON
    Global Ouput Enable Optimization            : ON
    Input Limit                                 : 54
    Pterm Limit                                 : 25