Signal Name | Total Product Terms | Product Terms | Location | Power Mode | Pin Number | PinType | Pin Use
--- | --- | --- | --- | --- | --- | --- | ---
ram/RefUrg | 1 | 1_1 | MC1 | STD |  | (b) | (b)
ram/RefReqSync | 1 | 2_1 | MC2 | STD | 11 | I/O | I
ram/RefReq | 1 | 3_1 | MC3 | STD | 12 | I/O | I
iobs/IOACTr | 1 | 4_1 | MC4 | STD |  | (b) | (b)
iobm/Er | 1 | 5_1 | MC5 | STD | 13 | I/O | I
iobm/DTACKrr | 1 | 6_1 | MC6 | STD | 14 | I/O | I
iobm/DTACKrf | 1 | 7_1 | MC7 | STD |  | (b) | (b)
iobm/BERRrr | 1 | 8_1 | MC8 | STD | 15 | I/O | I
iobm/BERRrf | 1 | 9_1 | MC9 | STD | 16 | I/O | I
cnt/nIPL2r | 1 | 10_1 | MC10 | STD |  | (b) | (b)
cnt/Er<0> | 1 | 11_1 | MC11 | STD | 17 | I/O | I
ALE0S | 1 | 12_1 | MC12 | STD | 18 | I/O | I
ram/RS_FSM_FFd1 | 2 | 13_1 13_2 | MC13 | STD |  | (b) | (b)
iobs/IOU1 | 2 | 14_1 14_2 | MC14 | STD | 19 | I/O | I
iobs/IOL1 | 2 | 15_1 15_2 | MC15 | STD | 20 | I/O | I
iobm/IOS_FSM_FFd1 | 2 | 16_1 16_2 | MC16 | STD |  | (b) | (b)
ALE0M | 2 | 17_1 17_2 | MC17 | STD | 22 | I/O/GCK1 | GCK
ram/RefDone | 3 | 18_1 18_2 18_3 | MC18 | STD |  | (b) | (b)

Signals Used By Logic in Function Block

1. E
2. IOACT
3. RefReq
4. iobm/IOREQr
5. iobm/IOS_FSM_FFd1
6. iobm/IOS_FSM_FFd2
7. iobm/IOS_FSM_FFd3
8. iobs/Load1
9. iobs/PS_FSM_FFd1
10. iobs/PS_FSM_FFd2
11. nBERR_IOB
12. nDTACK_IOB
13. nIPL2
14. nLDS_FSB
15. nUDS_FSB
16. ram/RS_FSM_FFd1
17. ram/RS_FSM_FFd2
18. ram/RS_FSM_FFd3
19. ram/RefDone
20. ram/RefReqSync
21. ram/RegUrgSync