(kicad_pcb (version 20171130) (host pcbnew "(5.1.8-0-10_14)")

  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 0)
    (zones 0)
    (modules 1)
    (nets 27)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 /I_O)
  (net 2 GND)
  (net 3 /REQ)
  (net 4 /C_D)
  (net 5 /SEL)
  (net 6 /MSG)
  (net 7 /RST)
  (net 8 "Net-(J1-Pad38)")
  (net 9 /BSY)
  (net 10 "Net-(J1-Pad34)")
  (net 11 /ATN)
  (net 12 "Net-(J1-Pad30)")
  (net 13 "Net-(J1-Pad28)")
  (net 14 /TERMPWR)
  (net 15 "Net-(J1-Pad24)")
  (net 16 "Net-(J1-Pad22)")
  (net 17 "Net-(J1-Pad20)")
  (net 18 /DBP)
  (net 19 /DB7)
  (net 20 /DB6)
  (net 21 /DB5)
  (net 22 /DB4)
  (net 23 /DB3)
  (net 24 /DB2)
  (net 25 /DB1)
  (net 26 /DB0)

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ATN)
    (add_net /BSY)
    (add_net /C_D)
    (add_net /DB0)
    (add_net /DB1)
    (add_net /DB2)
    (add_net /DB3)
    (add_net /DB4)
    (add_net /DB5)
    (add_net /DB6)
    (add_net /DB7)
    (add_net /DBP)
    (add_net /I_O)
    (add_net /MSG)
    (add_net /REQ)
    (add_net /RST)
    (add_net /SEL)
    (add_net /TERMPWR)
    (add_net GND)
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad24)")
    (add_net "Net-(J1-Pad28)")
    (add_net "Net-(J1-Pad30)")
    (add_net "Net-(J1-Pad34)")
    (add_net "Net-(J1-Pad38)")
  )

  (module Connector_PinSocket_2.54mm:PinSocket_2x25_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A421) (tstamp 609D94CC)
    (at 124.46 124.46)
    (descr "Through hole straight socket strip, 2x25, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x25 2.54mm double row")
    (path /609D92C9)
    (fp_text reference J1 (at -1.27 2.77) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Conn_02x25_Odd_Even (at -1.27 -63.73) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at -1.27 -30.48 -90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -3.81 1.27) (end 0.27 1.27) (layer B.Fab) (width 0.1))
    (fp_line (start 0.27 1.27) (end 1.27 0.27) (layer B.Fab) (width 0.1))
    (fp_line (start 1.27 0.27) (end 1.27 -62.23) (layer B.Fab) (width 0.1))
    (fp_line (start 1.27 -62.23) (end -3.81 -62.23) (layer B.Fab) (width 0.1))
    (fp_line (start -3.81 -62.23) (end -3.81 1.27) (layer B.Fab) (width 0.1))
    (fp_line (start -3.87 1.33) (end -1.27 1.33) (layer B.SilkS) (width 0.12))
    (fp_line (start -3.87 1.33) (end -3.87 -62.29) (layer B.SilkS) (width 0.12))
    (fp_line (start -3.87 -62.29) (end 1.33 -62.29) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.33 -1.27) (end 1.33 -62.29) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.27 -1.27) (end 1.33 -1.27) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.27 1.33) (end -1.27 -1.27) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.33 1.33) (end 1.33 0) (layer B.SilkS) (width 0.12))
    (fp_line (start 0 1.33) (end 1.33 1.33) (layer B.SilkS) (width 0.12))
    (fp_line (start -4.34 1.8) (end 1.76 1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.76 1.8) (end 1.76 -62.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.76 -62.7) (end -4.34 -62.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -4.34 -62.7) (end -4.34 1.8) (layer B.CrtYd) (width 0.05))
    (pad 50 thru_hole oval (at -2.54 -60.96) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /I_O))
    (pad 49 thru_hole oval (at 0 -60.96) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 48 thru_hole oval (at -2.54 -58.42) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /REQ))
    (pad 47 thru_hole oval (at 0 -58.42) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 46 thru_hole oval (at -2.54 -55.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /C_D))
    (pad 45 thru_hole oval (at 0 -55.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 44 thru_hole oval (at -2.54 -53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /SEL))
    (pad 43 thru_hole oval (at 0 -53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 42 thru_hole oval (at -2.54 -50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /MSG))
    (pad 41 thru_hole oval (at 0 -50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 40 thru_hole oval (at -2.54 -48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /RST))
    (pad 39 thru_hole oval (at 0 -48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 38 thru_hole oval (at -2.54 -45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad38)"))
    (pad 37 thru_hole oval (at 0 -45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 36 thru_hole oval (at -2.54 -43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /BSY))
    (pad 35 thru_hole oval (at 0 -43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 34 thru_hole oval (at -2.54 -40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad34)"))
    (pad 33 thru_hole oval (at 0 -40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 32 thru_hole oval (at -2.54 -38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /ATN))
    (pad 31 thru_hole oval (at 0 -38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 30 thru_hole oval (at -2.54 -35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad30)"))
    (pad 29 thru_hole oval (at 0 -35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 28 thru_hole oval (at -2.54 -33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad28)"))
    (pad 27 thru_hole oval (at 0 -33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 26 thru_hole oval (at -2.54 -30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /TERMPWR))
    (pad 25 thru_hole oval (at 0 -30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 24 thru_hole oval (at -2.54 -27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad24)"))
    (pad 23 thru_hole oval (at 0 -27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 22 thru_hole oval (at -2.54 -25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad22)"))
    (pad 21 thru_hole oval (at 0 -25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 20 thru_hole oval (at -2.54 -22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad20)"))
    (pad 19 thru_hole oval (at 0 -22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 18 thru_hole oval (at -2.54 -20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /DBP))
    (pad 17 thru_hole oval (at 0 -20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 16 thru_hole oval (at -2.54 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /DB7))
    (pad 15 thru_hole oval (at 0 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 14 thru_hole oval (at -2.54 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /DB6))
    (pad 13 thru_hole oval (at 0 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 12 thru_hole oval (at -2.54 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /DB5))
    (pad 11 thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at -2.54 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /DB4))
    (pad 9 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at -2.54 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /DB3))
    (pad 7 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at -2.54 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /DB2))
    (pad 5 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at -2.54 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /DB1))
    (pad 3 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /DB0))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x25_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 127 127) (end 127 60.96) (layer Edge.Cuts) (width 0.05) (tstamp 609D9A47))
  (gr_line (start 114.3 127) (end 127 127) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 88.9 66.04) (end 88.9 60.96) (layer Edge.Cuts) (width 0.05) (tstamp 609D9A45))
  (gr_line (start 114.3 111.76) (end 88.9 66.04) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 114.3 127) (end 114.3 111.76) (layer Edge.Cuts) (width 0.05))
  (dimension 15.24 (width 0.15) (layer Dwgs.User)
    (gr_text "15.240 mm" (at 107.92 119.38 270) (layer Dwgs.User)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (feature1 (pts (xy 111.76 127) (xy 108.633579 127)))
    (feature2 (pts (xy 111.76 111.76) (xy 108.633579 111.76)))
    (crossbar (pts (xy 109.22 111.76) (xy 109.22 127)))
    (arrow1a (pts (xy 109.22 127) (xy 108.633579 125.873496)))
    (arrow1b (pts (xy 109.22 127) (xy 109.806421 125.873496)))
    (arrow2a (pts (xy 109.22 111.76) (xy 108.633579 112.886504)))
    (arrow2b (pts (xy 109.22 111.76) (xy 109.806421 112.886504)))
  )
  (dimension 60.96 (width 0.15) (layer Dwgs.User)
    (gr_text "60.960 mm" (at 85.06 96.52 90) (layer Dwgs.User)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (feature1 (pts (xy 88.9 66.04) (xy 85.773579 66.04)))
    (feature2 (pts (xy 88.9 127) (xy 85.773579 127)))
    (crossbar (pts (xy 86.36 127) (xy 86.36 66.04)))
    (arrow1a (pts (xy 86.36 66.04) (xy 86.946421 67.166504)))
    (arrow1b (pts (xy 86.36 66.04) (xy 85.773579 67.166504)))
    (arrow2a (pts (xy 86.36 127) (xy 86.946421 125.873496)))
    (arrow2b (pts (xy 86.36 127) (xy 85.773579 125.873496)))
  )
  (dimension 38.1 (width 0.15) (layer Dwgs.User)
    (gr_text "38.100 mm" (at 107.95 54.58) (layer Dwgs.User)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (feature1 (pts (xy 88.9 58.42) (xy 88.9 55.293579)))
    (feature2 (pts (xy 127 58.42) (xy 127 55.293579)))
    (crossbar (pts (xy 127 55.88) (xy 88.9 55.88)))
    (arrow1a (pts (xy 88.9 55.88) (xy 90.026504 55.293579)))
    (arrow1b (pts (xy 88.9 55.88) (xy 90.026504 56.466421)))
    (arrow2a (pts (xy 127 55.88) (xy 125.873496 55.293579)))
    (arrow2b (pts (xy 127 55.88) (xy 125.873496 56.466421)))
  )
  (gr_line (start 127 60.96) (end 88.9 60.96) (layer Edge.Cuts) (width 0.05))

)
