<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="45" width="0" layer="20"/>
<wire x1="100" y1="45" x2="0" y2="45" width="0" layer="20"/>
<wire x1="0" y1="45" x2="0" y2="0" width="0" layer="20"/>
<text>PREV</text>
<text>SELECT</text>
<text>NEXT</text>
<text>RESET</text>
<text>STATUS</text>
<text>ISP</text>
<text>LCD1</text>
<text>LCD2</text>
<text>CPLD</text>
<text>AVR</text>
<text>244</text>
<text>X1</text>
<text>R4</text>
<text>R1</text>
<text>R3</text>
<text>C12</text>
<text>C13</text>
<text>C11</text>
<text>1117</text>
<text>MACINTOSH FLOPPY EMU</text>
<text>VERSION 1.2</text>
<text>WWW.BIGMESSOWIRES.COM</text>
<text>3V3</text>
<text>LED</text>
<text>CE</text>
<text>RST</text>
<text>D/C</text>
<text>MOSI</text>
<text>SCLK</text>
<text>POWER</text>
<text>R5</text>
<text>C10</text>
<text>C8</text>
<text>IC1</text>
<text>IC2</text>
<text>IC3</text>
<text>IC4</text>
<text>J1</text>
<text>J2</text>
<text>J3</text>
<text>C2</text>
<text>C1</text>
<text>C3</text>
<text>C9</text>
<text>C4</text>
<text>C6</text>
<text>C5</text>
<text>C7</text>
<text>U1</text>
<text>SD Card</text>
<text>DESIGNED AND PRODUCED BY</text>
<text>LIGHT</text>
</plain>
<libraries>
<library name="big-mess-o-wires">
<packages>
<package name="BIG-MESS-O-WIRES_TQFP44-LONGPADS">
<description>Extra-long pads for easier hand soldering</description>
</package>
<package name="TQFP44-LONGPADS">
<description>Extra-long pads for easier hand soldering</description>
</package>
<package name="DB19EDGE">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="BIG-MESS-O-WIRES_2X3-SHROUDED">
</package>
<package name="B3FS">
<description>Omron B3FS SMD tactile switch</description>
</package>
<package name="SSOP20">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type SS</description>
</package>
<package name="IDC20">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
series 057 contact pc board low profile headers&lt;p&gt;
straight</description>
</package>
<package name="ADAFRUIT_06132">
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="1X08">
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="NX5032">
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
<library name="burr-brown">
<packages>
<package name="SOT223">
<description>&lt;b&gt;Smal Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="P1-13">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA3528">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1/6W-RES">
<description>1/6W Thru-hole Resistor - *UNPROVEN*</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC2" library="big-mess-o-wires" package="BIG-MESS-O-WIRES_TQFP44-LONGPADS" value="BIG-MESS-O-WIRES_ATMEGA1284"/>
<element name="IC1" library="big-mess-o-wires" package="TQFP44-LONGPADS" value="XC9572XLTQFP44"/>
<element name="J4" library="SparkFun" package="1X08" value="LCD1"/>
<element name="J3" library="big-mess-o-wires" package="DB19EDGE" value="DB19"/>
<element name="U1" library="big-mess-o-wires" package="ADAFRUIT_06132" value="ADAFRUIT_SDMMC06132"/>
<element name="J2" library="big-mess-o-wires" package="IDC20" value="IDC20"/>
<element name="J1" library="big-mess-o-wires" package="BIG-MESS-O-WIRES_2X3-SHROUDED" value="BIG-MESS-O-WIRES_AVR_ISP"/>
<element name="C1" library="SparkFun" package="0805" value="0.1uF"/>
<element name="C2" library="SparkFun" package="0805" value="0.1uF"/>
<element name="C3" library="SparkFun" package="0805" value="0.1uF"/>
<element name="C4" library="SparkFun" package="0805" value="0.1uF"/>
<element name="C5" library="SparkFun" package="0805" value="0.1uF"/>
<element name="C6" library="SparkFun" package="0805" value="0.1uF"/>
<element name="C7" library="SparkFun" package="0805" value="0.1uF"/>
<element name="C8" library="SparkFun" package="0805" value="0.1uF"/>
<element name="C9" library="SparkFun" package="0805" value="0.1uF"/>
<element name="C10" library="SparkFun" package="0805" value="0.1uF"/>
<element name="PREV" library="big-mess-o-wires" package="B3FS" value="B3FS-10XX"/>
<element name="SELECT" library="big-mess-o-wires" package="B3FS" value="B3FS-10XX"/>
<element name="NEXT" library="big-mess-o-wires" package="B3FS" value="B3FS-10XX"/>
<element name="RESET" library="big-mess-o-wires" package="B3FS" value="B3FS-10XX"/>
<element name="POWER" library="led" package="CHIPLED_0805" value=""/>
<element name="STATUS" library="led" package="CHIPLED_0805" value=""/>
<element name="R1" library="SparkFun" package="0805" value="220R"/>
<element name="R3" library="SparkFun" package="0805" value="220R"/>
<element name="C12" library="SparkFun" package="0805" value="18pF"/>
<element name="C13" library="SparkFun" package="0805" value="18pF"/>
<element name="IC3" library="big-mess-o-wires" package="SSOP20" value="74LVC244"/>
<element name="IC4" library="burr-brown" package="SOT223" value="REG1117">
<attribute name="MF" value=""/>
<attribute name="MPN" value="REG1117"/>
<attribute name="OC_FARNELL" value="1097566"/>
<attribute name="OC_NEWARK" value="14P6981"/>
</element>
<element name="X1" library="adafruit" package="NX5032" value="20 MHz"/>
<element name="R4" library="SparkFun" package="0805" value="10K"/>
<element name="LCD2" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="STANDOFF1" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="STANDOFF2" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="STANDOFF3" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="STANDOFF4" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="R2" library="SparkFun-Resistors" package="1/6W-RES" value="220"/>
<element name="TP1" library="testpad" package="P1-13" value="PTR1PAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="C11" library="SparkFun-Capacitors" package="EIA3528" value="33uF">
<attribute name="PROD_ID" value="CAP-08310"/>
<attribute name="VALUE" value="47uF"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC2" pad="18"/>
<contactref element="IC2" pad="6"/>
<contactref element="IC2" pad="28"/>
<contactref element="IC2" pad="39"/>
<contactref element="IC1" pad="25"/>
<contactref element="IC3" pad="10"/>
<contactref element="PREV" pad="A'"/>
<contactref element="PREV" pad="A"/>
<contactref element="SELECT" pad="A'"/>
<contactref element="SELECT" pad="A"/>
<contactref element="NEXT" pad="A'"/>
<contactref element="NEXT" pad="A"/>
<contactref element="RESET" pad="A'"/>
<contactref element="RESET" pad="A"/>
<contactref element="IC4" pad="1"/>
<contactref element="C10" pad="2"/>
<contactref element="J1" pad="6"/>
<contactref element="J2" pad="7"/>
<contactref element="J2" pad="5"/>
<contactref element="J2" pad="3"/>
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="J3" pad="2"/>
<contactref element="J3" pad="3"/>
<contactref element="J3" pad="4"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="17"/>
<contactref element="U1" pad="GP"/>
<contactref element="C9" pad="1"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="3"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="POWER" pad="C"/>
<contactref element="IC3" pad="17"/>
<contactref element="IC3" pad="1"/>
<contactref element="IC3" pad="19"/>
<contactref element="C11" pad="C"/>
<contactref element="J4" pad="8"/>
</signal>
<signal name="+5V">
<contactref element="R1" pad="1"/>
<contactref element="IC4" pad="3"/>
<contactref element="C10" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="J2" pad="11"/>
<contactref element="J3" pad="6"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="IC2" pad="38"/>
<contactref element="IC2" pad="17"/>
<contactref element="IC2" pad="5"/>
<contactref element="C7" pad="1"/>
<contactref element="IC2" pad="27"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="2"/>
<contactref element="POWER" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="2"/>
<contactref element="STATUS" pad="A"/>
</signal>
<signal name="+3V3">
<contactref element="IC4" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="C9" pad="2"/>
<contactref element="IC1" pad="15"/>
<contactref element="IC1" pad="35"/>
<contactref element="IC1" pad="26"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="IC3" pad="20"/>
<contactref element="C8" pad="1"/>
<contactref element="C11" pad="A"/>
<contactref element="J4" pad="6"/>
</signal>
<signal name="RESET">
<contactref element="J1" pad="5"/>
<contactref element="IC2" pad="4"/>
<contactref element="RESET" pad="B'"/>
<contactref element="RESET" pad="B"/>
</signal>
<signal name="SCK">
<contactref element="J1" pad="3"/>
<contactref element="IC2" pad="3"/>
<contactref element="IC3" pad="11"/>
<contactref element="IC3" pad="13"/>
</signal>
<signal name="MISO">
<contactref element="J1" pad="1"/>
<contactref element="IC2" pad="2"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="MOSI">
<contactref element="J1" pad="4"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC3" pad="8"/>
</signal>
<signal name="PH0">
<contactref element="J2" pad="2"/>
<contactref element="J3" pad="11"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="PH1">
<contactref element="J2" pad="4"/>
<contactref element="J3" pad="12"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="PH2">
<contactref element="J2" pad="6"/>
<contactref element="IC1" pad="14"/>
<contactref element="J3" pad="13"/>
</signal>
<signal name="PH3">
<contactref element="J2" pad="8"/>
<contactref element="J3" pad="14"/>
<contactref element="IC1" pad="16"/>
</signal>
<signal name="/WREQ">
<contactref element="J2" pad="10"/>
<contactref element="J3" pad="15"/>
<contactref element="IC1" pad="18"/>
</signal>
<signal name="SEL">
<contactref element="J2" pad="12"/>
<contactref element="J3" pad="16"/>
<contactref element="IC1" pad="19"/>
</signal>
<signal name="RD">
<contactref element="J2" pad="16"/>
<contactref element="J3" pad="18"/>
<contactref element="IC1" pad="21"/>
</signal>
<signal name="WR">
<contactref element="J2" pad="18"/>
<contactref element="J3" pad="19"/>
<contactref element="IC1" pad="22"/>
</signal>
<signal name="/ENBL.EXT">
<contactref element="J3" pad="17"/>
<contactref element="J2" pad="14"/>
<contactref element="IC1" pad="20"/>
</signal>
<signal name="TMS">
<contactref element="IC1" pad="10"/>
<contactref element="IC2" pad="22"/>
</signal>
<signal name="TDO">
<contactref element="IC1" pad="24"/>
<contactref element="IC2" pad="23"/>
</signal>
<signal name="BYTER/TDI">
<contactref element="IC1" pad="9"/>
<contactref element="IC2" pad="24"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="LCDE33">
<contactref element="IC3" pad="18"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="RST33">
<contactref element="IC3" pad="16"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="DC33">
<contactref element="IC3" pad="14"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="MOSI33">
<contactref element="U1" pad="2"/>
<contactref element="IC3" pad="12"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="SCK33">
<contactref element="U1" pad="5"/>
<contactref element="IC3" pad="9"/>
</signal>
<signal name="SDE33">
<contactref element="U1" pad="1"/>
<contactref element="IC3" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="IC2" pad="8"/>
<contactref element="C13" pad="1"/>
<contactref element="X1" pad="P$2"/>
</signal>
<signal name="D4">
<contactref element="IC2" pad="33"/>
<contactref element="IC1" pad="36"/>
</signal>
<signal name="LCDE">
<contactref element="IC3" pad="2"/>
<contactref element="IC2" pad="42"/>
</signal>
<signal name="RST">
<contactref element="IC3" pad="4"/>
<contactref element="IC2" pad="40"/>
<contactref element="IC1" pad="37"/>
</signal>
<signal name="DC">
<contactref element="IC3" pad="6"/>
<contactref element="IC2" pad="15"/>
</signal>
<signal name="SDE">
<contactref element="IC3" pad="15"/>
<contactref element="IC2" pad="44"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="CLKO">
<contactref element="IC2" pad="41"/>
<contactref element="IC1" pad="43"/>
</signal>
<signal name="TACH">
<contactref element="IC2" pad="14"/>
<contactref element="IC1" pad="28"/>
</signal>
<signal name="/WREQM">
<contactref element="IC2" pad="19"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="SIDE">
<contactref element="IC1" pad="3"/>
<contactref element="IC2" pad="20"/>
</signal>
<signal name="STPDIR_MOTOR">
<contactref element="IC2" pad="26"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="STPREQ">
<contactref element="IC1" pad="39"/>
<contactref element="IC2" pad="9"/>
</signal>
<signal name="D1">
<contactref element="IC2" pad="36"/>
<contactref element="IC1" pad="32"/>
</signal>
<signal name="D6">
<contactref element="IC2" pad="31"/>
<contactref element="IC1" pad="41"/>
</signal>
<signal name="D2">
<contactref element="IC2" pad="35"/>
<contactref element="IC1" pad="33"/>
</signal>
<signal name="D3">
<contactref element="IC2" pad="34"/>
<contactref element="IC1" pad="34"/>
</signal>
<signal name="D5">
<contactref element="IC2" pad="32"/>
<contactref element="IC1" pad="38"/>
</signal>
<signal name="DIN/STA/TCK">
<contactref element="IC2" pad="21"/>
<contactref element="IC1" pad="11"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="EJECT">
<contactref element="IC2" pad="12"/>
<contactref element="IC1" pad="30"/>
</signal>
<signal name="D0">
<contactref element="IC2" pad="37"/>
<contactref element="IC1" pad="31"/>
</signal>
<signal name="RDAWRT">
<contactref element="IC2" pad="30"/>
<contactref element="IC1" pad="44"/>
</signal>
<signal name="OE">
<contactref element="IC2" pad="25"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="LEDD">
<contactref element="STATUS" pad="C"/>
<contactref element="IC2" pad="43"/>
</signal>
<signal name="NEXT">
<contactref element="NEXT" pad="B"/>
<contactref element="NEXT" pad="B'"/>
<contactref element="IC2" pad="11"/>
</signal>
<signal name="PREV">
<contactref element="IC2" pad="10"/>
<contactref element="PREV" pad="B"/>
<contactref element="PREV" pad="B'"/>
</signal>
<signal name="SELECT">
<contactref element="IC2" pad="13"/>
<contactref element="SELECT" pad="B"/>
<contactref element="SELECT" pad="B'"/>
</signal>
<signal name="N$3">
<contactref element="C12" pad="1"/>
<contactref element="X1" pad="P$1"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="SCK33A">
<contactref element="IC3" pad="7"/>
<contactref element="J4" pad="5"/>
</signal>
<signal name="WPROT">
<contactref element="U1" pad="WP"/>
<contactref element="IC2" pad="16"/>
</signal>
<signal name="TEST">
<contactref element="TP1" pad="TP"/>
<contactref element="IC1" pad="27"/>
</signal>
<signal name="PWM">
<contactref element="J3" pad="10"/>
<contactref element="J2" pad="20"/>
<contactref element="IC1" pad="23"/>
</signal>
<signal name="N$10">
<contactref element="R2" pad="2"/>
<contactref element="J4" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
