(export (version D)
  (design
    (source "/Users/demik/github/oldworld/EDA/TashTwenty Tiny/TashTwenty Tiny.sch")
    (date "2021 November 28, Sunday 23:04:41")
    (tool "Eeschema (5.1.9-0-10_14)")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "TashTwenty Tiny.sch")
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name "/TashTwenty Tiny Connector/") (tstamps /61A14260/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "TashTwenty Tiny Connector.sch")
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name "/TashTwenty Tiny LEDs/") (tstamps /61A5C73E/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "TashTwenty Tiny LEDs.sch")
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U1)
      (value PIC16F1825-IP)
      (footprint Package_DIP:DIP-14_W7.62mm)
      (datasheet http://ww1.microchip.com/downloads/en/DeviceDoc/41440C.pdf)
      (libsource (lib PIC16F1825-IP) (part PIC16F1825-IP) (description "Flash-Based, 8-Bit CMOS Microcontrollers, PDIP"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61A1F7E1))
    (comp (ref J1)
      (value SD_Card)
      (footprint Connector_Card:SD_TE_2041021)
      (datasheet http://portal.fciconnect.com/Comergent//fci/drawing/10067847.pdf)
      (libsource (lib Connector) (part SD_Card) (description "SD Card Reader"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61A25F7D))
    (comp (ref R1)
      (value 1200)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 61A3BBD3))
    (comp (ref R2)
      (value 2200)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 61A3C308))
    (comp (ref R3)
      (value 1200)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 61A42F61))
    (comp (ref R4)
      (value 2200)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 61A42F6B))
    (comp (ref R5)
      (value 1200)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 61A45B51))
    (comp (ref R6)
      (value 2200)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 61A45B5B))
    (comp (ref U2)
      (value 74HCT08)
      (footprint Package_DIP:DIP-14_W7.62mm)
      (datasheet http://www.ti.com/lit/gpn/sn74LS08)
      (libsource (lib 74xx) (part 74LS08) (description "Quad And2"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61A48A46))
    (comp (ref R7)
      (value 10k)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 61A58D06))
    (comp (ref C3)
      (value 100nF)
      (footprint Capacitor_THT:C_Rect_L7.0mm_W2.0mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61A75BA9))
    (comp (ref R14)
      (value 10k)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 61A3FDCC))
    (comp (ref U3)
      (value MCP1700-3302E_TO92)
      (footprint Package_TO_SOT_THT:TO-92_Inline)
      (datasheet http://ww1.microchip.com/downloads/en/DeviceDoc/20001826D.pdf)
      (libsource (lib Regulator_Linear) (part MCP1700-3302E_TO92) (description "250mA Low Quiscent Current LDO, 3.3V output, TO-92"))
      (sheetpath (names "/TashTwenty Tiny Connector/") (tstamps /61A14260/))
      (tstamp 61A62B21))
    (comp (ref C2)
      (value 2.2uF)
      (footprint Capacitor_THT:CP_Radial_D4.0mm_P1.50mm)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names "/TashTwenty Tiny Connector/") (tstamps /61A14260/))
      (tstamp 61A6754A))
    (comp (ref C1)
      (value 2.2uF)
      (footprint Capacitor_THT:CP_Radial_D4.0mm_P1.50mm)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names "/TashTwenty Tiny Connector/") (tstamps /61A14260/))
      (tstamp 61A68F66))
    (comp (ref C4)
      (value 100nF)
      (footprint Capacitor_THT:C_Rect_L7.0mm_W2.0mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/TashTwenty Tiny Connector/") (tstamps /61A14260/))
      (tstamp 61AA1BC9))
    (comp (ref J2)
      (value IDC20)
      (footprint Connector_IDC:IDC-Header_2x10_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x10_Odd_Even) (description "Generic connector, double row, 02x10, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names "/TashTwenty Tiny Connector/") (tstamps /61A14260/))
      (tstamp 61AFDBC1))
    (comp (ref J3)
      (value Conn_01x02)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x02) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names "/TashTwenty Tiny Connector/") (tstamps /61A14260/))
      (tstamp 61A1A4B6))
    (comp (ref H1)
      (value M3)
      (footprint MountingHole:MountingHole_3.2mm_M3_Pad)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names "/TashTwenty Tiny Connector/") (tstamps /61A14260/))
      (tstamp 61A418A3))
    (comp (ref H3)
      (value M3)
      (footprint MountingHole:MountingHole_3.2mm_M3_Pad)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names "/TashTwenty Tiny Connector/") (tstamps /61A14260/))
      (tstamp 61A44BCB))
    (comp (ref H2)
      (value M3)
      (footprint MountingHole:MountingHole_3.2mm_M3_Pad)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names "/TashTwenty Tiny Connector/") (tstamps /61A14260/))
      (tstamp 61A45CB6))
    (comp (ref D1)
      (value LED)
      (footprint LED_THT:LED_D5.0mm)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names "/TashTwenty Tiny LEDs/") (tstamps /61A5C73E/))
      (tstamp 61A7E10E))
    (comp (ref R8)
      (value 1200)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/TashTwenty Tiny LEDs/") (tstamps /61A5C73E/))
      (tstamp 61A7F7FD))
    (comp (ref D2)
      (value LED_Dual_ACA)
      (footprint LED_THT:LED_D5.0mm-3)
      (datasheet ~)
      (libsource (lib Device) (part LED_Dual_ACA) (description "Dual LED, common cathode on pin 2"))
      (sheetpath (names "/TashTwenty Tiny LEDs/") (tstamps /61A5C73E/))
      (tstamp 61A8E744))
    (comp (ref R11)
      (value 330)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/TashTwenty Tiny LEDs/") (tstamps /61A5C73E/))
      (tstamp 61A90834))
    (comp (ref R10)
      (value 330)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/TashTwenty Tiny LEDs/") (tstamps /61A5C73E/))
      (tstamp 61A90C1F))
    (comp (ref R9)
      (value 10k)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/TashTwenty Tiny LEDs/") (tstamps /61A5C73E/))
      (tstamp 61A96CB0))
    (comp (ref R13)
      (value 10k)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/TashTwenty Tiny LEDs/") (tstamps /61A5C73E/))
      (tstamp 61AB25BF))
    (comp (ref Q1)
      (value BC337)
      (footprint Package_TO_SOT_THT:TO-92_Inline)
      (datasheet https://diotec.com/tl_files/diotec/files/pdf/datasheets/bc337.pdf)
      (libsource (lib Transistor_BJT) (part BC337) (description "0.8A Ic, 45V Vce, NPN Transistor, TO-92"))
      (sheetpath (names "/TashTwenty Tiny LEDs/") (tstamps /61A5C73E/))
      (tstamp 61AB9694))
    (comp (ref R12)
      (value 10k)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/TashTwenty Tiny LEDs/") (tstamps /61A5C73E/))
      (tstamp 61ABBEBE)))
  (libparts
    (libpart (lib 74xx) (part 74LS08)
      (description "Quad And2")
      (docs http://www.ti.com/lit/gpn/sn74LS08)
      (footprints
        (fp DIP*W7.62mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS08))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type input))
        (pin (num 3) (name ~) (type output))
        (pin (num 4) (name ~) (type input))
        (pin (num 5) (name ~) (type input))
        (pin (num 6) (name ~) (type output))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name ~) (type output))
        (pin (num 9) (name ~) (type input))
        (pin (num 10) (name ~) (type input))
        (pin (num 11) (name ~) (type output))
        (pin (num 12) (name ~) (type input))
        (pin (num 13) (name ~) (type input))
        (pin (num 14) (name VCC) (type power_in))))
    (libpart (lib Connector) (part SD_Card)
      (description "SD Card Reader")
      (docs http://portal.fciconnect.com/Comergent//fci/drawing/10067847.pdf)
      (footprints
        (fp SD*))
      (fields
        (field (name Reference) J)
        (field (name Value) SD_Card))
      (pins
        (pin (num 1) (name CD/DAT3) (type input))
        (pin (num 2) (name CMD) (type input))
        (pin (num 3) (name VSS) (type power_in))
        (pin (num 4) (name VDD) (type power_in))
        (pin (num 5) (name CLK) (type input))
        (pin (num 6) (name VSS) (type power_in))
        (pin (num 7) (name DAT0) (type input))
        (pin (num 8) (name DAT1) (type input))
        (pin (num 9) (name DAT2) (type input))
        (pin (num 10) (name CARD_DETECT) (type input))
        (pin (num 11) (name WRITE_PROTECT) (type input))
        (pin (num 12) (name SHELL1) (type input))
        (pin (num 13) (name SHELL2) (type input))))
    (libpart (lib Connector_Generic) (part Conn_01x02)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x10_Odd_Even)
      (description "Generic connector, double row, 02x10, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x10_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))
        (pin (num 17) (name Pin_17) (type passive))
        (pin (num 18) (name Pin_18) (type passive))
        (pin (num 19) (name Pin_19) (type passive))
        (pin (num 20) (name Pin_20) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part CP)
      (description "Polarized capacitor")
      (docs ~)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part LED)
      (description "Light emitting diode")
      (docs ~)
      (footprints
        (fp LED*)
        (fp LED_SMD:*)
        (fp LED_THT:*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part LED_Dual_ACA)
      (description "Dual LED, common cathode on pin 2")
      (docs ~)
      (footprints
        (fp LED*)
        (fp LED_SMD:*)
        (fp LED_THT:*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED_Dual_ACA))
      (pins
        (pin (num 1) (name A1) (type input))
        (pin (num 2) (name K) (type input))
        (pin (num 3) (name A2) (type input))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Mechanical) (part MountingHole)
      (description "Mounting Hole without connection")
      (docs ~)
      (footprints
        (fp MountingHole*))
      (fields
        (field (name Reference) H)
        (field (name Value) MountingHole)))
    (libpart (lib PIC16F1825-IP) (part PIC16F1825-IP)
      (aliases
        (alias PIC16F1825-ISL)
        (alias PIC16F1825-ISO)
        (alias PIC16F1825-ISS)
        (alias PIC16F1825-IST))
      (description "Flash-Based, 8-Bit CMOS Microcontrollers, PDIP")
      (docs http://ww1.microchip.com/downloads/en/DeviceDoc/41440C.pdf)
      (footprints
        (fp DIP*W7.62mm*)
        (fp SOIC*3.9x8.7mm*P1.27mm*)
        (fp TSSOP*4.4x5mm*P0.65mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) PIC16F1825-IP))
      (pins
        (pin (num 1) (name VDD) (type power_in))
        (pin (num 2) (name RA5) (type BiDi))
        (pin (num 3) (name RA4) (type BiDi))
        (pin (num 4) (name RA3/MCLR/VPP) (type BiDi))
        (pin (num 5) (name RC5) (type BiDi))
        (pin (num 6) (name RC4) (type BiDi))
        (pin (num 7) (name RC3) (type BiDi))
        (pin (num 8) (name RC2) (type BiDi))
        (pin (num 9) (name RC1) (type BiDi))
        (pin (num 10) (name RC0) (type BiDi))
        (pin (num 11) (name RA2) (type BiDi))
        (pin (num 12) (name RA1/ICSPCLK) (type BiDi))
        (pin (num 13) (name RA0/ICSPDAT) (type BiDi))
        (pin (num 14) (name VSS) (type power_in))))
    (libpart (lib Regulator_Linear) (part LM79L05_TO92)
      (aliases
        (alias LM79L12_TO92)
        (alias LM79L15_TO92)
        (alias L79L05_TO92)
        (alias L79L08_TO92)
        (alias L79L12_TO92)
        (alias L79L15_TO92)
        (alias MCP1700-3002E_TO92)
        (alias MCP1700-1202E_TO92)
        (alias MCP1700-1802E_TO92)
        (alias MCP1700-2502E_TO92)
        (alias MCP1700-2802E_TO92)
        (alias MCP1700-3302E_TO92)
        (alias MCP1700-5002E_TO92))
      (description "3-Terminal Negative Regulator, -5V, TO-92")
      (docs http://www.ti.com/lit/ds/symlink/lm79l.pdf)
      (footprints
        (fp TO?92*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM79L05_TO92)
        (field (name Footprint) Package_TO_SOT_THT:TO-92_Inline))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name VI) (type power_in))
        (pin (num 3) (name VO) (type power_out))))
    (libpart (lib Transistor_BJT) (part BC547)
      (aliases
        (alias BC546)
        (alias BC548)
        (alias BC549)
        (alias BC550)
        (alias BC337)
        (alias BC338))
      (description "0.1A Ic, 45V Vce, Small Signal NPN Transistor, TO-92")
      (docs https://www.onsemi.com/pub/Collateral/BC550-D.pdf)
      (footprints
        (fp TO?92*))
      (fields
        (field (name Reference) Q)
        (field (name Value) BC547)
        (field (name Footprint) Package_TO_SOT_THT:TO-92_Inline))
      (pins
        (pin (num 1) (name C) (type passive))
        (pin (num 2) (name B) (type input))
        (pin (num 3) (name E) (type passive)))))
  (libraries
    (library (logical 74xx)
      (uri "/Library/Application Support/kicad/library/74xx.lib"))
    (library (logical Connector)
      (uri "/Library/Application Support/kicad/library/Connector.lib"))
    (library (logical Connector_Generic)
      (uri "/Library/Application Support/kicad/library/Connector_Generic.lib"))
    (library (logical Device)
      (uri "/Library/Application Support/kicad/library/Device.lib"))
    (library (logical Mechanical)
      (uri "/Library/Application Support/kicad/library/Mechanical.lib"))
    (library (logical PIC16F1825-IP)
      (uri "/Users/demik/github/oldworld/EDA/TashTwenty Tiny/PIC16F1825-IP.lib"))
    (library (logical Regulator_Linear)
      (uri "/Library/Application Support/kicad/library/Regulator_Linear.lib"))
    (library (logical Transistor_BJT)
      (uri "/Library/Application Support/kicad/library/Transistor_BJT.lib")))
  (nets
    (net (code 1) (name +5V)
      (node (ref U1) (pin 1))
      (node (ref R7) (pin 1))
      (node (ref R13) (pin 1))
      (node (ref R9) (pin 1))
      (node (ref J2) (pin 11))
      (node (ref C3) (pin 2))
      (node (ref U3) (pin 2))
      (node (ref C2) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref U2) (pin 14)))
    (net (code 2) (name "Net-(U1-Pad13)")
      (node (ref U1) (pin 13)))
    (net (code 3) (name "Net-(J1-Pad10)")
      (node (ref J1) (pin 10)))
    (net (code 4) (name "Net-(J1-Pad11)")
      (node (ref J1) (pin 11)))
    (net (code 5) (name "Net-(J1-Pad13)")
      (node (ref J1) (pin 13)))
    (net (code 6) (name "Net-(J1-Pad8)")
      (node (ref J1) (pin 8)))
    (net (code 7) (name "Net-(J1-Pad9)")
      (node (ref J1) (pin 9)))
    (net (code 8) (name +3V3)
      (node (ref C1) (pin 1))
      (node (ref U3) (pin 3))
      (node (ref J1) (pin 4))
      (node (ref R14) (pin 1)))
    (net (code 9) (name /MMC_SCK)
      (node (ref U1) (pin 10))
      (node (ref R1) (pin 1)))
    (net (code 10) (name /MMC_SCK_LV)
      (node (ref R2) (pin 1))
      (node (ref J1) (pin 5))
      (node (ref R1) (pin 2)))
    (net (code 11) (name GND)
      (node (ref J2) (pin 3))
      (node (ref R6) (pin 2))
      (node (ref Q1) (pin 3))
      (node (ref U1) (pin 14))
      (node (ref D2) (pin 2))
      (node (ref U2) (pin 7))
      (node (ref D1) (pin 1))
      (node (ref C4) (pin 2))
      (node (ref C3) (pin 1))
      (node (ref R4) (pin 2))
      (node (ref R2) (pin 2))
      (node (ref J2) (pin 7))
      (node (ref U3) (pin 1))
      (node (ref J2) (pin 5))
      (node (ref J2) (pin 1))
      (node (ref C2) (pin 2))
      (node (ref J1) (pin 12))
      (node (ref C1) (pin 2))
      (node (ref J1) (pin 3))
      (node (ref J1) (pin 6)))
    (net (code 12) (name /~MMC_CS)
      (node (ref R3) (pin 1))
      (node (ref U1) (pin 7)))
    (net (code 13) (name RD)
      (node (ref J2) (pin 16))
      (node (ref U2) (pin 5))
      (node (ref U1) (pin 6)))
    (net (code 14) (name WR)
      (node (ref U2) (pin 10))
      (node (ref J2) (pin 18))
      (node (ref U1) (pin 5)))
    (net (code 15) (name /MMC_MOSI)
      (node (ref U1) (pin 8))
      (node (ref R5) (pin 1)))
    (net (code 16) (name /MMC_MISO)
      (node (ref U1) (pin 9))
      (node (ref U2) (pin 11)))
    (net (code 17) (name ~ENABLE)
      (node (ref U2) (pin 2))
      (node (ref U1) (pin 2))
      (node (ref J3) (pin 2)))
    (net (code 18) (name PH3)
      (node (ref U1) (pin 3))
      (node (ref J2) (pin 8)))
    (net (code 19) (name PH2)
      (node (ref U1) (pin 4))
      (node (ref J2) (pin 6)))
    (net (code 20) (name PH1)
      (node (ref U1) (pin 11))
      (node (ref J2) (pin 4)))
    (net (code 21) (name PH0)
      (node (ref J2) (pin 2))
      (node (ref U1) (pin 12)))
    (net (code 22) (name /~MMC_CS_LV)
      (node (ref R3) (pin 2))
      (node (ref J1) (pin 1))
      (node (ref R4) (pin 1)))
    (net (code 23) (name /MMC_MOSI_LV)
      (node (ref R5) (pin 2))
      (node (ref R6) (pin 1))
      (node (ref J1) (pin 2)))
    (net (code 24) (name "Net-(R7-Pad2)")
      (node (ref U2) (pin 12))
      (node (ref R7) (pin 2)))
    (net (code 25) (name /MMC_MISO_LV)
      (node (ref U2) (pin 13))
      (node (ref J1) (pin 7))
      (node (ref R14) (pin 2)))
    (net (code 26) (name +12V)
      (node (ref J2) (pin 17))
      (node (ref J2) (pin 19))
      (node (ref R8) (pin 1))
      (node (ref J2) (pin 15))
      (node (ref J2) (pin 13)))
    (net (code 27) (name "Net-(J2-Pad10)")
      (node (ref J2) (pin 10)))
    (net (code 28) (name "Net-(J2-Pad12)")
      (node (ref J2) (pin 12)))
    (net (code 29) (name "Net-(J2-Pad20)")
      (node (ref J2) (pin 20)))
    (net (code 30) (name "Net-(J2-Pad9)")
      (node (ref J2) (pin 9)))
    (net (code 31) (name "Net-(J2-Pad14)")
      (node (ref J3) (pin 1))
      (node (ref J2) (pin 14)))
    (net (code 32) (name "Net-(D1-Pad2)")
      (node (ref D1) (pin 2))
      (node (ref R8) (pin 2)))
    (net (code 33) (name "Net-(Q1-Pad1)")
      (node (ref R13) (pin 2))
      (node (ref Q1) (pin 1))
      (node (ref U2) (pin 9))
      (node (ref U2) (pin 4)))
    (net (code 34) (name "Net-(D2-Pad3)")
      (node (ref R10) (pin 1))
      (node (ref D2) (pin 3)))
    (net (code 35) (name "Net-(D2-Pad1)")
      (node (ref R11) (pin 1))
      (node (ref D2) (pin 1)))
    (net (code 36) (name "Net-(R11-Pad2)")
      (node (ref R11) (pin 2))
      (node (ref U2) (pin 8)))
    (net (code 37) (name "Net-(R10-Pad2)")
      (node (ref U2) (pin 6))
      (node (ref R10) (pin 2)))
    (net (code 38) (name "Net-(R9-Pad2)")
      (node (ref R9) (pin 2))
      (node (ref U2) (pin 1)))
    (net (code 39) (name "Net-(Q1-Pad2)")
      (node (ref R12) (pin 1))
      (node (ref Q1) (pin 2)))
    (net (code 40) (name "Net-(R12-Pad2)")
      (node (ref R12) (pin 2))
      (node (ref U2) (pin 3)))))