(module PowerMac_PDS (layer F.Cu) (tedit 5EB2A446)
  (fp_text reference "PowerMac PDS" (at 0 -5.08) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value PowerMac_PDS (at 0 -3.04) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user 92 (at -58.42 -2.54 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user 140 (at 2.54 -2.54 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user 141 (at 6.35 -2.54 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.2)))
  )
  (fp_text user 182 (at 58.42 -2.54 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.2)))
  )
  (fp_text user 1 (at -58.42 -2.54 90) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (fp_text user 49 (at 2.54 -2.54 90) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (fp_text user 50 (at 6.35 -2.54 90) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (fp_text user 91 (at 58.42 -2.54 90) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (pad 92 connect rect (at -58.42 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 93 connect rect (at -57.15 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 94 connect rect (at -55.88 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 95 connect rect (at -54.61 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 96 connect rect (at -53.34 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 97 connect rect (at -52.07 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 98 connect rect (at -50.8 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 99 connect rect (at -49.53 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 100 connect rect (at -48.26 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 101 connect rect (at -46.99 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 102 connect rect (at -45.72 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 103 connect rect (at -44.45 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 104 connect rect (at -43.18 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 105 connect rect (at -41.91 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 106 connect rect (at -40.64 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 107 connect rect (at -39.37 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 108 connect rect (at -38.1 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 109 connect rect (at -36.83 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 110 connect rect (at -35.56 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 111 connect rect (at -34.29 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 112 connect rect (at -33.02 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 113 connect rect (at -31.75 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 114 connect rect (at -30.48 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 115 connect rect (at -29.21 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 116 connect rect (at -27.94 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 117 connect rect (at -26.67 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 118 connect rect (at -25.4 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 119 connect rect (at -24.13 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 120 connect rect (at -22.86 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 121 connect rect (at -21.59 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 122 connect rect (at -20.32 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 123 connect rect (at -19.05 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 124 connect rect (at -17.78 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 125 connect rect (at -16.51 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 126 connect rect (at -15.24 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 127 connect rect (at -13.97 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 128 connect rect (at -12.7 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 129 connect rect (at -11.43 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 130 connect rect (at -10.16 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 131 connect rect (at -8.89 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 132 connect rect (at -7.62 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 133 connect rect (at -6.35 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 134 connect rect (at -5.08 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 135 connect rect (at -3.81 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 136 connect rect (at -2.54 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 137 connect rect (at -1.27 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 138 connect rect (at 0 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 139 connect rect (at 1.27 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 140 connect rect (at 2.54 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 141 connect rect (at 6.35 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 142 connect rect (at 7.62 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 143 connect rect (at 8.89 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 144 connect rect (at 10.16 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 145 connect rect (at 11.43 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 146 connect rect (at 12.7 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 147 connect rect (at 13.97 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 148 connect rect (at 15.24 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 149 connect rect (at 16.51 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 150 connect rect (at 17.78 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 151 connect rect (at 19.05 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 152 connect rect (at 20.32 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 153 connect rect (at 21.59 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 154 connect rect (at 22.86 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 155 connect rect (at 24.13 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 156 connect rect (at 25.4 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 157 connect rect (at 26.67 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 158 connect rect (at 27.94 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 159 connect rect (at 29.21 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 160 connect rect (at 30.48 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 161 connect rect (at 31.75 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 162 connect rect (at 33.02 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 163 connect rect (at 34.29 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 164 connect rect (at 35.56 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 165 connect rect (at 36.83 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 166 connect rect (at 38.1 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 167 connect rect (at 39.37 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 168 connect rect (at 40.64 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 169 connect rect (at 41.91 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 170 connect rect (at 43.18 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 171 connect rect (at 44.45 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 172 connect rect (at 45.72 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 173 connect rect (at 46.99 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 174 connect rect (at 48.26 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 175 connect rect (at 49.53 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 176 connect rect (at 50.8 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 177 connect rect (at 52.07 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 178 connect rect (at 53.34 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 179 connect rect (at 54.61 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 180 connect rect (at 55.88 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 181 connect rect (at 57.15 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 182 connect rect (at 58.42 0) (size 1.04 3.81) (layers F.Cu F.Mask))
  (pad 1 connect rect (at -58.42 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 2 connect rect (at -57.15 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 3 connect rect (at -55.88 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 4 connect rect (at -54.61 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 5 connect rect (at -53.34 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 6 connect rect (at -52.07 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 7 connect rect (at -50.8 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 8 connect rect (at -49.53 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 9 connect rect (at -48.26 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 10 connect rect (at -46.99 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 11 connect rect (at -45.72 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 12 connect rect (at -44.45 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 13 connect rect (at -43.18 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 14 connect rect (at -41.91 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 15 connect rect (at -40.64 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 16 connect rect (at -39.37 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 17 connect rect (at -38.1 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 18 connect rect (at -36.83 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 19 connect rect (at -35.56 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 20 connect rect (at -34.29 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 21 connect rect (at -33.02 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 22 connect rect (at -31.75 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 23 connect rect (at -30.48 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 24 connect rect (at -29.21 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 25 connect rect (at -27.94 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 26 connect rect (at -26.67 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 27 connect rect (at -25.4 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 28 connect rect (at -24.13 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 29 connect rect (at -22.86 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 30 connect rect (at -21.59 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 31 connect rect (at -20.32 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 32 connect rect (at -19.05 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 33 connect rect (at -17.78 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 34 connect rect (at -16.51 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 35 connect rect (at -15.24 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 36 connect rect (at -13.97 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 37 connect rect (at -12.7 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 38 connect rect (at -11.43 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 39 connect rect (at -10.16 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 40 connect rect (at -8.89 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 41 connect rect (at -7.62 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 42 connect rect (at -6.35 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 43 connect rect (at -5.08 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 44 connect rect (at -3.81 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 45 connect rect (at -2.54 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 46 connect rect (at -1.27 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 47 connect rect (at 0 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 48 connect rect (at 1.27 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 49 connect rect (at 2.54 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 50 connect rect (at 6.35 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 51 connect rect (at 7.62 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 52 connect rect (at 8.89 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 53 connect rect (at 10.16 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 54 connect rect (at 11.43 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 55 connect rect (at 12.7 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 56 connect rect (at 13.97 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 57 connect rect (at 15.24 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 58 connect rect (at 16.51 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 59 connect rect (at 17.78 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 60 connect rect (at 19.05 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 61 connect rect (at 20.32 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 62 connect rect (at 21.59 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 63 connect rect (at 22.86 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 64 connect rect (at 24.13 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 65 connect rect (at 25.4 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 66 connect rect (at 26.67 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 67 connect rect (at 27.94 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 68 connect rect (at 29.21 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 69 connect rect (at 30.48 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 70 connect rect (at 31.75 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 71 connect rect (at 33.02 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 72 connect rect (at 34.29 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 73 connect rect (at 35.56 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 74 connect rect (at 36.83 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 75 connect rect (at 38.1 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 76 connect rect (at 39.37 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 77 connect rect (at 40.64 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 78 connect rect (at 41.91 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 79 connect rect (at 43.18 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 80 connect rect (at 44.45 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 81 connect rect (at 45.72 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 82 connect rect (at 46.99 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 83 connect rect (at 48.26 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 84 connect rect (at 49.53 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 85 connect rect (at 50.8 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 86 connect rect (at 52.07 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 87 connect rect (at 53.34 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 88 connect rect (at 54.61 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 89 connect rect (at 55.88 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 90 connect rect (at 57.15 0) (size 1.04 3.81) (layers B.Cu B.Mask))
  (pad 91 connect rect (at 58.42 0) (size 1.04 3.81) (layers B.Cu B.Mask))
)
