(kicad_pcb (version 20171130) (host pcbnew "(5.1.5-0-10_14)")

  (general
    (thickness 1.6)
    (drawings 26)
    (tracks 1229)
    (zones 0)
    (modules 34)
    (nets 100)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu power)
    (2 In2.Cu signal)
    (31 B.Cu power)
    (32 B.Adhes user)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.15)
    (user_trace_width 0.15)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.35)
    (user_trace_width 0.4)
    (user_trace_width 0.45)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (user_trace_width 1.27)
    (user_trace_width 1.524)
    (trace_clearance 0.15)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.15)
    (via_size 0.5)
    (via_drill 0.2)
    (via_min_size 0.5)
    (via_min_drill 0.2)
    (user_via 0.6 0.3)
    (user_via 0.8 0.4)
    (user_via 1 0.5)
    (user_via 1.524 0.762)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.1524)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.05 1.4)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0762)
    (solder_mask_min_width 0.127)
    (pad_to_paste_clearance -0.0381)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f8_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )

  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 /A4)
  (net 4 /D7)
  (net 5 /D6)
  (net 6 /A8)
  (net 7 /A7)
  (net 8 /A6)
  (net 9 /A5)
  (net 10 /A3)
  (net 11 /A2)
  (net 12 /A1)
  (net 13 /A0)
  (net 14 /A9)
  (net 15 /D1)
  (net 16 /D5)
  (net 17 /D0)
  (net 18 /D2)
  (net 19 /D3)
  (net 20 /D4)
  (net 21 /A10)
  (net 22 +12V)
  (net 23 -12V)
  (net 24 -5V)
  (net 25 /~IOSEL~)
  (net 26 /A11)
  (net 27 /A12)
  (net 28 /A13)
  (net 29 /A14)
  (net 30 /A15)
  (net 31 /~IOSTRB~)
  (net 32 /RDY)
  (net 33 /DMA)
  (net 34 /~NMI~)
  (net 35 /~IRQ~)
  (net 36 /~RES~)
  (net 37 /~INH~)
  (net 38 /COLORREF)
  (net 39 /7M)
  (net 40 /Q3)
  (net 41 /PHI1)
  (net 42 /USER1)
  (net 43 /PHI0)
  (net 44 /~DEVSEL~)
  (net 45 /INTin)
  (net 46 /DMAin)
  (net 47 /VIDSYNC)
  (net 48 /R~CS~)
  (net 49 /RA15)
  (net 50 /RA16)
  (net 51 /RA14)
  (net 52 /RA12)
  (net 53 /RD7)
  (net 54 /RD6)
  (net 55 /RD5)
  (net 56 /RD4)
  (net 57 /RD3)
  (net 58 /RD2)
  (net 59 /RD1)
  (net 60 /RD0)
  (net 61 /BankAB)
  (net 62 /ENWR1)
  (net 63 /ENRD)
  (net 64 /ENWR)
  (net 65 "Net-(U1-Pad9)")
  (net 66 /ENWR1A0)
  (net 67 "Net-(U3-Pad12)")
  (net 68 /~A0XOR1~)
  (net 69 "Net-(U5-Pad2)")
  (net 70 "Net-(U5-Pad4)")
  (net 71 "Net-(U5-Pad6)")
  (net 72 "Net-(U5-Pad8)")
  (net 73 /RCS)
  (net 74 "Net-(U5-Pad12)")
  (net 75 "Net-(U10-Pad1)")
  (net 76 "Net-(U10-Pad2)")
  (net 77 "Net-(U10-Pad4)")
  (net 78 "Net-(U10-Pad5)")
  (net 79 "Net-(U10-Pad10)")
  (net 80 "Net-(U8-Pad11)")
  (net 81 "Net-(U10-Pad9)")
  (net 82 "Net-(U9-Pad10)")
  (net 83 "Net-(U10-Pad8)")
  (net 84 /INHOE)
  (net 85 "Net-(U10-Pad11)")
  (net 86 "Net-(U3-Pad15)")
  (net 87 "Net-(U4-Pad15)")
  (net 88 "Net-(U3-Pad16)")
  (net 89 "Net-(U4-Pad16)")
  (net 90 "Net-(U4-Pad12)")
  (net 91 "Net-(U4-Pad9)")
  (net 92 "Net-(U3-Pad19)")
  (net 93 "Net-(U4-Pad19)")
  (net 94 "Net-(U7-Pad11)")
  (net 95 "Net-(U7-Pad8)")
  (net 96 "Net-(U6-Pad8)")
  (net 97 /~A2~clk)
  (net 98 /A2clk)
  (net 99 /R~W~)

  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.15)
    (via_dia 0.5)
    (via_drill 0.2)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +5V)
    (add_net -12V)
    (add_net -5V)
    (add_net /7M)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A2)
    (add_net /A2clk)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /BankAB)
    (add_net /COLORREF)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /DMA)
    (add_net /DMAin)
    (add_net /ENRD)
    (add_net /ENWR)
    (add_net /ENWR1)
    (add_net /ENWR1A0)
    (add_net /INHOE)
    (add_net /INTin)
    (add_net /PHI0)
    (add_net /PHI1)
    (add_net /Q3)
    (add_net /RA12)
    (add_net /RA14)
    (add_net /RA15)
    (add_net /RA16)
    (add_net /RCS)
    (add_net /RD0)
    (add_net /RD1)
    (add_net /RD2)
    (add_net /RD3)
    (add_net /RD4)
    (add_net /RD5)
    (add_net /RD6)
    (add_net /RD7)
    (add_net /RDY)
    (add_net /R~CS~)
    (add_net /R~W~)
    (add_net /USER1)
    (add_net /VIDSYNC)
    (add_net /~A0XOR1~)
    (add_net /~A2~clk)
    (add_net /~DEVSEL~)
    (add_net /~INH~)
    (add_net /~IOSEL~)
    (add_net /~IOSTRB~)
    (add_net /~IRQ~)
    (add_net /~NMI~)
    (add_net /~RES~)
    (add_net GND)
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U10-Pad1)")
    (add_net "Net-(U10-Pad10)")
    (add_net "Net-(U10-Pad11)")
    (add_net "Net-(U10-Pad2)")
    (add_net "Net-(U10-Pad4)")
    (add_net "Net-(U10-Pad5)")
    (add_net "Net-(U10-Pad8)")
    (add_net "Net-(U10-Pad9)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U3-Pad15)")
    (add_net "Net-(U3-Pad16)")
    (add_net "Net-(U3-Pad19)")
    (add_net "Net-(U4-Pad12)")
    (add_net "Net-(U4-Pad15)")
    (add_net "Net-(U4-Pad16)")
    (add_net "Net-(U4-Pad19)")
    (add_net "Net-(U4-Pad9)")
    (add_net "Net-(U5-Pad12)")
    (add_net "Net-(U5-Pad2)")
    (add_net "Net-(U5-Pad4)")
    (add_net "Net-(U5-Pad6)")
    (add_net "Net-(U5-Pad8)")
    (add_net "Net-(U6-Pad8)")
    (add_net "Net-(U7-Pad11)")
    (add_net "Net-(U7-Pad8)")
    (add_net "Net-(U8-Pad11)")
    (add_net "Net-(U9-Pad10)")
  )

  (module stdpads:C_0805 (layer F.Cu) (tedit 5F02840E) (tstamp 5DE2B4F2)
    (at 136.31 127.889 180)
    (tags capacitor)
    (path /5F64DEF7)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference C11 (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 10u (at 0 0.35) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text user %R (at 0 0 180) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_line (start 1.7 1) (end -1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1) (end 1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1) (end 1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1) (end -1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.15))
    (pad 2 smd roundrect (at 0.85 0 180) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.85 0 180) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0805 (layer F.Cu) (tedit 5F02840E) (tstamp 5F5E73A5)
    (at 71.25 126.3 180)
    (tags capacitor)
    (path /5E8640A9)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference C12 (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 10u (at 0 0.35) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text user %R (at 0 0 180) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_line (start 1.7 1) (end -1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1) (end 1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1) (end 1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1) (end -1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.15))
    (pad 2 smd roundrect (at 0.85 0 180) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.85 0 180) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:R_0805 (layer F.Cu) (tedit 5F027DD1) (tstamp 5F5D2D24)
    (at 118.3 125.55 180)
    (tags resistor)
    (path /5E6C502A)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference R1 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 3k3 (at 0 0.35) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text user %R (at 0 0 180) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_line (start 1.7 1) (end -1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1) (end 1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1) (end 1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1) (end -1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.1))
    (pad 2 smd roundrect (at 0.95 0 180) (size 0.85 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 /~INH~))
    (pad 1 smd roundrect (at -0.95 0 180) (size 0.85 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:PasteHole_1.152mm_NPTH (layer F.Cu) (tedit 5F27B084) (tstamp 5F7416FC)
    (at 136.906 122.301 270)
    (descr "Circular Fiducial, 1mm bare copper top; 2mm keepout (Level A)")
    (tags marker)
    (path /5F924B0A)
    (attr virtual)
    (fp_text reference H5 (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (fp_text value " " (at 0 2 90) (layer F.Fab) hide
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_circle (center 0 0) (end 1 0) (layer F.Fab) (width 0.1))
    (pad "" np_thru_hole circle (at 0 0 270) (size 1.152 1.152) (drill 1.152) (layers *.Cu *.Mask)
      (solder_mask_margin 0.148))
  )

  (module stdpads:SOT-353 (layer F.Cu) (tedit 5F739FE4) (tstamp 5F5D2CCD)
    (at 118.3 122.65 90)
    (tags "SOT-353 SC-70-5")
    (path /61E07386)
    (solder_mask_margin 0.04)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U11 (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 74AHCT1G126GW (at -1 0 180) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_line (start -1.6 -1.3) (end 1.6 -1.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 1.3) (end -1.6 -1.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.6 1.3) (end -1.6 1.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.6 -1.3) (end 1.6 1.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.73 1.16) (end 1.3 1.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.68 -1.16) (end -0.73 -1.16) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.67 1.1) (end 0.18 1.1) (layer F.Fab) (width 0.1))
    (fp_line (start 0.68 0.6) (end 0.68 -1.1) (layer F.Fab) (width 0.1))
    (fp_line (start -0.67 1.1) (end -0.67 -1.1) (layer F.Fab) (width 0.1))
    (fp_line (start -0.67 -1.1) (end 0.68 -1.1) (layer F.Fab) (width 0.1))
    (fp_line (start 0.18 1.1) (end 0.68 0.6) (layer F.Fab) (width 0.1))
    (pad 5 smd roundrect (at -0.85 0.65 270) (size 1 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 4 smd roundrect (at -0.85 -0.65 270) (size 1 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 /~INH~))
    (pad 2 smd roundrect (at 0.85 0 270) (size 1 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at 0.85 0.65 270) (size 1 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 /INHOE))
    (pad 3 smd roundrect (at 0.85 -0.65 270) (size 1 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-353_SC-70-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module stdpads:TSSOP-14_4.4x5mm_P0.65mm (layer F.Cu) (tedit 5F37C96A) (tstamp 5F8B1AFE)
    (at 104.45 122.6 180)
    (descr "14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /61D074CA)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U7 (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74HCT32PW (at 0 1 180) (layer F.Fab)
      (effects (font (size 0.381 0.381) (thickness 0.09525)))
    )
    (fp_text user %R (at 0 0 180) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_line (start -2.5 2.325) (end -2.5 3.675) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.625 2.325) (end 2.625 -2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.625 2.325) (end -2.625 -2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.625 2.325) (end 2.4 2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.625 -2.325) (end 2.4 -2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.625 -2.325) (end -2.4 -2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.625 2.325) (end -2.5 2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.8 3.95) (end 2.8 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.8 3.95) (end -2.8 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.8 -3.95) (end 2.8 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.8 3.95) (end 2.8 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.5 2.2) (end -2.5 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start 2.5 2.2) (end -1.5 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 2.5 -2.2) (end 2.5 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -2.5 -2.2) (end 2.5 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -2.5 1.2) (end -2.5 -2.2) (layer F.Fab) (width 0.15))
    (pad 14 smd roundrect (at -1.95 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 13 smd roundrect (at -1.3 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 12 smd roundrect (at -0.65 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 11 smd roundrect (at 0 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 "Net-(U7-Pad11)"))
    (pad 10 smd roundrect (at 0.65 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 9 smd roundrect (at 1.3 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 8 smd roundrect (at 1.95 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 95 "Net-(U7-Pad8)"))
    (pad 7 smd roundrect (at 1.95 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 6 smd roundrect (at 1.3 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 97 /~A2~clk))
    (pad 5 smd roundrect (at 0.65 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 /~DEVSEL~))
    (pad 4 smd roundrect (at 0 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /A2))
    (pad 3 smd roundrect (at -0.65 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 /A2clk))
    (pad 2 smd roundrect (at -1.3 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 /~DEVSEL~))
    (pad 1 smd roundrect (at -1.95 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(U5-Pad6)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:TSSOP-14_4.4x5mm_P0.65mm (layer F.Cu) (tedit 5F37C96A) (tstamp 5F8B1E88)
    (at 97.15 122.6 180)
    (descr "14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /61D062D6)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U6 (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74HCT08PW (at 0 1 180) (layer F.Fab)
      (effects (font (size 0.381 0.381) (thickness 0.09525)))
    )
    (fp_line (start -2.5 1.2) (end -2.5 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -2.5 -2.2) (end 2.5 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 2.5 -2.2) (end 2.5 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 2.5 2.2) (end -1.5 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -1.5 2.2) (end -2.5 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start -2.8 3.95) (end 2.8 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.8 -3.95) (end 2.8 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.8 3.95) (end -2.8 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.8 3.95) (end 2.8 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.625 2.325) (end -2.5 2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.625 -2.325) (end -2.4 -2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.625 -2.325) (end 2.4 -2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.625 2.325) (end 2.4 2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.625 2.325) (end -2.625 -2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.625 2.325) (end 2.625 -2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.5 2.325) (end -2.5 3.675) (layer F.SilkS) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 1 smd roundrect (at -1.95 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(U5-Pad2)"))
    (pad 2 smd roundrect (at -1.3 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(U5-Pad4)"))
    (pad 3 smd roundrect (at -0.65 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(U10-Pad1)"))
    (pad 4 smd roundrect (at 0 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /A0))
    (pad 5 smd roundrect (at 0.65 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /A1))
    (pad 6 smd roundrect (at 1.3 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(U10-Pad2)"))
    (pad 7 smd roundrect (at 1.95 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 8 smd roundrect (at 1.95 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 "Net-(U6-Pad8)"))
    (pad 9 smd roundrect (at 1.3 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 10 smd roundrect (at 0.65 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 11 smd roundrect (at 0 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 /ENWR1A0))
    (pad 12 smd roundrect (at -0.65 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 /ENWR1))
    (pad 13 smd roundrect (at -1.3 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /A0))
    (pad 14 smd roundrect (at -1.95 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:TSSOP-14_4.4x5mm_P0.65mm (layer F.Cu) (tedit 5F37C96A) (tstamp 5F8AB3FE)
    (at 128.6 112.45 270)
    (descr "14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /61D0A2BD)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U10 (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74HCT32PW (at 0 1 270) (layer F.Fab)
      (effects (font (size 0.381 0.381) (thickness 0.09525)))
    )
    (fp_text user %R (at 0 0 270) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_line (start -2.5 2.325) (end -2.5 3.675) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.625 2.325) (end 2.625 -2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.625 2.325) (end -2.625 -2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.625 2.325) (end 2.4 2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.625 -2.325) (end 2.4 -2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.625 -2.325) (end -2.4 -2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.625 2.325) (end -2.5 2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.8 3.95) (end 2.8 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.8 3.95) (end -2.8 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.8 -3.95) (end 2.8 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.8 3.95) (end 2.8 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.5 2.2) (end -2.5 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start 2.5 2.2) (end -1.5 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 2.5 -2.2) (end 2.5 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -2.5 -2.2) (end 2.5 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -2.5 1.2) (end -2.5 -2.2) (layer F.Fab) (width 0.15))
    (pad 14 smd roundrect (at -1.95 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 13 smd roundrect (at -1.3 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 /A12))
    (pad 12 smd roundrect (at -0.65 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /A13))
    (pad 11 smd roundrect (at 0 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 "Net-(U10-Pad11)"))
    (pad 10 smd roundrect (at 0.65 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "Net-(U10-Pad10)"))
    (pad 9 smd roundrect (at 1.3 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(U10-Pad9)"))
    (pad 8 smd roundrect (at 1.95 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(U10-Pad8)"))
    (pad 7 smd roundrect (at 1.95 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 6 smd roundrect (at 1.3 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 /RA12))
    (pad 5 smd roundrect (at 0.65 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 "Net-(U10-Pad5)"))
    (pad 4 smd roundrect (at 0 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 "Net-(U10-Pad4)"))
    (pad 3 smd roundrect (at -0.65 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 /~A0XOR1~))
    (pad 2 smd roundrect (at -1.3 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(U10-Pad2)"))
    (pad 1 smd roundrect (at -1.95 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(U10-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 5F5CC4AD)
    (at 107.95 124.8 90)
    (tags capacitor)
    (path /61D5AB0B)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C7 (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.75 0 90) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.75 0 90) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:TSOP-I-32_18.4x8mm_P0.5mm (layer F.Cu) (tedit 5F599AB1) (tstamp 5F5EB7FE)
    (at 92.1 112.15 180)
    (descr "TSOP I, 32 pins, 18.4x8mm body (https://www.micron.com/~/media/documents/products/technical-note/nor-flash/tn1225_land_pad_design.pdf, http://www.fujitsu.com/downloads/MICRO/fma/pdfmcu/f32pm25.pdf)")
    (tags "TSOP I 32")
    (path /61C2B655)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.035)
    (attr smd)
    (fp_text reference U1 (at 0 0) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 621024 (at 0 1.25) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_line (start -8.2 -4) (end 9.2 -4) (layer F.Fab) (width 0.1))
    (fp_line (start -9.2 4) (end -9.2 -3) (layer F.Fab) (width 0.1))
    (fp_line (start 9.2 4) (end -9.2 4) (layer F.Fab) (width 0.1))
    (fp_line (start 9.2 -4) (end 9.2 4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_line (start -8.2 -4) (end -9.2 -3) (layer F.Fab) (width 0.1))
    (fp_line (start 9.2 -4.12) (end -10.2 -4.12) (layer F.SilkS) (width 0.1))
    (fp_line (start -9.2 4.12) (end 9.2 4.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -10.55 -4.25) (end 10.55 -4.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 10.55 -4.25) (end 10.55 4.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 10.55 4.25) (end -10.55 4.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -10.55 4.25) (end -10.55 -4.25) (layer F.CrtYd) (width 0.05))
    (pad 32 smd roundrect (at 9.75 -3.75 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 31 smd roundrect (at 9.75 -3.25 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /A13))
    (pad 30 smd roundrect (at 9.75 -2.75 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 /R~CS~))
    (pad 29 smd roundrect (at 9.75 -2.25 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 /RD3))
    (pad 28 smd roundrect (at 9.75 -1.75 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 /RD2))
    (pad 27 smd roundrect (at 9.75 -1.25 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 /RD1))
    (pad 26 smd roundrect (at 9.75 -0.75 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 /RD0))
    (pad 25 smd roundrect (at 9.75 -0.25 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 /RD7))
    (pad 24 smd roundrect (at 9.75 0.25 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 23 smd roundrect (at 9.75 0.75 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 /RD6))
    (pad 22 smd roundrect (at 9.75 1.25 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 /RD5))
    (pad 21 smd roundrect (at 9.75 1.75 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 /RD4))
    (pad 20 smd roundrect (at 9.75 2.25 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 /A11))
    (pad 19 smd roundrect (at 9.75 2.75 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /A10))
    (pad 18 smd roundrect (at 9.75 3.25 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /A9))
    (pad 16 smd roundrect (at -9.75 3.75 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /A4))
    (pad 15 smd roundrect (at -9.75 3.25 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /A5))
    (pad 14 smd roundrect (at -9.75 2.75 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 /RA12))
    (pad 13 smd roundrect (at -9.75 2.25 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /A6))
    (pad 12 smd roundrect (at -9.75 1.75 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 /RA14))
    (pad 11 smd roundrect (at -9.75 1.25 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 /RA15))
    (pad 10 smd roundrect (at -9.75 0.75 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 /RA16))
    (pad 9 smd roundrect (at -9.75 0.25 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(U1-Pad9)"))
    (pad 8 smd roundrect (at -9.75 -0.25 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 7 smd roundrect (at -9.75 -0.75 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /A7))
    (pad 6 smd roundrect (at -9.75 -1.25 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 5 smd roundrect (at -9.75 -1.75 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 /R~W~))
    (pad 4 smd roundrect (at -9.75 -2.25 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /A3))
    (pad 3 smd roundrect (at -9.75 -2.75 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /A2))
    (pad 2 smd roundrect (at -9.75 -3.25 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /A1))
    (pad 17 smd roundrect (at 9.75 3.75 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /A8))
    (pad 1 smd roundrect (at -9.75 -3.75 180) (size 1.1 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /A0))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSOP-I-32_18.4x8mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 5F8B1CE1)
    (at 86.05 124.8 90)
    (tags capacitor)
    (path /5D14D1B0)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C2 (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (pad 2 smd roundrect (at 0.75 0 90) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.75 0 90) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 5F8B1BF1)
    (at 126.3 124.8 90)
    (tags capacitor)
    (path /61D3AEA2)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C9 (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.75 0 90) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.75 0 90) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 5F8B1C21)
    (at 115.25 124.8 90)
    (tags capacitor)
    (path /61D3AE9C)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C8 (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (pad 2 smd roundrect (at 0.75 0 90) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.75 0 90) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 5F8B1C51)
    (at 93.35 124.8 90)
    (tags capacitor)
    (path /5E988E8B)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C5 (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.75 0 90) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.75 0 90) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:AppleIIBus_Edge (layer F.Cu) (tedit 5CFDB600) (tstamp 5D312B09)
    (at 106.68 135.382)
    (path /5CFC517D)
    (attr virtual)
    (fp_text reference J1 (at 25.4 -5.08) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AppleIIBus (at 0 5.207) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.1524)))
    )
    (fp_line (start -32.512 4.318) (end -32.512 -3.81) (layer B.Fab) (width 0.127))
    (fp_line (start 32.512 4.318) (end -32.512 4.318) (layer B.Fab) (width 0.127))
    (fp_line (start 32.512 -3.81) (end 32.512 4.318) (layer F.Fab) (width 0.127))
    (fp_line (start 32.512 4.318) (end -32.512 4.318) (layer F.Fab) (width 0.127))
    (fp_line (start -32.512 4.318) (end -32.512 -3.81) (layer F.Fab) (width 0.127))
    (fp_line (start 32.512 -3.81) (end 32.512 4.318) (layer B.Fab) (width 0.127))
    (fp_text user J1 (at 25.4 -5.08) (layer B.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (pad 26 smd roundrect (at 30.48 -0.1 180) (size 1.524 7.34) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 27 smd roundrect (at 27.94 -0.1 180) (size 1.524 7.34) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 46 /DMAin))
    (pad 28 smd roundrect (at 25.4 -0.1 180) (size 1.524 7.34) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 45 /INTin))
    (pad 50 smd roundrect (at -30.48 -0.1 180) (size 1.524 7.34) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 22 +12V))
    (pad 49 smd roundrect (at -27.94 -0.1 180) (size 1.524 7.34) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 17 /D0))
    (pad 48 smd roundrect (at -25.4 -0.1 180) (size 1.524 7.34) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 15 /D1))
    (pad 47 smd roundrect (at -22.86 -0.1 180) (size 1.524 7.34) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 18 /D2))
    (pad 46 smd roundrect (at -20.32 -0.1 180) (size 1.524 7.34) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 19 /D3))
    (pad 45 smd roundrect (at -17.78 -0.1 180) (size 1.524 7.34) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 20 /D4))
    (pad 44 smd roundrect (at -15.24 -0.1 180) (size 1.524 7.34) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 16 /D5))
    (pad 43 smd roundrect (at -12.7 -0.1 180) (size 1.524 7.34) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 5 /D6))
    (pad 42 smd roundrect (at -10.16 -0.1 180) (size 1.524 7.34) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 4 /D7))
    (pad 41 smd roundrect (at -7.62 -0.1 180) (size 1.524 7.34) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 44 /~DEVSEL~))
    (pad 40 smd roundrect (at -5.08 -0.1 180) (size 1.524 7.34) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 43 /PHI0))
    (pad 39 smd roundrect (at -2.54 -0.1 180) (size 1.524 7.34) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 42 /USER1))
    (pad 38 smd roundrect (at 0 -0.1 180) (size 1.524 7.34) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 41 /PHI1))
    (pad 37 smd roundrect (at 2.54 -0.1 180) (size 1.524 7.34) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 40 /Q3))
    (pad 36 smd roundrect (at 5.08 -0.1 180) (size 1.524 7.34) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 39 /7M))
    (pad 35 smd roundrect (at 7.62 -0.1 180) (size 1.524 7.34) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 38 /COLORREF))
    (pad 34 smd roundrect (at 10.16 -0.1 180) (size 1.524 7.34) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 24 -5V))
    (pad 33 smd roundrect (at 12.7 -0.1 180) (size 1.524 7.34) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 23 -12V))
    (pad 32 smd roundrect (at 15.24 -0.1 180) (size 1.524 7.34) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 37 /~INH~))
    (pad 31 smd roundrect (at 17.78 -0.1 180) (size 1.524 7.34) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 36 /~RES~))
    (pad 30 smd roundrect (at 20.32 -0.1 180) (size 1.524 7.34) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 35 /~IRQ~))
    (pad 29 smd roundrect (at 22.86 -0.1 180) (size 1.524 7.34) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 34 /~NMI~))
    (pad 25 smd roundrect (at 30.48 -0.1 180) (size 1.524 7.34) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 24 smd roundrect (at 27.94 -0.1 180) (size 1.524 7.34) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 46 /DMAin))
    (pad 23 smd roundrect (at 25.4 -0.1 180) (size 1.524 7.34) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 45 /INTin))
    (pad 22 smd roundrect (at 22.86 -0.1 180) (size 1.524 7.34) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 33 /DMA))
    (pad 21 smd roundrect (at 20.32 -0.1 180) (size 1.524 7.34) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 32 /RDY))
    (pad 20 smd roundrect (at 17.78 -0.1 180) (size 1.524 7.34) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 31 /~IOSTRB~))
    (pad 19 smd roundrect (at 15.24 -0.1 180) (size 1.524 7.34) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 47 /VIDSYNC))
    (pad 18 smd roundrect (at 12.7 -0.1 180) (size 1.524 7.34) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 99 /R~W~))
    (pad 17 smd roundrect (at 10.16 -0.1 180) (size 1.524 7.34) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 30 /A15))
    (pad 16 smd roundrect (at 7.62 -0.1 180) (size 1.524 7.34) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 29 /A14))
    (pad 15 smd roundrect (at 5.08 -0.1 180) (size 1.524 7.34) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 28 /A13))
    (pad 14 smd roundrect (at 2.54 -0.1 180) (size 1.524 7.34) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 27 /A12))
    (pad 13 smd roundrect (at 0 -0.1 180) (size 1.524 7.34) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 26 /A11))
    (pad 12 smd roundrect (at -2.54 -0.1 180) (size 1.524 7.34) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 21 /A10))
    (pad 11 smd roundrect (at -5.08 -0.1 180) (size 1.524 7.34) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 14 /A9))
    (pad 10 smd roundrect (at -7.62 -0.1 180) (size 1.524 7.34) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 6 /A8))
    (pad 9 smd roundrect (at -10.16 -0.1 180) (size 1.524 7.34) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 7 /A7))
    (pad 8 smd roundrect (at -12.7 -0.1 180) (size 1.524 7.34) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 8 /A6))
    (pad 7 smd roundrect (at -15.24 -0.1 180) (size 1.524 7.34) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 9 /A5))
    (pad 6 smd roundrect (at -17.78 -0.1 180) (size 1.524 7.34) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 3 /A4))
    (pad 5 smd roundrect (at -20.32 -0.1 180) (size 1.524 7.34) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 10 /A3))
    (pad 4 smd roundrect (at -22.86 -0.1 180) (size 1.524 7.34) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 11 /A2))
    (pad 3 smd roundrect (at -25.4 -0.1 180) (size 1.524 7.34) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 12 /A1))
    (pad 2 smd roundrect (at -27.94 -0.1 180) (size 1.524 7.34) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 13 /A0))
    (pad 1 smd roundrect (at -30.48 -0.1 180) (size 1.524 7.34) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 25 /~IOSEL~))
  )

  (module stdpads:Fiducial (layer F.Cu) (tedit 5CFD71CD) (tstamp 5F74E679)
    (at 70.358 117.729 90)
    (descr "Circular Fiducial, 1mm bare copper top; 2mm keepout (Level A)")
    (tags marker)
    (path /5D321D2B)
    (attr smd)
    (fp_text reference FID2 (at 0 -1.6 90) (layer F.SilkS) hide
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_text value Fiducial (at 0 2 90) (layer F.Fab) hide
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_circle (center 0 0) (end 1.25 0) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.06)))
    )
    (fp_circle (center 0 0) (end 1 0) (layer F.Fab) (width 0.1))
    (pad ~ smd circle (at 0 0 90) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.5) (clearance 0.575))
  )

  (module stdpads:Fiducial (layer F.Cu) (tedit 5CFD71CD) (tstamp 5DE2B53A)
    (at 136.906 106.553 270)
    (descr "Circular Fiducial, 1mm bare copper top; 2mm keepout (Level A)")
    (tags marker)
    (path /5D321DA8)
    (attr smd)
    (fp_text reference FID3 (at 0 -1.6 90) (layer F.SilkS) hide
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_text value Fiducial (at 0 2 90) (layer F.Fab) hide
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_circle (center 0 0) (end 1 0) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.06)))
    )
    (fp_circle (center 0 0) (end 1.25 0) (layer F.CrtYd) (width 0.05))
    (pad ~ smd circle (at 0 0 270) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.5) (clearance 0.575))
  )

  (module stdpads:Fiducial (layer F.Cu) (tedit 5CFD71CD) (tstamp 5DE2C9B7)
    (at 70.358 129.54)
    (descr "Circular Fiducial, 1mm bare copper top; 2mm keepout (Level A)")
    (tags marker)
    (path /5D319AED)
    (attr smd)
    (fp_text reference FID1 (at 0 -1.6) (layer F.SilkS) hide
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_text value Fiducial (at 0 2) (layer F.Fab) hide
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_circle (center 0 0) (end 1 0) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.06)))
    )
    (fp_circle (center 0 0) (end 1.25 0) (layer F.CrtYd) (width 0.05))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.5) (clearance 0.575))
  )

  (module stdpads:Fiducial (layer F.Cu) (tedit 5CFD71CD) (tstamp 5F8AC618)
    (at 136.906 124.841)
    (descr "Circular Fiducial, 1mm bare copper top; 2mm keepout (Level A)")
    (tags marker)
    (path /5D322056)
    (attr smd)
    (fp_text reference FID4 (at 2.032 0) (layer F.SilkS) hide
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_text value Fiducial (at 0 2) (layer F.Fab) hide
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_circle (center 0 0) (end 1 0) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.06)))
    )
    (fp_circle (center 0 0) (end 1.25 0) (layer F.CrtYd) (width 0.05))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.5) (clearance 0.575))
  )

  (module stdpads:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5F27C9F6) (tstamp 5F8B1DF0)
    (at 81.675 122.6 180)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /5F96867C)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U2 (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74HCT245PW (at 0 1.016 180) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -3.25 1.2) (end -3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 -2.2) (end 3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 -2.2) (end 3.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 2.2) (end -2.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -2.25 2.2) (end -3.25 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.55 3.95) (end 3.55 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 -3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end -3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.45 2.225) (end 3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.45 3.75) (end -3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_text user %R (at 0 0) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 1 smd roundrect (at -2.925 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 /R~W~))
    (pad 2 smd roundrect (at -2.275 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 /RD3))
    (pad 3 smd roundrect (at -1.625 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 /RD2))
    (pad 4 smd roundrect (at -0.975 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 /RD1))
    (pad 5 smd roundrect (at -0.325 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 /RD0))
    (pad 6 smd roundrect (at 0.325 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 /RD7))
    (pad 7 smd roundrect (at 0.975 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 /RD6))
    (pad 8 smd roundrect (at 1.625 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 /RD5))
    (pad 9 smd roundrect (at 2.275 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 /RD4))
    (pad 10 smd roundrect (at 2.925 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 11 smd roundrect (at 2.925 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /D0))
    (pad 12 smd roundrect (at 2.275 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /D1))
    (pad 13 smd roundrect (at 1.625 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /D2))
    (pad 14 smd roundrect (at 0.975 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /D3))
    (pad 15 smd roundrect (at 0.325 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /D4))
    (pad 16 smd roundrect (at -0.325 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /D5))
    (pad 17 smd roundrect (at -0.975 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /D6))
    (pad 18 smd roundrect (at -1.625 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /D7))
    (pad 19 smd roundrect (at -2.275 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 /R~CS~))
    (pad 20 smd roundrect (at -2.925 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:TSSOP-14_4.4x5mm_P0.65mm (layer F.Cu) (tedit 5F37C96A) (tstamp 5F8B1D23)
    (at 122.8 122.6 180)
    (descr "14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /61D098B2)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U9 (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74HCT08PW (at 0 1 180) (layer F.Fab)
      (effects (font (size 0.381 0.381) (thickness 0.09525)))
    )
    (fp_line (start -2.5 1.2) (end -2.5 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -2.5 -2.2) (end 2.5 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 2.5 -2.2) (end 2.5 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 2.5 2.2) (end -1.5 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -1.5 2.2) (end -2.5 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start -2.8 3.95) (end 2.8 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.8 -3.95) (end 2.8 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.8 3.95) (end -2.8 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.8 3.95) (end 2.8 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.625 2.325) (end -2.5 2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.625 -2.325) (end -2.4 -2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.625 -2.325) (end 2.4 -2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.625 2.325) (end 2.4 2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.625 2.325) (end -2.625 -2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.625 2.325) (end 2.625 -2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.5 2.325) (end -2.5 3.675) (layer F.SilkS) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 1 smd roundrect (at -1.95 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(U8-Pad11)"))
    (pad 2 smd roundrect (at -1.3 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 "Net-(U10-Pad11)"))
    (pad 3 smd roundrect (at -0.65 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(U9-Pad10)"))
    (pad 4 smd roundrect (at 0 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 /INHOE))
    (pad 5 smd roundrect (at 0.65 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 /PHI0))
    (pad 6 smd roundrect (at 1.3 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 /RCS))
    (pad 7 smd roundrect (at 1.95 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 8 smd roundrect (at 1.95 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 /INHOE))
    (pad 9 smd roundrect (at 1.3 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(U10-Pad8)"))
    (pad 10 smd roundrect (at 0.65 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(U9-Pad10)"))
    (pad 11 smd roundrect (at 0 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(U10-Pad9)"))
    (pad 12 smd roundrect (at -0.65 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 /ENRD))
    (pad 13 smd roundrect (at -1.3 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 /R~W~))
    (pad 14 smd roundrect (at -1.95 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:TSSOP-14_4.4x5mm_P0.65mm (layer F.Cu) (tedit 5F37C96A) (tstamp 5F8B1D89)
    (at 111.75 122.6 180)
    (descr "14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /61D08FB5)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U8 (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74HCT08PW (at 0 1 180) (layer F.Fab)
      (effects (font (size 0.381 0.381) (thickness 0.09525)))
    )
    (fp_line (start -2.5 1.2) (end -2.5 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -2.5 -2.2) (end 2.5 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 2.5 -2.2) (end 2.5 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 2.5 2.2) (end -1.5 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -1.5 2.2) (end -2.5 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start -2.8 3.95) (end 2.8 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.8 -3.95) (end 2.8 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.8 3.95) (end -2.8 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.8 3.95) (end 2.8 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.625 2.325) (end -2.5 2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.625 -2.325) (end -2.4 -2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.625 -2.325) (end 2.4 -2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.625 2.325) (end 2.4 2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.625 2.325) (end -2.625 -2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.625 2.325) (end 2.625 -2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.5 2.325) (end -2.5 3.675) (layer F.SilkS) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 1 smd roundrect (at -1.95 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(U5-Pad8)"))
    (pad 2 smd roundrect (at -1.3 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 /BankAB))
    (pad 3 smd roundrect (at -0.65 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 "Net-(U10-Pad4)"))
    (pad 4 smd roundrect (at 0 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /A13))
    (pad 5 smd roundrect (at 0.65 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 /A12))
    (pad 6 smd roundrect (at 1.3 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 "Net-(U10-Pad5)"))
    (pad 7 smd roundrect (at 1.95 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 8 smd roundrect (at 1.95 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "Net-(U10-Pad10)"))
    (pad 9 smd roundrect (at 1.3 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 /ENWR))
    (pad 10 smd roundrect (at 0.65 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(U5-Pad12)"))
    (pad 11 smd roundrect (at 0 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(U8-Pad11)"))
    (pad 12 smd roundrect (at -0.65 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /A14))
    (pad 13 smd roundrect (at -1.3 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /A15))
    (pad 14 smd roundrect (at -1.95 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:TSSOP-14_4.4x5mm_P0.65mm (layer F.Cu) (tedit 5F37C96A) (tstamp 5F8B1B64)
    (at 89.85 122.6 180)
    (descr "14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /61D05E00)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U5 (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74HCT04PW (at 0 1 180) (layer F.Fab)
      (effects (font (size 0.381 0.381) (thickness 0.09525)))
    )
    (fp_text user %R (at 0 0 180) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_line (start -2.5 2.325) (end -2.5 3.675) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.625 2.325) (end 2.625 -2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.625 2.325) (end -2.625 -2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.625 2.325) (end 2.4 2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.625 -2.325) (end 2.4 -2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.625 -2.325) (end -2.4 -2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.625 2.325) (end -2.5 2.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.8 3.95) (end 2.8 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.8 3.95) (end -2.8 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.8 -3.95) (end 2.8 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.8 3.95) (end 2.8 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.5 2.2) (end -2.5 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start 2.5 2.2) (end -1.5 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 2.5 -2.2) (end 2.5 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -2.5 -2.2) (end 2.5 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -2.5 1.2) (end -2.5 -2.2) (layer F.Fab) (width 0.15))
    (pad 14 smd roundrect (at -1.95 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 13 smd roundrect (at -1.3 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 /R~W~))
    (pad 12 smd roundrect (at -0.65 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(U5-Pad12)"))
    (pad 11 smd roundrect (at 0 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 /RCS))
    (pad 10 smd roundrect (at 0.65 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 /R~CS~))
    (pad 9 smd roundrect (at 1.3 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /A13))
    (pad 8 smd roundrect (at 1.95 -2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(U5-Pad8)"))
    (pad 7 smd roundrect (at 1.95 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 6 smd roundrect (at 1.3 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(U5-Pad6)"))
    (pad 5 smd roundrect (at 0.65 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /A2))
    (pad 4 smd roundrect (at 0 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(U5-Pad4)"))
    (pad 3 smd roundrect (at -0.65 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /A1))
    (pad 2 smd roundrect (at -1.3 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(U5-Pad2)"))
    (pad 1 smd roundrect (at -1.95 2.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /A0))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 5F8B1C81)
    (at 100.65 124.8 90)
    (tags capacitor)
    (path /5E988E8B)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C6 (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (pad 2 smd roundrect (at 0.75 0 90) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.75 0 90) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 5F8B2817)
    (at 130.8 108.75 180)
    (tags capacitor)
    (path /61D3AEA8)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C10 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (pad 2 smd roundrect (at 0.75 0 180) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.75 0 180) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 5F8B2828)
    (at 104.35 112.4)
    (tags capacitor)
    (path /5D136B08)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C1 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 5F5EECAC)
    (at 113.45 107.1 180)
    (tags capacitor)
    (path /607FA429)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C4 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (pad 2 smd roundrect (at 0.75 0 180) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.75 0 180) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 5F5EAEB4)
    (at 122.3 107.1 180)
    (tags capacitor)
    (path /5D14D1AA)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C3 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (pad 2 smd roundrect (at 0.75 0 180) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.75 0 180) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5F27C9F6) (tstamp 5F5EAE5E)
    (at 120.1 111.475 270)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /5FA968ED)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U3 (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74HCT273PW (at 0 1.016 270) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_text user %R (at 0 0 90) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_line (start -3.45 3.75) (end -3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.45 2.225) (end 3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.55 3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end -3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 -3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end 3.55 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 2.2) (end -3.25 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 2.2) (end -2.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 -2.2) (end 3.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 -2.2) (end 3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 1.2) (end -3.25 -2.2) (layer F.Fab) (width 0.15))
    (pad 20 smd roundrect (at -2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 19 smd roundrect (at -2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 92 "Net-(U3-Pad19)"))
    (pad 18 smd roundrect (at -1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 17 smd roundrect (at -0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 16 smd roundrect (at -0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 88 "Net-(U3-Pad16)"))
    (pad 15 smd roundrect (at 0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(U3-Pad15)"))
    (pad 14 smd roundrect (at 0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 13 smd roundrect (at 1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 12 smd roundrect (at 2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 "Net-(U3-Pad12)"))
    (pad 11 smd roundrect (at 2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 97 /~A2~clk))
    (pad 10 smd roundrect (at 2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 9 smd roundrect (at 2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 /ENWR))
    (pad 8 smd roundrect (at 1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 /ENWR1A0))
    (pad 7 smd roundrect (at 0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /A0))
    (pad 6 smd roundrect (at 0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 /ENWR1))
    (pad 5 smd roundrect (at -0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 /ENRD))
    (pad 4 smd roundrect (at -0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 /~A0XOR1~))
    (pad 3 smd roundrect (at -1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /A3))
    (pad 2 smd roundrect (at -2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 /BankAB))
    (pad 1 smd roundrect (at -2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 /~RES~))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5F27C9F6) (tstamp 5F5EECEF)
    (at 111.25 111.475 270)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /5FB03A58)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U4 (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74HCT273PW (at 0 1.016 270) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -3.25 1.2) (end -3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 -2.2) (end 3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 -2.2) (end 3.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 2.2) (end -2.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -2.25 2.2) (end -3.25 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.55 3.95) (end 3.55 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 -3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end -3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.45 2.225) (end 3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.45 3.75) (end -3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_text user %R (at 0 0 90) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 1 smd roundrect (at -2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 /~RES~))
    (pad 2 smd roundrect (at -2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 /RA14))
    (pad 3 smd roundrect (at -1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /A0))
    (pad 4 smd roundrect (at -0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /A1))
    (pad 5 smd roundrect (at -0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 /RA15))
    (pad 6 smd roundrect (at 0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 /RA16))
    (pad 7 smd roundrect (at 0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /A3))
    (pad 8 smd roundrect (at 1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 9 smd roundrect (at 2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 91 "Net-(U4-Pad9)"))
    (pad 10 smd roundrect (at 2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 11 smd roundrect (at 2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 /A2clk))
    (pad 12 smd roundrect (at 2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 90 "Net-(U4-Pad12)"))
    (pad 13 smd roundrect (at 1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 14 smd roundrect (at 0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 15 smd roundrect (at 0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(U4-Pad15)"))
    (pad 16 smd roundrect (at -0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 "Net-(U4-Pad16)"))
    (pad 17 smd roundrect (at -0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 18 smd roundrect (at -1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 19 smd roundrect (at -2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 "Net-(U4-Pad19)"))
    (pad 20 smd roundrect (at -2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:PasteHole_1.152mm_NPTH (layer F.Cu) (tedit 5F27B084) (tstamp 5F744B15)
    (at 70.358 115.189 90)
    (descr "Circular Fiducial, 1mm bare copper top; 2mm keepout (Level A)")
    (tags marker)
    (path /607FA434)
    (attr virtual)
    (fp_text reference H2 (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (fp_text value " " (at 0 2 90) (layer F.Fab) hide
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_circle (center 0 0) (end 1 0) (layer F.Fab) (width 0.1))
    (pad "" np_thru_hole circle (at 0 0 90) (size 1.152 1.152) (drill 1.152) (layers *.Cu *.Mask)
      (solder_mask_margin 0.148))
  )

  (module stdpads:PasteHole_1.152mm_NPTH (layer F.Cu) (tedit 5F27B084) (tstamp 5F744B1A)
    (at 134.366 106.553 270)
    (descr "Circular Fiducial, 1mm bare copper top; 2mm keepout (Level A)")
    (tags marker)
    (path /607FA435)
    (attr virtual)
    (fp_text reference H3 (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (fp_text value " " (at 0 2 90) (layer F.Fab) hide
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_circle (center 0 0) (end 1 0) (layer F.Fab) (width 0.1))
    (pad "" np_thru_hole circle (at 0 0 270) (size 1.152 1.152) (drill 1.152) (layers *.Cu *.Mask)
      (solder_mask_margin 0.148))
  )

  (module stdpads:PasteHole_1.152mm_NPTH (layer F.Cu) (tedit 5F27B084) (tstamp 5F7411AF)
    (at 72.898 129.54)
    (descr "Circular Fiducial, 1mm bare copper top; 2mm keepout (Level A)")
    (tags marker)
    (path /607FA433)
    (attr virtual)
    (fp_text reference H1 (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (fp_text value " " (at 0 2) (layer F.Fab) hide
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_circle (center 0 0) (end 1 0) (layer F.Fab) (width 0.1))
    (pad "" np_thru_hole circle (at 0 0) (size 1.152 1.152) (drill 1.152) (layers *.Cu *.Mask)
      (solder_mask_margin 0.148))
  )

  (module stdpads:PasteHole_1.1mm_PTH (layer F.Cu) (tedit 5E892B4B) (tstamp 5F7411B4)
    (at 133.35 129.54)
    (descr "Circular Fiducial, 1mm bare copper top; 2mm keepout (Level A)")
    (tags marker)
    (path /5CC7E0C0)
    (zone_connect 2)
    (attr virtual)
    (fp_text reference H4 (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (fp_text value " " (at 0 2) (layer F.Fab) hide
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_circle (center 0 0) (end 1 0) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )

  (gr_text "128 kB RAM" (at 75.819 109.982 45) (layer F.SilkS) (tstamp 5F74F688)
    (effects (font (size 1.4 1.4) (thickness 0.3)))
  )
  (gr_text "for Apple II" (at 77.089 111.252 45) (layer F.SilkS) (tstamp 5F74F685)
    (effects (font (size 1.016 1.016) (thickness 0.2)))
  )
  (gr_text JLCJLCJLCJLC (at 92.1 113.45) (layer F.SilkS) (tstamp 5F5EB79D)
    (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
  )
  (gr_text "Garrett’s Workshop" (at 90.805 106.299) (layer B.SilkS) (tstamp 5F66B30E)
    (effects (font (size 1.5 1.5) (thickness 0.225)) (justify mirror))
  )
  (gr_line (start 139.446 106.553) (end 139.446 132.08) (layer Edge.Cuts) (width 0.15) (tstamp 5DE2B8E6))
  (gr_line (start 68.326001 113.664999) (end 77.47 104.521) (layer Edge.Cuts) (width 0.15) (tstamp 5DE2CA1A))
  (gr_line (start 67.818 115.189) (end 67.818 129.54) (layer Edge.Cuts) (width 0.15) (tstamp 5DE2C9A8))
  (gr_arc (start 78.994 106.553) (end 78.994 104.521) (angle -53.1) (layer Dwgs.User) (width 0.01) (tstamp 5DE2C9ED))
  (gr_arc (start 78.994 106.553) (end 78.994 104.013) (angle -36.86989765) (layer Edge.Cuts) (width 0.15) (tstamp 5DE2C9E1))
  (gr_line (start 78.994 104.013) (end 136.906 104.013) (layer Edge.Cuts) (width 0.15) (tstamp 5DE2B4E0))
  (gr_line (start 70.358 132.08) (end 73.914 132.08) (layer Edge.Cuts) (width 0.15) (tstamp 5DE2C9DB))
  (gr_arc (start 70.358 115.189) (end 67.818 115.189) (angle 36.86992923) (layer Edge.Cuts) (width 0.15) (tstamp 5DE2C9EA))
  (gr_arc (start 70.358 115.189) (end 68.326 115.189) (angle 36.9) (layer Dwgs.User) (width 0.01) (tstamp 5DE2C9E7))
  (gr_arc (start 136.906 106.553) (end 139.446 106.553) (angle -90) (layer Edge.Cuts) (width 0.15) (tstamp 5DE2B52E))
  (gr_arc (start 136.906 106.553) (end 138.938 106.553) (angle -90) (layer Dwgs.User) (width 0.01) (tstamp 5DE2B52B))
  (gr_poly (pts (xy 139.7 139.446) (xy 139.192 139.954) (xy 74.168 139.954) (xy 73.66 139.446) (xy 73.66 132.08) (xy 139.7 132.08)) (layer F.Mask) (width 0) (tstamp 5D312690))
  (gr_text GW (at 94.615 108.839) (layer B.SilkS) (tstamp 5F66B311)
    (effects (font (size 1.524 1.524) (thickness 0.3)) (justify mirror))
  )
  (gr_line (start 139.446 132.08) (end 139.446 139.192) (layer Edge.Cuts) (width 0.15) (tstamp 5D312687))
  (gr_arc (start 70.358 129.54) (end 68.326 129.54) (angle -90) (layer Dwgs.User) (width 0.01) (tstamp 5DE2C9DE))
  (gr_arc (start 70.358 129.54) (end 67.818 129.54) (angle -90) (layer Edge.Cuts) (width 0.15) (tstamp 5DE2C9E4))
  (gr_text 4208B (at 89.027 108.839) (layer B.SilkS) (tstamp 5F66B314)
    (effects (font (size 1.524 1.524) (thickness 0.3)) (justify mirror))
  )
  (gr_line (start 73.914 132.08) (end 73.914 139.192) (layer Edge.Cuts) (width 0.15) (tstamp 5D312678))
  (gr_poly (pts (xy 139.7 139.446) (xy 139.192 139.954) (xy 74.168 139.954) (xy 73.66 139.446) (xy 73.66 132.08) (xy 139.7 132.08)) (layer B.Mask) (width 0) (tstamp 5D312675))
  (gr_arc (start 138.938 139.192) (end 138.938 139.7) (angle -90) (layer Edge.Cuts) (width 0.15) (tstamp 5D312672))
  (gr_arc (start 74.422 139.192) (end 73.914 139.192) (angle -90) (layer Edge.Cuts) (width 0.15) (tstamp 5D31266F))
  (gr_line (start 138.938 139.7) (end 74.422 139.7) (layer Edge.Cuts) (width 0.15) (tstamp 5D312663))

  (via (at 137.16 129.54) (size 1.524) (drill 0.762) (layers F.Cu B.Cu) (net 1))
  (segment (start 137.16 135.382) (end 137.16 129.54) (width 1.524) (layer F.Cu) (net 1))
  (via (at 137.16 126.619) (size 0.6) (drill 0.3) (layers F.Cu B.Cu) (net 1))
  (segment (start 137.16 127.889) (end 137.16 126.619) (width 0.762) (layer F.Cu) (net 1))
  (segment (start 137.16 127.889) (end 137.16 129.54) (width 0.762) (layer F.Cu) (net 1))
  (segment (start 137.16 129.54) (end 137.16 126.619) (width 1.27) (layer B.Cu) (net 1))
  (via (at 84.6 126.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 84.6 125.55) (end 84.6 126.65) (width 0.45) (layer F.Cu) (net 1))
  (via (at 85.2 125.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 84.6 125.55) (end 85.2 125.55) (width 0.45) (layer F.Cu) (net 1))
  (segment (start 85.2 125.55) (end 86.05 125.55) (width 0.5) (layer F.Cu) (net 1))
  (via (at 86.05 126.35) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 86.05 125.55) (end 86.05 126.35) (width 0.5) (layer F.Cu) (net 1))
  (via (at 86.9 125.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 86.05 125.55) (end 86.9 125.55) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 91.8 125.55) (end 92.45 125.55) (width 0.45) (layer F.Cu) (net 1))
  (via (at 92.45 125.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 92.45 125.55) (end 93.35 125.55) (width 0.5) (layer F.Cu) (net 1))
  (via (at 93.35 126.35) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 93.35 125.55) (end 93.35 126.35) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 99.1 125.55) (end 99.1 126.65) (width 0.45) (layer F.Cu) (net 1) (tstamp 5F5CCA65))
  (via (at 99.1 126.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 5F5CCA66))
  (via (at 101.5 125.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 5F5CCA68))
  (segment (start 100.65 125.55) (end 100.65 126.35) (width 0.5) (layer F.Cu) (net 1) (tstamp 5F5CCA69))
  (segment (start 99.75 125.55) (end 100.65 125.55) (width 0.5) (layer F.Cu) (net 1) (tstamp 5F5CCA6A))
  (segment (start 100.65 125.55) (end 101.5 125.55) (width 0.5) (layer F.Cu) (net 1) (tstamp 5F5CCA6B))
  (via (at 100.65 126.35) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 5F5CCA6C))
  (via (at 99.75 125.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 5F5CCA6F))
  (segment (start 99.1 125.55) (end 99.75 125.55) (width 0.45) (layer F.Cu) (net 1) (tstamp 5F5CCA70))
  (segment (start 107.05 125.55) (end 107.95 125.55) (width 0.5) (layer F.Cu) (net 1) (tstamp 5F5CCBB4))
  (via (at 107.05 125.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 5F5CCBB5))
  (via (at 108.8 125.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 5F5CCBB6))
  (segment (start 106.4 125.55) (end 106.4 126.65) (width 0.45) (layer F.Cu) (net 1) (tstamp 5F5CCBB8))
  (segment (start 106.4 125.55) (end 107.05 125.55) (width 0.45) (layer F.Cu) (net 1) (tstamp 5F5CCBBB))
  (via (at 106.4 126.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 5F5CCBBD))
  (segment (start 107.95 125.55) (end 108.8 125.55) (width 0.5) (layer F.Cu) (net 1) (tstamp 5F5CCBBE))
  (via (at 107.95 126.35) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 5F5CCBC0))
  (segment (start 107.95 125.55) (end 107.95 126.35) (width 0.5) (layer F.Cu) (net 1) (tstamp 5F5CCBC6))
  (via (at 113.7 126.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 5F5CCBE2))
  (segment (start 115.25 125.55) (end 116.1 125.55) (width 0.5) (layer F.Cu) (net 1) (tstamp 5F5CCBE4))
  (via (at 116.1 125.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 5F5CCBE5))
  (segment (start 113.7 125.55) (end 113.7 126.65) (width 0.45) (layer F.Cu) (net 1) (tstamp 5F5CCBE7))
  (via (at 115.25 126.35) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 5F5CCBE9))
  (segment (start 113.7 125.55) (end 114.35 125.55) (width 0.45) (layer F.Cu) (net 1) (tstamp 5F5CCBEA))
  (via (at 114.35 125.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 5F5CCBED))
  (via (at 113.7 124.45) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 5F5CCBF0))
  (segment (start 113.7 125.55) (end 113.7 124.45) (width 0.45) (layer F.Cu) (net 1) (tstamp 5F5CCBF1))
  (segment (start 115.25 125.55) (end 115.25 126.35) (width 0.5) (layer F.Cu) (net 1) (tstamp 5F5CCBF6))
  (segment (start 114.35 125.55) (end 115.25 125.55) (width 0.5) (layer F.Cu) (net 1) (tstamp 5F5CCBF7))
  (segment (start 124.75 125.55) (end 124.75 126.65) (width 0.45) (layer F.Cu) (net 1) (tstamp 5F5CCC13))
  (via (at 127.15 125.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 5F5CCC14))
  (segment (start 126.3 125.55) (end 126.3 126.35) (width 0.5) (layer F.Cu) (net 1) (tstamp 5F5CCC16))
  (segment (start 124.75 125.55) (end 125.4 125.55) (width 0.45) (layer F.Cu) (net 1) (tstamp 5F5CCC1A))
  (via (at 125.4 125.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 5F5CCC1B))
  (segment (start 125.4 125.55) (end 126.3 125.55) (width 0.5) (layer F.Cu) (net 1) (tstamp 5F5CCC1C))
  (via (at 124.75 126.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 5F5CCC1D))
  (via (at 126.3 126.35) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 5F5CCC1F))
  (segment (start 126.3 125.55) (end 127.15 125.55) (width 0.5) (layer F.Cu) (net 1) (tstamp 5F5CCC25))
  (via (at 119.25 124.45) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 119.25 125.55) (end 119.25 124.45) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 118.95 123.5) (end 118.95 124.2) (width 0.4) (layer F.Cu) (net 1))
  (segment (start 119.2 124.45) (end 119.25 124.45) (width 0.4) (layer F.Cu) (net 1))
  (segment (start 118.95 124.2) (end 119.2 124.45) (width 0.4) (layer F.Cu) (net 1))
  (via (at 131.55 107.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 131.55 108.75) (end 131.55 107.9) (width 0.5) (layer F.Cu) (net 1))
  (via (at 132.35 108.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 131.55 108.75) (end 132.35 108.75) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 131.55 108.75) (end 131.55 109.6) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 131.55 110.5) (end 131.55 109.6) (width 0.45) (layer F.Cu) (net 1))
  (via (at 131.55 109.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (via (at 132.65 110.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 131.55 110.5) (end 132.65 110.5) (width 0.45) (layer F.Cu) (net 1))
  (via (at 130.45 110.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 131.55 110.5) (end 130.45 110.5) (width 0.45) (layer F.Cu) (net 1))
  (via (at 100.9 112.4) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 101.85 112.4) (end 100.9 112.4) (width 0.3) (layer F.Cu) (net 1))
  (via (at 102.8 112.4) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 101.85 112.4) (end 102.8 112.4) (width 0.3) (layer F.Cu) (net 1))
  (via (at 103.6 111.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 103.6 112.4) (end 103.6 111.55) (width 0.5) (layer F.Cu) (net 1))
  (via (at 103.6 113.25) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 103.6 112.4) (end 103.6 113.25) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 103.6 112.4) (end 102.8 112.4) (width 0.5) (layer F.Cu) (net 1))
  (via (at 100.9 113.4) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 101.85 113.4) (end 100.9 113.4) (width 0.15) (layer F.Cu) (net 1))
  (via (at 114.2 107.95) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 5F5EED6F))
  (segment (start 114.2 108.55) (end 114.2 107.95) (width 0.45) (layer F.Cu) (net 1) (tstamp 5F5EED6C))
  (via (at 123.05 107.95) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 123.05 108.55) (end 123.05 107.95) (width 0.45) (layer F.Cu) (net 1))
  (segment (start 114.2 107.1) (end 114.2 107.95) (width 0.5) (layer F.Cu) (net 1) (tstamp 5F5EED57))
  (segment (start 123.05 107.1) (end 123.05 107.95) (width 0.5) (layer F.Cu) (net 1))
  (via (at 123.05 106.25) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 123.05 107.1) (end 123.05 106.25) (width 0.5) (layer F.Cu) (net 1))
  (via (at 121.95 108.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 123.05 108.55) (end 121.95 108.55) (width 0.45) (layer F.Cu) (net 1))
  (via (at 124.15 108.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 123.05 108.55) (end 124.15 108.55) (width 0.45) (layer F.Cu) (net 1))
  (via (at 113.1 108.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 5F5EED54))
  (segment (start 114.2 108.55) (end 113.1 108.55) (width 0.45) (layer F.Cu) (net 1) (tstamp 5F5EED45))
  (via (at 115.3 108.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 5F5EED3F))
  (segment (start 114.2 108.55) (end 115.3 108.55) (width 0.45) (layer F.Cu) (net 1) (tstamp 5F5EED3C))
  (via (at 114.2 106.25) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 5F5EED4B))
  (segment (start 114.2 107.1) (end 114.2 106.25) (width 0.5) (layer F.Cu) (net 1) (tstamp 5F5EED4E))
  (via (at 115 107.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 5F5EED48))
  (segment (start 114.2 107.1) (end 115 107.1) (width 0.5) (layer F.Cu) (net 1) (tstamp 5F5EED51))
  (segment (start 91.8 126.65) (end 91.8 125.55) (width 0.45) (layer F.Cu) (net 1))
  (via (at 91.8 126.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 137.16 126.619) (end 137.287 126.492) (width 1.016) (layer B.Cu) (net 1))
  (segment (start 94.1 125.55) (end 93.35 125.55) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 94.2 125.65) (end 94.1 125.55) (width 0.5) (layer F.Cu) (net 1))
  (via (at 94.2 125.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 106.4 124.5) (end 106.3 124.4) (width 0.45) (layer F.Cu) (net 1))
  (segment (start 106.4 125.55) (end 106.4 124.5) (width 0.45) (layer F.Cu) (net 1))
  (via (at 106.3 124.4) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (via (at 68.834 114.427) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F6116F9) (status 40000))
  (via (at 68.58 124.841) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5DE2CA3B) (status 40000))
  (via (at 117.983 104.775) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5DE2B56D) (status 40000))
  (via (at 112.903 104.775) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5DE2B573) (status 40000))
  (via (at 107.823 104.775) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5DE2B564) (status 40000))
  (via (at 102.743 104.775) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5DE2B561) (status 40000))
  (via (at 97.663 104.775) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5DE2B55E) (status 40000))
  (via (at 92.583 104.775) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5DE2B56A) (status 40000))
  (via (at 69.977 131.191) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5DE2CA2F) (status 40000))
  (via (at 68.707 129.921) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5DE2CA35) (status 40000))
  (via (at 138.557 106.172) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5DE2B570) (status 40000))
  (via (at 137.287 104.902) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F6116E0) (status 40000))
  (via (at 102.87 131.318) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5D3131F1) (status 40000))
  (via (at 105.41 131.318) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5D313170) (status 40000))
  (via (at 107.95 131.318) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5D313152) (status 40000))
  (via (at 110.49 131.318) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5D313176) (status 40000))
  (via (at 113.03 131.318) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5D313182) (status 40000))
  (via (at 115.57 131.318) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5D31318E) (status 40000))
  (via (at 118.11 131.318) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5D313194) (status 40000))
  (via (at 100.33 131.318) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5D3131A0))
  (via (at 77.47 131.318) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5DE2CA23))
  (via (at 138.684 110.236) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5DE2B555) (status 40000))
  (via (at 133.223 104.775) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5DE2B54C) (status 40000))
  (via (at 128.143 104.775) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5DE2B558) (status 40000))
  (via (at 123.063 104.775) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5DE2B552) (status 40000))
  (via (at 120.65 131.318) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5D31411E))
  (via (at 125.73 131.318) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5D314112))
  (via (at 128.27 131.318) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5D314106))
  (via (at 130.81 131.318) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5D3140FA))
  (via (at 133.35 131.318) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5D3140E8))
  (via (at 135.89 131.318) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5D3140DC))
  (via (at 123.19 131.318) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5D3140D0))
  (via (at 138.684 131.318) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5D33C184))
  (via (at 95.25 131.318) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5D3131A6))
  (via (at 97.79 131.318) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5D31314F))
  (via (at 92.71 131.318) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5D3131AC))
  (via (at 90.17 131.318) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5D3131B2))
  (via (at 87.63 131.318) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5D313137))
  (via (at 87.503 104.775) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5DE2B567) (status 40000))
  (segment (start 137.16 135.382) (end 137.16 131.445) (width 1.524) (layer B.Cu) (net 2))
  (via (at 135.509 126.619) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 135.46 126.668) (end 135.509 126.619) (width 0.762) (layer F.Cu) (net 2))
  (segment (start 135.46 127.889) (end 135.46 126.668) (width 0.762) (layer F.Cu) (net 2))
  (via (at 134.366 127.889) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 135.46 127.889) (end 134.366 127.889) (width 0.762) (layer F.Cu) (net 2))
  (segment (start 135.46 129.11) (end 135.509 129.159) (width 0.762) (layer F.Cu) (net 2))
  (via (at 135.509 129.159) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 135.46 127.889) (end 135.46 129.11) (width 0.762) (layer F.Cu) (net 2))
  (via (at 74.93 131.318) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5DE556D0))
  (via (at 82.423 104.775) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5DE823FD) (status 40000))
  (via (at 71.882 111.379) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5DE82728) (status 40000))
  (via (at 75.184 108.077) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5DE8272D) (status 40000))
  (via (at 68.58 119.761) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5DE828DB) (status 40000))
  (via (at 138.684 115.316) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5DE829F5) (status 40000))
  (via (at 138.684 120.396) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5DE829FB) (status 40000))
  (via (at 138.684 125.476) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5DE829FD) (status 40000))
  (via (at 72.644 117.094) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2) (tstamp 5E53C06E))
  (via (at 82.55 131.318) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5D3131D3))
  (via (at 80.01 131.318) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5D3131B8))
  (via (at 85.2 124.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 86.05 124.05) (end 85.2 124.05) (width 0.5) (layer F.Cu) (net 2))
  (via (at 86.05 123.25) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 86.05 124.05) (end 86.05 123.25) (width 0.5) (layer F.Cu) (net 2))
  (via (at 86.9 124.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 86.05 124.05) (end 86.9 124.05) (width 0.5) (layer F.Cu) (net 2))
  (via (at 78.75 120.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 78.75 119.65) (end 78.75 120.75) (width 0.45) (layer F.Cu) (net 2))
  (via (at 78.75 118.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 78.75 119.65) (end 78.75 118.55) (width 0.45) (layer F.Cu) (net 2))
  (via (at 78.15 119.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 78.75 119.65) (end 78.15 119.65) (width 0.45) (layer F.Cu) (net 2))
  (via (at 87.3 119.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 87.9 119.65) (end 87.3 119.65) (width 0.45) (layer F.Cu) (net 2))
  (via (at 87.9 118.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 87.9 119.65) (end 87.9 118.55) (width 0.45) (layer F.Cu) (net 2))
  (via (at 92.5 124.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 93.35 124.05) (end 92.5 124.05) (width 0.5) (layer F.Cu) (net 2))
  (via (at 93.35 123.25) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 93.35 124.05) (end 93.35 123.25) (width 0.5) (layer F.Cu) (net 2))
  (via (at 94.2 124.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 93.35 124.05) (end 94.2 124.05) (width 0.5) (layer F.Cu) (net 2))
  (via (at 100.65 123.25) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5CCA5A))
  (segment (start 100.65 124.05) (end 100.65 123.25) (width 0.5) (layer F.Cu) (net 2) (tstamp 5F5CCA5B))
  (segment (start 100.65 124.05) (end 101.5 124.05) (width 0.5) (layer F.Cu) (net 2) (tstamp 5F5CCA5C))
  (via (at 101.5 124.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5CCA5D))
  (via (at 94.6 119.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5CCA60))
  (segment (start 95.2 119.65) (end 94.6 119.65) (width 0.45) (layer F.Cu) (net 2) (tstamp 5F5CCA61))
  (segment (start 95.2 119.65) (end 95.2 120.75) (width 0.45) (layer F.Cu) (net 2) (tstamp 5F5CCA6D))
  (via (at 95.2 120.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5CCA6E))
  (via (at 102.5 120.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5CCBB9))
  (via (at 108.8 124.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5CCBBA))
  (segment (start 107.95 124.05) (end 107.1 124.05) (width 0.5) (layer F.Cu) (net 2) (tstamp 5F5CCBBC))
  (via (at 101.9 119.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5CCBC1))
  (segment (start 102.5 119.65) (end 101.9 119.65) (width 0.45) (layer F.Cu) (net 2) (tstamp 5F5CCBC2))
  (segment (start 107.95 124.05) (end 108.8 124.05) (width 0.5) (layer F.Cu) (net 2) (tstamp 5F5CCBC3))
  (segment (start 102.5 119.65) (end 102.5 120.75) (width 0.45) (layer F.Cu) (net 2) (tstamp 5F5CCBC4))
  (via (at 107.1 124.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5CCBC5))
  (via (at 107.95 123.25) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5CCBC8))
  (segment (start 107.95 124.05) (end 107.95 123.25) (width 0.5) (layer F.Cu) (net 2) (tstamp 5F5CCBC9))
  (segment (start 115.25 124.05) (end 114.4 124.05) (width 0.5) (layer F.Cu) (net 2) (tstamp 5F5CCBE1))
  (via (at 116.1 124.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5CCBE3))
  (via (at 109.8 118.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5CCBE8))
  (segment (start 115.25 124.05) (end 116.1 124.05) (width 0.5) (layer F.Cu) (net 2) (tstamp 5F5CCBEB))
  (via (at 115.25 123.25) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5CCBEC))
  (via (at 109.8 120.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5CCBEE))
  (segment (start 115.25 124.05) (end 115.25 123.25) (width 0.5) (layer F.Cu) (net 2) (tstamp 5F5CCBEF))
  (segment (start 109.8 119.65) (end 109.8 120.75) (width 0.45) (layer F.Cu) (net 2) (tstamp 5F5CCBF2))
  (segment (start 109.8 119.65) (end 109.8 118.55) (width 0.45) (layer F.Cu) (net 2) (tstamp 5F5CCBF4))
  (via (at 114.4 124.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5CCBF5))
  (segment (start 120.85 119.65) (end 120.85 118.55) (width 0.45) (layer F.Cu) (net 2) (tstamp 5F5CCC0F))
  (via (at 120.85 120.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5CCC10))
  (via (at 120.85 118.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5CCC11))
  (via (at 120.25 119.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5CCC12))
  (via (at 125.45 124.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5CCC17))
  (segment (start 126.3 124.05) (end 125.45 124.05) (width 0.5) (layer F.Cu) (net 2) (tstamp 5F5CCC18))
  (segment (start 126.3 124.05) (end 127.15 124.05) (width 0.5) (layer F.Cu) (net 2) (tstamp 5F5CCC19))
  (segment (start 120.85 119.65) (end 120.25 119.65) (width 0.45) (layer F.Cu) (net 2) (tstamp 5F5CCC1E))
  (segment (start 126.3 124.05) (end 126.3 123.25) (width 0.5) (layer F.Cu) (net 2) (tstamp 5F5CCC21))
  (via (at 126.3 123.25) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5CCC22))
  (segment (start 120.85 119.65) (end 120.85 120.75) (width 0.45) (layer F.Cu) (net 2) (tstamp 5F5CCC23))
  (via (at 127.15 124.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5CCC24))
  (via (at 83.3 115.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 82.35 115.9) (end 83.3 115.9) (width 0.3) (layer F.Cu) (net 2))
  (via (at 81.4 111.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 82.35 111.9) (end 81.4 111.9) (width 0.3) (layer F.Cu) (net 2))
  (via (at 83.3 111.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 82.35 111.9) (end 83.3 111.9) (width 0.3) (layer F.Cu) (net 2))
  (via (at 117.65 120.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 117.65 121.8) (end 117.65 120.9) (width 0.4) (layer F.Cu) (net 2))
  (via (at 117.05 121.8) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 117.65 121.8) (end 117.05 121.8) (width 0.4) (layer F.Cu) (net 2))
  (via (at 130.05 109.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 130.05 108.75) (end 130.05 109.6) (width 0.5) (layer F.Cu) (net 2))
  (via (at 129.25 108.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 130.05 108.75) (end 129.25 108.75) (width 0.5) (layer F.Cu) (net 2))
  (via (at 130.05 107.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 130.05 108.75) (end 130.05 107.9) (width 0.5) (layer F.Cu) (net 2))
  (via (at 124.55 114.4) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 125.65 114.4) (end 124.55 114.4) (width 0.45) (layer F.Cu) (net 2))
  (segment (start 125.65 114.4) (end 126.75 114.4) (width 0.45) (layer F.Cu) (net 2))
  (segment (start 125.65 114.4) (end 125.65 115) (width 0.45) (layer F.Cu) (net 2))
  (via (at 105.1 111.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 105.1 112.4) (end 105.1 111.55) (width 0.5) (layer F.Cu) (net 2))
  (via (at 105.1 113.25) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 105.1 112.4) (end 105.1 113.25) (width 0.5) (layer F.Cu) (net 2))
  (via (at 105.9 112.4) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 105.1 112.4) (end 105.9 112.4) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 82.35 115.9) (end 82.35 116.45) (width 0.3) (layer F.Cu) (net 2))
  (via (at 82.35 116.45) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (via (at 85.09 131.318) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5A87B8))
  (via (at 78.25 113.8) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5D31CC))
  (via (at 79.9 113.45) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5D31D9))
  (via (at 70.4 125) (size 1) (drill 0.5) (layers F.Cu B.Cu) (net 2) (tstamp 5F5E73D2))
  (segment (start 70.4 126.3) (end 70.4 125) (width 1) (layer F.Cu) (net 2) (tstamp 5F5E73D8))
  (via (at 69.25 126.3) (size 1) (drill 0.5) (layers F.Cu B.Cu) (net 2) (tstamp 5F5E73E7))
  (segment (start 70.4 126.3) (end 69.25 126.3) (width 1) (layer F.Cu) (net 2) (tstamp 5F5E73E4))
  (via (at 70.4 127.6) (size 1) (drill 0.5) (layers F.Cu B.Cu) (net 2) (tstamp 5F5E73D5))
  (segment (start 70.4 126.3) (end 70.4 127.6) (width 1) (layer F.Cu) (net 2) (tstamp 5F5E73DB))
  (via (at 121.55 107.95) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 121.55 107.1) (end 121.55 107.95) (width 0.5) (layer F.Cu) (net 2))
  (via (at 112.7 107.95) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5EED36))
  (segment (start 112.7 107.1) (end 112.7 107.95) (width 0.5) (layer F.Cu) (net 2) (tstamp 5F5EED39))
  (via (at 111.9 107.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5EED8D))
  (segment (start 112.7 107.1) (end 111.9 107.1) (width 0.5) (layer F.Cu) (net 2) (tstamp 5F5EED8A))
  (via (at 118.25 114.4) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 117.15 114.4) (end 118.25 114.4) (width 0.45) (layer F.Cu) (net 2))
  (via (at 116.05 114.4) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 117.15 114.4) (end 116.05 114.4) (width 0.45) (layer F.Cu) (net 2))
  (via (at 117.15 115) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 117.15 114.4) (end 117.15 115) (width 0.45) (layer F.Cu) (net 2))
  (via (at 107.2 114.4) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5EED84))
  (segment (start 108.3 114.4) (end 107.2 114.4) (width 0.45) (layer F.Cu) (net 2) (tstamp 5F5EED7B))
  (via (at 108.3 115) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5EED69))
  (segment (start 108.3 114.4) (end 108.3 115) (width 0.45) (layer F.Cu) (net 2) (tstamp 5F5EED87))
  (via (at 109.4 114.4) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5EED75))
  (segment (start 108.3 114.4) (end 109.4 114.4) (width 0.45) (layer F.Cu) (net 2) (tstamp 5F5EED72))
  (via (at 103.15 126.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (via (at 125.65 115) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (via (at 78.232 105.029) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5DE2CA1D) (status 40000))
  (via (at 99.6 109.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F6179C4))
  (via (at 100.2 112.4) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F617C61))
  (via (at 89.5 126.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F627A71))
  (via (at 111.85 129.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F627A98))
  (via (at 110.3 127.35) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F627AA7))
  (via (at 120.7 122.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F629768))
  (via (at 124.4 121.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F62B3E3))
  (segment (start 120.9 107.1) (end 121.55 107.1) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 120.75 106.95) (end 120.9 107.1) (width 0.5) (layer F.Cu) (net 2))
  (via (at 120.75 106.95) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (via (at 89.7 118.2) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F62F04B))
  (via (at 88.7 123.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F630AE0))
  (via (at 94.95 128.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F633A69))
  (via (at 115.3 112.45) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 114.2 112.45) (end 115.3 112.45) (width 0.15) (layer F.Cu) (net 2))
  (via (at 107.2 113.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 108.3 113.1) (end 107.2 113.1) (width 0.15) (layer F.Cu) (net 2))
  (via (at 121.95 113.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 123.05 113.1) (end 121.95 113.1) (width 0.15) (layer F.Cu) (net 2))
  (via (at 124.15 109.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 123.05 109.85) (end 124.15 109.85) (width 0.15) (layer F.Cu) (net 2))
  (via (at 92.5 126.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F639B44))
  (segment (start 102.5 119.65) (end 102.5 118.55) (width 0.45) (layer F.Cu) (net 2) (tstamp 5F5CCBB7))
  (segment (start 95.2 119.65) (end 95.2 118.55) (width 0.45) (layer F.Cu) (net 2) (tstamp 5F5CCA67))
  (via (at 125.15 108.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5CA093))
  (segment (start 114.2 110.5) (end 115.3 110.5) (width 0.15) (layer F.Cu) (net 2))
  (via (at 115.3 110.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (via (at 102.9 129.25) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5D320E) (status 40000))
  (via (at 100.65 129.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5D3419) (status 40000))
  (via (at 98.4 129.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5D362F) (status 40000))
  (via (at 97.2 127.95) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5D3A64) (status 40000))
  (via (at 99.2 127.95) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5D4184))
  (via (at 94.35 126.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5D439E))
  (via (at 107.1 129.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5D49C3))
  (via (at 111.6 127.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5D49C5))
  (via (at 124.05 128.2) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5D49C7))
  (via (at 121.35 128.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5D4BE8))
  (via (at 118.5 128.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5D4BE3))
  (via (at 112.8 114.95) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F75FD63))
  (via (at 99.3 116.15) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5D5E38))
  (via (at 99 113.4) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5D5E33))
  (via (at 121.5 124.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F5D6BC9))
  (via (at 127.3 118.2) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F657934))
  (via (at 132.35 121.25) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F657B4F))
  (via (at 129.75 123.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F658186))
  (via (at 125.45 129.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F65818D))
  (via (at 105.85 122.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F6597AD))
  (via (at 107.15 121.25) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F6597AF))
  (via (at 127.65 116.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F659BA0))
  (via (at 120.85 115) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F659BA2))
  (via (at 71.12 122.301) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F668F5B) (status 40000))
  (via (at 73.66 119.761) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F668F5D) (status 40000))
  (via (at 73.66 124.841) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F668F5F) (status 40000))
  (via (at 136.144 112.776) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F669179) (status 40000))
  (via (at 136.144 107.696) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F669180) (status 40000))
  (via (at 134.366 110.236) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F66939B) (status 40000))
  (via (at 134.366 115.316) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F6693A1) (status 40000))
  (via (at 134.366 125.476) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F6693A5) (status 40000))
  (via (at 131.826 128.016) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F6695BB) (status 40000))
  (via (at 99.8 124.25) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 100.65 124.05) (end 99.85 124.05) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 99.8 124.1) (end 99.8 124.25) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 99.85 124.05) (end 99.8 124.1) (width 0.5) (layer F.Cu) (net 2))
  (via (at 108.8 121) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F7563BD))
  (via (at 112.7 106.25) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 112.7 107.1) (end 112.7 106.25) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 121.55 107.1) (end 121.55 106.4) (width 0.5) (layer F.Cu) (net 2))
  (via (at 121.95 106.2) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 121.75 106.2) (end 121.95 106.2) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 121.55 106.4) (end 121.75 106.2) (width 0.5) (layer F.Cu) (net 2))
  (via (at 136.144 117.856) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 5F741708) (status 40000))
  (segment (start 75.55 112.55) (end 81.05 107.05) (width 0.15) (layer F.Cu) (net 3))
  (segment (start 81.05 107.05) (end 88.85 107.05) (width 0.15) (layer F.Cu) (net 3))
  (segment (start 88.9 131.191) (end 87.309 129.6) (width 0.15) (layer F.Cu) (net 3))
  (segment (start 75.55 128) (end 75.55 112.55) (width 0.15) (layer F.Cu) (net 3))
  (segment (start 87.309 129.6) (end 77.15 129.6) (width 0.15) (layer F.Cu) (net 3))
  (segment (start 90.2 108.4) (end 101.85 108.4) (width 0.15) (layer F.Cu) (net 3))
  (segment (start 88.85 107.05) (end 90.2 108.4) (width 0.15) (layer F.Cu) (net 3))
  (segment (start 77.15 129.6) (end 75.55 128) (width 0.15) (layer F.Cu) (net 3))
  (segment (start 88.9 135.282) (end 88.9 131.191) (width 0.15) (layer F.Cu) (net 3))
  (via (at 83.3 126.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 4))
  (segment (start 83.3 125.55) (end 83.3 126.65) (width 0.15) (layer F.Cu) (net 4))
  (segment (start 83.3 128.4) (end 83.3 126.65) (width 0.15) (layer B.Cu) (net 4))
  (segment (start 84.35 129.45) (end 83.3 128.4) (width 0.15) (layer B.Cu) (net 4))
  (segment (start 94.779 129.45) (end 84.35 129.45) (width 0.15) (layer B.Cu) (net 4))
  (segment (start 96.52 131.191) (end 94.779 129.45) (width 0.15) (layer B.Cu) (net 4))
  (segment (start 96.52 135.282) (end 96.52 131.191) (width 0.15) (layer B.Cu) (net 4))
  (via (at 82.65 124.45) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 5))
  (segment (start 82.65 125.55) (end 82.65 124.45) (width 0.15) (layer F.Cu) (net 5))
  (segment (start 93.98 131.191) (end 93.98 135.282) (width 0.15) (layer B.Cu) (net 5))
  (segment (start 92.539 129.75) (end 93.98 131.191) (width 0.15) (layer B.Cu) (net 5))
  (segment (start 84.2 129.75) (end 92.539 129.75) (width 0.15) (layer B.Cu) (net 5))
  (segment (start 82.65 128.2) (end 84.2 129.75) (width 0.15) (layer B.Cu) (net 5))
  (segment (start 82.65 124.45) (end 82.65 128.2) (width 0.15) (layer B.Cu) (net 5))
  (segment (start 99.06 131.191) (end 99.06 135.282) (width 0.15) (layer F.Cu) (net 6))
  (segment (start 96.4 129.65) (end 97.519 129.65) (width 0.15) (layer F.Cu) (net 6))
  (segment (start 97.519 129.65) (end 99.06 131.191) (width 0.15) (layer F.Cu) (net 6))
  (segment (start 95.15 128.4) (end 96.4 129.65) (width 0.15) (layer F.Cu) (net 6))
  (segment (start 77.75 128.4) (end 95.15 128.4) (width 0.15) (layer F.Cu) (net 6))
  (segment (start 76.75 127.4) (end 77.75 128.4) (width 0.15) (layer F.Cu) (net 6))
  (segment (start 76.75 113.15) (end 76.75 127.4) (width 0.15) (layer F.Cu) (net 6))
  (segment (start 81.5 108.4) (end 76.75 113.15) (width 0.15) (layer F.Cu) (net 6))
  (segment (start 82.35 108.4) (end 81.5 108.4) (width 0.15) (layer F.Cu) (net 6))
  (segment (start 100 112.9) (end 101.85 112.9) (width 0.15) (layer F.Cu) (net 7))
  (segment (start 99.7 112.6) (end 100 112.9) (width 0.15) (layer F.Cu) (net 7))
  (segment (start 94.029 128.7) (end 77.6 128.7) (width 0.15) (layer F.Cu) (net 7))
  (segment (start 77.6 128.7) (end 76.45 127.55) (width 0.15) (layer F.Cu) (net 7))
  (segment (start 99.7 110.3) (end 99.7 112.6) (width 0.15) (layer F.Cu) (net 7))
  (segment (start 96.52 135.282) (end 96.52 131.191) (width 0.15) (layer F.Cu) (net 7))
  (segment (start 98.7 109.3) (end 99.7 110.3) (width 0.15) (layer F.Cu) (net 7))
  (segment (start 89.75 109.3) (end 98.7 109.3) (width 0.15) (layer F.Cu) (net 7))
  (segment (start 96.52 131.191) (end 94.029 128.7) (width 0.15) (layer F.Cu) (net 7))
  (segment (start 76.45 113) (end 81.5 107.95) (width 0.15) (layer F.Cu) (net 7))
  (segment (start 81.5 107.95) (end 88.4 107.95) (width 0.15) (layer F.Cu) (net 7))
  (segment (start 88.4 107.95) (end 89.75 109.3) (width 0.15) (layer F.Cu) (net 7))
  (segment (start 76.45 127.55) (end 76.45 113) (width 0.15) (layer F.Cu) (net 7))
  (segment (start 76.15 127.7) (end 76.15 112.85) (width 0.15) (layer F.Cu) (net 8))
  (segment (start 76.15 112.85) (end 81.35 107.65) (width 0.15) (layer F.Cu) (net 8))
  (segment (start 91.789 129) (end 77.45 129) (width 0.15) (layer F.Cu) (net 8))
  (segment (start 77.45 129) (end 76.15 127.7) (width 0.15) (layer F.Cu) (net 8))
  (segment (start 93.98 131.191) (end 91.789 129) (width 0.15) (layer F.Cu) (net 8))
  (segment (start 93.98 135.282) (end 93.98 131.191) (width 0.15) (layer F.Cu) (net 8))
  (segment (start 101.85 109.9) (end 100.7 109.9) (width 0.15) (layer F.Cu) (net 8))
  (segment (start 100.7 109.9) (end 99.8 109) (width 0.15) (layer F.Cu) (net 8))
  (segment (start 99.8 109) (end 89.9 109) (width 0.15) (layer F.Cu) (net 8))
  (segment (start 88.55 107.65) (end 89.9 109) (width 0.15) (layer F.Cu) (net 8))
  (segment (start 81.35 107.65) (end 88.55 107.65) (width 0.15) (layer F.Cu) (net 8))
  (segment (start 91.44 131.191) (end 91.44 135.282) (width 0.15) (layer F.Cu) (net 9))
  (segment (start 77.3 129.3) (end 89.549 129.3) (width 0.15) (layer F.Cu) (net 9))
  (segment (start 89.549 129.3) (end 91.44 131.191) (width 0.15) (layer F.Cu) (net 9))
  (segment (start 75.85 127.85) (end 77.3 129.3) (width 0.15) (layer F.Cu) (net 9))
  (segment (start 75.85 112.7) (end 75.85 127.85) (width 0.15) (layer F.Cu) (net 9))
  (segment (start 88.7 107.35) (end 81.2 107.35) (width 0.15) (layer F.Cu) (net 9))
  (segment (start 81.2 107.35) (end 75.85 112.7) (width 0.15) (layer F.Cu) (net 9))
  (segment (start 101.85 108.9) (end 101.15 108.9) (width 0.15) (layer F.Cu) (net 9))
  (segment (start 101.15 108.9) (end 100.95 108.7) (width 0.15) (layer F.Cu) (net 9))
  (segment (start 90.05 108.7) (end 88.7 107.35) (width 0.15) (layer F.Cu) (net 9))
  (segment (start 100.95 108.7) (end 90.05 108.7) (width 0.15) (layer F.Cu) (net 9))
  (via (at 102.8 114.4) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 10))
  (segment (start 102.8 114.4) (end 101.85 114.4) (width 0.15) (layer F.Cu) (net 10))
  (via (at 93.85 107.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 10))
  (via (at 109.4 112.45) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 10) (tstamp 5F5EED5D))
  (segment (start 108.3 112.45) (end 109.4 112.45) (width 0.15) (layer F.Cu) (net 10) (tstamp 5F5EED63))
  (segment (start 85.069 129.9) (end 86.36 131.191) (width 0.15) (layer F.Cu) (net 10))
  (segment (start 77 129.9) (end 85.069 129.9) (width 0.15) (layer F.Cu) (net 10))
  (segment (start 86.36 131.191) (end 86.36 135.282) (width 0.15) (layer F.Cu) (net 10))
  (segment (start 75.25 128.15) (end 77 129.9) (width 0.15) (layer F.Cu) (net 10))
  (segment (start 75.25 112.4) (end 75.25 128.15) (width 0.15) (layer F.Cu) (net 10))
  (segment (start 88.9875 106.75) (end 80.9 106.75) (width 0.15) (layer F.Cu) (net 10))
  (segment (start 80.9 106.75) (end 75.25 112.4) (width 0.15) (layer F.Cu) (net 10))
  (segment (start 90.3375 108.1) (end 88.9875 106.75) (width 0.15) (layer F.Cu) (net 10))
  (segment (start 93.65 108.1) (end 90.3375 108.1) (width 0.15) (layer F.Cu) (net 10))
  (segment (start 93.85 107.9) (end 93.65 108.1) (width 0.15) (layer F.Cu) (net 10))
  (segment (start 117.15 109.85) (end 116.05 109.85) (width 0.15) (layer F.Cu) (net 10))
  (via (at 116.05 109.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 10))
  (segment (start 100.7 114.4) (end 102.8 114.4) (width 0.15) (layer B.Cu) (net 10))
  (segment (start 100.5 114.6) (end 100.7 114.4) (width 0.15) (layer B.Cu) (net 10))
  (segment (start 93.85 109) (end 99.45 114.6) (width 0.15) (layer B.Cu) (net 10))
  (segment (start 99.45 114.6) (end 100.5 114.6) (width 0.15) (layer B.Cu) (net 10))
  (segment (start 93.85 107.9) (end 93.85 109) (width 0.15) (layer B.Cu) (net 10))
  (segment (start 108.15 113.7) (end 109.4 112.45) (width 0.15) (layer B.Cu) (net 10))
  (segment (start 105.35 113.7) (end 108.15 113.7) (width 0.15) (layer B.Cu) (net 10))
  (segment (start 104.65 114.4) (end 105.35 113.7) (width 0.15) (layer B.Cu) (net 10))
  (segment (start 102.8 114.4) (end 104.65 114.4) (width 0.15) (layer B.Cu) (net 10))
  (segment (start 109.55 112.6) (end 109.4 112.45) (width 0.15) (layer B.Cu) (net 10))
  (segment (start 110.75 112.6) (end 109.55 112.6) (width 0.15) (layer B.Cu) (net 10))
  (segment (start 113.5 109.85) (end 110.75 112.6) (width 0.15) (layer B.Cu) (net 10))
  (segment (start 116.05 109.85) (end 113.5 109.85) (width 0.15) (layer B.Cu) (net 10))
  (segment (start 101.85 114.9) (end 100.8 114.9) (width 0.15) (layer F.Cu) (net 11))
  (segment (start 100.8 114.9) (end 100.9 114.9) (width 0.15) (layer F.Cu) (net 11))
  (via (at 100.9 114.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 11))
  (via (at 92.85 107.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 11))
  (segment (start 83.82 131.191) (end 83.82 135.282) (width 0.15) (layer F.Cu) (net 11))
  (segment (start 82.829 130.2) (end 83.82 131.191) (width 0.15) (layer F.Cu) (net 11))
  (segment (start 76.85 130.2) (end 82.829 130.2) (width 0.15) (layer F.Cu) (net 11))
  (segment (start 74.95 128.3) (end 76.85 130.2) (width 0.15) (layer F.Cu) (net 11))
  (segment (start 74.95 112.25) (end 74.95 128.3) (width 0.15) (layer F.Cu) (net 11))
  (segment (start 80.75 106.45) (end 74.95 112.25) (width 0.15) (layer F.Cu) (net 11))
  (segment (start 89.1375 106.45) (end 80.75 106.45) (width 0.15) (layer F.Cu) (net 11))
  (segment (start 90.4875 107.8) (end 89.1375 106.45) (width 0.15) (layer F.Cu) (net 11))
  (segment (start 92.65 107.8) (end 90.4875 107.8) (width 0.15) (layer F.Cu) (net 11))
  (segment (start 92.85 107.6) (end 92.65 107.8) (width 0.15) (layer F.Cu) (net 11))
  (segment (start 89.2 118) (end 89.2 119.65) (width 0.15) (layer F.Cu) (net 11))
  (segment (start 92.3 114.9) (end 89.2 118) (width 0.15) (layer F.Cu) (net 11))
  (segment (start 100.8 114.9) (end 92.3 114.9) (width 0.15) (layer F.Cu) (net 11))
  (segment (start 99.325 114.9) (end 100.9 114.9) (width 0.15) (layer B.Cu) (net 11))
  (segment (start 92.85 108.425) (end 99.325 114.9) (width 0.15) (layer B.Cu) (net 11))
  (segment (start 92.85 107.6) (end 92.85 108.425) (width 0.15) (layer B.Cu) (net 11))
  (segment (start 104.45 114.9) (end 100.9 114.9) (width 0.15) (layer B.Cu) (net 11))
  (segment (start 104.8 115.25) (end 104.45 114.9) (width 0.15) (layer B.Cu) (net 11))
  (segment (start 104.8 116.65) (end 104.8 115.25) (width 0.15) (layer B.Cu) (net 11))
  (segment (start 104.45 117) (end 104.8 116.65) (width 0.15) (layer B.Cu) (net 11))
  (segment (start 104.45 118) (end 104.45 117) (width 0.15) (layer B.Cu) (net 11))
  (segment (start 104.45 118) (end 104.45 119.65) (width 0.15) (layer F.Cu) (net 11))
  (via (at 104.45 118) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 11))
  (via (at 102.8 115.4) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 12))
  (segment (start 101.85 115.4) (end 102.8 115.4) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 74.65 112.7) (end 74.65 112.6) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 74.65 128.45) (end 74.65 112.7) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 76.7 130.5) (end 74.65 128.45) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 80.589 130.5) (end 76.7 130.5) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 81.28 131.191) (end 80.589 130.5) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 81.28 135.282) (end 81.28 131.191) (width 0.15) (layer F.Cu) (net 12))
  (via (at 91.85 107.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 12))
  (segment (start 74.65 112.1) (end 74.65 112.7) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 91.85 107.3) (end 91.65 107.5) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 80.6 106.15) (end 74.65 112.1) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 90.65 107.5) (end 89.3 106.15) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 89.3 106.15) (end 80.6 106.15) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 91.65 107.5) (end 90.65 107.5) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 103.8 115.4) (end 102.8 115.4) (width 0.15) (layer B.Cu) (net 12))
  (via (at 103.8 115.4) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 12))
  (segment (start 100.7 115.4) (end 102.8 115.4) (width 0.15) (layer B.Cu) (net 12))
  (segment (start 100.5 115.2) (end 100.7 115.4) (width 0.15) (layer B.Cu) (net 12))
  (segment (start 99.175 115.2) (end 100.5 115.2) (width 0.15) (layer B.Cu) (net 12))
  (segment (start 91.85 107.875) (end 99.175 115.2) (width 0.15) (layer B.Cu) (net 12))
  (segment (start 91.85 107.3) (end 91.85 107.875) (width 0.15) (layer B.Cu) (net 12))
  (segment (start 90.5 118.05) (end 90.5 119.65) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 92.65 115.9) (end 90.5 118.05) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 94.65 115.9) (end 92.65 115.9) (width 0.15) (layer F.Cu) (net 12))
  (via (at 94.65 115.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 12))
  (segment (start 94.2 116.35) (end 94.65 115.9) (width 0.15) (layer B.Cu) (net 12))
  (segment (start 94.2 117.7) (end 94.2 116.35) (width 0.15) (layer B.Cu) (net 12))
  (via (at 94.2 117.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 12))
  (segment (start 96.5 118) (end 96.5 119.65) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 96.2 117.7) (end 96.5 118) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 94.2 117.7) (end 96.2 117.7) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 100.65 115.4) (end 101.85 115.4) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 100.15 115.9) (end 100.65 115.4) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 94.65 115.9) (end 98.7 115.9) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 98.95 115.65) (end 99.5 115.65) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 98.7 115.9) (end 98.95 115.65) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 99.75 115.9) (end 100.15 115.9) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 99.5 115.65) (end 99.75 115.9) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 106.7 111) (end 107.2 110.5) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 107.2 110.5) (end 108.3 110.5) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 104 115.2) (end 104.51875 115.2) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 104.51875 115.2) (end 106.7 113.01875) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 106.7 113.01875) (end 106.7 111) (width 0.15) (layer F.Cu) (net 12))
  (segment (start 103.8 115.4) (end 104 115.2) (width 0.15) (layer F.Cu) (net 12))
  (via (at 100.9 115.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 13))
  (segment (start 101 115.9) (end 100.9 115.9) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 101 115.9) (end 101.85 115.9) (width 0.15) (layer F.Cu) (net 13))
  (via (at 92.45 119.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 13))
  (segment (start 92.45 119.65) (end 91.8 119.65) (width 0.15) (layer F.Cu) (net 13))
  (via (at 90.85 107) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 13))
  (segment (start 78.74 131.191) (end 78.74 135.282) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 78.349 130.8) (end 78.74 131.191) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 76.55 130.8) (end 78.349 130.8) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 74.35 128.6) (end 76.55 130.8) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 74.35 111.95) (end 74.35 128.6) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 90.85 107) (end 90.575 107) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 89.425 105.85) (end 80.45 105.85) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 90.575 107) (end 89.425 105.85) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 80.45 105.85) (end 74.35 111.95) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 101.85 115.9) (end 103.15 115.9) (width 0.15) (layer F.Cu) (net 13))
  (via (at 100.2 119.15) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 13))
  (segment (start 100.2 116.6) (end 100.9 115.9) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 100.2 119.15) (end 100.2 116.6) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 103.3 115.9) (end 103.15 115.9) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 103.45 115.9) (end 103.3 115.9) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 103.3 115.75) (end 103.45 115.9) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 103.3 115.75) (end 103.3 115.9) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 103.3 115.75) (end 103.15 115.9) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 99.05 115.5) (end 100.35 115.5) (width 0.15) (layer B.Cu) (net 13))
  (segment (start 90.85 107.3) (end 99.05 115.5) (width 0.15) (layer B.Cu) (net 13))
  (segment (start 100.75 115.9) (end 100.9 115.9) (width 0.15) (layer B.Cu) (net 13))
  (segment (start 100.35 115.5) (end 100.75 115.9) (width 0.15) (layer B.Cu) (net 13))
  (segment (start 90.85 107) (end 90.85 107.3) (width 0.15) (layer B.Cu) (net 13))
  (segment (start 95.825001 120.125001) (end 92.925001 120.125001) (width 0.15) (layer B.Cu) (net 13))
  (segment (start 96.45 120.75) (end 95.825001 120.125001) (width 0.15) (layer B.Cu) (net 13))
  (segment (start 92.925001 120.125001) (end 92.45 119.65) (width 0.15) (layer B.Cu) (net 13))
  (segment (start 97.15 120.75) (end 96.45 120.75) (width 0.15) (layer B.Cu) (net 13))
  (segment (start 99.05 118.85) (end 99.9 118.85) (width 0.15) (layer B.Cu) (net 13))
  (segment (start 99.9 118.85) (end 100.2 119.15) (width 0.15) (layer B.Cu) (net 13))
  (segment (start 97.15 120.75) (end 99.05 118.85) (width 0.15) (layer B.Cu) (net 13))
  (segment (start 103.3 115.15) (end 103.3 115.75) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 103.55 114.9) (end 103.3 115.15) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 104.35 114.9) (end 103.55 114.9) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 106.4 110.8375) (end 106.4 112.85) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 106.4 112.85) (end 104.35 114.9) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 107.3875 109.85) (end 106.4 110.8375) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 108.3 109.85) (end 107.3875 109.85) (width 0.15) (layer F.Cu) (net 13))
  (via (at 97.15 120.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 13))
  (segment (start 97.15 120.75) (end 97.15 119.65) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 98.45 125.55) (end 98.45 123.55) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 100.2 121.8) (end 100.2 119.15) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 98.45 123.55) (end 100.2 121.8) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 105.6 116.2) (end 105.3 115.9) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 110.8 115.45) (end 110.05 116.2) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 105.3 115.9) (end 103.45 115.9) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 110.05 116.2) (end 105.6 116.2) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 116.25 112.45) (end 115.55 113.15) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 115.05 115.45) (end 110.8 115.45) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 117.15 112.45) (end 116.25 112.45) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 115.55 114.95) (end 115.05 115.45) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 115.55 113.15) (end 115.55 114.95) (width 0.15) (layer F.Cu) (net 13))
  (segment (start 99.759 129.35) (end 101.6 131.191) (width 0.15) (layer F.Cu) (net 14))
  (segment (start 95.3 128.1) (end 96.55 129.35) (width 0.15) (layer F.Cu) (net 14))
  (segment (start 101.6 131.191) (end 101.6 135.282) (width 0.15) (layer F.Cu) (net 14))
  (segment (start 77.05 127.25) (end 77.9 128.1) (width 0.15) (layer F.Cu) (net 14))
  (segment (start 96.55 129.35) (end 99.759 129.35) (width 0.15) (layer F.Cu) (net 14))
  (segment (start 77.05 113.3) (end 77.05 127.25) (width 0.15) (layer F.Cu) (net 14))
  (segment (start 81.45 108.9) (end 77.05 113.3) (width 0.15) (layer F.Cu) (net 14))
  (segment (start 77.9 128.1) (end 95.3 128.1) (width 0.15) (layer F.Cu) (net 14))
  (segment (start 82.35 108.9) (end 81.45 108.9) (width 0.15) (layer F.Cu) (net 14))
  (via (at 79.4 126.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 15))
  (segment (start 79.4 125.55) (end 79.4 126.65) (width 0.15) (layer F.Cu) (net 15))
  (segment (start 81.28 131.191) (end 81.28 135.282) (width 0.15) (layer B.Cu) (net 15))
  (segment (start 79.4 129.311) (end 81.28 131.191) (width 0.15) (layer B.Cu) (net 15))
  (segment (start 79.4 126.65) (end 79.4 129.311) (width 0.15) (layer B.Cu) (net 15))
  (via (at 82 126.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 16))
  (segment (start 82 125.55) (end 82 126.65) (width 0.15) (layer F.Cu) (net 16))
  (segment (start 82 128) (end 82 126.65) (width 0.15) (layer B.Cu) (net 16))
  (segment (start 84.05 130.05) (end 82 128) (width 0.15) (layer B.Cu) (net 16))
  (segment (start 90.299 130.05) (end 84.05 130.05) (width 0.15) (layer B.Cu) (net 16))
  (segment (start 91.44 131.191) (end 90.299 130.05) (width 0.15) (layer B.Cu) (net 16))
  (segment (start 91.44 135.282) (end 91.44 131.191) (width 0.15) (layer B.Cu) (net 16))
  (segment (start 78.75 135.372) (end 78.74 135.382) (width 0.15) (layer B.Cu) (net 17) (tstamp 5F5D1442))
  (segment (start 78.75 125.55) (end 78.75 124.45) (width 0.15) (layer F.Cu) (net 17))
  (via (at 78.75 124.45) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 17))
  (segment (start 78.74 124.46) (end 78.75 124.45) (width 0.15) (layer B.Cu) (net 17))
  (segment (start 78.74 135.282) (end 78.74 124.46) (width 0.15) (layer B.Cu) (net 17))
  (via (at 80.05 124.45) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 18))
  (segment (start 80.05 125.55) (end 80.05 124.45) (width 0.15) (layer F.Cu) (net 18))
  (segment (start 80.05 127.2) (end 80.05 124.45) (width 0.15) (layer B.Cu) (net 18))
  (segment (start 80.05 127.422) (end 80.05 127.2) (width 0.15) (layer B.Cu) (net 18))
  (segment (start 83.82 131.192) (end 80.05 127.422) (width 0.15) (layer B.Cu) (net 18))
  (segment (start 83.82 135.282) (end 83.82 131.192) (width 0.15) (layer B.Cu) (net 18))
  (via (at 80.7 126.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 19))
  (segment (start 80.7 125.55) (end 80.7 126.65) (width 0.15) (layer F.Cu) (net 19))
  (segment (start 80.7 127.4) (end 80.7 126.65) (width 0.15) (layer B.Cu) (net 19))
  (segment (start 83.72525 130.65) (end 80.7 127.62475) (width 0.15) (layer B.Cu) (net 19))
  (segment (start 80.7 127.62475) (end 80.7 127.4) (width 0.15) (layer B.Cu) (net 19))
  (segment (start 85.819 130.65) (end 83.72525 130.65) (width 0.15) (layer B.Cu) (net 19))
  (segment (start 86.36 131.191) (end 85.819 130.65) (width 0.15) (layer B.Cu) (net 19))
  (segment (start 86.36 135.282) (end 86.36 131.191) (width 0.15) (layer B.Cu) (net 19))
  (via (at 81.35 124.45) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 20))
  (segment (start 81.35 125.55) (end 81.35 124.45) (width 0.15) (layer F.Cu) (net 20))
  (segment (start 88.9 131.191) (end 88.9 135.282) (width 0.15) (layer B.Cu) (net 20))
  (segment (start 88.059 130.35) (end 88.9 131.191) (width 0.15) (layer B.Cu) (net 20))
  (segment (start 83.8975 130.35) (end 88.059 130.35) (width 0.15) (layer B.Cu) (net 20))
  (segment (start 81.35 127.8025) (end 83.8975 130.35) (width 0.15) (layer B.Cu) (net 20))
  (segment (start 81.35 124.45) (end 81.35 127.8025) (width 0.15) (layer B.Cu) (net 20))
  (segment (start 96.7 129.05) (end 101.999 129.05) (width 0.15) (layer F.Cu) (net 21))
  (segment (start 104.14 131.191) (end 104.14 135.282) (width 0.15) (layer F.Cu) (net 21))
  (segment (start 81.4 109.4) (end 77.35 113.45) (width 0.15) (layer F.Cu) (net 21))
  (segment (start 78.05 127.8) (end 95.45 127.8) (width 0.15) (layer F.Cu) (net 21))
  (segment (start 101.999 129.05) (end 104.14 131.191) (width 0.15) (layer F.Cu) (net 21))
  (segment (start 77.35 127.1) (end 78.05 127.8) (width 0.15) (layer F.Cu) (net 21))
  (segment (start 95.45 127.8) (end 96.7 129.05) (width 0.15) (layer F.Cu) (net 21))
  (segment (start 77.35 113.45) (end 77.35 127.1) (width 0.15) (layer F.Cu) (net 21))
  (segment (start 82.35 109.4) (end 81.4 109.4) (width 0.15) (layer F.Cu) (net 21))
  (via (at 73.25 126.3) (size 1) (drill 0.5) (layers F.Cu B.Cu) (net 22) (tstamp 5F5E73C6))
  (segment (start 72.1 126.3) (end 73.25 126.3) (width 1) (layer F.Cu) (net 22) (tstamp 5F5E73C9))
  (via (at 72.1 125) (size 1) (drill 0.5) (layers F.Cu B.Cu) (net 22) (tstamp 5F5E73CC))
  (segment (start 72.1 126.3) (end 72.1 125) (width 1) (layer F.Cu) (net 22) (tstamp 5F5E73CF))
  (via (at 72.1 127.6) (size 1) (drill 0.5) (layers F.Cu B.Cu) (net 22) (tstamp 5F5E73E1))
  (segment (start 72.1 126.3) (end 72.1 127.6) (width 1) (layer F.Cu) (net 22) (tstamp 5F5E73DE))
  (segment (start 76.2 129.25) (end 73.25 126.3) (width 1.524) (layer B.Cu) (net 22))
  (segment (start 76.2 135.282) (end 76.2 129.25) (width 1.524) (layer B.Cu) (net 22))
  (segment (start 72.1 127.6) (end 72.1 125) (width 1.524) (layer B.Cu) (net 22) (tstamp 5F668F57))
  (segment (start 76.2 129.1) (end 76.2 129.25) (width 1.524) (layer B.Cu) (net 22))
  (segment (start 72.1 125) (end 76.2 129.1) (width 1.524) (layer B.Cu) (net 22))
  (segment (start 72.2 127.5) (end 72.1 127.6) (width 1.524) (layer B.Cu) (net 22))
  (segment (start 74.45 127.5) (end 72.2 127.5) (width 1.524) (layer B.Cu) (net 22))
  (segment (start 76.2 129.25) (end 74.45 127.5) (width 1.524) (layer B.Cu) (net 22))
  (segment (start 81.35 109.9) (end 82.35 109.9) (width 0.15) (layer F.Cu) (net 26))
  (segment (start 77.65 113.6) (end 81.35 109.9) (width 0.15) (layer F.Cu) (net 26))
  (segment (start 77.65 126.95) (end 77.65 113.6) (width 0.15) (layer F.Cu) (net 26))
  (segment (start 78.2 127.5) (end 77.65 126.95) (width 0.15) (layer F.Cu) (net 26))
  (segment (start 95.6 127.5) (end 78.2 127.5) (width 0.15) (layer F.Cu) (net 26))
  (segment (start 96.85 128.75) (end 95.6 127.5) (width 0.15) (layer F.Cu) (net 26))
  (segment (start 104.239 128.75) (end 96.85 128.75) (width 0.15) (layer F.Cu) (net 26))
  (segment (start 106.68 131.191) (end 104.239 128.75) (width 0.15) (layer F.Cu) (net 26))
  (segment (start 106.68 135.282) (end 106.68 131.191) (width 0.15) (layer F.Cu) (net 26))
  (segment (start 109.22 131.191) (end 109.22 135.382) (width 0.1524) (layer F.Cu) (net 27))
  (via (at 109.22 131.191) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 27))
  (segment (start 111.1 119.65) (end 111.1 120.75) (width 0.15) (layer F.Cu) (net 27))
  (via (at 111.1 120.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 27))
  (segment (start 109.22 131.13) (end 109.22 131.191) (width 0.15) (layer B.Cu) (net 27))
  (segment (start 110.8 123.85) (end 110.8 129.55) (width 0.15) (layer B.Cu) (net 27))
  (segment (start 111.1 120.75) (end 111.45 121.1) (width 0.15) (layer B.Cu) (net 27))
  (segment (start 111.45 123.2) (end 110.8 123.85) (width 0.15) (layer B.Cu) (net 27))
  (segment (start 110.8 129.55) (end 109.22 131.13) (width 0.15) (layer B.Cu) (net 27))
  (segment (start 111.45 121.1) (end 111.45 123.2) (width 0.15) (layer B.Cu) (net 27))
  (segment (start 111.1 118.5) (end 111.1 119.65) (width 0.15) (layer F.Cu) (net 27))
  (segment (start 112.2 117.4) (end 111.1 118.5) (width 0.15) (layer F.Cu) (net 27))
  (segment (start 131.55 111.15) (end 130.65 111.15) (width 0.15) (layer F.Cu) (net 27))
  (segment (start 127.9 117.4) (end 112.2 117.4) (width 0.15) (layer F.Cu) (net 27))
  (segment (start 129.35 115.95) (end 127.9 117.4) (width 0.15) (layer F.Cu) (net 27))
  (segment (start 129.35 112.45) (end 129.35 115.95) (width 0.15) (layer F.Cu) (net 27))
  (segment (start 130.65 111.15) (end 129.35 112.45) (width 0.15) (layer F.Cu) (net 27))
  (via (at 81.4 115.4) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 28))
  (segment (start 82.35 115.4) (end 81.4 115.4) (width 0.15) (layer F.Cu) (net 28))
  (segment (start 111.76 135.382) (end 111.76 131.206875) (width 0.1524) (layer F.Cu) (net 28))
  (via (at 111.76 131.191) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 28))
  (segment (start 111.76 131.206875) (end 111.76 131.191) (width 0.15) (layer F.Cu) (net 28))
  (via (at 111.75 118.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 28))
  (segment (start 111.75 119.65) (end 111.75 118.55) (width 0.15) (layer F.Cu) (net 28))
  (segment (start 88.55 124.05) (end 88.55 125.55) (width 0.15) (layer F.Cu) (net 28))
  (segment (start 86.4 121.9) (end 88.55 124.05) (width 0.15) (layer F.Cu) (net 28))
  (segment (start 86.4 121.25) (end 86.4 121.9) (width 0.15) (layer F.Cu) (net 28))
  (via (at 86.4 121.25) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 28))
  (segment (start 86.65 121) (end 86.65 115.95) (width 0.15) (layer B.Cu) (net 28))
  (segment (start 86.1 115.4) (end 81.4 115.4) (width 0.15) (layer B.Cu) (net 28))
  (segment (start 86.65 115.95) (end 86.1 115.4) (width 0.15) (layer B.Cu) (net 28))
  (segment (start 86.4 121.25) (end 86.65 121) (width 0.15) (layer B.Cu) (net 28))
  (segment (start 97 128.45) (end 109.019 128.45) (width 0.15) (layer F.Cu) (net 28))
  (segment (start 95.75 127.2) (end 97 128.45) (width 0.15) (layer F.Cu) (net 28))
  (segment (start 109.019 128.45) (end 111.76 131.191) (width 0.15) (layer F.Cu) (net 28))
  (segment (start 89.3 127.2) (end 95.75 127.2) (width 0.15) (layer F.Cu) (net 28))
  (segment (start 88.55 126.45) (end 89.3 127.2) (width 0.15) (layer F.Cu) (net 28))
  (segment (start 88.55 125.55) (end 88.55 126.45) (width 0.15) (layer F.Cu) (net 28))
  (segment (start 111.75 123.35) (end 111.75 118.55) (width 0.15) (layer B.Cu) (net 28))
  (segment (start 111.1 124) (end 111.75 123.35) (width 0.15) (layer B.Cu) (net 28))
  (segment (start 111.1 130.531) (end 111.1 124) (width 0.15) (layer B.Cu) (net 28))
  (segment (start 111.76 131.191) (end 111.1 130.531) (width 0.15) (layer B.Cu) (net 28))
  (segment (start 130.65 111.8) (end 131.55 111.8) (width 0.15) (layer F.Cu) (net 28))
  (segment (start 129.65 112.8) (end 130.65 111.8) (width 0.15) (layer F.Cu) (net 28))
  (segment (start 111.75 118.55) (end 111.75 118.3) (width 0.15) (layer F.Cu) (net 28))
  (segment (start 129.65 116.1) (end 129.65 112.8) (width 0.15) (layer F.Cu) (net 28))
  (segment (start 128.05 117.7) (end 129.65 116.1) (width 0.15) (layer F.Cu) (net 28))
  (segment (start 112.35 117.7) (end 128.05 117.7) (width 0.15) (layer F.Cu) (net 28))
  (segment (start 111.75 118.3) (end 112.35 117.7) (width 0.15) (layer F.Cu) (net 28))
  (segment (start 112.4 129.23675) (end 112.4 126.9) (width 0.15) (layer F.Cu) (net 29))
  (segment (start 112.4 126.9) (end 112.4 125.55) (width 0.15) (layer F.Cu) (net 29))
  (segment (start 114.3 131.13675) (end 112.4 129.23675) (width 0.15) (layer F.Cu) (net 29))
  (segment (start 114.3 135.282) (end 114.3 131.13675) (width 0.15) (layer F.Cu) (net 29))
  (segment (start 116.84 131.191) (end 116.84 135.282) (width 0.15) (layer F.Cu) (net 30))
  (segment (start 113.05 127.401) (end 116.84 131.191) (width 0.15) (layer F.Cu) (net 30))
  (segment (start 113.05 125.55) (end 113.05 127.401) (width 0.15) (layer F.Cu) (net 30))
  (via (at 126.65 106.2) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 36))
  (segment (start 131.3 106.2) (end 126.65 106.2) (width 0.15) (layer B.Cu) (net 36))
  (segment (start 133.85 108.75) (end 131.3 106.2) (width 0.15) (layer B.Cu) (net 36))
  (segment (start 133.85 121.801) (end 133.85 108.75) (width 0.15) (layer B.Cu) (net 36))
  (segment (start 124.46 131.191) (end 133.85 121.801) (width 0.15) (layer B.Cu) (net 36))
  (segment (start 124.46 135.282) (end 124.46 131.191) (width 0.15) (layer B.Cu) (net 36))
  (segment (start 109.45 105.4) (end 114.65 105.4) (width 0.15) (layer F.Cu) (net 36))
  (segment (start 108.3 106.55) (end 109.45 105.4) (width 0.15) (layer F.Cu) (net 36))
  (segment (start 108.3 108.55) (end 108.3 106.55) (width 0.15) (layer F.Cu) (net 36))
  (segment (start 117.15 107.9) (end 117.15 108.55) (width 0.15) (layer F.Cu) (net 36))
  (segment (start 119.65 105.4) (end 118.15 106.9) (width 0.15) (layer F.Cu) (net 36))
  (segment (start 125.85 105.4) (end 119.65 105.4) (width 0.15) (layer F.Cu) (net 36))
  (segment (start 126.65 106.2) (end 125.85 105.4) (width 0.15) (layer F.Cu) (net 36))
  (segment (start 117.25 107.8) (end 117.05 107.8) (width 0.15) (layer F.Cu) (net 36))
  (segment (start 117.05 107.8) (end 117.15 107.9) (width 0.15) (layer F.Cu) (net 36))
  (segment (start 114.65 105.4) (end 117.05 107.8) (width 0.15) (layer F.Cu) (net 36))
  (segment (start 118.15 106.9) (end 117.25 107.8) (width 0.15) (layer F.Cu) (net 36))
  (segment (start 117.25 107.8) (end 117.15 107.9) (width 0.15) (layer F.Cu) (net 36))
  (segment (start 117.35 124.55) (end 117.35 125.55) (width 0.15) (layer F.Cu) (net 37))
  (segment (start 117.65 124.25) (end 117.35 124.55) (width 0.15) (layer F.Cu) (net 37))
  (segment (start 117.65 123.5) (end 117.65 124.25) (width 0.15) (layer F.Cu) (net 37))
  (segment (start 119.35 130.05) (end 120.779 130.05) (width 0.15) (layer B.Cu) (net 37))
  (segment (start 117.35 128.05) (end 117.35 125.55) (width 0.15) (layer F.Cu) (net 37))
  (segment (start 119.35 130.05) (end 117.35 128.05) (width 0.15) (layer F.Cu) (net 37))
  (segment (start 121.92 131.191) (end 121.92 135.382) (width 0.15) (layer B.Cu) (net 37))
  (segment (start 120.779 130.05) (end 121.92 131.191) (width 0.15) (layer B.Cu) (net 37))
  (via (at 119.35 130.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 37))
  (via (at 110.3 122.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 43))
  (segment (start 101.6 131.191) (end 101.6 135.282) (width 0.15) (layer B.Cu) (net 43))
  (segment (start 101.991 130.8) (end 101.6 131.191) (width 0.15) (layer B.Cu) (net 43))
  (segment (start 106.1 130.8) (end 101.991 130.8) (width 0.15) (layer B.Cu) (net 43))
  (segment (start 110.1 126.8) (end 106.1 130.8) (width 0.15) (layer B.Cu) (net 43))
  (segment (start 110.1 123.05) (end 110.1 126.8) (width 0.15) (layer B.Cu) (net 43))
  (segment (start 110.3 122.85) (end 110.1 123.05) (width 0.15) (layer B.Cu) (net 43))
  (segment (start 122.15 120.6) (end 122.15 119.65) (width 0.15) (layer F.Cu) (net 43))
  (segment (start 121.2 121.55) (end 122.15 120.6) (width 0.15) (layer F.Cu) (net 43))
  (segment (start 119.2875 120.35) (end 120.4875 121.55) (width 0.15) (layer F.Cu) (net 43))
  (segment (start 110.9 123.45) (end 112.9 123.45) (width 0.15) (layer F.Cu) (net 43))
  (segment (start 116 120.35) (end 119.2875 120.35) (width 0.15) (layer F.Cu) (net 43))
  (segment (start 120.4875 121.55) (end 121.2 121.55) (width 0.15) (layer F.Cu) (net 43))
  (segment (start 112.9 123.45) (end 116 120.35) (width 0.15) (layer F.Cu) (net 43))
  (segment (start 110.3 122.85) (end 110.9 123.45) (width 0.15) (layer F.Cu) (net 43))
  (segment (start 103.8 120.75) (end 103.8 119.65) (width 0.15) (layer F.Cu) (net 44))
  (segment (start 103.8 120.75) (end 104.05 121) (width 0.15) (layer F.Cu) (net 44))
  (segment (start 105.75 120.7) (end 105.75 119.65) (width 0.15) (layer F.Cu) (net 44))
  (via (at 103.8 120.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 44))
  (segment (start 105.45 121) (end 105.75 120.7) (width 0.15) (layer F.Cu) (net 44))
  (segment (start 104.05 121) (end 105.45 121) (width 0.15) (layer F.Cu) (net 44))
  (segment (start 96 128.2) (end 99.06 131.26) (width 0.15) (layer B.Cu) (net 44))
  (segment (start 94.05 128.55) (end 94.4 128.2) (width 0.15) (layer B.Cu) (net 44))
  (segment (start 99.06 131.26) (end 99.06 135.282) (width 0.15) (layer B.Cu) (net 44))
  (segment (start 87.35 128.55) (end 94.05 128.55) (width 0.15) (layer B.Cu) (net 44))
  (segment (start 84.15 125.35) (end 87.35 128.55) (width 0.15) (layer B.Cu) (net 44))
  (segment (start 94.4 128.2) (end 96 128.2) (width 0.15) (layer B.Cu) (net 44))
  (segment (start 84.15 124.25) (end 84.15 125.35) (width 0.15) (layer B.Cu) (net 44))
  (segment (start 80.45 120.55) (end 84.15 124.25) (width 0.15) (layer B.Cu) (net 44))
  (segment (start 80.45 114.5) (end 80.45 120.55) (width 0.15) (layer B.Cu) (net 44))
  (segment (start 88.85 118.125) (end 88.85 115.7) (width 0.15) (layer B.Cu) (net 44))
  (segment (start 91.925 121.2) (end 88.85 118.125) (width 0.15) (layer B.Cu) (net 44))
  (segment (start 99.85 121.95) (end 95.3 121.95) (width 0.15) (layer B.Cu) (net 44))
  (segment (start 100.55 121.25) (end 99.85 121.95) (width 0.15) (layer B.Cu) (net 44))
  (segment (start 94.55 121.2) (end 91.925 121.2) (width 0.15) (layer B.Cu) (net 44))
  (segment (start 103.8 120.75) (end 103.25 120.75) (width 0.15) (layer B.Cu) (net 44))
  (segment (start 87 113.85) (end 81.1 113.85) (width 0.15) (layer B.Cu) (net 44))
  (segment (start 102.75 121.25) (end 100.55 121.25) (width 0.15) (layer B.Cu) (net 44))
  (segment (start 95.3 121.95) (end 94.55 121.2) (width 0.15) (layer B.Cu) (net 44))
  (segment (start 81.1 113.85) (end 80.45 114.5) (width 0.15) (layer B.Cu) (net 44))
  (segment (start 103.25 120.75) (end 102.75 121.25) (width 0.15) (layer B.Cu) (net 44))
  (segment (start 88.85 115.7) (end 87 113.85) (width 0.15) (layer B.Cu) (net 44))
  (via (at 132.08 131.064) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 45) (tstamp 5D3137A3))
  (segment (start 132.08 135.382) (end 132.08 131.064) (width 0.15) (layer B.Cu) (net 45) (tstamp 5D3137A0))
  (segment (start 132.08 131.064) (end 132.08 135.382) (width 0.15) (layer F.Cu) (net 45) (tstamp 5D31379D))
  (via (at 134.62 131.064) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 46) (tstamp 5D31379A))
  (segment (start 134.62 135.382) (end 134.62 131.064) (width 0.15) (layer B.Cu) (net 46) (tstamp 5D313956))
  (segment (start 134.62 131.064) (end 134.62 135.382) (width 0.15) (layer F.Cu) (net 46) (tstamp 5D313953))
  (segment (start 83.05 114.9) (end 86.2 118.05) (width 0.15) (layer F.Cu) (net 48))
  (segment (start 82.35 114.9) (end 83.05 114.9) (width 0.15) (layer F.Cu) (net 48))
  (segment (start 86.2 118.05) (end 86.2 119.75) (width 0.15) (layer F.Cu) (net 48))
  (segment (start 86.2 119.75) (end 89.2 122.75) (width 0.15) (layer F.Cu) (net 48))
  (segment (start 89.2 125.55) (end 89.2 122.75) (width 0.15) (layer F.Cu) (net 48))
  (segment (start 83.95 123.175) (end 83.95 125.55) (width 0.15) (layer F.Cu) (net 48))
  (segment (start 85.5 121.625) (end 83.95 123.175) (width 0.15) (layer F.Cu) (net 48))
  (segment (start 85.5 120.45) (end 85.5 121.625) (width 0.15) (layer F.Cu) (net 48))
  (segment (start 86.2 119.75) (end 85.5 120.45) (width 0.15) (layer F.Cu) (net 48))
  (via (at 109.4 111.15) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 49) (tstamp 5F5EED78))
  (segment (start 108.3 111.15) (end 109.4 111.15) (width 0.15) (layer F.Cu) (net 49) (tstamp 5F5EED7E))
  (via (at 102.8 110.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 49))
  (segment (start 101.85 110.9) (end 102.8 110.9) (width 0.15) (layer F.Cu) (net 49))
  (segment (start 103.05 110.9) (end 102.8 110.9) (width 0.15) (layer B.Cu) (net 49))
  (segment (start 108.75 110.75) (end 103.2 110.75) (width 0.15) (layer B.Cu) (net 49))
  (segment (start 103.2 110.75) (end 103.05 110.9) (width 0.15) (layer B.Cu) (net 49))
  (segment (start 109.15 111.15) (end 108.75 110.75) (width 0.15) (layer B.Cu) (net 49))
  (segment (start 109.4 111.15) (end 109.15 111.15) (width 0.15) (layer B.Cu) (net 49))
  (via (at 100.9 111.4) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 50))
  (segment (start 101.85 111.4) (end 100.9 111.4) (width 0.15) (layer F.Cu) (net 50))
  (segment (start 108.3 111.8) (end 110.2 111.8) (width 0.15) (layer F.Cu) (net 50))
  (via (at 110.2 111.8) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 50))
  (segment (start 103 111.4) (end 100.9 111.4) (width 0.15) (layer B.Cu) (net 50))
  (segment (start 103.35 111.05) (end 103 111.4) (width 0.15) (layer B.Cu) (net 50))
  (segment (start 109.2 111.65) (end 108.6 111.05) (width 0.15) (layer B.Cu) (net 50))
  (segment (start 108.6 111.05) (end 103.35 111.05) (width 0.15) (layer B.Cu) (net 50))
  (segment (start 110.05 111.65) (end 109.2 111.65) (width 0.15) (layer B.Cu) (net 50))
  (segment (start 110.2 111.8) (end 110.05 111.65) (width 0.15) (layer B.Cu) (net 50))
  (segment (start 101.85 110.4) (end 102.55 110.4) (width 0.15) (layer F.Cu) (net 51))
  (segment (start 102.55 110.4) (end 103.75 109.2) (width 0.15) (layer F.Cu) (net 51))
  (segment (start 103.75 109.2) (end 108.3 109.2) (width 0.15) (layer F.Cu) (net 51))
  (segment (start 125.65 113.75) (end 126.75 113.75) (width 0.15) (layer F.Cu) (net 52))
  (via (at 126.75 113.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 52))
  (via (at 100.9 109.4) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 52))
  (segment (start 100.9 109.4) (end 101.85 109.4) (width 0.15) (layer F.Cu) (net 52))
  (segment (start 104.9 105.4) (end 100.9 109.4) (width 0.15) (layer B.Cu) (net 52))
  (segment (start 120.45 105.4) (end 104.9 105.4) (width 0.15) (layer B.Cu) (net 52))
  (segment (start 121.85 106.8) (end 120.45 105.4) (width 0.15) (layer B.Cu) (net 52))
  (segment (start 126.75 113.75) (end 127.25 113.25) (width 0.15) (layer B.Cu) (net 52))
  (segment (start 127.25 109.8) (end 124.25 106.8) (width 0.15) (layer B.Cu) (net 52))
  (segment (start 124.25 106.8) (end 121.85 106.8) (width 0.15) (layer B.Cu) (net 52))
  (segment (start 127.25 113.25) (end 127.25 109.8) (width 0.15) (layer B.Cu) (net 52))
  (segment (start 81.35 118.75) (end 81.35 119.65) (width 0.15) (layer F.Cu) (net 53))
  (segment (start 79.7 117.1) (end 81.35 118.75) (width 0.15) (layer F.Cu) (net 53))
  (segment (start 79.7 114.35) (end 79.7 117.1) (width 0.15) (layer F.Cu) (net 53))
  (segment (start 81.65 112.4) (end 79.7 114.35) (width 0.15) (layer F.Cu) (net 53))
  (segment (start 82.35 112.4) (end 81.65 112.4) (width 0.15) (layer F.Cu) (net 53))
  (segment (start 81.2 111.4) (end 82.35 111.4) (width 0.15) (layer F.Cu) (net 54))
  (segment (start 79.4 113.2) (end 81.2 111.4) (width 0.15) (layer F.Cu) (net 54))
  (segment (start 79.4 117.45) (end 79.4 113.2) (width 0.15) (layer F.Cu) (net 54))
  (segment (start 80.7 118.75) (end 79.4 117.45) (width 0.15) (layer F.Cu) (net 54))
  (segment (start 80.7 119.65) (end 80.7 118.75) (width 0.15) (layer F.Cu) (net 54))
  (segment (start 80.05 118.7) (end 80.05 119.65) (width 0.15) (layer F.Cu) (net 55))
  (segment (start 79.1 117.75) (end 80.05 118.7) (width 0.15) (layer F.Cu) (net 55))
  (segment (start 79.1 113.05) (end 79.1 117.75) (width 0.15) (layer F.Cu) (net 55))
  (segment (start 81.25 110.9) (end 79.1 113.05) (width 0.15) (layer F.Cu) (net 55))
  (segment (start 82.35 110.9) (end 81.25 110.9) (width 0.15) (layer F.Cu) (net 55))
  (segment (start 81.3 110.4) (end 82.35 110.4) (width 0.15) (layer F.Cu) (net 56))
  (segment (start 78.8 112.9) (end 81.3 110.4) (width 0.15) (layer F.Cu) (net 56))
  (segment (start 78.8 117.9) (end 78.8 112.9) (width 0.15) (layer F.Cu) (net 56))
  (segment (start 79.4 118.5) (end 78.8 117.9) (width 0.15) (layer F.Cu) (net 56))
  (segment (start 79.4 119.65) (end 79.4 118.5) (width 0.15) (layer F.Cu) (net 56))
  (segment (start 81.65 114.4) (end 82.35 114.4) (width 0.15) (layer F.Cu) (net 57))
  (segment (start 80.9 115.15) (end 81.65 114.4) (width 0.15) (layer F.Cu) (net 57))
  (segment (start 80.9 115.7) (end 80.9 115.15) (width 0.15) (layer F.Cu) (net 57))
  (segment (start 83.95 118.75) (end 80.9 115.7) (width 0.15) (layer F.Cu) (net 57))
  (segment (start 83.95 119.65) (end 83.95 118.75) (width 0.15) (layer F.Cu) (net 57))
  (segment (start 81.65 113.9) (end 82.35 113.9) (width 0.15) (layer F.Cu) (net 58))
  (segment (start 80.6 114.95) (end 81.65 113.9) (width 0.15) (layer F.Cu) (net 58))
  (segment (start 80.6 116.05) (end 80.6 114.95) (width 0.15) (layer F.Cu) (net 58))
  (segment (start 83.3 118.75) (end 80.6 116.05) (width 0.15) (layer F.Cu) (net 58))
  (segment (start 83.3 119.65) (end 83.3 118.75) (width 0.15) (layer F.Cu) (net 58))
  (segment (start 80.3 116.4) (end 82.65 118.75) (width 0.15) (layer F.Cu) (net 59))
  (segment (start 80.3 114.75) (end 80.3 116.4) (width 0.15) (layer F.Cu) (net 59))
  (segment (start 81.65 113.4) (end 80.3 114.75) (width 0.15) (layer F.Cu) (net 59))
  (segment (start 82.65 118.75) (end 82.65 119.65) (width 0.15) (layer F.Cu) (net 59))
  (segment (start 82.35 113.4) (end 81.65 113.4) (width 0.15) (layer F.Cu) (net 59))
  (segment (start 80 116.75) (end 80 114.55) (width 0.15) (layer F.Cu) (net 60))
  (segment (start 81.65 112.9) (end 82.35 112.9) (width 0.15) (layer F.Cu) (net 60))
  (segment (start 80 114.55) (end 81.65 112.9) (width 0.15) (layer F.Cu) (net 60))
  (segment (start 82 118.75) (end 80 116.75) (width 0.15) (layer F.Cu) (net 60))
  (segment (start 82 119.65) (end 82 118.75) (width 0.15) (layer F.Cu) (net 60))
  (via (at 119.25 110.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 61))
  (segment (start 118.05 109.2) (end 117.15 109.2) (width 0.15) (layer F.Cu) (net 61))
  (segment (start 119.25 110.4) (end 118.05 109.2) (width 0.15) (layer F.Cu) (net 61))
  (segment (start 119.25 110.5) (end 119.25 110.4) (width 0.15) (layer F.Cu) (net 61))
  (segment (start 113.05 118.55) (end 113.05 119.65) (width 0.15) (layer F.Cu) (net 61))
  (via (at 113.05 118.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 61))
  (segment (start 119.25 110.775) (end 119.25 110.5) (width 0.15) (layer B.Cu) (net 61))
  (segment (start 119.8 111.325) (end 119.25 110.775) (width 0.15) (layer B.Cu) (net 61))
  (segment (start 119.8 112.2) (end 119.8 111.325) (width 0.15) (layer B.Cu) (net 61))
  (segment (start 119.05 112.95) (end 119.8 112.2) (width 0.15) (layer B.Cu) (net 61))
  (segment (start 119.05 115.05) (end 119.05 112.95) (width 0.15) (layer B.Cu) (net 61))
  (segment (start 117.5 116.6) (end 119.05 115.05) (width 0.15) (layer B.Cu) (net 61))
  (segment (start 114.675 116.6) (end 117.5 116.6) (width 0.15) (layer B.Cu) (net 61))
  (segment (start 113.05 118.225) (end 114.675 116.6) (width 0.15) (layer B.Cu) (net 61))
  (segment (start 113.05 118.55) (end 113.05 118.225) (width 0.15) (layer B.Cu) (net 61))
  (via (at 97.8 124.45) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 62))
  (segment (start 97.8 125.55) (end 97.8 124.45) (width 0.15) (layer F.Cu) (net 62))
  (via (at 118.25 111.8) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 62))
  (segment (start 117.15 111.8) (end 118.25 111.8) (width 0.15) (layer F.Cu) (net 62))
  (segment (start 98.7 124.45) (end 97.8 124.45) (width 0.15) (layer B.Cu) (net 62))
  (segment (start 100.25 123.75) (end 99.4 123.75) (width 0.15) (layer B.Cu) (net 62))
  (segment (start 100.4 123.9) (end 100.25 123.75) (width 0.15) (layer B.Cu) (net 62))
  (segment (start 101.15 123.55) (end 100.8 123.9) (width 0.15) (layer B.Cu) (net 62))
  (segment (start 100.8 123.9) (end 100.4 123.9) (width 0.15) (layer B.Cu) (net 62))
  (segment (start 105.25 122) (end 105.25 122.55) (width 0.15) (layer B.Cu) (net 62))
  (segment (start 112.6 114.45) (end 107.85 119.2) (width 0.15) (layer B.Cu) (net 62))
  (segment (start 106.65 120.6) (end 105.25 122) (width 0.15) (layer B.Cu) (net 62))
  (segment (start 107.3 120.6) (end 106.65 120.6) (width 0.15) (layer B.Cu) (net 62))
  (segment (start 107.85 119.2) (end 107.85 120.05) (width 0.15) (layer B.Cu) (net 62))
  (segment (start 105.25 122.55) (end 104.25 123.55) (width 0.15) (layer B.Cu) (net 62))
  (segment (start 104.25 123.55) (end 101.15 123.55) (width 0.15) (layer B.Cu) (net 62))
  (segment (start 117.1 111.8) (end 114.45 114.45) (width 0.15) (layer B.Cu) (net 62))
  (segment (start 114.45 114.45) (end 112.6 114.45) (width 0.15) (layer B.Cu) (net 62))
  (segment (start 107.85 120.05) (end 107.3 120.6) (width 0.15) (layer B.Cu) (net 62))
  (segment (start 99.4 123.75) (end 98.7 124.45) (width 0.15) (layer B.Cu) (net 62))
  (segment (start 118.25 111.8) (end 117.1 111.8) (width 0.15) (layer B.Cu) (net 62))
  (segment (start 123.45 126.55) (end 123.45 125.55) (width 0.15) (layer F.Cu) (net 63))
  (segment (start 123.35 126.65) (end 123.45 126.55) (width 0.15) (layer F.Cu) (net 63))
  (segment (start 123.2 126.65) (end 123.35 126.65) (width 0.15) (layer F.Cu) (net 63))
  (via (at 123.2 126.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 63))
  (segment (start 121.25 111.15) (end 117.15 111.15) (width 0.15) (layer F.Cu) (net 63))
  (via (at 121.25 111.15) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 63))
  (segment (start 124.15 127.6) (end 123.2 126.65) (width 0.15) (layer B.Cu) (net 63))
  (segment (start 126.2375 127.6) (end 124.15 127.6) (width 0.15) (layer B.Cu) (net 63))
  (segment (start 129.25 124.5875) (end 126.2375 127.6) (width 0.15) (layer B.Cu) (net 63))
  (segment (start 129.25 121.85) (end 129.25 124.5875) (width 0.15) (layer B.Cu) (net 63))
  (segment (start 121.25 113.85) (end 129.25 121.85) (width 0.15) (layer B.Cu) (net 63))
  (segment (start 121.25 111.15) (end 121.25 113.85) (width 0.15) (layer B.Cu) (net 63))
  (segment (start 119.55 113.75) (end 117.15 113.75) (width 0.15) (layer F.Cu) (net 64))
  (via (at 119.55 113.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 64))
  (segment (start 119.35 115.2) (end 119.35 113.95) (width 0.15) (layer B.Cu) (net 64))
  (segment (start 113.05 121.5) (end 119.35 115.2) (width 0.15) (layer B.Cu) (net 64))
  (segment (start 113.05 122.55) (end 113.05 121.5) (width 0.15) (layer B.Cu) (net 64))
  (segment (start 110.45 124.7) (end 110.45 125.55) (width 0.15) (layer F.Cu) (net 64))
  (segment (start 119.35 113.95) (end 119.55 113.75) (width 0.15) (layer B.Cu) (net 64))
  (segment (start 108.8 122.65) (end 108.8 123.05) (width 0.15) (layer F.Cu) (net 64))
  (segment (start 112.85 122.35) (end 109.1 122.35) (width 0.15) (layer F.Cu) (net 64))
  (segment (start 113.05 122.55) (end 112.85 122.35) (width 0.15) (layer F.Cu) (net 64))
  (segment (start 109.1 122.35) (end 108.8 122.65) (width 0.15) (layer F.Cu) (net 64))
  (segment (start 108.8 123.05) (end 110.45 124.7) (width 0.15) (layer F.Cu) (net 64))
  (via (at 113.05 122.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 64))
  (segment (start 97.15 124.4) (end 96.65 123.9) (width 0.15) (layer F.Cu) (net 66))
  (via (at 96.65 123.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 66))
  (segment (start 97.15 125.55) (end 97.15 124.4) (width 0.15) (layer F.Cu) (net 66))
  (via (at 118.25 113.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 66))
  (segment (start 118.25 113.1) (end 117.15 113.1) (width 0.15) (layer F.Cu) (net 66))
  (segment (start 98.15 125.5) (end 97.25 125.5) (width 0.15) (layer B.Cu) (net 66))
  (segment (start 98.65 125) (end 98.15 125.5) (width 0.15) (layer B.Cu) (net 66))
  (segment (start 104.1 125) (end 98.65 125) (width 0.15) (layer B.Cu) (net 66))
  (segment (start 112.65 117.75) (end 111.35 117.75) (width 0.15) (layer B.Cu) (net 66))
  (segment (start 114.4 116) (end 112.65 117.75) (width 0.15) (layer B.Cu) (net 66))
  (segment (start 96.65 124.9) (end 96.65 123.9) (width 0.15) (layer B.Cu) (net 66))
  (segment (start 115.4 116) (end 114.4 116) (width 0.15) (layer B.Cu) (net 66))
  (segment (start 111.35 117.75) (end 104.1 125) (width 0.15) (layer B.Cu) (net 66))
  (segment (start 118.25 113.15) (end 115.4 116) (width 0.15) (layer B.Cu) (net 66))
  (segment (start 97.25 125.5) (end 96.65 124.9) (width 0.15) (layer B.Cu) (net 66))
  (segment (start 118.25 113.1) (end 118.25 113.15) (width 0.15) (layer B.Cu) (net 66))
  (segment (start 125.65 111.8) (end 126.75 111.8) (width 0.15) (layer F.Cu) (net 68))
  (via (at 126.75 111.8) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 68))
  (segment (start 117.15 110.5) (end 118.25 110.5) (width 0.15) (layer F.Cu) (net 68))
  (via (at 118.25 110.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 68))
  (segment (start 118.8 109.7) (end 122.4 109.7) (width 0.15) (layer B.Cu) (net 68))
  (segment (start 124.5 111.8) (end 126.75 111.8) (width 0.15) (layer B.Cu) (net 68))
  (segment (start 118.25 110.25) (end 118.8 109.7) (width 0.15) (layer B.Cu) (net 68))
  (segment (start 122.4 109.7) (end 124.5 111.8) (width 0.15) (layer B.Cu) (net 68))
  (segment (start 118.25 110.5) (end 118.25 110.25) (width 0.15) (layer B.Cu) (net 68))
  (segment (start 91.15 118.5) (end 91.15 119.65) (width 0.15) (layer F.Cu) (net 69))
  (segment (start 92.85 116.8) (end 91.15 118.5) (width 0.15) (layer F.Cu) (net 69))
  (segment (start 97.6 116.8) (end 92.85 116.8) (width 0.15) (layer F.Cu) (net 69))
  (segment (start 99.1 118.3) (end 97.6 116.8) (width 0.15) (layer F.Cu) (net 69))
  (segment (start 99.1 119.65) (end 99.1 118.3) (width 0.15) (layer F.Cu) (net 69))
  (segment (start 98.45 119.65) (end 98.45 120.95) (width 0.15) (layer F.Cu) (net 70))
  (segment (start 98.45 120.95) (end 97.9 121.5) (width 0.15) (layer F.Cu) (net 70))
  (segment (start 97.9 121.5) (end 90.55 121.5) (width 0.15) (layer F.Cu) (net 70))
  (segment (start 89.85 120.8) (end 89.85 119.65) (width 0.15) (layer F.Cu) (net 70))
  (segment (start 90.55 121.5) (end 89.85 120.8) (width 0.15) (layer F.Cu) (net 70))
  (segment (start 88.55 119.65) (end 88.55 120.7) (width 0.15) (layer F.Cu) (net 71))
  (segment (start 88.55 120.7) (end 90.05 122.2) (width 0.15) (layer F.Cu) (net 71))
  (via (at 99.4 121.25) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 71))
  (segment (start 98.45 122.2) (end 99.4 121.25) (width 0.15) (layer F.Cu) (net 71))
  (segment (start 90.05 122.2) (end 98.45 122.2) (width 0.15) (layer F.Cu) (net 71))
  (segment (start 99.4 121.25) (end 100.05 120.6) (width 0.15) (layer B.Cu) (net 71))
  (segment (start 100.05 120.6) (end 101.8 120.6) (width 0.15) (layer B.Cu) (net 71))
  (via (at 107.05 119.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 71))
  (segment (start 102.75 119.65) (end 107.05 119.65) (width 0.15) (layer B.Cu) (net 71))
  (segment (start 101.8 120.6) (end 102.75 119.65) (width 0.15) (layer B.Cu) (net 71))
  (segment (start 107.05 119.65) (end 106.4 119.65) (width 0.15) (layer F.Cu) (net 71))
  (via (at 87.9 124.4) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 72))
  (segment (start 87.9 125.55) (end 87.9 124.4) (width 0.15) (layer F.Cu) (net 72))
  (via (at 104.2 122.25) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 72))
  (segment (start 113.7 120.55) (end 113.7 119.65) (width 0.15) (layer F.Cu) (net 72))
  (segment (start 105.425 121.75) (end 112.5 121.75) (width 0.15) (layer F.Cu) (net 72))
  (segment (start 112.5 121.75) (end 113.7 120.55) (width 0.15) (layer F.Cu) (net 72))
  (segment (start 104.925 122.25) (end 105.425 121.75) (width 0.15) (layer F.Cu) (net 72))
  (segment (start 104.2 122.25) (end 104.925 122.25) (width 0.15) (layer F.Cu) (net 72))
  (segment (start 88.75 125.25) (end 87.9 124.4) (width 0.15) (layer B.Cu) (net 72))
  (segment (start 91.5 125.25) (end 88.75 125.25) (width 0.15) (layer B.Cu) (net 72))
  (segment (start 91.95 124.8) (end 91.5 125.25) (width 0.15) (layer B.Cu) (net 72))
  (segment (start 91.95 123.9) (end 91.95 124.8) (width 0.15) (layer B.Cu) (net 72))
  (segment (start 93.1 122.75) (end 91.95 123.9) (width 0.15) (layer B.Cu) (net 72))
  (segment (start 94 122.75) (end 93.1 122.75) (width 0.15) (layer B.Cu) (net 72))
  (segment (start 94.35 123.1) (end 94 122.75) (width 0.15) (layer B.Cu) (net 72))
  (segment (start 100.1 123.1) (end 94.35 123.1) (width 0.15) (layer B.Cu) (net 72))
  (segment (start 100.45 122.75) (end 100.1 123.1) (width 0.15) (layer B.Cu) (net 72))
  (segment (start 103.7 122.75) (end 100.45 122.75) (width 0.15) (layer B.Cu) (net 72))
  (segment (start 104.2 122.25) (end 103.7 122.75) (width 0.15) (layer B.Cu) (net 72))
  (via (at 89.85 124.45) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 73))
  (segment (start 89.85 125.55) (end 89.85 124.45) (width 0.15) (layer F.Cu) (net 73))
  (segment (start 121.5 120.8) (end 121.5 119.65) (width 0.15) (layer F.Cu) (net 73))
  (segment (start 120.65 121.25) (end 121.05 121.25) (width 0.15) (layer F.Cu) (net 73))
  (segment (start 119.45 120.05) (end 120.65 121.25) (width 0.15) (layer F.Cu) (net 73))
  (segment (start 121.05 121.25) (end 121.5 120.8) (width 0.15) (layer F.Cu) (net 73))
  (segment (start 105.55 122.05) (end 113.85 122.05) (width 0.15) (layer F.Cu) (net 73))
  (segment (start 113.85 122.05) (end 115.85 120.05) (width 0.15) (layer F.Cu) (net 73))
  (segment (start 104.85 122.75) (end 105.55 122.05) (width 0.15) (layer F.Cu) (net 73))
  (segment (start 115.85 120.05) (end 119.45 120.05) (width 0.15) (layer F.Cu) (net 73))
  (segment (start 103.8 122.75) (end 104.85 122.75) (width 0.15) (layer F.Cu) (net 73))
  (segment (start 103.15 122.1) (end 103.8 122.75) (width 0.15) (layer F.Cu) (net 73))
  (via (at 103.15 122.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 73))
  (segment (start 102.8 122.45) (end 103.15 122.1) (width 0.15) (layer B.Cu) (net 73))
  (segment (start 100.3 122.45) (end 102.8 122.45) (width 0.15) (layer B.Cu) (net 73))
  (segment (start 92.95 122.45) (end 94.15 122.45) (width 0.15) (layer B.Cu) (net 73))
  (segment (start 94.5 122.8) (end 99.95 122.8) (width 0.15) (layer B.Cu) (net 73))
  (segment (start 91.65 123.75) (end 92.95 122.45) (width 0.15) (layer B.Cu) (net 73))
  (segment (start 91.65 124.65) (end 91.65 123.75) (width 0.15) (layer B.Cu) (net 73))
  (segment (start 90.35 124.95) (end 91.35 124.95) (width 0.15) (layer B.Cu) (net 73))
  (segment (start 99.95 122.8) (end 100.3 122.45) (width 0.15) (layer B.Cu) (net 73))
  (segment (start 91.35 124.95) (end 91.65 124.65) (width 0.15) (layer B.Cu) (net 73))
  (segment (start 94.15 122.45) (end 94.5 122.8) (width 0.15) (layer B.Cu) (net 73))
  (segment (start 89.85 124.45) (end 90.35 124.95) (width 0.15) (layer B.Cu) (net 73))
  (via (at 90.5 126.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 74))
  (segment (start 90.5 125.55) (end 90.5 126.65) (width 0.15) (layer F.Cu) (net 74))
  (segment (start 111.1 124.65) (end 111.1 125.55) (width 0.15) (layer F.Cu) (net 74))
  (via (at 109.3 122.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 74))
  (segment (start 109.3 122.85) (end 111.1 124.65) (width 0.15) (layer F.Cu) (net 74))
  (segment (start 107.85 128.6) (end 99.15 128.6) (width 0.15) (layer B.Cu) (net 74))
  (segment (start 99.15 128.6) (end 97.75 127.2) (width 0.15) (layer B.Cu) (net 74))
  (segment (start 91.075 126.65) (end 90.5 126.65) (width 0.15) (layer B.Cu) (net 74))
  (segment (start 91.625 127.2) (end 91.075 126.65) (width 0.15) (layer B.Cu) (net 74))
  (segment (start 97.75 127.2) (end 91.625 127.2) (width 0.15) (layer B.Cu) (net 74))
  (segment (start 109.8 126.65) (end 107.85 128.6) (width 0.15) (layer B.Cu) (net 74))
  (segment (start 109.8 123.35) (end 109.8 126.65) (width 0.15) (layer B.Cu) (net 74))
  (segment (start 109.3 122.85) (end 109.8 123.35) (width 0.15) (layer B.Cu) (net 74))
  (segment (start 126.75 110.5) (end 125.65 110.5) (width 0.15) (layer F.Cu) (net 75))
  (via (at 126.75 110.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 75))
  (via (at 97.8 118.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 75))
  (segment (start 97.8 119.65) (end 97.8 118.55) (width 0.15) (layer F.Cu) (net 75))
  (segment (start 101.05 118.55) (end 97.8 118.55) (width 0.15) (layer B.Cu) (net 75))
  (via (at 101.05 118.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 75))
  (segment (start 107.3 117.15) (end 107.9 117.15) (width 0.15) (layer B.Cu) (net 75))
  (segment (start 121.59375 107.1) (end 124.1 107.1) (width 0.15) (layer B.Cu) (net 75))
  (segment (start 120.55 106.45) (end 120.94375 106.45) (width 0.15) (layer B.Cu) (net 75))
  (segment (start 120.25 106.75) (end 120.55 106.45) (width 0.15) (layer B.Cu) (net 75))
  (segment (start 116.4 111.2) (end 120.25 107.35) (width 0.15) (layer B.Cu) (net 75))
  (segment (start 120.25 107.35) (end 120.25 106.75) (width 0.15) (layer B.Cu) (net 75))
  (segment (start 126.75 109.75) (end 126.75 110.5) (width 0.15) (layer B.Cu) (net 75))
  (segment (start 124.1 107.1) (end 126.75 109.75) (width 0.15) (layer B.Cu) (net 75))
  (segment (start 120.94375 106.45) (end 121.59375 107.1) (width 0.15) (layer B.Cu) (net 75))
  (segment (start 113.85 111.2) (end 116.4 111.2) (width 0.15) (layer B.Cu) (net 75))
  (segment (start 107.9 117.15) (end 113.85 111.2) (width 0.15) (layer B.Cu) (net 75))
  (via (at 107.3 117.15) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 75))
  (segment (start 102.75 116.85) (end 101.05 118.55) (width 0.15) (layer F.Cu) (net 75))
  (segment (start 107 116.85) (end 102.75 116.85) (width 0.15) (layer F.Cu) (net 75))
  (segment (start 107.3 117.15) (end 107 116.85) (width 0.15) (layer F.Cu) (net 75))
  (segment (start 95.85 118.55) (end 95.85 119.65) (width 0.15) (layer F.Cu) (net 76))
  (via (at 95.85 118.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 76))
  (via (at 124.55 111.15) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 76))
  (segment (start 125.65 111.15) (end 124.55 111.15) (width 0.15) (layer F.Cu) (net 76))
  (segment (start 97.15 117.25) (end 95.85 118.55) (width 0.15) (layer B.Cu) (net 76))
  (segment (start 101.8 117.25) (end 97.15 117.25) (width 0.15) (layer B.Cu) (net 76))
  (segment (start 103.4 118.85) (end 101.8 117.25) (width 0.15) (layer B.Cu) (net 76))
  (segment (start 106.65 118.85) (end 103.4 118.85) (width 0.15) (layer B.Cu) (net 76))
  (segment (start 114 111.5) (end 106.65 118.85) (width 0.15) (layer B.Cu) (net 76))
  (segment (start 116.55 111.5) (end 114 111.5) (width 0.15) (layer B.Cu) (net 76))
  (segment (start 124 107.45) (end 120.6 107.45) (width 0.15) (layer B.Cu) (net 76))
  (segment (start 120.6 107.45) (end 116.55 111.5) (width 0.15) (layer B.Cu) (net 76))
  (segment (start 124.65 108.1) (end 124 107.45) (width 0.15) (layer B.Cu) (net 76))
  (segment (start 124.65 111.05) (end 124.65 108.1) (width 0.15) (layer B.Cu) (net 76))
  (segment (start 124.55 111.15) (end 124.65 111.05) (width 0.15) (layer B.Cu) (net 76))
  (segment (start 124.55 112.45) (end 125.65 112.45) (width 0.15) (layer F.Cu) (net 77))
  (via (at 124.55 112.45) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 77))
  (segment (start 112.4 120.65) (end 112.4 119.65) (width 0.15) (layer F.Cu) (net 77))
  (segment (start 112.55 120.8) (end 112.4 120.65) (width 0.15) (layer F.Cu) (net 77))
  (via (at 112.55 120.8) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 77))
  (segment (start 112.35 120.6) (end 112.55 120.8) (width 0.15) (layer B.Cu) (net 77))
  (segment (start 112.35 119.1) (end 112.35 120.6) (width 0.15) (layer B.Cu) (net 77))
  (segment (start 112.55 118.3) (end 112.55 118.9) (width 0.15) (layer B.Cu) (net 77))
  (segment (start 114.55 116.3) (end 112.55 118.3) (width 0.15) (layer B.Cu) (net 77))
  (segment (start 118.75 112.8) (end 118.75 114.9) (width 0.15) (layer B.Cu) (net 77))
  (segment (start 119.5 112.05) (end 118.75 112.8) (width 0.15) (layer B.Cu) (net 77))
  (segment (start 119.5 111.45) (end 119.5 112.05) (width 0.15) (layer B.Cu) (net 77))
  (segment (start 124.55 112.3) (end 122.25 110) (width 0.15) (layer B.Cu) (net 77))
  (segment (start 118.75 114.9) (end 117.35 116.3) (width 0.15) (layer B.Cu) (net 77))
  (segment (start 118.75 110.2) (end 118.75 110.7) (width 0.15) (layer B.Cu) (net 77))
  (segment (start 117.35 116.3) (end 114.55 116.3) (width 0.15) (layer B.Cu) (net 77))
  (segment (start 118.95 110) (end 118.75 110.2) (width 0.15) (layer B.Cu) (net 77))
  (segment (start 118.75 110.7) (end 119.5 111.45) (width 0.15) (layer B.Cu) (net 77))
  (segment (start 112.55 118.9) (end 112.35 119.1) (width 0.15) (layer B.Cu) (net 77))
  (segment (start 122.25 110) (end 118.95 110) (width 0.15) (layer B.Cu) (net 77))
  (segment (start 124.55 112.45) (end 124.55 112.3) (width 0.15) (layer B.Cu) (net 77))
  (segment (start 128 113.1) (end 125.65 113.1) (width 0.15) (layer F.Cu) (net 78))
  (segment (start 129.05 115.8) (end 129.05 114.15) (width 0.15) (layer F.Cu) (net 78))
  (segment (start 127.75 117.1) (end 129.05 115.8) (width 0.15) (layer F.Cu) (net 78))
  (segment (start 112.075 117.1) (end 127.75 117.1) (width 0.15) (layer F.Cu) (net 78))
  (segment (start 110.45 118.725) (end 112.075 117.1) (width 0.15) (layer F.Cu) (net 78))
  (segment (start 129.05 114.15) (end 128 113.1) (width 0.15) (layer F.Cu) (net 78))
  (segment (start 110.45 119.65) (end 110.45 118.725) (width 0.15) (layer F.Cu) (net 78))
  (via (at 132.65 113.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 79))
  (segment (start 132.65 113.1) (end 131.55 113.1) (width 0.15) (layer F.Cu) (net 79))
  (segment (start 109.8 127.9) (end 109.8 125.55) (width 0.15) (layer F.Cu) (net 79))
  (segment (start 112.1 130.2) (end 109.8 127.9) (width 0.15) (layer F.Cu) (net 79))
  (via (at 112.1 130.2) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 79))
  (segment (start 133.15 113.6) (end 132.65 113.1) (width 0.15) (layer B.Cu) (net 79))
  (segment (start 133.15 121.6125) (end 133.15 113.6) (width 0.15) (layer B.Cu) (net 79))
  (segment (start 125.7625 129) (end 133.15 121.6125) (width 0.15) (layer B.Cu) (net 79))
  (segment (start 113.3 129) (end 125.7625 129) (width 0.15) (layer B.Cu) (net 79))
  (segment (start 112.1 130.2) (end 113.3 129) (width 0.15) (layer B.Cu) (net 79))
  (segment (start 125.4 119.65) (end 124.75 119.65) (width 0.15) (layer F.Cu) (net 80))
  (via (at 125.4 119.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 80))
  (segment (start 111.75 124.55) (end 111.75 125.55) (width 0.15) (layer F.Cu) (net 80))
  (segment (start 111.9 124.4) (end 111.75 124.55) (width 0.15) (layer F.Cu) (net 80))
  (via (at 111.9 124.4) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 80))
  (segment (start 111.9 124.4) (end 112.55 124.4) (width 0.15) (layer B.Cu) (net 80))
  (segment (start 112.55 124.4) (end 114.4 122.55) (width 0.15) (layer B.Cu) (net 80))
  (segment (start 124.65 122.55) (end 125.4 121.8) (width 0.15) (layer B.Cu) (net 80))
  (segment (start 114.4 122.55) (end 124.65 122.55) (width 0.15) (layer B.Cu) (net 80))
  (segment (start 125.4 121.8) (end 125.4 119.65) (width 0.15) (layer B.Cu) (net 80))
  (segment (start 122.8 123.825) (end 122.8 125.55) (width 0.15) (layer F.Cu) (net 81))
  (segment (start 130.65 113.75) (end 130.25 114.15) (width 0.15) (layer F.Cu) (net 81))
  (segment (start 130.25 116.375) (end 122.8 123.825) (width 0.15) (layer F.Cu) (net 81))
  (segment (start 130.25 114.15) (end 130.25 116.375) (width 0.15) (layer F.Cu) (net 81))
  (segment (start 131.55 113.75) (end 130.65 113.75) (width 0.15) (layer F.Cu) (net 81))
  (segment (start 123.45 120.55) (end 122.15 121.85) (width 0.15) (layer F.Cu) (net 82))
  (segment (start 122.15 121.85) (end 122.15 125.55) (width 0.15) (layer F.Cu) (net 82))
  (segment (start 123.45 119.65) (end 123.45 120.55) (width 0.15) (layer F.Cu) (net 82))
  (segment (start 132.65 114.4) (end 131.55 114.4) (width 0.15) (layer F.Cu) (net 83))
  (via (at 132.65 114.4) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 83))
  (segment (start 121.5 126.65) (end 121.5 125.55) (width 0.15) (layer F.Cu) (net 83))
  (via (at 121.5 126.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 83))
  (segment (start 121.5 126.75) (end 121.5 126.65) (width 0.15) (layer B.Cu) (net 83))
  (segment (start 123.45 128.7) (end 121.5 126.75) (width 0.15) (layer B.Cu) (net 83))
  (segment (start 132.85 121.45) (end 125.6 128.7) (width 0.15) (layer B.Cu) (net 83))
  (segment (start 132.85 114.6) (end 132.85 121.45) (width 0.15) (layer B.Cu) (net 83))
  (segment (start 125.6 128.7) (end 123.45 128.7) (width 0.15) (layer B.Cu) (net 83))
  (segment (start 132.65 114.4) (end 132.85 114.6) (width 0.15) (layer B.Cu) (net 83))
  (segment (start 120.85 122.9) (end 120.85 125.55) (width 0.15) (layer F.Cu) (net 84))
  (segment (start 119.75 121.8) (end 120.85 122.9) (width 0.15) (layer F.Cu) (net 84))
  (segment (start 118.95 121.8) (end 119.75 121.8) (width 0.15) (layer F.Cu) (net 84))
  (segment (start 121.2 122.55) (end 120.85 122.9) (width 0.15) (layer F.Cu) (net 84))
  (segment (start 121.2 122.15) (end 121.2 122.55) (width 0.15) (layer F.Cu) (net 84))
  (segment (start 122.8 120.55) (end 121.2 122.15) (width 0.15) (layer F.Cu) (net 84))
  (segment (start 122.8 119.65) (end 122.8 120.55) (width 0.15) (layer F.Cu) (net 84))
  (segment (start 124.1 120.55) (end 124.1 119.65) (width 0.15) (layer F.Cu) (net 85))
  (segment (start 124.55 121) (end 124.1 120.55) (width 0.15) (layer F.Cu) (net 85))
  (segment (start 125.2 121) (end 124.55 121) (width 0.15) (layer F.Cu) (net 85))
  (segment (start 129.95 116.25) (end 125.2 121) (width 0.15) (layer F.Cu) (net 85))
  (segment (start 129.95 113.15) (end 129.95 116.25) (width 0.15) (layer F.Cu) (net 85))
  (segment (start 130.65 112.45) (end 129.95 113.15) (width 0.15) (layer F.Cu) (net 85))
  (segment (start 131.55 112.45) (end 130.65 112.45) (width 0.15) (layer F.Cu) (net 85))
  (segment (start 121.3 116.45) (end 123.05 114.7) (width 0.15) (layer F.Cu) (net 97))
  (segment (start 110.75 116.45) (end 121.3 116.45) (width 0.15) (layer F.Cu) (net 97))
  (segment (start 108.2 120.45) (end 108.2 119) (width 0.15) (layer F.Cu) (net 97))
  (segment (start 106.95 120.75) (end 107.9 120.75) (width 0.15) (layer F.Cu) (net 97))
  (segment (start 107.9 120.75) (end 108.2 120.45) (width 0.15) (layer F.Cu) (net 97))
  (segment (start 106.4 121.3) (end 106.95 120.75) (width 0.15) (layer F.Cu) (net 97))
  (segment (start 103.55 121.3) (end 106.4 121.3) (width 0.15) (layer F.Cu) (net 97))
  (segment (start 103.15 120.9) (end 103.55 121.3) (width 0.15) (layer F.Cu) (net 97))
  (segment (start 123.05 114.7) (end 123.05 114.4) (width 0.15) (layer F.Cu) (net 97))
  (segment (start 108.2 119) (end 110.75 116.45) (width 0.15) (layer F.Cu) (net 97))
  (segment (start 103.15 119.65) (end 103.15 120.9) (width 0.15) (layer F.Cu) (net 97))
  (via (at 106.15 115.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 98))
  (via (at 106.25 117.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 98))
  (segment (start 106.15 117.65) (end 106.25 117.75) (width 0.15) (layer B.Cu) (net 98))
  (segment (start 106.15 115.1) (end 106.15 117.65) (width 0.15) (layer B.Cu) (net 98))
  (segment (start 105.1 118.7) (end 105.1 119.65) (width 0.15) (layer F.Cu) (net 98))
  (segment (start 106.05 117.75) (end 105.1 118.7) (width 0.15) (layer F.Cu) (net 98))
  (segment (start 106.25 117.75) (end 106.05 117.75) (width 0.15) (layer F.Cu) (net 98))
  (segment (start 106.55 115.5) (end 106.15 115.1) (width 0.15) (layer F.Cu) (net 98))
  (segment (start 109.65 115.5) (end 106.55 115.5) (width 0.15) (layer F.Cu) (net 98))
  (segment (start 110.75 114.4) (end 109.65 115.5) (width 0.15) (layer F.Cu) (net 98))
  (segment (start 114.2 114.4) (end 110.75 114.4) (width 0.15) (layer F.Cu) (net 98))
  (via (at 84.6 120.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 99))
  (segment (start 84.6 119.65) (end 84.6 120.75) (width 0.15) (layer F.Cu) (net 99))
  (via (at 91.15 124.45) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 99))
  (segment (start 91.15 125.55) (end 91.15 124.45) (width 0.15) (layer F.Cu) (net 99))
  (segment (start 84.6 117.6) (end 84.6 120.75) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 85.8 116.4) (end 84.6 117.6) (width 0.15) (layer B.Cu) (net 99))
  (via (at 85.8 116.4) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 99))
  (segment (start 124.1 124.45) (end 124.1 125.55) (width 0.15) (layer F.Cu) (net 99))
  (via (at 124.1 124.45) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 99))
  (segment (start 124.1 126.471) (end 124.1 125.55) (width 0.15) (layer F.Cu) (net 99))
  (segment (start 119.38 135.282) (end 119.38 131.191) (width 0.15) (layer F.Cu) (net 99))
  (segment (start 119.38 131.191) (end 124.1 126.471) (width 0.15) (layer F.Cu) (net 99))
  (segment (start 116.189 128) (end 115.3 128) (width 0.15) (layer F.Cu) (net 99))
  (via (at 115.3 128) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 99))
  (segment (start 119.38 131.191) (end 116.189 128) (width 0.15) (layer F.Cu) (net 99))
  (segment (start 88.4 113.9) (end 101.85 113.9) (width 0.15) (layer F.Cu) (net 99))
  (segment (start 85.9 116.4) (end 88.4 113.9) (width 0.15) (layer F.Cu) (net 99))
  (segment (start 85.8 116.4) (end 85.9 116.4) (width 0.15) (layer F.Cu) (net 99))
  (segment (start 86.55 122.7) (end 84.6 120.75) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 89.4 122.7) (end 86.55 122.7) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 91.15 124.45) (end 89.4 122.7) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 88.2 126.1) (end 84.6 122.5) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 94 124.7) (end 92.6 126.1) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 92.6 126.1) (end 88.2 126.1) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 94.5 124.7) (end 94 124.7) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 96.05 126.25) (end 94.5 124.7) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 98.9 127.15) (end 98 126.25) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 115.3 128) (end 112.7 128) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 98 126.25) (end 96.05 126.25) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 104.75 127.15) (end 98.9 127.15) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 107.45 123.5) (end 107.6 123.65) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 107.6 124.3) (end 104.75 127.15) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 84.6 122.5) (end 84.6 120.75) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 107.6 123.65) (end 107.6 124.3) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 109.3 120.3) (end 109.3 121.2) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 109.3 121.2) (end 107.45 123.05) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 111.55 118.05) (end 109.3 120.3) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 107.45 123.05) (end 107.45 123.5) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 112.25 118.35) (end 111.95 118.05) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 112.25 118.75) (end 112.25 118.35) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 112.05 123.5) (end 112.05 118.95) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 112.05 118.95) (end 112.25 118.75) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 111.95 118.05) (end 111.55 118.05) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 111.4 124.15) (end 112.05 123.5) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 111.4 126.7) (end 111.4 124.15) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 112.7 128) (end 111.4 126.7) (width 0.15) (layer B.Cu) (net 99))

  (zone (net 2) (net_name GND) (layer F.Cu) (tstamp 5DE6C357) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 137.541 104.648) (xy 138.176 105.029) (xy 138.557 105.41) (xy 138.811 105.918) (xy 138.938 106.553)
        (xy 138.938 131.572) (xy 70.358 131.572) (xy 69.723 131.445) (xy 69.215 131.191) (xy 68.707 130.683)
        (xy 68.453 130.175) (xy 68.326 129.54) (xy 68.326 115.189) (xy 68.453 114.554) (xy 68.707 114.046)
        (xy 77.851 104.902) (xy 78.359 104.648) (xy 78.994 104.521) (xy 136.906 104.521)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (tstamp 5DE6C368) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 137.541 104.648) (xy 138.176 105.029) (xy 138.557 105.41) (xy 138.811 105.918) (xy 138.938 106.553)
        (xy 138.938 131.572) (xy 70.358 131.572) (xy 69.723 131.445) (xy 69.215 131.191) (xy 68.707 130.683)
        (xy 68.453 130.175) (xy 68.326 129.54) (xy 68.326 115.189) (xy 68.453 114.554) (xy 68.707 114.046)
        (xy 77.851 104.902) (xy 78.359 104.648) (xy 78.994 104.521) (xy 136.906 104.521)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer In1.Cu) (tstamp 5F5CD030) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 137.541 104.648) (xy 138.176 105.029) (xy 138.557 105.41) (xy 138.811 105.918) (xy 138.938 106.553)
        (xy 138.938 131.572) (xy 139.446 131.572) (xy 139.446 139.7) (xy 73.914 139.7) (xy 73.914 131.572)
        (xy 70.358 131.572) (xy 69.723 131.445) (xy 69.215 131.191) (xy 68.707 130.683) (xy 68.453 130.175)
        (xy 68.326 129.54) (xy 68.326 115.189) (xy 68.453 114.554) (xy 68.707 114.046) (xy 77.851 104.902)
        (xy 78.359 104.648) (xy 78.994 104.521) (xy 136.906 104.521)
      )
    )
  )
  (zone (net 1) (net_name +5V) (layer In2.Cu) (tstamp 5F5CD031) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 137.541 104.648) (xy 138.176 105.029) (xy 138.557 105.41) (xy 138.811 105.918) (xy 138.938 106.553)
        (xy 138.938 131.572) (xy 139.446 131.572) (xy 139.446 139.7) (xy 73.914 139.7) (xy 73.914 131.572)
        (xy 70.358 131.572) (xy 69.723 131.445) (xy 69.215 131.191) (xy 68.707 130.683) (xy 68.453 130.175)
        (xy 68.326 129.54) (xy 68.326 115.189) (xy 68.453 114.554) (xy 68.707 114.046) (xy 77.851 104.902)
        (xy 78.359 104.648) (xy 78.994 104.521) (xy 136.906 104.521)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1652) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.887 137.668) (xy 111.887 138.049) (xy 112.268 138.049) (xy 112.268 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1651) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.252 132.588) (xy 111.252 132.969) (xy 111.633 132.969) (xy 111.633 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1650) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.252 135.128) (xy 111.252 135.509) (xy 111.633 135.509) (xy 111.633 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D164F) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.587 133.223) (xy 124.587 133.604) (xy 124.968 133.604) (xy 124.968 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D164E) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.967 135.763) (xy 116.967 136.144) (xy 117.348 136.144) (xy 117.348 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D164D) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.332 135.763) (xy 116.332 136.144) (xy 116.713 136.144) (xy 116.713 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D164C) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.427 137.668) (xy 114.427 138.049) (xy 114.808 138.049) (xy 114.808 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D164B) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.792 136.398) (xy 113.792 136.779) (xy 114.173 136.779) (xy 114.173 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D164A) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.427 135.763) (xy 114.427 136.144) (xy 114.808 136.144) (xy 114.808 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1649) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.792 135.763) (xy 113.792 136.144) (xy 114.173 136.144) (xy 114.173 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1648) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.427 136.398) (xy 114.427 136.779) (xy 114.808 136.779) (xy 114.808 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1647) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.792 134.493) (xy 113.792 134.874) (xy 114.173 134.874) (xy 114.173 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1646) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.427 135.128) (xy 114.427 135.509) (xy 114.808 135.509) (xy 114.808 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1645) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.792 137.668) (xy 113.792 138.049) (xy 114.173 138.049) (xy 114.173 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1644) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.887 131.953) (xy 111.887 132.334) (xy 112.268 132.334) (xy 112.268 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1643) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.252 133.858) (xy 111.252 134.239) (xy 111.633 134.239) (xy 111.633 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1642) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.887 133.223) (xy 111.887 133.604) (xy 112.268 133.604) (xy 112.268 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1641) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.252 133.223) (xy 111.252 133.604) (xy 111.633 133.604) (xy 111.633 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1640) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.887 133.858) (xy 111.887 134.239) (xy 112.268 134.239) (xy 112.268 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D163F) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.252 131.953) (xy 111.252 132.334) (xy 111.633 132.334) (xy 111.633 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D163E) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.887 137.033) (xy 111.887 137.414) (xy 112.268 137.414) (xy 112.268 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D163D) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.887 132.588) (xy 111.887 132.969) (xy 112.268 132.969) (xy 112.268 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D163C) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.172 137.033) (xy 106.172 137.414) (xy 106.553 137.414) (xy 106.553 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D163B) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.807 137.668) (xy 106.807 138.049) (xy 107.188 138.049) (xy 107.188 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D163A) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.172 132.588) (xy 106.172 132.969) (xy 106.553 132.969) (xy 106.553 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1639) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.427 134.493) (xy 114.427 134.874) (xy 114.808 134.874) (xy 114.808 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1638) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.507 131.953) (xy 119.507 132.334) (xy 119.888 132.334) (xy 119.888 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1637) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.872 133.858) (xy 118.872 134.239) (xy 119.253 134.239) (xy 119.253 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1636) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.172 135.763) (xy 106.172 136.144) (xy 106.553 136.144) (xy 106.553 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1635) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.967 137.668) (xy 116.967 138.049) (xy 117.348 138.049) (xy 117.348 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1634) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.332 132.588) (xy 116.332 132.969) (xy 116.713 132.969) (xy 116.713 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1633) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.332 135.128) (xy 116.332 135.509) (xy 116.713 135.509) (xy 116.713 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1632) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.967 134.493) (xy 116.967 134.874) (xy 117.348 134.874) (xy 117.348 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1631) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.332 136.398) (xy 116.332 136.779) (xy 116.713 136.779) (xy 116.713 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1630) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.872 135.128) (xy 118.872 135.509) (xy 119.253 135.509) (xy 119.253 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D162F) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.967 138.303) (xy 116.967 138.684) (xy 117.348 138.684) (xy 117.348 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D162E) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.332 138.303) (xy 116.332 138.684) (xy 116.713 138.684) (xy 116.713 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D162D) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.332 137.033) (xy 116.332 137.414) (xy 116.713 137.414) (xy 116.713 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D162C) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.552 137.033) (xy 98.552 137.414) (xy 98.933 137.414) (xy 98.933 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D162B) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.187 137.668) (xy 99.187 138.049) (xy 99.568 138.049) (xy 99.568 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D162A) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.552 132.588) (xy 98.552 132.969) (xy 98.933 132.969) (xy 98.933 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1629) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.967 132.588) (xy 116.967 132.969) (xy 117.348 132.969) (xy 117.348 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1628) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.012 136.398) (xy 96.012 136.779) (xy 96.393 136.779) (xy 96.393 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1627) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.187 133.858) (xy 99.187 134.239) (xy 99.568 134.239) (xy 99.568 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1626) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.552 131.953) (xy 98.552 132.334) (xy 98.933 132.334) (xy 98.933 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1625) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.187 137.033) (xy 99.187 137.414) (xy 99.568 137.414) (xy 99.568 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1624) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.187 132.588) (xy 99.187 132.969) (xy 99.568 132.969) (xy 99.568 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1623) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.187 138.303) (xy 99.187 138.684) (xy 99.568 138.684) (xy 99.568 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1622) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.552 138.303) (xy 98.552 138.684) (xy 98.933 138.684) (xy 98.933 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1621) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.647 134.493) (xy 96.647 134.874) (xy 97.028 134.874) (xy 97.028 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1620) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.012 138.303) (xy 96.012 138.684) (xy 96.393 138.684) (xy 96.393 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D161F) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.012 137.033) (xy 96.012 137.414) (xy 96.393 137.414) (xy 96.393 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D161E) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.647 137.668) (xy 96.647 138.049) (xy 97.028 138.049) (xy 97.028 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D161D) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.012 132.588) (xy 96.012 132.969) (xy 96.393 132.969) (xy 96.393 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D161C) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.012 135.128) (xy 96.012 135.509) (xy 96.393 135.509) (xy 96.393 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D161B) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.867 134.493) (xy 78.867 134.874) (xy 79.248 134.874) (xy 79.248 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D161A) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.232 136.398) (xy 78.232 136.779) (xy 78.613 136.779) (xy 78.613 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1619) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.867 135.763) (xy 78.867 136.144) (xy 79.248 136.144) (xy 79.248 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1618) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.232 135.763) (xy 78.232 136.144) (xy 78.613 136.144) (xy 78.613 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1617) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.867 137.033) (xy 78.867 137.414) (xy 79.248 137.414) (xy 79.248 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1616) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.867 132.588) (xy 78.867 132.969) (xy 79.248 132.969) (xy 79.248 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1615) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 81.407 138.303) (xy 81.407 138.684) (xy 81.788 138.684) (xy 81.788 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1614) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.772 138.303) (xy 80.772 138.684) (xy 81.153 138.684) (xy 81.153 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1613) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.772 137.033) (xy 80.772 137.414) (xy 81.153 137.414) (xy 81.153 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1612) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 81.407 137.668) (xy 81.407 138.049) (xy 81.788 138.049) (xy 81.788 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1611) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.772 132.588) (xy 80.772 132.969) (xy 81.153 132.969) (xy 81.153 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1610) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.772 135.128) (xy 80.772 135.509) (xy 81.153 135.509) (xy 81.153 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D160F) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 81.407 134.493) (xy 81.407 134.874) (xy 81.788 134.874) (xy 81.788 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D160E) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.772 136.398) (xy 80.772 136.779) (xy 81.153 136.779) (xy 81.153 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D160D) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 81.407 135.763) (xy 81.407 136.144) (xy 81.788 136.144) (xy 81.788 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D160C) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.772 135.763) (xy 80.772 136.144) (xy 81.153 136.144) (xy 81.153 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D160B) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 81.407 136.398) (xy 81.407 136.779) (xy 81.788 136.779) (xy 81.788 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D160A) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.772 134.493) (xy 80.772 134.874) (xy 81.153 134.874) (xy 81.153 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1609) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 81.407 135.128) (xy 81.407 135.509) (xy 81.788 135.509) (xy 81.788 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1608) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.772 137.668) (xy 80.772 138.049) (xy 81.153 138.049) (xy 81.153 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1607) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.867 137.668) (xy 78.867 138.049) (xy 79.248 138.049) (xy 79.248 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1606) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.232 132.588) (xy 78.232 132.969) (xy 78.613 132.969) (xy 78.613 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1605) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.232 135.128) (xy 78.232 135.509) (xy 78.613 135.509) (xy 78.613 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1604) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.692 138.303) (xy 75.692 138.684) (xy 76.073 138.684) (xy 76.073 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1603) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.692 137.033) (xy 75.692 137.414) (xy 76.073 137.414) (xy 76.073 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1602) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.327 137.668) (xy 76.327 138.049) (xy 76.708 138.049) (xy 76.708 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1601) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.867 138.303) (xy 78.867 138.684) (xy 79.248 138.684) (xy 79.248 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1600) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.232 138.303) (xy 78.232 138.684) (xy 78.613 138.684) (xy 78.613 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15FF) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.232 137.033) (xy 78.232 137.414) (xy 78.613 137.414) (xy 78.613 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15FE) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.112 137.033) (xy 134.112 137.414) (xy 134.493 137.414) (xy 134.493 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D15FD) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.327 137.033) (xy 76.327 137.414) (xy 76.708 137.414) (xy 76.708 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D15FC) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.327 138.303) (xy 76.327 138.684) (xy 76.708 138.684) (xy 76.708 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D15FB) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.692 135.128) (xy 75.692 135.509) (xy 76.073 135.509) (xy 76.073 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D15FA) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.327 134.493) (xy 76.327 134.874) (xy 76.708 134.874) (xy 76.708 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D15F9) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.327 133.858) (xy 76.327 134.239) (xy 76.708 134.239) (xy 76.708 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D15F8) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.692 133.858) (xy 75.692 134.239) (xy 76.073 134.239) (xy 76.073 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D15F7) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.327 133.223) (xy 76.327 133.604) (xy 76.708 133.604) (xy 76.708 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D15F6) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.692 133.223) (xy 75.692 133.604) (xy 76.073 133.604) (xy 76.073 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D15F5) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.327 132.588) (xy 76.327 132.969) (xy 76.708 132.969) (xy 76.708 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D15F4) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.692 132.588) (xy 75.692 132.969) (xy 76.073 132.969) (xy 76.073 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D15F3) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.692 136.398) (xy 75.692 136.779) (xy 76.073 136.779) (xy 76.073 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D15F2) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.327 135.763) (xy 76.327 136.144) (xy 76.708 136.144) (xy 76.708 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D15F1) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.692 135.763) (xy 75.692 136.144) (xy 76.073 136.144) (xy 76.073 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D15F0) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.327 136.398) (xy 76.327 136.779) (xy 76.708 136.779) (xy 76.708 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D15EF) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.692 134.493) (xy 75.692 134.874) (xy 76.073 134.874) (xy 76.073 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D15EE) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.327 135.128) (xy 76.327 135.509) (xy 76.708 135.509) (xy 76.708 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D15ED) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.692 137.668) (xy 75.692 138.049) (xy 76.073 138.049) (xy 76.073 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15EC) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.747 135.128) (xy 134.747 135.509) (xy 135.128 135.509) (xy 135.128 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15EB) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.112 138.303) (xy 134.112 138.684) (xy 134.493 138.684) (xy 134.493 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15EA) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.747 138.303) (xy 134.747 138.684) (xy 135.128 138.684) (xy 135.128 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D15E9) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.872 138.303) (xy 118.872 138.684) (xy 119.253 138.684) (xy 119.253 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15E8) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.127 134.493) (xy 127.127 134.874) (xy 127.508 134.874) (xy 127.508 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15E7) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.127 136.398) (xy 127.127 136.779) (xy 127.508 136.779) (xy 127.508 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15E6) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.112 132.588) (xy 134.112 132.969) (xy 134.493 132.969) (xy 134.493 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15E5) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.412 137.668) (xy 121.412 138.049) (xy 121.793 138.049) (xy 121.793 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15E4) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.127 135.128) (xy 127.127 135.509) (xy 127.508 135.509) (xy 127.508 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15E3) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.172 137.668) (xy 106.172 138.049) (xy 106.553 138.049) (xy 106.553 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15E2) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.807 135.128) (xy 106.807 135.509) (xy 107.188 135.509) (xy 107.188 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15E1) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.172 134.493) (xy 106.172 134.874) (xy 106.553 134.874) (xy 106.553 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15E0) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.792 133.223) (xy 113.792 133.604) (xy 114.173 133.604) (xy 114.173 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15DF) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.572 135.128) (xy 131.572 135.509) (xy 131.953 135.509) (xy 131.953 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15DE) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.747 137.668) (xy 134.747 138.049) (xy 135.128 138.049) (xy 135.128 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15DD) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.587 135.763) (xy 124.587 136.144) (xy 124.968 136.144) (xy 124.968 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15DC) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.587 131.953) (xy 124.587 132.334) (xy 124.968 132.334) (xy 124.968 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15DB) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.492 135.763) (xy 126.492 136.144) (xy 126.873 136.144) (xy 126.873 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15DA) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.127 135.763) (xy 127.127 136.144) (xy 127.508 136.144) (xy 127.508 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15D9) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.412 137.033) (xy 121.412 137.414) (xy 121.793 137.414) (xy 121.793 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15D8) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.412 134.493) (xy 121.412 134.874) (xy 121.793 134.874) (xy 121.793 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15D7) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.047 134.493) (xy 122.047 134.874) (xy 122.428 134.874) (xy 122.428 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15D6) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.412 136.398) (xy 121.412 136.779) (xy 121.793 136.779) (xy 121.793 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15D5) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.952 133.858) (xy 123.952 134.239) (xy 124.333 134.239) (xy 124.333 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15D4) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.807 136.398) (xy 106.807 136.779) (xy 107.188 136.779) (xy 107.188 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15D3) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.412 135.763) (xy 121.412 136.144) (xy 121.793 136.144) (xy 121.793 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15D2) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.952 136.398) (xy 123.952 136.779) (xy 124.333 136.779) (xy 124.333 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15D1) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.047 135.128) (xy 122.047 135.509) (xy 122.428 135.509) (xy 122.428 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15D0) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.047 136.398) (xy 122.047 136.779) (xy 122.428 136.779) (xy 122.428 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15CF) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.047 135.763) (xy 122.047 136.144) (xy 122.428 136.144) (xy 122.428 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15CE) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.492 136.398) (xy 126.492 136.779) (xy 126.873 136.779) (xy 126.873 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15CD) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.047 137.668) (xy 122.047 138.049) (xy 122.428 138.049) (xy 122.428 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15CC) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.587 134.493) (xy 124.587 134.874) (xy 124.968 134.874) (xy 124.968 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15CB) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.492 137.668) (xy 126.492 138.049) (xy 126.873 138.049) (xy 126.873 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15CA) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.412 132.588) (xy 121.412 132.969) (xy 121.793 132.969) (xy 121.793 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15C9) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.952 135.128) (xy 123.952 135.509) (xy 124.333 135.509) (xy 124.333 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15C8) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.492 134.493) (xy 126.492 134.874) (xy 126.873 134.874) (xy 126.873 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15C7) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.092 133.223) (xy 101.092 133.604) (xy 101.473 133.604) (xy 101.473 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15C6) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.092 133.858) (xy 101.092 134.239) (xy 101.473 134.239) (xy 101.473 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15C5) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.727 137.033) (xy 101.727 137.414) (xy 102.108 137.414) (xy 102.108 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15C4) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.727 133.858) (xy 101.727 134.239) (xy 102.108 134.239) (xy 102.108 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15C3) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.487 138.303) (xy 86.487 138.684) (xy 86.868 138.684) (xy 86.868 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15C2) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.852 138.303) (xy 85.852 138.684) (xy 86.233 138.684) (xy 86.233 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15C1) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.852 137.033) (xy 85.852 137.414) (xy 86.233 137.414) (xy 86.233 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15C0) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.487 137.668) (xy 86.487 138.049) (xy 86.868 138.049) (xy 86.868 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15BF) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.852 132.588) (xy 85.852 132.969) (xy 86.233 132.969) (xy 86.233 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15BE) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.852 135.128) (xy 85.852 135.509) (xy 86.233 135.509) (xy 86.233 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15BD) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.487 134.493) (xy 86.487 134.874) (xy 86.868 134.874) (xy 86.868 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15BC) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.852 136.398) (xy 85.852 136.779) (xy 86.233 136.779) (xy 86.233 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15BB) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.487 135.763) (xy 86.487 136.144) (xy 86.868 136.144) (xy 86.868 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15BA) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.852 135.763) (xy 85.852 136.144) (xy 86.233 136.144) (xy 86.233 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15B9) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.487 136.398) (xy 86.487 136.779) (xy 86.868 136.779) (xy 86.868 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15B8) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.852 134.493) (xy 85.852 134.874) (xy 86.233 134.874) (xy 86.233 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15B7) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.487 135.128) (xy 86.487 135.509) (xy 86.868 135.509) (xy 86.868 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15B6) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.852 137.668) (xy 85.852 138.049) (xy 86.233 138.049) (xy 86.233 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15B5) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.027 131.953) (xy 89.027 132.334) (xy 89.408 132.334) (xy 89.408 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15B4) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.392 133.858) (xy 88.392 134.239) (xy 88.773 134.239) (xy 88.773 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15B3) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.632 137.668) (xy 103.632 138.049) (xy 104.013 138.049) (xy 104.013 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15B2) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.727 131.953) (xy 101.727 132.334) (xy 102.108 132.334) (xy 102.108 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15B1) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.727 132.588) (xy 101.727 132.969) (xy 102.108 132.969) (xy 102.108 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15B0) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 94.107 133.223) (xy 94.107 133.604) (xy 94.488 133.604) (xy 94.488 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15AF) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.092 131.953) (xy 101.092 132.334) (xy 101.473 132.334) (xy 101.473 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15AE) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.472 133.223) (xy 93.472 133.604) (xy 93.853 133.604) (xy 93.853 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15AD) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 94.107 133.858) (xy 94.107 134.239) (xy 94.488 134.239) (xy 94.488 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15AC) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.472 131.953) (xy 93.472 132.334) (xy 93.853 132.334) (xy 93.853 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15AB) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.092 137.668) (xy 101.092 138.049) (xy 101.473 138.049) (xy 101.473 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15AA) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.727 133.223) (xy 101.727 133.604) (xy 102.108 133.604) (xy 102.108 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15A9) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.567 132.588) (xy 91.567 132.969) (xy 91.948 132.969) (xy 91.948 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15A8) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.647 138.303) (xy 96.647 138.684) (xy 97.028 138.684) (xy 97.028 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15A7) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 94.107 137.033) (xy 94.107 137.414) (xy 94.488 137.414) (xy 94.488 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15A6) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 94.107 132.588) (xy 94.107 132.969) (xy 94.488 132.969) (xy 94.488 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15A5) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 94.107 138.303) (xy 94.107 138.684) (xy 94.488 138.684) (xy 94.488 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15A4) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.472 138.303) (xy 93.472 138.684) (xy 93.853 138.684) (xy 93.853 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15A3) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.472 137.033) (xy 93.472 137.414) (xy 93.853 137.414) (xy 93.853 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15A2) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 94.107 137.668) (xy 94.107 138.049) (xy 94.488 138.049) (xy 94.488 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15A1) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.472 132.588) (xy 93.472 132.969) (xy 93.853 132.969) (xy 93.853 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D15A0) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.472 135.128) (xy 93.472 135.509) (xy 93.853 135.509) (xy 93.853 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D159F) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.647 135.763) (xy 96.647 136.144) (xy 97.028 136.144) (xy 97.028 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D159E) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.012 135.763) (xy 96.012 136.144) (xy 96.393 136.144) (xy 96.393 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D159D) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.647 136.398) (xy 96.647 136.779) (xy 97.028 136.779) (xy 97.028 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D159C) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.012 134.493) (xy 96.012 134.874) (xy 96.393 134.874) (xy 96.393 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D159B) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.647 135.128) (xy 96.647 135.509) (xy 97.028 135.509) (xy 97.028 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D159A) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.012 137.668) (xy 96.012 138.049) (xy 96.393 138.049) (xy 96.393 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1599) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.187 131.953) (xy 99.187 132.334) (xy 99.568 132.334) (xy 99.568 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1598) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.552 133.858) (xy 98.552 134.239) (xy 98.933 134.239) (xy 98.933 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1597) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.187 133.223) (xy 99.187 133.604) (xy 99.568 133.604) (xy 99.568 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1596) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.552 133.223) (xy 98.552 133.604) (xy 98.933 133.604) (xy 98.933 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1595) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.507 133.223) (xy 119.507 133.604) (xy 119.888 133.604) (xy 119.888 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1594) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.872 133.223) (xy 118.872 133.604) (xy 119.253 133.604) (xy 119.253 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1593) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.507 133.858) (xy 119.507 134.239) (xy 119.888 134.239) (xy 119.888 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1592) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.872 131.953) (xy 118.872 132.334) (xy 119.253 132.334) (xy 119.253 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1591) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.507 137.033) (xy 119.507 137.414) (xy 119.888 137.414) (xy 119.888 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1590) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.507 132.588) (xy 119.507 132.969) (xy 119.888 132.969) (xy 119.888 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D158F) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.507 138.303) (xy 119.507 138.684) (xy 119.888 138.684) (xy 119.888 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D158E) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.172 135.128) (xy 106.172 135.509) (xy 106.553 135.509) (xy 106.553 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D158D) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.807 134.493) (xy 106.807 134.874) (xy 107.188 134.874) (xy 107.188 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D158C) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.172 136.398) (xy 106.172 136.779) (xy 106.553 136.779) (xy 106.553 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D158B) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.807 135.763) (xy 106.807 136.144) (xy 107.188 136.144) (xy 107.188 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D158A) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.792 135.128) (xy 113.792 135.509) (xy 114.173 135.509) (xy 114.173 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1589) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.872 137.033) (xy 118.872 137.414) (xy 119.253 137.414) (xy 119.253 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1588) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.507 137.668) (xy 119.507 138.049) (xy 119.888 138.049) (xy 119.888 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1587) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.872 132.588) (xy 118.872 132.969) (xy 119.253 132.969) (xy 119.253 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1586) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.392 137.033) (xy 88.392 137.414) (xy 88.773 137.414) (xy 88.773 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1585) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.027 137.668) (xy 89.027 138.049) (xy 89.408 138.049) (xy 89.408 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1584) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.392 132.588) (xy 88.392 132.969) (xy 88.773 132.969) (xy 88.773 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1583) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.567 138.303) (xy 91.567 138.684) (xy 91.948 138.684) (xy 91.948 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1582) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.932 138.303) (xy 90.932 138.684) (xy 91.313 138.684) (xy 91.313 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1581) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.932 137.033) (xy 90.932 137.414) (xy 91.313 137.414) (xy 91.313 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1580) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.567 137.668) (xy 91.567 138.049) (xy 91.948 138.049) (xy 91.948 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D157F) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.932 132.588) (xy 90.932 132.969) (xy 91.313 132.969) (xy 91.313 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D157E) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.187 134.493) (xy 99.187 134.874) (xy 99.568 134.874) (xy 99.568 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D157D) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.552 136.398) (xy 98.552 136.779) (xy 98.933 136.779) (xy 98.933 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D157C) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.187 135.763) (xy 99.187 136.144) (xy 99.568 136.144) (xy 99.568 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D157B) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.552 135.763) (xy 98.552 136.144) (xy 98.933 136.144) (xy 98.933 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D157A) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.187 136.398) (xy 99.187 136.779) (xy 99.568 136.779) (xy 99.568 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1579) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.552 134.493) (xy 98.552 134.874) (xy 98.933 134.874) (xy 98.933 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1578) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.187 135.128) (xy 99.187 135.509) (xy 99.568 135.509) (xy 99.568 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1577) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.552 137.668) (xy 98.552 138.049) (xy 98.933 138.049) (xy 98.933 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1576) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.647 131.953) (xy 96.647 132.334) (xy 97.028 132.334) (xy 97.028 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1575) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.012 133.858) (xy 96.012 134.239) (xy 96.393 134.239) (xy 96.393 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1574) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.647 133.223) (xy 96.647 133.604) (xy 97.028 133.604) (xy 97.028 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1573) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.012 133.223) (xy 96.012 133.604) (xy 96.393 133.604) (xy 96.393 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1572) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.647 133.858) (xy 96.647 134.239) (xy 97.028 134.239) (xy 97.028 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1571) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.012 131.953) (xy 96.012 132.334) (xy 96.393 132.334) (xy 96.393 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1570) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.647 137.033) (xy 96.647 137.414) (xy 97.028 137.414) (xy 97.028 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D156F) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.647 132.588) (xy 96.647 132.969) (xy 97.028 132.969) (xy 97.028 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D156E) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.727 135.763) (xy 101.727 136.144) (xy 102.108 136.144) (xy 102.108 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D156D) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.092 135.763) (xy 101.092 136.144) (xy 101.473 136.144) (xy 101.473 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D156C) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.552 135.128) (xy 98.552 135.509) (xy 98.933 135.509) (xy 98.933 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D156B) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.632 137.033) (xy 103.632 137.414) (xy 104.013 137.414) (xy 104.013 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D156A) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.267 137.668) (xy 104.267 138.049) (xy 104.648 138.049) (xy 104.648 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1569) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.632 132.588) (xy 103.632 132.969) (xy 104.013 132.969) (xy 104.013 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1568) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.472 137.668) (xy 93.472 138.049) (xy 93.853 138.049) (xy 93.853 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1567) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.567 131.953) (xy 91.567 132.334) (xy 91.948 132.334) (xy 91.948 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1566) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.727 135.128) (xy 101.727 135.509) (xy 102.108 135.509) (xy 102.108 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1565) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.932 133.858) (xy 90.932 134.239) (xy 91.313 134.239) (xy 91.313 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1564) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.567 133.223) (xy 91.567 133.604) (xy 91.948 133.604) (xy 91.948 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1563) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.932 133.223) (xy 90.932 133.604) (xy 91.313 133.604) (xy 91.313 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1562) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.567 133.858) (xy 91.567 134.239) (xy 91.948 134.239) (xy 91.948 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1561) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.932 131.953) (xy 90.932 132.334) (xy 91.313 132.334) (xy 91.313 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1560) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.727 136.398) (xy 101.727 136.779) (xy 102.108 136.779) (xy 102.108 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D155F) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.472 134.493) (xy 93.472 134.874) (xy 93.853 134.874) (xy 93.853 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D155E) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 94.107 135.128) (xy 94.107 135.509) (xy 94.488 135.509) (xy 94.488 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D155D) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.267 133.223) (xy 104.267 133.604) (xy 104.648 133.604) (xy 104.648 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D155C) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.632 133.223) (xy 103.632 133.604) (xy 104.013 133.604) (xy 104.013 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D155B) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.267 133.858) (xy 104.267 134.239) (xy 104.648 134.239) (xy 104.648 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D155A) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.632 131.953) (xy 103.632 132.334) (xy 104.013 132.334) (xy 104.013 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1559) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.267 137.033) (xy 104.267 137.414) (xy 104.648 137.414) (xy 104.648 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1558) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.267 132.588) (xy 104.267 132.969) (xy 104.648 132.969) (xy 104.648 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1557) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.267 138.303) (xy 104.267 138.684) (xy 104.648 138.684) (xy 104.648 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1556) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.932 135.128) (xy 90.932 135.509) (xy 91.313 135.509) (xy 91.313 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1555) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.567 134.493) (xy 91.567 134.874) (xy 91.948 134.874) (xy 91.948 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1554) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.932 136.398) (xy 90.932 136.779) (xy 91.313 136.779) (xy 91.313 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1553) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.567 135.763) (xy 91.567 136.144) (xy 91.948 136.144) (xy 91.948 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1552) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.932 135.763) (xy 90.932 136.144) (xy 91.313 136.144) (xy 91.313 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1551) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.567 136.398) (xy 91.567 136.779) (xy 91.948 136.779) (xy 91.948 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1550) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.267 134.493) (xy 104.267 134.874) (xy 104.648 134.874) (xy 104.648 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D154F) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.632 136.398) (xy 103.632 136.779) (xy 104.013 136.779) (xy 104.013 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D154E) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.267 135.763) (xy 104.267 136.144) (xy 104.648 136.144) (xy 104.648 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D154D) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.632 135.763) (xy 103.632 136.144) (xy 104.013 136.144) (xy 104.013 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D154C) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.267 136.398) (xy 104.267 136.779) (xy 104.648 136.779) (xy 104.648 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D154B) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.632 134.493) (xy 103.632 134.874) (xy 104.013 134.874) (xy 104.013 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D154A) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.267 135.128) (xy 104.267 135.509) (xy 104.648 135.509) (xy 104.648 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1549) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.632 135.128) (xy 103.632 135.509) (xy 104.013 135.509) (xy 104.013 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1548) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.727 138.303) (xy 101.727 138.684) (xy 102.108 138.684) (xy 102.108 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1547) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.092 138.303) (xy 101.092 138.684) (xy 101.473 138.684) (xy 101.473 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1546) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.092 137.033) (xy 101.092 137.414) (xy 101.473 137.414) (xy 101.473 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1545) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.727 137.668) (xy 101.727 138.049) (xy 102.108 138.049) (xy 102.108 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1544) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.092 132.588) (xy 101.092 132.969) (xy 101.473 132.969) (xy 101.473 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1543) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.092 135.128) (xy 101.092 135.509) (xy 101.473 135.509) (xy 101.473 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1542) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.727 134.493) (xy 101.727 134.874) (xy 102.108 134.874) (xy 102.108 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1541) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.092 136.398) (xy 101.092 136.779) (xy 101.473 136.779) (xy 101.473 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1540) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.267 131.953) (xy 104.267 132.334) (xy 104.648 132.334) (xy 104.648 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D153F) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.632 133.858) (xy 103.632 134.239) (xy 104.013 134.239) (xy 104.013 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D153E) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.947 133.223) (xy 83.947 133.604) (xy 84.328 133.604) (xy 84.328 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D153D) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.312 133.223) (xy 83.312 133.604) (xy 83.693 133.604) (xy 83.693 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D153C) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.947 133.858) (xy 83.947 134.239) (xy 84.328 134.239) (xy 84.328 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D153B) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.567 137.033) (xy 91.567 137.414) (xy 91.948 137.414) (xy 91.948 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D153A) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.947 131.953) (xy 83.947 132.334) (xy 84.328 132.334) (xy 84.328 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1539) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.772 131.953) (xy 80.772 132.334) (xy 81.153 132.334) (xy 81.153 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1538) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 81.407 137.033) (xy 81.407 137.414) (xy 81.788 137.414) (xy 81.788 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1537) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 81.407 132.588) (xy 81.407 132.969) (xy 81.788 132.969) (xy 81.788 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1536) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.027 134.493) (xy 89.027 134.874) (xy 89.408 134.874) (xy 89.408 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1535) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.392 136.398) (xy 88.392 136.779) (xy 88.773 136.779) (xy 88.773 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1534) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.027 135.763) (xy 89.027 136.144) (xy 89.408 136.144) (xy 89.408 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1533) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.392 135.763) (xy 88.392 136.144) (xy 88.773 136.144) (xy 88.773 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1532) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.027 136.398) (xy 89.027 136.779) (xy 89.408 136.779) (xy 89.408 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1531) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.392 134.493) (xy 88.392 134.874) (xy 88.773 134.874) (xy 88.773 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1530) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.027 135.128) (xy 89.027 135.509) (xy 89.408 135.509) (xy 89.408 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D152F) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.392 137.668) (xy 88.392 138.049) (xy 88.773 138.049) (xy 88.773 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D152E) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.487 131.953) (xy 86.487 132.334) (xy 86.868 132.334) (xy 86.868 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D152D) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.852 133.858) (xy 85.852 134.239) (xy 86.233 134.239) (xy 86.233 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D152C) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.487 133.223) (xy 86.487 133.604) (xy 86.868 133.604) (xy 86.868 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D152B) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.852 133.223) (xy 85.852 133.604) (xy 86.233 133.604) (xy 86.233 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D152A) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.487 133.858) (xy 86.487 134.239) (xy 86.868 134.239) (xy 86.868 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1529) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.852 131.953) (xy 85.852 132.334) (xy 86.233 132.334) (xy 86.233 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1528) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.487 137.033) (xy 86.487 137.414) (xy 86.868 137.414) (xy 86.868 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1527) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.487 132.588) (xy 86.487 132.969) (xy 86.868 132.969) (xy 86.868 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1526) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.392 135.128) (xy 88.392 135.509) (xy 88.773 135.509) (xy 88.773 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1525) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.312 133.858) (xy 83.312 134.239) (xy 83.693 134.239) (xy 83.693 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1524) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.312 131.953) (xy 83.312 132.334) (xy 83.693 132.334) (xy 83.693 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1523) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.947 137.033) (xy 83.947 137.414) (xy 84.328 137.414) (xy 84.328 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1522) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.947 132.588) (xy 83.947 132.969) (xy 84.328 132.969) (xy 84.328 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1521) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.947 138.303) (xy 83.947 138.684) (xy 84.328 138.684) (xy 84.328 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1520) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.312 138.303) (xy 83.312 138.684) (xy 83.693 138.684) (xy 83.693 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D151F) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.312 137.033) (xy 83.312 137.414) (xy 83.693 137.414) (xy 83.693 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D151E) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.947 137.668) (xy 83.947 138.049) (xy 84.328 138.049) (xy 84.328 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D151D) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 81.407 133.858) (xy 81.407 134.239) (xy 81.788 134.239) (xy 81.788 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D151C) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.092 134.493) (xy 101.092 134.874) (xy 101.473 134.874) (xy 101.473 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D151B) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.932 134.493) (xy 90.932 134.874) (xy 91.313 134.874) (xy 91.313 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D151A) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.567 135.128) (xy 91.567 135.509) (xy 91.948 135.509) (xy 91.948 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1519) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.932 137.668) (xy 90.932 138.049) (xy 91.313 138.049) (xy 91.313 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1518) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.632 138.303) (xy 103.632 138.684) (xy 104.013 138.684) (xy 104.013 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1517) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 94.107 131.953) (xy 94.107 132.334) (xy 94.488 132.334) (xy 94.488 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1516) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.472 133.858) (xy 93.472 134.239) (xy 93.853 134.239) (xy 93.853 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1515) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 94.107 134.493) (xy 94.107 134.874) (xy 94.488 134.874) (xy 94.488 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1514) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.472 136.398) (xy 93.472 136.779) (xy 93.853 136.779) (xy 93.853 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1513) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 94.107 135.763) (xy 94.107 136.144) (xy 94.488 136.144) (xy 94.488 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1512) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.472 135.763) (xy 93.472 136.144) (xy 93.853 136.144) (xy 93.853 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1511) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 94.107 136.398) (xy 94.107 136.779) (xy 94.488 136.779) (xy 94.488 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1510) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.807 133.858) (xy 106.807 134.239) (xy 107.188 134.239) (xy 107.188 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D150F) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.172 131.953) (xy 106.172 132.334) (xy 106.553 132.334) (xy 106.553 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D150E) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.967 136.398) (xy 116.967 136.779) (xy 117.348 136.779) (xy 117.348 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D150D) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.332 134.493) (xy 116.332 134.874) (xy 116.713 134.874) (xy 116.713 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D150C) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.807 137.033) (xy 106.807 137.414) (xy 107.188 137.414) (xy 107.188 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D150B) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.807 132.588) (xy 106.807 132.969) (xy 107.188 132.969) (xy 107.188 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D150A) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.347 135.128) (xy 109.347 135.509) (xy 109.728 135.509) (xy 109.728 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1509) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.712 137.668) (xy 108.712 138.049) (xy 109.093 138.049) (xy 109.093 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1508) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.712 135.763) (xy 108.712 136.144) (xy 109.093 136.144) (xy 109.093 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1507) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.347 136.398) (xy 109.347 136.779) (xy 109.728 136.779) (xy 109.728 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1506) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.712 134.493) (xy 108.712 134.874) (xy 109.093 134.874) (xy 109.093 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1505) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.507 136.398) (xy 119.507 136.779) (xy 119.888 136.779) (xy 119.888 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1504) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.872 134.493) (xy 118.872 134.874) (xy 119.253 134.874) (xy 119.253 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1503) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.507 135.128) (xy 119.507 135.509) (xy 119.888 135.509) (xy 119.888 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1502) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.872 137.668) (xy 118.872 138.049) (xy 119.253 138.049) (xy 119.253 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1501) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.967 131.953) (xy 116.967 132.334) (xy 117.348 132.334) (xy 117.348 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1500) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.332 133.858) (xy 116.332 134.239) (xy 116.713 134.239) (xy 116.713 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D14FF) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.332 137.668) (xy 116.332 138.049) (xy 116.713 138.049) (xy 116.713 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D14FE) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.967 133.223) (xy 116.967 133.604) (xy 117.348 133.604) (xy 117.348 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14FD) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.427 137.033) (xy 114.427 137.414) (xy 114.808 137.414) (xy 114.808 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14FC) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.427 132.588) (xy 114.427 132.969) (xy 114.808 132.969) (xy 114.808 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14FB) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.427 138.303) (xy 114.427 138.684) (xy 114.808 138.684) (xy 114.808 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14FA) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.792 138.303) (xy 113.792 138.684) (xy 114.173 138.684) (xy 114.173 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14F9) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.792 137.033) (xy 113.792 137.414) (xy 114.173 137.414) (xy 114.173 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14F8) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.712 138.303) (xy 108.712 138.684) (xy 109.093 138.684) (xy 109.093 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14F7) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.712 137.033) (xy 108.712 137.414) (xy 109.093 137.414) (xy 109.093 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14F6) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.347 137.668) (xy 109.347 138.049) (xy 109.728 138.049) (xy 109.728 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14F5) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.712 132.588) (xy 108.712 132.969) (xy 109.093 132.969) (xy 109.093 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14F4) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.712 135.128) (xy 108.712 135.509) (xy 109.093 135.509) (xy 109.093 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14F3) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.347 134.493) (xy 109.347 134.874) (xy 109.728 134.874) (xy 109.728 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14F2) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.712 136.398) (xy 108.712 136.779) (xy 109.093 136.779) (xy 109.093 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14F1) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.347 135.763) (xy 109.347 136.144) (xy 109.728 136.144) (xy 109.728 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D14F0) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.507 134.493) (xy 119.507 134.874) (xy 119.888 134.874) (xy 119.888 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D14EF) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.872 136.398) (xy 118.872 136.779) (xy 119.253 136.779) (xy 119.253 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14EE) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.207 134.493) (xy 132.207 134.874) (xy 132.588 134.874) (xy 132.588 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14ED) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.572 136.398) (xy 131.572 136.779) (xy 131.953 136.779) (xy 131.953 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14EC) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.207 135.763) (xy 132.207 136.144) (xy 132.588 136.144) (xy 132.588 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14EB) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.572 135.763) (xy 131.572 136.144) (xy 131.953 136.144) (xy 131.953 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14EA) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.207 136.398) (xy 132.207 136.779) (xy 132.588 136.779) (xy 132.588 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14E9) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.572 134.493) (xy 131.572 134.874) (xy 131.953 134.874) (xy 131.953 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14E8) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.207 135.128) (xy 132.207 135.509) (xy 132.588 135.509) (xy 132.588 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14E7) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.572 137.668) (xy 131.572 138.049) (xy 131.953 138.049) (xy 131.953 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14E6) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.667 131.953) (xy 129.667 132.334) (xy 130.048 132.334) (xy 130.048 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14E5) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.032 133.858) (xy 129.032 134.239) (xy 129.413 134.239) (xy 129.413 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14E4) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.667 133.223) (xy 129.667 133.604) (xy 130.048 133.604) (xy 130.048 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14E3) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.032 133.223) (xy 129.032 133.604) (xy 129.413 133.604) (xy 129.413 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14E2) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.667 133.858) (xy 129.667 134.239) (xy 130.048 134.239) (xy 130.048 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14E1) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.032 131.953) (xy 129.032 132.334) (xy 129.413 132.334) (xy 129.413 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14E0) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.667 137.033) (xy 129.667 137.414) (xy 130.048 137.414) (xy 130.048 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14DF) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.667 132.588) (xy 129.667 132.969) (xy 130.048 132.969) (xy 130.048 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14DE) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.747 135.763) (xy 134.747 136.144) (xy 135.128 136.144) (xy 135.128 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14DD) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.112 135.763) (xy 134.112 136.144) (xy 134.493 136.144) (xy 134.493 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14DC) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.747 131.953) (xy 134.747 132.334) (xy 135.128 132.334) (xy 135.128 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14DB) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.112 133.858) (xy 134.112 134.239) (xy 134.493 134.239) (xy 134.493 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14DA) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.112 137.668) (xy 134.112 138.049) (xy 134.493 138.049) (xy 134.493 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14D9) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.747 133.223) (xy 134.747 133.604) (xy 135.128 133.604) (xy 135.128 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14D8) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.207 137.033) (xy 132.207 137.414) (xy 132.588 137.414) (xy 132.588 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14D7) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.207 132.588) (xy 132.207 132.969) (xy 132.588 132.969) (xy 132.588 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14D6) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.207 138.303) (xy 132.207 138.684) (xy 132.588 138.684) (xy 132.588 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14D5) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.572 138.303) (xy 131.572 138.684) (xy 131.953 138.684) (xy 131.953 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14D4) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.572 137.033) (xy 131.572 137.414) (xy 131.953 137.414) (xy 131.953 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14D3) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.207 137.668) (xy 132.207 138.049) (xy 132.588 138.049) (xy 132.588 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14D2) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.572 132.588) (xy 131.572 132.969) (xy 131.953 132.969) (xy 131.953 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14D1) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.412 131.953) (xy 121.412 132.334) (xy 121.793 132.334) (xy 121.793 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14D0) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.047 137.033) (xy 122.047 137.414) (xy 122.428 137.414) (xy 122.428 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14CF) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.047 132.588) (xy 122.047 132.969) (xy 122.428 132.969) (xy 122.428 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14CE) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.047 138.303) (xy 122.047 138.684) (xy 122.428 138.684) (xy 122.428 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14CD) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.747 132.588) (xy 134.747 132.969) (xy 135.128 132.969) (xy 135.128 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14CC) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.952 135.763) (xy 123.952 136.144) (xy 124.333 136.144) (xy 124.333 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14CB) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.952 137.033) (xy 123.952 137.414) (xy 124.333 137.414) (xy 124.333 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14CA) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.587 137.668) (xy 124.587 138.049) (xy 124.968 138.049) (xy 124.968 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14C9) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.887 138.303) (xy 111.887 138.684) (xy 112.268 138.684) (xy 112.268 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14C8) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.252 138.303) (xy 111.252 138.684) (xy 111.633 138.684) (xy 111.633 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14C7) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.252 137.033) (xy 111.252 137.414) (xy 111.633 137.414) (xy 111.633 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14C6) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.347 131.953) (xy 109.347 132.334) (xy 109.728 132.334) (xy 109.728 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14C5) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.712 133.858) (xy 108.712 134.239) (xy 109.093 134.239) (xy 109.093 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14C4) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.347 133.223) (xy 109.347 133.604) (xy 109.728 133.604) (xy 109.728 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14C3) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.712 133.223) (xy 108.712 133.604) (xy 109.093 133.604) (xy 109.093 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14C2) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.792 131.953) (xy 113.792 132.334) (xy 114.173 132.334) (xy 114.173 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14C1) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.347 133.858) (xy 109.347 134.239) (xy 109.728 134.239) (xy 109.728 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14C0) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.712 131.953) (xy 108.712 132.334) (xy 109.093 132.334) (xy 109.093 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14BF) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.792 133.858) (xy 113.792 134.239) (xy 114.173 134.239) (xy 114.173 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14BE) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.427 133.223) (xy 114.427 133.604) (xy 114.808 133.604) (xy 114.808 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D14BD) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.967 137.033) (xy 116.967 137.414) (xy 117.348 137.414) (xy 117.348 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14BC) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.347 137.033) (xy 109.347 137.414) (xy 109.728 137.414) (xy 109.728 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14BB) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.347 132.588) (xy 109.347 132.969) (xy 109.728 132.969) (xy 109.728 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14BA) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.807 138.303) (xy 106.807 138.684) (xy 107.188 138.684) (xy 107.188 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14B9) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.172 138.303) (xy 106.172 138.684) (xy 106.553 138.684) (xy 106.553 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D14B8) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.332 133.223) (xy 116.332 133.604) (xy 116.713 133.604) (xy 116.713 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D14B7) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.967 133.858) (xy 116.967 134.239) (xy 117.348 134.239) (xy 117.348 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D14B6) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.332 131.953) (xy 116.332 132.334) (xy 116.713 132.334) (xy 116.713 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14B5) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.412 135.128) (xy 121.412 135.509) (xy 121.793 135.509) (xy 121.793 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14B4) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.047 131.953) (xy 122.047 132.334) (xy 122.428 132.334) (xy 122.428 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14B3) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.412 133.858) (xy 121.412 134.239) (xy 121.793 134.239) (xy 121.793 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14B2) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.047 133.223) (xy 122.047 133.604) (xy 122.428 133.604) (xy 122.428 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14B1) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.412 133.223) (xy 121.412 133.604) (xy 121.793 133.604) (xy 121.793 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14B0) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.047 133.858) (xy 122.047 134.239) (xy 122.428 134.239) (xy 122.428 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14AF) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.807 131.953) (xy 106.807 132.334) (xy 107.188 132.334) (xy 107.188 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D14AE) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.967 135.128) (xy 116.967 135.509) (xy 117.348 135.509) (xy 117.348 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14AD) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.172 133.858) (xy 106.172 134.239) (xy 106.553 134.239) (xy 106.553 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14AC) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.807 133.223) (xy 106.807 133.604) (xy 107.188 133.604) (xy 107.188 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14AB) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.172 133.223) (xy 106.172 133.604) (xy 106.553 133.604) (xy 106.553 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14AA) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 81.407 133.223) (xy 81.407 133.604) (xy 81.788 133.604) (xy 81.788 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14A9) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.772 133.223) (xy 80.772 133.604) (xy 81.153 133.604) (xy 81.153 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14A8) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.027 133.223) (xy 89.027 133.604) (xy 89.408 133.604) (xy 89.408 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14A7) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.867 133.223) (xy 78.867 133.604) (xy 79.248 133.604) (xy 79.248 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14A6) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.232 133.223) (xy 78.232 133.604) (xy 78.613 133.604) (xy 78.613 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14A5) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.867 133.858) (xy 78.867 134.239) (xy 79.248 134.239) (xy 79.248 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14A4) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.232 131.953) (xy 78.232 132.334) (xy 78.613 132.334) (xy 78.613 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14A3) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.867 136.398) (xy 78.867 136.779) (xy 79.248 136.779) (xy 79.248 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14A2) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.232 137.668) (xy 78.232 138.049) (xy 78.613 138.049) (xy 78.613 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14A1) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.867 131.953) (xy 78.867 132.334) (xy 79.248 132.334) (xy 79.248 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D14A0) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.232 133.858) (xy 78.232 134.239) (xy 78.613 134.239) (xy 78.613 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D149F) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.232 134.493) (xy 78.232 134.874) (xy 78.613 134.874) (xy 78.613 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D149E) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.867 135.128) (xy 78.867 135.509) (xy 79.248 135.509) (xy 79.248 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D149D) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.692 131.953) (xy 75.692 132.334) (xy 76.073 132.334) (xy 76.073 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D149C) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.327 131.953) (xy 76.327 132.334) (xy 76.708 132.334) (xy 76.708 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D149B) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.112 136.398) (xy 134.112 136.779) (xy 134.493 136.779) (xy 134.493 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D149A) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.747 134.493) (xy 134.747 134.874) (xy 135.128 134.874) (xy 135.128 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1499) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.412 138.303) (xy 121.412 138.684) (xy 121.793 138.684) (xy 121.793 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1498) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.112 135.128) (xy 134.112 135.509) (xy 134.493 135.509) (xy 134.493 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1497) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.747 133.858) (xy 134.747 134.239) (xy 135.128 134.239) (xy 135.128 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1496) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.112 131.953) (xy 134.112 132.334) (xy 134.493 132.334) (xy 134.493 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1495) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.032 137.668) (xy 129.032 138.049) (xy 129.413 138.049) (xy 129.413 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1494) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.207 131.953) (xy 132.207 132.334) (xy 132.588 132.334) (xy 132.588 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1493) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.127 138.303) (xy 127.127 138.684) (xy 127.508 138.684) (xy 127.508 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1492) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.492 138.303) (xy 126.492 138.684) (xy 126.873 138.684) (xy 126.873 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1491) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.492 137.033) (xy 126.492 137.414) (xy 126.873 137.414) (xy 126.873 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1490) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.127 137.668) (xy 127.127 138.049) (xy 127.508 138.049) (xy 127.508 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D148F) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.492 132.588) (xy 126.492 132.969) (xy 126.873 132.969) (xy 126.873 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D148E) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.492 135.128) (xy 126.492 135.509) (xy 126.873 135.509) (xy 126.873 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D148D) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.952 133.223) (xy 123.952 133.604) (xy 124.333 133.604) (xy 124.333 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D148C) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.587 133.858) (xy 124.587 134.239) (xy 124.968 134.239) (xy 124.968 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D148B) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.952 131.953) (xy 123.952 132.334) (xy 124.333 132.334) (xy 124.333 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D148A) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.747 136.398) (xy 134.747 136.779) (xy 135.128 136.779) (xy 135.128 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1489) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.112 134.493) (xy 134.112 134.874) (xy 134.493 134.874) (xy 134.493 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1488) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.587 137.033) (xy 124.587 137.414) (xy 124.968 137.414) (xy 124.968 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1487) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.587 132.588) (xy 124.587 132.969) (xy 124.968 132.969) (xy 124.968 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1486) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.667 138.303) (xy 129.667 138.684) (xy 130.048 138.684) (xy 130.048 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1485) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.032 138.303) (xy 129.032 138.684) (xy 129.413 138.684) (xy 129.413 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1484) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.032 137.033) (xy 129.032 137.414) (xy 129.413 137.414) (xy 129.413 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1483) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.667 137.668) (xy 129.667 138.049) (xy 130.048 138.049) (xy 130.048 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1482) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.032 132.588) (xy 129.032 132.969) (xy 129.413 132.969) (xy 129.413 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1481) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.032 135.128) (xy 129.032 135.509) (xy 129.413 135.509) (xy 129.413 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1480) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.667 134.493) (xy 129.667 134.874) (xy 130.048 134.874) (xy 130.048 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D147F) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.032 136.398) (xy 129.032 136.779) (xy 129.413 136.779) (xy 129.413 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D147E) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.572 133.223) (xy 131.572 133.604) (xy 131.953 133.604) (xy 131.953 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D147D) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.207 133.858) (xy 132.207 134.239) (xy 132.588 134.239) (xy 132.588 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D147C) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.587 136.398) (xy 124.587 136.779) (xy 124.968 136.779) (xy 124.968 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D147B) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.952 134.493) (xy 123.952 134.874) (xy 124.333 134.874) (xy 124.333 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D147A) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.587 135.128) (xy 124.587 135.509) (xy 124.968 135.509) (xy 124.968 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1479) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.952 137.668) (xy 123.952 138.049) (xy 124.333 138.049) (xy 124.333 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1478) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.127 131.953) (xy 127.127 132.334) (xy 127.508 132.334) (xy 127.508 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1477) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.492 133.858) (xy 126.492 134.239) (xy 126.873 134.239) (xy 126.873 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1476) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.127 133.223) (xy 127.127 133.604) (xy 127.508 133.604) (xy 127.508 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1475) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.492 133.223) (xy 126.492 133.604) (xy 126.873 133.604) (xy 126.873 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1474) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.572 131.953) (xy 131.572 132.334) (xy 131.953 132.334) (xy 131.953 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1473) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.127 133.858) (xy 127.127 134.239) (xy 127.508 134.239) (xy 127.508 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1472) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.492 131.953) (xy 126.492 132.334) (xy 126.873 132.334) (xy 126.873 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1471) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.572 133.858) (xy 131.572 134.239) (xy 131.953 134.239) (xy 131.953 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1470) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.207 133.223) (xy 132.207 133.604) (xy 132.588 133.604) (xy 132.588 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D146F) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.747 137.033) (xy 134.747 137.414) (xy 135.128 137.414) (xy 135.128 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D146E) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.127 137.033) (xy 127.127 137.414) (xy 127.508 137.414) (xy 127.508 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D146D) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.127 132.588) (xy 127.127 132.969) (xy 127.508 132.969) (xy 127.508 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D146C) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.587 138.303) (xy 124.587 138.684) (xy 124.968 138.684) (xy 124.968 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D146B) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.952 138.303) (xy 123.952 138.684) (xy 124.333 138.684) (xy 124.333 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D146A) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.112 133.223) (xy 134.112 133.604) (xy 134.493 133.604) (xy 134.493 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1469) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.667 136.398) (xy 129.667 136.779) (xy 130.048 136.779) (xy 130.048 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1468) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.032 134.493) (xy 129.032 134.874) (xy 129.413 134.874) (xy 129.413 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1467) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.667 135.128) (xy 129.667 135.509) (xy 130.048 135.509) (xy 130.048 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1466) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.667 135.763) (xy 129.667 136.144) (xy 130.048 136.144) (xy 130.048 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1465) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.032 135.763) (xy 129.032 136.144) (xy 129.413 136.144) (xy 129.413 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1464) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.952 132.588) (xy 123.952 132.969) (xy 124.333 132.969) (xy 124.333 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1463) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.312 132.588) (xy 83.312 132.969) (xy 83.693 132.969) (xy 83.693 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1462) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.312 135.128) (xy 83.312 135.509) (xy 83.693 135.509) (xy 83.693 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1461) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.947 134.493) (xy 83.947 134.874) (xy 84.328 134.874) (xy 84.328 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1460) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.312 136.398) (xy 83.312 136.779) (xy 83.693 136.779) (xy 83.693 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D145F) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.947 135.763) (xy 83.947 136.144) (xy 84.328 136.144) (xy 84.328 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D145E) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.312 135.763) (xy 83.312 136.144) (xy 83.693 136.144) (xy 83.693 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D145D) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.947 136.398) (xy 83.947 136.779) (xy 84.328 136.779) (xy 84.328 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D145C) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.312 134.493) (xy 83.312 134.874) (xy 83.693 134.874) (xy 83.693 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D145B) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.947 135.128) (xy 83.947 135.509) (xy 84.328 135.509) (xy 84.328 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D145A) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.312 137.668) (xy 83.312 138.049) (xy 83.693 138.049) (xy 83.693 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1459) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 81.407 131.953) (xy 81.407 132.334) (xy 81.788 132.334) (xy 81.788 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1458) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.772 133.858) (xy 80.772 134.239) (xy 81.153 134.239) (xy 81.153 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D1457) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.872 135.763) (xy 118.872 136.144) (xy 119.253 136.144) (xy 119.253 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1456) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.027 138.303) (xy 89.027 138.684) (xy 89.408 138.684) (xy 89.408 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1455) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.392 138.303) (xy 88.392 138.684) (xy 88.773 138.684) (xy 88.773 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1454) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.027 137.033) (xy 89.027 137.414) (xy 89.408 137.414) (xy 89.408 137.033)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1453) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.027 132.588) (xy 89.027 132.969) (xy 89.408 132.969) (xy 89.408 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1452) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.027 133.858) (xy 89.027 134.239) (xy 89.408 134.239) (xy 89.408 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1451) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.392 131.953) (xy 88.392 132.334) (xy 88.773 132.334) (xy 88.773 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1450) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.392 133.223) (xy 88.392 133.604) (xy 88.773 133.604) (xy 88.773 133.223)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D144F) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.347 138.303) (xy 109.347 138.684) (xy 109.728 138.684) (xy 109.728 138.303)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D144E) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.887 135.763) (xy 111.887 136.144) (xy 112.268 136.144) (xy 112.268 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (tstamp 5F5D144D) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.507 135.763) (xy 119.507 136.144) (xy 119.888 136.144) (xy 119.888 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D144C) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.252 135.763) (xy 111.252 136.144) (xy 111.633 136.144) (xy 111.633 135.763)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D144B) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.252 136.398) (xy 111.252 136.779) (xy 111.633 136.779) (xy 111.633 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D144A) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.427 131.953) (xy 114.427 132.334) (xy 114.808 132.334) (xy 114.808 131.953)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1449) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.252 137.668) (xy 111.252 138.049) (xy 111.633 138.049) (xy 111.633 137.668)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1448) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.887 135.128) (xy 111.887 135.509) (xy 112.268 135.509) (xy 112.268 135.128)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1447) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.252 134.493) (xy 111.252 134.874) (xy 111.633 134.874) (xy 111.633 134.493)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1446) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.792 132.588) (xy 113.792 132.969) (xy 114.173 132.969) (xy 114.173 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1445) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.427 133.858) (xy 114.427 134.239) (xy 114.808 134.239) (xy 114.808 133.858)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1444) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.887 136.398) (xy 111.887 136.779) (xy 112.268 136.779) (xy 112.268 136.398)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu) (tstamp 5F5D1443) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.887 134.493) (xy 111.887 134.874) (xy 112.268 134.874) (xy 112.268 134.493)
      )
    )
  )
)
