{ "Info" "IQEXE_SEPARATOR" "" "*******************************************************************" {  } {  } 3 0 "*******************************************************************" 0 0 "Quartus II" 0 -1 1591131666606 ""}
{ "Info" "IQEXE_START_BANNER_PRODUCT" "TimeQuest Timing Analyzer Quartus II 64-Bit " "Running Quartus II 64-Bit TimeQuest Timing Analyzer" { { "Info" "IQEXE_START_BANNER_VERSION" "Version 13.0.1 Build 232 06/12/2013 Service Pack 1 SJ Web Edition " "Version 13.0.1 Build 232 06/12/2013 Service Pack 1 SJ Web Edition" {  } {  } 0 0 "%1!s!" 0 0 "Quartus II" 0 -1 1591131666607 ""} { "Info" "IQEXE_START_BANNER_TIME" "Tue Jun 02 17:01:06 2020 " "Processing started: Tue Jun 02 17:01:06 2020" {  } {  } 0 0 "Processing started: %1!s!" 0 0 "Quartus II" 0 -1 1591131666607 ""}  } {  } 4 0 "Running %2!s! %1!s!" 0 0 "Quartus II" 0 -1 1591131666607 ""}
{ "Info" "IQEXE_START_BANNER_COMMANDLINE" "quartus_sta RAM2E -c RAM2E " "Command: quartus_sta RAM2E -c RAM2E" {  } {  } 0 0 "Command: %1!s!" 0 0 "Quartus II" 0 -1 1591131666607 ""}
{ "Info" "0" "" "qsta_default_script.tcl version: #1" {  } {  } 0 0 "qsta_default_script.tcl version: #1" 0 0 "Quartus II" 0 0 1591131666668 ""}
{ "Warning" "WQCU_PARALLEL_NO_LICENSE" "" "Parallel compilation is not licensed and has been disabled" {  } {  } 0 20028 "Parallel compilation is not licensed and has been disabled" 0 0 "Quartus II" 0 -1 1591131666769 ""}
{ "Info" "ICUT_CUT_USING_OPERATING_CONDITION" "Low junction temperature 0 degrees C " "Low junction temperature is 0 degrees C" {  } {  } 0 21077 "%1!s! is %2!s!" 0 0 "Quartus II" 0 -1 1591131666805 ""}
{ "Info" "ICUT_CUT_USING_OPERATING_CONDITION" "High junction temperature 85 degrees C " "High junction temperature is 85 degrees C" {  } {  } 0 21077 "%1!s! is %2!s!" 0 0 "Quartus II" 0 -1 1591131666805 ""}
{ "Info" "IDAT_DAT_STARTED" "" "Started post-fitting delay annotation" {  } {  } 0 306004 "Started post-fitting delay annotation" 0 0 "Quartus II" 0 -1 1591131666836 ""}
{ "Info" "IDAT_DAT_COMPLETED" "" "Delay annotation completed successfully" {  } {  } 0 306005 "Delay annotation completed successfully" 0 0 "Quartus II" 0 -1 1591131666999 ""}
{ "Info" "ISTA_SDC_FOUND" "constraints.sdc " "Reading SDC File: 'constraints.sdc'" {  } {  } 0 332104 "Reading SDC File: '%1!s!'" 0 0 "Quartus II" 0 -1 1591131667120 ""}
{ "Warning" "WSTA_NODE_FOUND_WITHOUT_CLOCK_ASSIGNMENT" "DRCLK " "Node: DRCLK was determined to be a clock but was found without an associated clock assignment." {  } {  } 0 332060 "Node: %1!s! was determined to be a clock but was found without an associated clock assignment." 0 0 "Quartus II" 0 -1 1591131667127 "|RAM2E|DRCLK"}
{ "Warning" "WSTA_NODE_FOUND_WITHOUT_CLOCK_ASSIGNMENT" "ARCLK " "Node: ARCLK was determined to be a clock but was found without an associated clock assignment." {  } {  } 0 332060 "Node: %1!s! was determined to be a clock but was found without an associated clock assignment." 0 0 "Quartus II" 0 -1 1591131667127 "|RAM2E|ARCLK"}
{ "Info" "0" "" "Found TIMEQUEST_REPORT_SCRIPT_INCLUDE_DEFAULT_ANALYSIS = ON" {  } {  } 0 0 "Found TIMEQUEST_REPORT_SCRIPT_INCLUDE_DEFAULT_ANALYSIS = ON" 0 0 "Quartus II" 0 0 1591131667130 ""}
{ "Info" "ISTA_WORST_CASE_SLACK" "setup 28.330 " "Worst-case setup slack is 28.330" { { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "    Slack End Point TNS Clock  " "    Slack End Point TNS Clock " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1591131667154 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "========= ============= ===================== " "========= ============= =====================" {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1591131667154 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "   28.330         0.000 C14M  " "   28.330         0.000 C14M " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1591131667154 ""}  } {  } 0 332146 "Worst-case %1!s! slack is %2!s!" 0 0 "Quartus II" 0 -1 1591131667154 ""}
{ "Info" "ISTA_WORST_CASE_SLACK" "hold 1.425 " "Worst-case hold slack is 1.425" { { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "    Slack End Point TNS Clock  " "    Slack End Point TNS Clock " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1591131667160 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "========= ============= ===================== " "========= ============= =====================" {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1591131667160 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "    1.425         0.000 C14M  " "    1.425         0.000 C14M " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1591131667160 ""}  } {  } 0 332146 "Worst-case %1!s! slack is %2!s!" 0 0 "Quartus II" 0 -1 1591131667160 ""}
{ "Info" "ISTA_NO_PATHS_TO_REPORT" "Recovery " "No Recovery paths to report" {  } {  } 0 332140 "No %1!s! paths to report" 0 0 "Quartus II" 0 -1 1591131667167 ""}
{ "Info" "ISTA_NO_PATHS_TO_REPORT" "Removal " "No Removal paths to report" {  } {  } 0 332140 "No %1!s! paths to report" 0 0 "Quartus II" 0 -1 1591131667172 ""}
{ "Info" "ISTA_WORST_CASE_SLACK" "minimum pulse width 34.654 " "Worst-case minimum pulse width slack is 34.654" { { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "    Slack End Point TNS Clock  " "    Slack End Point TNS Clock " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1591131667178 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "========= ============= ===================== " "========= ============= =====================" {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1591131667178 ""} { "Info" "ISTA_CREATE_TIMING_SUMMARY_INFO" "   34.654         0.000 C14M  " "   34.654         0.000 C14M " {  } {  } 0 332119 "%1!s!" 0 0 "Quartus II" 0 -1 1591131667178 ""}  } {  } 0 332146 "Worst-case %1!s! slack is %2!s!" 0 0 "Quartus II" 0 -1 1591131667178 ""}
{ "Info" "ISTA_METASTABILITY_REPORT_DISABLED" "" "The selected device family is not supported by the report_metastability command." {  } {  } 0 332001 "The selected device family is not supported by the report_metastability command." 0 0 "Quartus II" 0 -1 1591131667220 ""}
{ "Info" "ISTA_UCP_NOT_CONSTRAINED" "setup " "Design is not fully constrained for setup requirements" {  } {  } 0 332102 "Design is not fully constrained for %1!s! requirements" 0 0 "Quartus II" 0 -1 1591131667245 ""}
{ "Info" "ISTA_UCP_NOT_CONSTRAINED" "hold " "Design is not fully constrained for hold requirements" {  } {  } 0 332102 "Design is not fully constrained for %1!s! requirements" 0 0 "Quartus II" 0 -1 1591131667246 ""}
{ "Info" "IQEXE_ERROR_COUNT" "TimeQuest Timing Analyzer 0 s 3 s Quartus II 64-Bit " "Quartus II 64-Bit TimeQuest Timing Analyzer was successful. 0 errors, 3 warnings" { { "Info" "IQEXE_END_PEAK_VSIZE_MEMORY" "4522 " "Peak virtual memory: 4522 megabytes" {  } {  } 0 0 "Peak virtual memory: %1!s! megabytes" 0 0 "Quartus II" 0 -1 1591131667319 ""} { "Info" "IQEXE_END_BANNER_TIME" "Tue Jun 02 17:01:07 2020 " "Processing ended: Tue Jun 02 17:01:07 2020" {  } {  } 0 0 "Processing ended: %1!s!" 0 0 "Quartus II" 0 -1 1591131667319 ""} { "Info" "IQEXE_ELAPSED_TIME" "00:00:01 " "Elapsed time: 00:00:01" {  } {  } 0 0 "Elapsed time: %1!s!" 0 0 "Quartus II" 0 -1 1591131667319 ""} { "Info" "IQEXE_ELAPSED_CPU_TIME" "00:00:01 " "Total CPU time (on all processors): 00:00:01" {  } {  } 0 0 "Total CPU time (on all processors): %1!s!" 0 0 "Quartus II" 0 -1 1591131667319 ""}  } {  } 0 0 "%6!s! %1!s! was successful. %2!d! error%3!s!, %4!d! warning%5!s!" 0 0 "Quartus II" 0 -1 1591131667319 ""}
