<?xml version="1.0" encoding="UTF-8"?>
<simconf>
  <project EXPORT="discard">[CONTIKI_DIR]/tools/cooja/apps/mrm</project>
  <project EXPORT="discard">[CONTIKI_DIR]/tools/cooja/apps/mspsim</project>
  <project EXPORT="discard">[CONTIKI_DIR]/tools/cooja/apps/avrora</project>
  <project EXPORT="discard">[CONTIKI_DIR]/tools/cooja/apps/native_gateway</project>
  <simulation>
    <title>My simulation</title>
    <delaytime>0</delaytime>
    <randomseed>generated</randomseed>
    <motedelay_us>1000000</motedelay_us>
    <radiomedium>
      se.sics.cooja.radiomediums.UDGM
      <transmitting_range>50.0</transmitting_range>
      <interference_range>100.0</interference_range>
      <success_ratio_tx>1.0</success_ratio_tx>
      <success_ratio_rx>1.0</success_ratio_rx>
    </radiomedium>
    <events>
      <logoutput>40000</logoutput>
    </events>
    <motetype>
      se.sics.cooja.mspmote.SkyMoteType
      <identifier>sky1</identifier>
      <description>Sky Mote Type #1</description>
      <source EXPORT="discard">[CONTIKI_DIR]/examples/sky-shell/sky-shell.c</source>
      <commands EXPORT="discard">make clean TARGET=sky
make sky-shell.sky TARGET=sky</commands>
      <firmware EXPORT="copy">[CONTIKI_DIR]/examples/sky-shell/sky-shell.sky</firmware>
      <moteinterface>se.sics.cooja.interfaces.Position</moteinterface>
      <moteinterface>se.sics.cooja.interfaces.IPAddress</moteinterface>
      <moteinterface>se.sics.cooja.interfaces.Mote2MoteRelations</moteinterface>
      <moteinterface>se.sics.cooja.mspmote.interfaces.MspClock</moteinterface>
      <moteinterface>se.sics.cooja.mspmote.interfaces.MspMoteID</moteinterface>
      <moteinterface>se.sics.cooja.mspmote.interfaces.SkyButton</moteinterface>
      <moteinterface>se.sics.cooja.mspmote.interfaces.SkyFlash</moteinterface>
      <moteinterface>se.sics.cooja.mspmote.interfaces.SkyByteRadio</moteinterface>
      <moteinterface>se.sics.cooja.mspmote.interfaces.MspSerial</moteinterface>
      <moteinterface>se.sics.cooja.mspmote.interfaces.SkyLED</moteinterface>
      <moteinterface>se.sics.cooja.interfaces.RimeAddress</moteinterface>
      <moteinterface>se.sics.cooja.interfaces.MoteAttributes</moteinterface>
      <moteinterface>se.sics.cooja.mspmote.interfaces.SkyCoffeeFilesystem</moteinterface>
      <moteinterface>se.sics.cooja.mspmote.interfaces.MspDebugOutput</moteinterface>
      <moteinterface>se.sics.cooja.mspmote.interfaces.SkyTemperature</moteinterface>
    </motetype>
    <mote>
      <breakpoints />
      <interface_config>
        se.sics.cooja.interfaces.Position
        <x>62.86427076032819</x>
        <y>38.98246035522194</y>
        <z>0.0</z>
      </interface_config>
      <interface_config>
        se.sics.cooja.mspmote.interfaces.MspMoteID
        <id>1</id>
      </interface_config>
      <motetype_identifier>sky1</motetype_identifier>
    </mote>
  </simulation>
  <plugin>
    se.sics.cooja.plugins.SimControl
    <width>302</width>
    <z>2</z>
    <height>205</height>
    <location_x>0</location_x>
    <location_y>0</location_y>
    <minimized>false</minimized>
  </plugin>
  <plugin>
    se.sics.cooja.plugins.LogListener
    <plugin_config>
      <filter />
    </plugin_config>
    <width>690</width>
    <z>1</z>
    <height>190</height>
    <location_x>0</location_x>
    <location_y>457</location_y>
    <minimized>false</minimized>
  </plugin>
  <plugin>
    se.sics.cooja.plugins.ScriptRunner
    <plugin_config>
      <script>TIMEOUT(3000, log.log("last message: " + msg + "\n"));

/* Wait until node has booted */
WAIT_UNTIL(msg.startsWith('Starting'));
log.log("Shell started\n");

/* Test command: echo */
log.log("&gt; echo Hello\n");
write(mote, "echo Hello");
WAIT_UNTIL(msg.contains('Hello'));
WAIT_UNTIL(msg.contains('Contiki&gt;'));

/* Test command: help */
log.log("&gt; help\n");
write(mote, "help");
WAIT_UNTIL(msg.startsWith('Available commands:'));
WAIT_UNTIL(msg.contains('Contiki&gt;'));

log.testOK(); /* We are done! */</script>
      <active>true</active>
    </plugin_config>
    <width>600</width>
    <z>0</z>
    <height>648</height>
    <location_x>303</location_x>
    <location_y>0</location_y>
    <minimized>false</minimized>
  </plugin>
</simconf>

