                           Performance Summary Report
                           --------------------------

Design:     WarpSE
Device:     XC95144XL-10-TQ100
Speed File: Version 3.0
Program:    Timing Report Generator:  version P.20131013
Date:       Mon Mar 28 09:28:06 2022

Timing Constraint Summary:

TS_CLK_IOB=PERIOD:CLK_IOB:142.857nS:HIGH:71.428nS                            N/A
TS_CLK_FSB=PERIOD:CLK_FSB:40.000nS:HIGH:20.000nS                             Met
TS_CLK2X_IOB=PERIOD:CLK2X_IOB:66.666nS:HIGH:33.333nS                         Met

Performance Summary:

Pad to Pad (tPD)                          :         11.0ns (1 macrocell levels)
Pad 'A_FSB<11>' to Pad 'RA<1>'                                    

Clock net 'CLK_IOB' path delays:

Setup to Clock at the Pad (tSU)           :          6.5ns (0 macrocell levels)
Data signal 'E_IOB' to DFF D input Pin at 'iobm/Er.D'
Clock pad 'CLK_IOB'                                                       (GCK)

                          Minimum Clock Period: 9.0ns
                     Maximum Internal Clock Speed: 111.1Mhz
                         (Limited by Clock Pulse Width)

Clock net 'CLK_FSB' path delays:

Clock Pad to Output Pad (tCO)             :         14.5ns (2 macrocell levels)
Clock Pad 'CLK_FSB' to Output Pad 'RA<1>'                                 (GCK)

Clock to Setup (tCYC)                     :         20.1ns (2 macrocell levels)
Clock to Q, net 'cs/nOverlay1.Q' to DFF Setup(D) at 'fsb/VPA.D'           (GCK)
Target FF drives output net 'fsb/VPA'

Setup to Clock at the Pad (tSU)           :         16.6ns (1 macrocell levels)
Data signal 'A_FSB<23>' to DFF D input Pin at 'fsb/VPA.D'
Clock pad 'CLK_FSB'                                                       (GCK)

                          Minimum Clock Period: 20.1ns
                     Maximum Internal Clock Speed: 49.7Mhz
                            (Limited by Cycle Time)

Clock net 'CLK2X_IOB' path delays:

Clock Pad to Output Pad (tCO)             :         14.5ns (2 macrocell levels)
Clock Pad 'CLK2X_IOB' to Output Pad 'nVMA_IOB'                            (GCK)

Clock to Setup (tCYC)                     :         11.0ns (1 macrocell levels)
Clock to Q, net 'iobm/IOS_FSM_FFd3.Q' to DFF Setup(D) at 'IOACT.D'        (GCK)
Target FF drives output net 'IOACT'

Setup to Clock at the Pad (tSU)           :          7.5ns (0 macrocell levels)
Data signal 'CLK_IOB' to DFF D input Pin at 'IOACT.D'
Clock pad 'CLK2X_IOB'                                                     (GCK)

                          Minimum Clock Period: 11.0ns
                     Maximum Internal Clock Speed: 90.9Mhz
                            (Limited by Cycle Time)

--------------------------------------------------------------------------------
                            Pad to Pad (tPD) (nsec)

\ From        A     A     A     A     A     A     A     A     A     A     A
 \            _     _     _     _     _     _     _     _     _     _     _
  \           F     F     F     F     F     F     F     F     F     F     F
   \          S     S     S     S     S     S     S     S     S     S     S
    \         B     B     B     B     B     B     B     B     B     B     B
     \        <     <     <     <     <     <     <     <     <     <     <
      \       1     1     1     1     1     1     1     1     1     1     1
       \      0     1     2     3     4     5     6     7     8     9     >
        \     >     >     >     >     >     >     >     >     >     >      
  To     \------------------------------------------------------------------

CLK20EN                                                                    
CLK25EN                                                                    
RA<0>      10.0                                                        10.0
RA<10>                                                                     
RA<11>                                                           10.0      
RA<1>            11.0                                                      
RA<2>                  11.0                                                
RA<3>                        10.0                                          
RA<4>                              11.0                                    
RA<5>                                    11.0                              
RA<6>                                          10.0                        
RA<7>                                                10.0                  
RA<8>                                                      10.0            
RA<9>                                                            10.0      
nBERR_FSB                                                                  
nDinOE                                                                     
nOE                                                                        
nRAMLWE                                                                    
nRAMUWE                                                                    
nRAS                                                                       
nROMCS                                                                     
nROMWE                                                                     
nVPA_FSB                                                                   

--------------------------------------------------------------------------------
                            Pad to Pad (tPD) (nsec)

\ From        A     A     A     A     A     A     A     A     A     A     A
 \            _     _     _     _     _     _     _     _     _     _     _
  \           F     F     F     F     F     F     F     F     F     F     F
   \          S     S     S     S     S     S     S     S     S     S     S
    \         B     B     B     B     B     B     B     B     B     B     B
     \        <     <     <     <     <     <     <     <     <     <     <
      \       2     2     2     2     2     3     4     5     6     7     8
       \      0     1     2     3     >     >     >     >     >     >     >
        \     >     >     >     >                                          
  To     \------------------------------------------------------------------

CLK20EN                                                                    
CLK25EN                                                                    
RA<0>                                                                      
RA<10>           10.0                                                      
RA<11>                                                                     
RA<1>                              11.0                                    
RA<2>                                    11.0                              
RA<3>                                          10.0                        
RA<4>                                                11.0                  
RA<5>                                                      11.0            
RA<6>                                                            10.0      
RA<7>                                                                  10.0
RA<8>            11.0  11.0  11.0                                          
RA<9>      10.0                                                            
nBERR_FSB  11.0  11.0  11.0  11.0                                          
nDinOE     10.0  10.0  10.0  10.0                                          
nOE                                                                        
nRAMLWE                                                                    
nRAMUWE                                                                    
nRAS             11.0  11.0  11.0                                          
nROMCS     11.0  11.0  11.0  11.0                                          
nROMWE                                                                     
nVPA_FSB                                                                   

--------------------------------------------------------------------------------
                            Pad to Pad (tPD) (nsec)

\ From        A     S     S     n     n     n     n
 \            _     W     W     A     L     U     W
  \           F     <     <     S     D     D     E
   \          S     0     1     _     S     S     _
    \         B     >     >     F     _     _     F
     \        <                 S     F     F     S
      \       9                 B     S     S     B
       \      >                       B     B      
        \                                          
  To     \------------------------------------------

CLK20EN          10.0                              
CLK25EN          10.0                              
RA<0>                                              
RA<10>                                             
RA<11>                                             
RA<1>                                              
RA<2>                                              
RA<3>                                              
RA<4>                                              
RA<5>                                              
RA<6>                                              
RA<7>                                              
RA<8>      11.0                                    
RA<9>                                              
nBERR_FSB                    10.0                  
nDinOE                 10.0  10.0              10.0
nOE                          10.0              10.0
nRAMLWE                      10.0  10.0        10.0
nRAMUWE                      11.0        11.0  11.0
nRAS                         11.0                  
nROMCS                 11.0                        
nROMWE                       10.0              10.0
nVPA_FSB                     10.0                  

--------------------------------------------------------------------------------
                      Clock Pad to Output Pad (tCO) (nsec)

\ From         C     C
 \             L     L
  \            K     K
   \           2     _
    \          X     F
     \         _     S
      \        I     B
       \       O      
        \      B      
         \            
  To      \------------

RA<0>             13.5
RA<1>             14.5
RA<2>             14.5
RA<3>             13.5
RA<4>             14.5
RA<5>             14.5
RA<6>             13.5
RA<7>             13.5
RA<8>             14.5
RA<9>             13.5
nADoutLE0   13.5  13.5
nADoutLE1          5.8
nAS_IOB     14.5      
nAoutOE      5.8      
nBERR_FSB         14.5
nBR_IOB            5.8
nCAS               5.8
nDTACK_FSB         5.8
nDinLE       5.8      
nDoutOE      5.8      
nLDS_IOB    14.5      
nRAMLWE           13.5
nRAMUWE           14.5
nRAS              14.5
nROMCS            14.5
nUDS_IOB    14.5      
nVMA_IOB    14.5      
nVPA_FSB          13.5

--------------------------------------------------------------------------------
                   Setup to Clock at Pad (tSU or tSUF) (nsec)

\ From         C     C     C
 \             L     L     L
  \            K     K     K
   \           2     _     _
    \          X     F     I
     \         _     S     O
      \        I     B     B
       \       O            
        \      B            
         \                  
  To      \------------------

A_FSB<10>          7.9      
A_FSB<11>          7.9      
A_FSB<12>          7.9      
A_FSB<13>          7.9      
A_FSB<14>          7.9      
A_FSB<15>          7.9      
A_FSB<16>          7.9      
A_FSB<17>          7.9      
A_FSB<18>          7.9      
A_FSB<19>          7.9      
A_FSB<20>         15.6      
A_FSB<21>         16.6      
A_FSB<22>         16.6      
A_FSB<23>         16.6      
A_FSB<8>           7.9      
A_FSB<9>           7.9      
CLK_IOB      7.5            
E_IOB                    6.5
SW<1>              7.9      
nAS_FSB           15.6      
nBERR_IOB    7.5            
nBG_IOB      6.5            
nDTACK_IOB   6.5            
nIPL2              6.5      
nLDS_FSB           6.5      
nRES         6.5   6.5      
nUDS_FSB           6.5      
nVPA_IOB     6.5            
nWE_FSB            7.9      

--------------------------------------------------------------------------------
                          Clock to Setup (tCYC) (nsec)
                                (Clock: CLK_FSB)

\ From                 B     I     I     I     R     R     R     R     R     T
 \                     E     O     P     P     E     E     E     E     e     i
  \                    R     R     L     L     S     S     S     S     f     m
   \                   R     W     2     2     D     r     r     r     A     e
    \                  _     0     r     r     o     0     1     2     c     o
     \                 I     .     0     1     n     .     .     .     k     u
      \                O     Q     .     .     e     Q     Q     Q     .     t
       \               B           Q     Q     .                       Q     A
        \              S                       Q                             .
         \             .                                                     Q
          \            Q                                                      
           \                                                                  
            \                                                                 
             \                                                                
              \                                                               
               \                                                              
                \                                                             
                 \                                                            
  To              \------------------------------------------------------------

ALE0S.D                                                                       
BERR_IOBS.D         10.0                                                      
IOL0.CE                                                                       
IOL0.D                                                                        
IOREQ.D                                                                       
IORW0.D                   11.4                                                
IOU0.CE                                                                       
IOU0.D                                                                        
IPL2r1.D                        10.0                                          
RESDone.CE                                        10.0  10.0  10.0            
RESr1.D                                           10.0                        
RESr2.D                                                 10.0                  
RefAck.D                                                                      
TimeoutA.D                                                                10.0
TimeoutB.D                                                                    
cnt/RefCnt<1>.D                                                               
cnt/RefCnt<2>.D                                                               
cnt/RefCnt<3>.D                                                               
cnt/RefCnt<4>.D                                                               
cnt/RefCnt<5>.D                                                               
cnt/RefCnt<6>.D                                                               
cnt/RefCnt<7>.D                                                               
cnt/RefDone.D                                                       10.0      
cnt/TimeoutBPre.D                                                             
cs/nOverlay0.D                                                                
cs/nOverlay1.CE                                                               
cs/nOverlay1.D                                                                
fsb/BERR0r.D                                                                  
fsb/BERR1r.D        10.0                                                      
fsb/Ready0r.D                                                                 
fsb/Ready1r.D                                                                 
fsb/Ready2r.D                                                             11.0
fsb/VPA.D           11.4                                                  11.4
iobs/Clear1.D                                                                 
iobs/IOL1.CE                                                                  
iobs/IORW1.D                                                                  
iobs/IOReady.D                                                                
iobs/IOU1.CE                                                                  
iobs/Load1.D                                                                  
iobs/Once.D                                                                   
iobs/PS_FSM_FFd1.D                                                            
iobs/PS_FSM_FFd2.D                                                            
nADoutLE1.D                                                                   
nBR_IOB.CE                      10.0  10.0  10.0  10.0  10.0  10.0            
nCAS.D                                                                        
nDTACK_FSB.D        11.4                                                  11.4
ram/BACTr.D                                                                   
ram/Once.D                                                                    
ram/RAMDIS1.D                                                                 
ram/RAMDIS2.D                                                                 
ram/RAMReady.D                                                                
ram/RASEL.D                                                                   
ram/RS_FSM_FFd1.D                                                             
ram/RS_FSM_FFd2.D                                                             
ram/RS_FSM_FFd3.D                                                             

--------------------------------------------------------------------------------
                          Clock to Setup (tCYC) (nsec)
                                (Clock: CLK_FSB)

\ From                 T     c     c     c     c     c     c     c     c     c
 \                     i     n     n     n     n     n     n     n     n     n
  \                    m     t     t     t     t     t     t     t     t     t
   \                   e     /     /     /     /     /     /     /     /     /
    \                  o     R     R     R     R     R     R     R     R     R
     \                 u     e     e     e     e     e     e     e     e     e
      \                t     f     f     f     f     f     f     f     f     f
       \               B     C     C     C     C     C     C     C     C     D
        \              .     n     n     n     n     n     n     n     n     o
         \             Q     t     t     t     t     t     t     t     t     n
          \                  <     <     <     <     <     <     <     <     e
           \                 0     1     2     3     4     5     6     7     .
            \                >     >     >     >     >     >     >     >     Q
             \               .     .     .     .     .     .     .     .      
              \              Q     Q     Q     Q     Q     Q     Q     Q      
               \                                                              
                \                                                             
                 \                                                            
  To              \------------------------------------------------------------

ALE0S.D                                                                       
BERR_IOBS.D                                                                   
IOL0.CE                                                                       
IOL0.D                                                                        
IOREQ.D                                                                       
IORW0.D                                                                       
IOU0.CE                                                                       
IOU0.D                                                                        
IPL2r1.D                                                                      
RESDone.CE                                                                    
RESr1.D                                                                       
RESr2.D                                                                       
RefAck.D                                                                      
TimeoutA.D                10.0  10.0  10.0  10.0  10.0  10.0  10.0            
TimeoutB.D          10.0  10.0  10.0  10.0  10.0  10.0  10.0  10.0  10.0      
cnt/RefCnt<1>.D           10.0                                                
cnt/RefCnt<2>.D           10.0  10.0                                          
cnt/RefCnt<3>.D           10.0  10.0  10.0                                    
cnt/RefCnt<4>.D           10.0  10.0  10.0  10.0                              
cnt/RefCnt<5>.D           10.0  10.0  10.0  10.0  10.0                        
cnt/RefCnt<6>.D           10.0  10.0  10.0  10.0  10.0  10.0                  
cnt/RefCnt<7>.D           10.0  10.0  10.0  10.0  10.0  10.0  10.0            
cnt/RefDone.D             10.0  10.0  10.0  10.0  10.0  10.0  10.0  10.0  10.0
cnt/TimeoutBPre.D         10.0  10.0  10.0  10.0  10.0  10.0  10.0  10.0      
cs/nOverlay0.D                                                                
cs/nOverlay1.CE                                                               
cs/nOverlay1.D                                                                
fsb/BERR0r.D        10.0                                                      
fsb/BERR1r.D                                                                  
fsb/Ready0r.D                                                                 
fsb/Ready1r.D                                                                 
fsb/Ready2r.D                                                                 
fsb/VPA.D           19.1                                                      
iobs/Clear1.D                                                                 
iobs/IOL1.CE                                                                  
iobs/IORW1.D                                                                  
iobs/IOReady.D                                                                
iobs/IOU1.CE                                                                  
iobs/Load1.D                                                                  
iobs/Once.D                                                                   
iobs/PS_FSM_FFd1.D                                                            
iobs/PS_FSM_FFd2.D                                                            
nADoutLE1.D                                                                   
nBR_IOB.CE                                                                    
nCAS.D                                                                        
nDTACK_FSB.D        19.1                                                      
ram/BACTr.D                                                                   
ram/Once.D                                                                    
ram/RAMDIS1.D                                           11.4  11.4  11.4  11.4
ram/RAMDIS2.D                                           11.0  11.0  11.0  11.0
ram/RAMReady.D                                          11.4  11.4  11.4  11.4
ram/RASEL.D                                             11.4  11.4  11.4  11.4
ram/RS_FSM_FFd1.D                                                             
ram/RS_FSM_FFd2.D                                       11.4  11.4  11.4  11.4
ram/RS_FSM_FFd3.D                                       11.0  11.0  11.0  11.0

--------------------------------------------------------------------------------
                          Clock to Setup (tCYC) (nsec)
                                (Clock: CLK_FSB)

\ From                 c     c     c     f     f     f     f     f     f     f
 \                     n     s     s     s     s     s     s     s     s     s
  \                    t     /     /     b     b     b     b     b     b     b
   \                   /     n     n     /     /     /     /     /     /     /
    \                  T     O     O     A     B     B     R     R     R     V
     \                 i     v     v     S     E     E     e     e     e     P
      \                m     e     e     r     R     R     a     a     a     A
       \               e     r     r     f     R     R     d     d     d     .
        \              o     l     l     .     0     1     y     y     y     Q
         \             u     a     a     Q     r     r     0     1     2      
          \            t     y     y           .     .     r     r     r      
           \           B     0     1           Q     Q     .     .     .      
            \          P     .     .                       Q     Q     Q      
             \         r     Q     Q                                          
              \        e                                                      
               \       .                                                      
                \      Q                                                      
                 \                                                            
  To              \------------------------------------------------------------

ALE0S.D                                                                       
BERR_IOBS.D                           10.0                                    
IOL0.CE                                                                       
IOL0.D                                                                        
IOREQ.D                         11.0  10.0                                    
IORW0.D                         10.0  11.0                                    
IOU0.CE                                                                       
IOU0.D                                                                        
IPL2r1.D                                                                      
RESDone.CE                                                                    
RESr1.D                                                                       
RESr2.D                                                                       
RefAck.D                                                                      
TimeoutA.D                            10.0                                    
TimeoutB.D          10.0              10.0                                    
cnt/RefCnt<1>.D                                                               
cnt/RefCnt<2>.D                                                               
cnt/RefCnt<3>.D                                                               
cnt/RefCnt<4>.D                                                               
cnt/RefCnt<5>.D                                                               
cnt/RefCnt<6>.D                                                               
cnt/RefCnt<7>.D                                                               
cnt/RefDone.D                                                                 
cnt/TimeoutBPre.D   10.0              10.0                                    
cs/nOverlay0.D            10.0        10.0                                    
cs/nOverlay1.CE                       10.0                                    
cs/nOverlay1.D            10.0                                                
fsb/BERR0r.D                          10.0  10.0                              
fsb/BERR1r.D                          10.0        10.0                        
fsb/Ready0r.D                   10.0  10.0              10.0                  
fsb/Ready1r.D                   11.0  10.0                    11.0            
fsb/Ready2r.D                   11.0  11.0                          11.0      
fsb/VPA.D                       20.1  19.1  11.4  11.4  20.1  11.4  11.4  11.4
iobs/Clear1.D                                                                 
iobs/IOL1.CE                                                                  
iobs/IORW1.D                    11.4  11.0                                    
iobs/IOReady.D                        10.0                                    
iobs/IOU1.CE                                                                  
iobs/Load1.D                    11.0  10.0                                    
iobs/Once.D                     11.4  10.0                                    
iobs/PS_FSM_FFd1.D                                                            
iobs/PS_FSM_FFd2.D              11.0  10.0                                    
nADoutLE1.D                                                                   
nBR_IOB.CE                                                                    
nCAS.D                                                                        
nDTACK_FSB.D                    20.1  11.0  11.4  11.4  20.1  11.4  11.4      
ram/BACTr.D                           10.0                                    
ram/Once.D                      10.0  10.0                                    
ram/RAMDIS1.D                   11.4  11.0                                    
ram/RAMDIS2.D                   11.0  11.0                                    
ram/RAMReady.D                  11.0  11.0                                    
ram/RASEL.D                     11.4  11.4                                    
ram/RS_FSM_FFd1.D               10.0  10.0                                    
ram/RS_FSM_FFd2.D               11.4  11.4                                    
ram/RS_FSM_FFd3.D               11.0  11.0                                    

--------------------------------------------------------------------------------
                          Clock to Setup (tCYC) (nsec)
                                (Clock: CLK_FSB)

\ From                 i     i     i     i     i     i     i     i     i     i
 \                     o     o     o     o     o     o     o     o     o     o
  \                    b     b     b     b     b     b     b     b     b     b
   \                   s     s     s     s     s     s     s     s     s     s
    \                  /     /     /     /     /     /     /     /     /     /
     \                 C     I     I     I     I     I     L     O     P     P
      \                l     O     O     O     O     O     o     n     S     S
       \               e     A     L     R     R     U     a     c     _     _
        \              a     C     1     W     e     1     d     e     F     F
         \             r     T     .     1     a     .     1     .     S     S
          \            1     r     Q     .     d     Q     .     Q     M     M
           \           .     .           Q     y           Q           _     _
            \          Q     Q                 .                       F     F
             \                                 Q                       F     F
              \                                                        d     d
               \                                                       1     2
                \                                                      .     .
                 \                                                     Q     Q
  To              \------------------------------------------------------------

ALE0S.D                                                             10.0  10.0
BERR_IOBS.D               10.0                                10.0        10.0
IOL0.CE                                                             10.0  10.0
IOL0.D                          10.0                                          
IOREQ.D                   10.0                                10.0  10.0  11.0
IORW0.D                               11.0                    11.4  11.4  11.4
IOU0.CE                                                             10.0  10.0
IOU0.D                                            10.0                        
IPL2r1.D                                                                      
RESDone.CE                                                                    
RESr1.D                                                                       
RESr2.D                                                                       
RefAck.D                                                                      
TimeoutA.D                                                                    
TimeoutB.D                                                                    
cnt/RefCnt<1>.D                                                               
cnt/RefCnt<2>.D                                                               
cnt/RefCnt<3>.D                                                               
cnt/RefCnt<4>.D                                                               
cnt/RefCnt<5>.D                                                               
cnt/RefCnt<6>.D                                                               
cnt/RefCnt<7>.D                                                               
cnt/RefDone.D                                                                 
cnt/TimeoutBPre.D                                                             
cs/nOverlay0.D                                                                
cs/nOverlay1.CE                                                               
cs/nOverlay1.D                                                                
fsb/BERR0r.D                                                                  
fsb/BERR1r.D                                                                  
fsb/Ready0r.D                                                                 
fsb/Ready1r.D                               11.0                              
fsb/Ready2r.D                                                                 
fsb/VPA.D                                   11.4                              
iobs/Clear1.D                                                       10.0  10.0
iobs/IOL1.CE                                            10.0                  
iobs/IORW1.D                          10.0                    10.0  11.0  11.0
iobs/IOReady.D            10.0              10.0              10.0        10.0
iobs/IOU1.CE                                            10.0                  
iobs/Load1.D                                                  10.0  10.0  10.0
iobs/Once.D                                                   11.4  11.0  10.0
iobs/PS_FSM_FFd1.D        10.0                                      10.0  10.0
iobs/PS_FSM_FFd2.D        10.0                                10.0  11.0  11.0
nADoutLE1.D         10.0                                10.0                  
nBR_IOB.CE                                                                    
nCAS.D                                                                        
nDTACK_FSB.D                                11.4                              
ram/BACTr.D                                                                   
ram/Once.D                                                                    
ram/RAMDIS1.D                                                                 
ram/RAMDIS2.D                                                                 
ram/RAMReady.D                                                                
ram/RASEL.D                                                                   
ram/RS_FSM_FFd1.D                                                             
ram/RS_FSM_FFd2.D                                                             
ram/RS_FSM_FFd3.D                                                             

--------------------------------------------------------------------------------
                          Clock to Setup (tCYC) (nsec)
                                (Clock: CLK_FSB)

\ From                 n     n     n     r     r     r     r     r     r     r
 \                     A     B     D     a     a     a     a     a     a     a
  \                    D     R     T     m     m     m     m     m     m     m
   \                   o     _     A     /     /     /     /     /     /     /
    \                  u     I     C     B     O     R     R     R     R     R
     \                 t     O     K     A     n     A     A     A     S     S
      \                L     B     _     C     c     M     M     S     _     _
       \               E     .     F     T     e     D     R     E     F     F
        \              1     Q     S     r     .     I     e     L     S     S
         \             .           B     .     Q     S     a     .     M     M
          \            Q           .     Q           2     d     Q     _     _
           \                       Q                 .     y           F     F
            \                                        Q     .           F     F
             \                                             Q           d     d
              \                                                        1     2
               \                                                       .     .
                \                                                      Q     Q
                 \                                                            
  To              \------------------------------------------------------------

ALE0S.D                                                                       
BERR_IOBS.D         10.0                                                      
IOL0.CE                                                                       
IOL0.D              10.0                                                      
IOREQ.D             11.0                                                      
IORW0.D             11.4                                                      
IOU0.CE                                                                       
IOU0.D              10.0                                                      
IPL2r1.D                                                                      
RESDone.CE                                                                    
RESr1.D                                                                       
RESr2.D                                                                       
RefAck.D                                                            10.0  10.0
TimeoutA.D                                                                    
TimeoutB.D                                                                    
cnt/RefCnt<1>.D                                                               
cnt/RefCnt<2>.D                                                               
cnt/RefCnt<3>.D                                                               
cnt/RefCnt<4>.D                                                               
cnt/RefCnt<5>.D                                                               
cnt/RefCnt<6>.D                                                               
cnt/RefCnt<7>.D                                                               
cnt/RefDone.D                                                                 
cnt/TimeoutBPre.D                                                             
cs/nOverlay0.D                                                                
cs/nOverlay1.CE                                                               
cs/nOverlay1.D                                                                
fsb/BERR0r.D                                                                  
fsb/BERR1r.D                                                                  
fsb/Ready0r.D                                           10.0                  
fsb/Ready1r.D       11.0                                                      
fsb/Ready2r.D                                                                 
fsb/VPA.D           11.0  11.4                          20.1                  
iobs/Clear1.D       10.0                                                      
iobs/IOL1.CE                                                                  
iobs/IORW1.D        10.0                                                      
iobs/IOReady.D      10.0                                                      
iobs/IOU1.CE                                                                  
iobs/Load1.D        10.0                                                      
iobs/Once.D         11.0                                                      
iobs/PS_FSM_FFd1.D                                                            
iobs/PS_FSM_FFd2.D  11.0                                                      
nADoutLE1.D         10.0                                                      
nBR_IOB.CE                                                                    
nCAS.D                                                        10.0            
nDTACK_FSB.D        11.0  11.4  11.4                    20.1                  
ram/BACTr.D                                                                   
ram/Once.D                                  10.0                    10.0  10.0
ram/RAMDIS1.D                         11.0  11.0                    11.4  11.0
ram/RAMDIS2.D                               11.0  11.0              11.0  11.0
ram/RAMReady.D                        11.0  11.0                    11.0  11.0
ram/RASEL.D                           11.0  11.4                    11.4  11.4
ram/RS_FSM_FFd1.D                           10.0                    10.0  10.0
ram/RS_FSM_FFd2.D                     11.0                          11.4  11.4
ram/RS_FSM_FFd3.D                           10.0                    11.0  11.0

--------------------------------------------------------------------------------
                          Clock to Setup (tCYC) (nsec)
                                (Clock: CLK_FSB)

\ From                 r
 \                     a
  \                    m
   \                   /
    \                  R
     \                 S
      \                _
       \               F
        \              S
         \             M
          \            _
           \           F
            \          F
             \         d
              \        3
               \       .
                \      Q
                 \      
  To              \------

ALE0S.D                 
BERR_IOBS.D             
IOL0.CE                 
IOL0.D                  
IOREQ.D                 
IORW0.D                 
IOU0.CE                 
IOU0.D                  
IPL2r1.D                
RESDone.CE              
RESr1.D                 
RESr2.D                 
RefAck.D                
TimeoutA.D              
TimeoutB.D              
cnt/RefCnt<1>.D         
cnt/RefCnt<2>.D         
cnt/RefCnt<3>.D         
cnt/RefCnt<4>.D         
cnt/RefCnt<5>.D         
cnt/RefCnt<6>.D         
cnt/RefCnt<7>.D         
cnt/RefDone.D           
cnt/TimeoutBPre.D       
cs/nOverlay0.D          
cs/nOverlay1.CE         
cs/nOverlay1.D          
fsb/BERR0r.D            
fsb/BERR1r.D            
fsb/Ready0r.D           
fsb/Ready1r.D           
fsb/Ready2r.D           
fsb/VPA.D               
iobs/Clear1.D           
iobs/IOL1.CE            
iobs/IORW1.D            
iobs/IOReady.D          
iobs/IOU1.CE            
iobs/Load1.D            
iobs/Once.D             
iobs/PS_FSM_FFd1.D      
iobs/PS_FSM_FFd2.D      
nADoutLE1.D             
nBR_IOB.CE              
nCAS.D                  
nDTACK_FSB.D            
ram/BACTr.D             
ram/Once.D          10.0
ram/RAMDIS1.D       11.0
ram/RAMDIS2.D       11.0
ram/RAMReady.D      11.0
ram/RASEL.D         11.0
ram/RS_FSM_FFd1.D   10.0
ram/RS_FSM_FFd2.D   11.4
ram/RS_FSM_FFd3.D   11.0

--------------------------------------------------------------------------------
                          Clock to Setup (tCYC) (nsec)
                               (Clock: CLK2X_IOB)

\ From                  I     I     i     i     i     i     i     i     i     i
 \                      O     O     o     o     o     o     o     o     o     o
  \                     A     B     b     b     b     b     b     b     b     b
   \                    C     E     m     m     m     m     m     m     m     m
    \                   T     R     /     /     /     /     /     /     /     /
     \                  .     R     B     B     B     B     D     D     E     E
      \                 Q     .     E     E     G     G     T     T     S     S
       \                      Q     R     R     r     r     A     A     <     <
        \                           R     R     0     1     C     C     0     1
         \                          r     r     .     .     K     K     >     >
          \                         f     r     Q     Q     r     r     .     .
           \                        .     .                 f     r     Q     Q
            \                       Q     Q                 .     .            
             \                                              Q     Q            
              \                                                                
               \                                                               
                \                                                              
                 \                                                             
                  \                                                            
  To               \------------------------------------------------------------

ALE0M.D                                                                        
IOACT.D                          10.0  10.0              11.0  11.0            
IOBERR.D                   11.0  11.0  11.0              11.0  11.0            
iobm/BGr1.D                                  10.0                              
iobm/ES<0>.D                                                         10.0  10.0
iobm/ES<1>.D                                                         10.0  10.0
iobm/ES<2>.D                                                         10.0  10.0
iobm/ES<3>.D                                                         10.0  10.0
iobm/ES<4>.D                                                         10.0  10.0
iobm/ETACK.D                                                         10.0  10.0
iobm/IOS_FSM_FFd1.D                                                            
iobm/IOS_FSM_FFd2.D              10.0  10.0              10.0  10.0            
iobm/IOS_FSM_FFd3.D                                                            
nAS_IOB.D                                                                      
nAoutOE.D                                    10.0  10.0                        
nDinLE.D                                                                       
nDoutOE.D                                                                      
nLDS_IOB.D                                                                     
nUDS_IOB.D                                                                     
nVMA_IOB.D           10.0                                            10.0  10.0

--------------------------------------------------------------------------------
                          Clock to Setup (tCYC) (nsec)
                               (Clock: CLK2X_IOB)

\ From                  i     i     i     i     i     i     i     i     i     i
 \                      o     o     o     o     o     o     o     o     o     o
  \                     b     b     b     b     b     b     b     b     b     b
   \                    m     m     m     m     m     m     m     m     m     m
    \                   /     /     /     /     /     /     /     /     /     /
     \                  E     E     E     E     E     I     I     I     I     R
      \                 S     S     S     T     r     O     O     O     O     E
       \                <     <     <     A     2     R     S     S     S     S
        \               2     3     4     C     .     E     _     _     _     r
         \              >     >     >     K     Q     Q     F     F     F     f
          \             .     .     .     .           r     S     S     S     .
           \            Q     Q     Q     Q           .     M     M     M     Q
            \                                         Q     _     _     _      
             \                                              F     F     F      
              \                                             F     F     F      
               \                                            d     d     d      
                \                                           1     2     3      
                 \                                          .     .     .      
                  \                                         Q     Q     Q      
  To               \------------------------------------------------------------

ALE0M.D                                            10.0  10.0  10.0  10.0      
IOACT.D                                10.0        10.0  11.0  10.0  11.0  11.0
IOBERR.D                               10.0              11.0  11.0  11.0  11.0
iobm/BGr1.D                                                                    
iobm/ES<0>.D         10.0  10.0  10.0        10.0                              
iobm/ES<1>.D                                 10.0                              
iobm/ES<2>.D         10.0  10.0  10.0        10.0                              
iobm/ES<3>.D         10.0  10.0              10.0                              
iobm/ES<4>.D         10.0  10.0  10.0        10.0                              
iobm/ETACK.D         10.0  10.0  10.0                                          
iobm/IOS_FSM_FFd1.D                                      10.0  10.0  10.0      
iobm/IOS_FSM_FFd2.D                    10.0              10.0  10.0  10.0  10.0
iobm/IOS_FSM_FFd3.D                                10.0  10.0  10.0  10.0      
nAS_IOB.D                                                10.0  10.0  10.0      
nAoutOE.D                                                                      
nDinLE.D                                                 10.0  10.0            
nDoutOE.D                                                      10.0  10.0      
nLDS_IOB.D                                               10.0  10.0  10.0      
nUDS_IOB.D                                               10.0  10.0  10.0      
nVMA_IOB.D           10.0  10.0  10.0                                          

--------------------------------------------------------------------------------
                          Clock to Setup (tCYC) (nsec)
                               (Clock: CLK2X_IOB)

\ From                  i     i     i     n     n     n
 \                      o     o     o     A     A     V
  \                     b     b     b     S     o     M
   \                    m     m     m     _     u     A
    \                   /     /     /     I     t     _
     \                  R     V     V     O     O     I
      \                 E     P     P     B     E     O
       \                S     A     A     .     .     B
        \               r     r     r     Q     Q     .
         \              r     f     r                 Q
          \             .     .     .                  
           \            Q     Q     Q                  
            \                                          
             \                                         
              \                                        
               \                                       
                \                                      
                 \                                     
                  \                                    
  To               \------------------------------------

ALE0M.D                                      10.0      
IOACT.D              11.0                    10.0      
IOBERR.D             11.0                              
iobm/BGr1.D                                            
iobm/ES<0>.D                                           
iobm/ES<1>.D                                           
iobm/ES<2>.D                                           
iobm/ES<3>.D                                           
iobm/ES<4>.D                                           
iobm/ETACK.D                                       10.0
iobm/IOS_FSM_FFd1.D                                    
iobm/IOS_FSM_FFd2.D  10.0                              
iobm/IOS_FSM_FFd3.D                          10.0      
nAS_IOB.D                                              
nAoutOE.D                              10.0  10.0      
nDinLE.D                                               
nDoutOE.D                                              
nLDS_IOB.D                                             
nUDS_IOB.D                                             
nVMA_IOB.D                 10.0  10.0              10.0

Path Type Definition: 

Pad to Pad (tPD) -                        Reports pad to pad paths that start 
                                          at input pads and end at output pads. 
                                          Paths are not traced through 
                                          registers. 

Clock Pad to Output Pad (tCO) -           Reports paths that start at input 
                                          pads trace through clock inputs of 
                                          registers and end at output pads. 
                                          Paths are not traced through PRE/CLR 
                                          inputs of registers. 

Setup to Clock at Pad (tSU or tSUF) -     Reports external setup time of data 
                                          to clock at pad. Data path starts at 
                                          an input pad and ends at register 
                                          (Fast Input Register for tSUF) D/T 
                                          input. Clock path starts at input pad 
                                          and ends at the register clock input. 
                                          Paths are not traced through 
                                          registers. Pin-to-pin setup 
                                          requirement is not reported or 
                                          guaranteed for product-term clocks 
                                          derived from macrocell feedback 
                                          signals. 

Clock to Setup (tCYC) -                   Register to register cycle time. 
                                          Include source register tCO and 
                                          destination register tSU. Note that 
                                          when the computed Maximum Clock Speed 
                                          is limited by tCYC it is computed 
                                          assuming that all registers are 
                                          rising-edge sensitive. 

