### Errors and Warnings

There are 0 error(s), 2 warning(s), and 0 information.

[Warning]:Cpld - Unable to retrieve the path to the iSE Project Repository. Will use the default filename of 'WarpSE.ise'.INFO:Cpld - Inferring BUFG constraint for signal 'CLK2X_IOB' based upon the LOC constraint 'P22'. It is recommended that you declare this BUFG explicitedly in your design. Note that for certain device families the output of a BUFG constraint can not drive a gated clock, and the BUFG constraint will be ignored.INFO:Cpld - Inferring BUFG constraint for signal 'CLK_FSB' based upon the LOC constraint 'P27'. It is recommended that you declare this BUFG explicitedly in your design. Note that for certain device families the output of a BUFG constraint can not drive a gated clock, and the BUFG constraint will be ignored.INFO:Cpld - Inferring BUFG constraint for signal 'CLK_IOB' based upon the LOC constraint 'P23'. It is recommended that you declare this BUFG explicitedly in your design. Note that for certain device families the output of a BUFG constraint can not drive a gated clock, and the BUFG constraint will be ignored.

[Warning]:Cpld:1007 - Removing unused input(s) 'SW<2>'. The input(s) are unused after optimization. Please verify functionality via simulation.